(kicad_pcb (version 20171130) (host pcbnew 5.1.6+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 37)
    (tracks 31)
    (zones 0)
    (modules 19)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.635)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2 2.2)
    (pad_drill 1.1)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 inputVOX)
  (net 3 GNDS)
  (net 4 "Net-(C2-Pad1)")
  (net 5 micHT)
  (net 6 PTT)
  (net 7 miccomp)
  (net 8 audiocomp)
  (net 9 gndcomp)
  (net 10 speakerHT)
  (net 11 "Net-(J3-PadT)")
  (net 12 "Net-(Q1-Pad2)")
  (net 13 "Net-(C4-Pad1)")
  (net 14 "Net-(J1-PadR1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.635)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GNDS)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J1-PadR1)")
    (add_net "Net-(J3-PadT)")
    (add_net "Net-(Q1-Pad2)")
    (add_net PTT)
    (add_net audiocomp)
    (add_net gndcomp)
    (add_net inputVOX)
    (add_net micHT)
    (add_net miccomp)
    (add_net speakerHT)
  )
  (module Symbol:OSHW-Logo_5.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 79.375 33.02)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 79.756 49.784 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at -2.794 1.016) (layer F.SilkS))
    (fp_text value 10u (at 1 3.75 90) (layer F.Fab))
    (fp_text user %R (at 1 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 miccomp))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 100.965 37.465)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 1.2k (at 7.62 -2.54) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GNDS))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 111.76 31.75 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GNDS))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 PTT))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 12 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 116.205 57.912)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 116.84 25.4)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 79.248 57.912)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 79.248 25.4)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 95.885 41.91 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 3.175 3.175) (layer F.SilkS))
    (fp_text value 10u (at 1 3.75) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 inputVOX))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 111.76 51.435 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at 4.445 0 180) (layer F.SilkS))
    (fp_text value 10u (at 1 3.75 90) (layer F.Fab))
    (fp_text user %R (at 1 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GNDS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm placed (layer F.Cu) (tedit 5AE50EF0)
    (at 110.49 26.67 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C3 (at 3.175 -3.175 90) (layer F.SilkS))
    (fp_text value 10u (at 1 3.75 90) (layer F.Fab))
    (fp_text user %R (at 1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 micHT))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 inputVOX))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal placed (layer F.Cu) (tedit 5AE50CD5)
    (at 100.965 41.91)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at -2.19 0 270) (layer F.SilkS))
    (fp_text value 1N5817 (at 5.08 2.47) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.SilkS))
    (fp_text user K (at 0 -2.1) (layer F.Fab))
    (fp_text user %R (at 5.47 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GNDS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal placed (layer F.Cu) (tedit 5AE50CD5)
    (at 111.125 45.72 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 12.7 0 90) (layer F.SilkS))
    (fp_text value 1N5817 (at 5.08 2.47) (layer F.Fab))
    (fp_text user %R (at 5.47 0) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digital_interface:Jack_3.5mm_PJ320A_Horizontal_CircularHoles (layer F.Cu) (tedit 600457FC)
    (at 86.995 39.37)
    (descr "TRRS headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320A-175.html)")
    (tags "3.5mm jack mic microphone phones headphones 4pins audio plug trrs")
    (fp_text reference J1 (at -4.8 -2.2) (layer F.SilkS))
    (fp_text value Computer (at -4.1 7.6) (layer F.Fab))
    (fp_text user %R (at -4.9 2.3) (layer F.Fab))
    (pad S thru_hole circle (at 1.1 4.6 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 13 "Net-(C4-Pad1)"))
    (pad T thru_hole rect (at 0 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 8 audiocomp))
    (pad R1 thru_hole circle (at -4 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-PadR1)"))
    (pad R2 thru_hole circle (at -7 0 180) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 9 gndcomp))
    (pad "" np_thru_hole circle (at -8.6 2.3 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.6 2.3 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320A_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digital_interface:Jack_3.5mm_PJ320A_Horizontal_CircularHoles (layer F.Cu) (tedit 600457FC)
    (at 105.029 32.893 270)
    (descr "TRRS headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320A-175.html)")
    (tags "3.5mm jack mic microphone phones headphones 4pins audio plug trrs")
    (fp_text reference J3 (at -4.445 6.223 90) (layer F.SilkS))
    (fp_text value "HT Out" (at -4.1 7.6 90) (layer F.Fab))
    (fp_text user %R (at -4.9 2.3 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.6 2.3 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -8.6 2.3 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad R2 thru_hole circle (at -7 0 90) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 6 PTT))
    (pad R1 thru_hole circle (at -4 0 90) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 5 micHT))
    (pad T thru_hole rect (at 0 0 90) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-PadT)"))
    (pad S thru_hole circle (at 1.1 4.6 90) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 6 PTT))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320A_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal placed (layer F.Cu) (tedit 5AE5139B)
    (at 114.3 37.465 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.905 0) (layer F.SilkS))
    (fp_text value 1.2k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digital_interface:Transformer_EI14 placed (layer F.Cu) (tedit 60062BDC)
    (at 84.836 50.8)
    (descr "EI14 Audio Transformer")
    (tags "Audio Transformer")
    (fp_text reference T1 (at 6 -5.2) (layer F.SilkS))
    (fp_text value 600:600 (at 6 10.5 180) (layer F.Fab))
    (fp_text user %R (at 6 2.5) (layer F.Fab))
    (pad 4 thru_hole circle (at 11 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 speakerHT))
    (pad 3 thru_hole circle (at 11 5) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 GNDS))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 miccomp))
    (pad 2 thru_hole circle (at 0 5) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 gndcomp))
    (model ${KISYS3DMOD}/Transformer_THT.3dshapes/Transformer_EI14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digital_interface:Transformer_EI14 placed (layer F.Cu) (tedit 6003A871)
    (at 84.836 27.432)
    (descr "EI14 Audio Transformer")
    (tags "Audio Transformer")
    (fp_text reference T2 (at 6 -5.2) (layer F.SilkS))
    (fp_text value 600:600 (at 6 10.5 180) (layer F.Fab))
    (fp_text user %R (at 6 2.5) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 5) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 gndcomp))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 8 audiocomp))
    (pad 3 thru_hole circle (at 11 5) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 GNDS))
    (pad 4 thru_hole circle (at 11 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 inputVOX))
    (model ${KISYS3DMOD}/Transformer_THT.3dshapes/Transformer_EI14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digital_interface:Jack_3.5mm_PJ320A_Horizontal_CircularHoles (layer F.Cu) (tedit 600457FC)
    (at 100.711 50.292 90)
    (descr "TRRS headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320A-175.html)")
    (tags "3.5mm jack mic microphone phones headphones 4pins audio plug trrs")
    (fp_text reference J2 (at -4.318 -2.286 90) (layer F.SilkS))
    (fp_text value "HT In" (at -4.1 7.6 90) (layer F.Fab))
    (fp_text user %R (at -4.9 2.3 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.6 2.3 270) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -8.6 2.3 270) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad R2 thru_hole circle (at -7 0 270) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 3 GNDS))
    (pad R1 thru_hole circle (at -4 0 270) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 3 GNDS))
    (pad T thru_hole rect (at 0 0 270) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 10 speakerHT))
    (pad S thru_hole circle (at 1.1 4.6 270) (size 2.55 2.55) (drill 1.55) (layers *.Cu *.Mask)
      (net 3 GNDS))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_PJ320A_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 40.005 (width 0.15) (layer Dwgs.User)
    (gr_text "1.5750 in" (at 48.23 41.5925 90) (layer Dwgs.User))
    (feature1 (pts (xy 75.565 21.59) (xy 48.943579 21.59)))
    (feature2 (pts (xy 75.565 61.595) (xy 48.943579 61.595)))
    (crossbar (pts (xy 49.53 61.595) (xy 49.53 21.59)))
    (arrow1a (pts (xy 49.53 21.59) (xy 50.116421 22.716504)))
    (arrow1b (pts (xy 49.53 21.59) (xy 48.943579 22.716504)))
    (arrow2a (pts (xy 49.53 61.595) (xy 50.116421 60.468496)))
    (arrow2b (pts (xy 49.53 61.595) (xy 48.943579 60.468496)))
  )
  (dimension 45.085 (width 0.15) (layer Dwgs.User)
    (gr_text "1.7750 in" (at 98.1075 71.920045) (layer Dwgs.User))
    (feature1 (pts (xy 75.565 61.595) (xy 75.565 71.206466)))
    (feature2 (pts (xy 120.65 61.595) (xy 120.65 71.206466)))
    (crossbar (pts (xy 120.65 70.620045) (xy 75.565 70.620045)))
    (arrow1a (pts (xy 75.565 70.620045) (xy 76.691504 70.033624)))
    (arrow1b (pts (xy 75.565 70.620045) (xy 76.691504 71.206466)))
    (arrow2a (pts (xy 120.65 70.620045) (xy 119.523496 70.033624)))
    (arrow2b (pts (xy 120.65 70.620045) (xy 119.523496 71.206466)))
  )
  (gr_text "XCVR Mic" (at 107.95 29.21 90) (layer B.SilkS))
  (gr_text PTT (at 100.457 28.829 90) (layer B.SilkS))
  (gr_text "XCVR gnd" (at 105.41 54.991 90) (layer B.SilkS))
  (gr_text "XCVR Speaker" (at 97.917 50.038 90) (layer B.SilkS))
  (gr_text "CPU gnd" (at 79.883 33.782 270) (layer B.SilkS))
  (gr_text "CPU Speaker" (at 90.17 35.56 270) (layer B.SilkS))
  (gr_text "CPU Mic" (at 90.932 46.355 270) (layer B.SilkS))
  (gr_text "DigiVox v0.1\nKD9PDP\nTAPR OHL\n" (at 118.11 41.91 270) (layer F.SilkS))
  (gr_line (start 120.65 21.59) (end 75.565 21.59) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.65 61.595) (end 120.65 21.59) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 75.565 61.595) (end 120.65 61.595) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 75.565 21.59) (end 75.565 61.595) (layer Edge.Cuts) (width 0.05))
  (zone (net 9) (net_name gndcomp) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.932 58.42) (xy 76.962 58.42) (xy 76.962 26.035) (xy 90.932 26.035)
      )
    )
  )
  (zone (net 3) (net_name GNDS) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.205 61.0235) (xy 93.345 60.96) (xy 93.345 22.225) (xy 116.205 22.2885)
      )
    )
  )
)
