(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 96)
    (no_connects 0)
    (area 68.5926 98 159.295258 153.2774)
    (thickness 1.6)
    (drawings 22)
    (tracks 220)
    (zones 0)
    (modules 32)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.3)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 /VOL_ADC)
  (net 4 "Net-(C6-Pad1)")
  (net 5 "Net-(C7-Pad1)")
  (net 6 /DAC_L)
  (net 7 "Net-(C8-Pad1)")
  (net 8 /DAC_R)
  (net 9 "Net-(C9-Pad1)")
  (net 10 "Net-(C9-Pad2)")
  (net 11 "Net-(C10-Pad1)")
  (net 12 "Net-(C10-Pad2)")
  (net 13 "Net-(J2-Pad3)")
  (net 14 /TIP_SW)
  (net 15 "Net-(J3-Pad2)")
  (net 16 "Net-(J4-Pad1)")
  (net 17 "Net-(J4-Pad2)")
  (net 18 +3V3)
  (net 19 "Net-(J5-Pad2)")
  (net 20 "Net-(J6-Pad1)")
  (net 21 "Net-(J6-Pad2)")
  (net 22 "Net-(R2-Pad1)")
  (net 23 "Net-(R6-Pad2)")
  (net 24 /~SHUTDOWN)
  (net 25 /MUTE)
  (net 26 "Net-(U2-Pad14)")
  (net 27 "Net-(U2-Pad17)")
  (net 28 "Net-(U2-Pad37)")
  (net 29 "Net-(U2-Pad38)")
  (net 30 "Net-(U2-Pad39)")
  (net 31 "Net-(U2-Pad40)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /DAC_L)
    (add_net /DAC_R)
    (add_net /MUTE)
    (add_net /TIP_SW)
    (add_net /VOL_ADC)
    (add_net /~SHUTDOWN)
    (add_net GND)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad38)")
    (add_net "Net-(U2-Pad39)")
    (add_net "Net-(U2-Pad40)")
    (add_net VDD)
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.1)
  )
  (net_class Speaker ""
    (clearance 0.1524)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.1)
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad2)")
  )
  (module Capacitors_SMD:C_0603 placed (layer F.Cu) (tedit 59F911CC)
    (at 113 146 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 10µF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 placed (layer F.Cu) (tedit 59F91368)
    (at 126.3 120.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 placed (layer F.Cu) (tedit 59F9135C)
    (at 123.7 120.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 placed (layer F.Cu) (tedit 59F91361)
    (at 129.6 125)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module audio-repair:C_0603_TH placed (layer F.Cu) (tedit 59F737C3)
    (at 118.5 132.05)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 6.5 -0.05) (layer F.SilkS))
    (fp_text value 10nF (at 2 1.9) (layer F.Fab))
    (pad 1 smd rect (at 1.25 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /VOL_ADC))
    (pad 2 smd rect (at 2.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 /VOL_ADC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0.0787402 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 placed (layer F.Cu) (tedit 59F91259)
    (at 120.4 125.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 1µF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module audio-repair:C_0603_TH placed (layer F.Cu) (tedit 59F9132C)
    (at 115.95 127.54 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 2 -1.9 180) (layer F.SilkS))
    (fp_text value 220nF (at 2 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at 1.25 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 2.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 /DAC_L))
    (pad 2 thru_hole circle (at 4 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 /DAC_L))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0.0787402 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module audio-repair:C_0603_TH placed (layer F.Cu) (tedit 59F91322)
    (at 115.95 125 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 2 1.9 180) (layer F.SilkS))
    (fp_text value 220nF (at 2 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at 1.25 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 2.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /DAC_R))
    (pad 2 thru_hole circle (at 4 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 /DAC_R))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0.0787402 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 placed (layer F.Cu) (tedit 59F9111F)
    (at 137.6 122)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C9 (at 0 -2.7) (layer F.SilkS) hide)
    (fp_text value 220µF (at 0 2.7) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 placed (layer F.Cu) (tedit 59F91119)
    (at 137.6 104)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C10 (at 0 -2.7) (layer F.SilkS) hide)
    (fp_text value 220µF (at 0 2.7) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm placed (layer F.Cu) (tedit 59FA1364)
    (at 108.89 144.78)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference "Ext Pwr" (at 2.61 1.22 90) (layer F.SilkS))
    (fp_text value "Ext. Power" (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module audio-repair:Switchcraft_35RAPC4BHN3 placed (layer F.Cu) (tedit 59F9108F)
    (at 150 113 180)
    (fp_text reference J2 (at 2.5 7 180) (layer F.SilkS) hide)
    (fp_text value Switchcraft_35RAPC4BHN3 (at 10 -7 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 2 0 180) (size 1.5 1.9) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole rect (at 9.8 -5.2 180) (size 1.9 1.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad2)"))
    (pad 3 thru_hole rect (at 8.4 -2.5 180) (size 1.9 1.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad3)"))
    (pad 4 thru_hole rect (at 13 4 180) (size 1.5 1.9) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 /TIP_SW))
    (pad 5 thru_hole rect (at 5.4 4.5 180) (size 1.9 1.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(C9-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm placed (layer F.Cu) (tedit 59F90F31)
    (at 108.89 104.68)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value PL (at 0 7.41) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm placed (layer F.Cu) (tedit 59F91103)
    (at 119.05 104.68)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value UVP (at 0 7.41) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module audio-repair:R_0603_TH placed (layer F.Cu) (tedit 59F912B2)
    (at 129.4 137.6 90)
    (fp_text reference R1 (at 2 -1.5 90) (layer F.SilkS))
    (fp_text value 100K (at 2 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at 1.25 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 2.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 /TIP_SW))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole circle (at 4 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 /TIP_SW))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0.07874015748031496 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module audio-repair:R_0603_TH placed (layer F.Cu) (tedit 59F737FF)
    (at 122.5 138.025 180)
    (fp_text reference R2 (at -2.5 0.025 180) (layer F.SilkS))
    (fp_text value 680K (at 2 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at 1.25 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 2.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /VOL_ADC))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 4 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 /VOL_ADC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0.07874015748031496 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module audio-repair:R_0603_TH placed (layer F.Cu) (tedit 59F737FF)
    (at 118.5 135.025)
    (fp_text reference R3 (at 6.5 -0.025) (layer F.SilkS))
    (fp_text value 1M (at 2 -1.5) (layer F.Fab))
    (pad 1 smd rect (at 1.25 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /VOL_ADC))
    (pad 2 smd rect (at 2.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 /VOL_ADC))
    (pad 2 thru_hole circle (at 4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0.07874015748031496 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module audio-repair:R_0603_TH placed (layer F.Cu) (tedit 59F737FF)
    (at 121.59 107.22)
    (fp_text reference R6 (at 6.41 -0.02) (layer F.SilkS))
    (fp_text value 100K (at 2 -1.5) (layer F.Fab))
    (pad 1 smd rect (at 1.25 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J5-Pad2)"))
    (pad 2 smd rect (at 2.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(J5-Pad2)"))
    (pad 2 thru_hole circle (at 4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0.07874 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module audio-repair:Potentiometer_Bourns_3352T placed (layer F.Cu) (tedit 59F9115B)
    (at 122.5 146.75 180)
    (fp_text reference RV1 (at 0 6 180) (layer F.SilkS) hide)
    (fp_text value 50K (at 0 -5.5 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 2.875 180) (size 1.1 1.1) (drill 0.55) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 2.875 180) (size 1.1 1.1) (drill 0.55) (layers *.Cu *.Mask)
      (net 22 "Net-(R2-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 2.875 180) (size 1.1 1.1) (drill 0.55) (layers *.Cu *.Mask)
      (net 1 VDD))
  )
  (module audio-repair:QFN-20-1EP_4x4mm_Pitch0.5mm placed (layer F.Cu) (tedit 59F910A6)
    (at 125 125)
    (descr "20-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -3.33) (layer F.SilkS) hide)
    (fp_text value PAM8019KGR (at 0 3.33) (layer F.Fab))
    (pad 1 smd oval (at -1.965 -1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J6-Pad2)"))
    (pad 2 smd oval (at -1.965 -0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad1)"))
    (pad 3 smd oval (at -1.965 0) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /~SHUTDOWN))
    (pad 4 smd oval (at -1.965 0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 5 smd oval (at -1.965 1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C8-Pad1)"))
    (pad 6 smd oval (at -1 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd oval (at -0.5 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 8 smd oval (at 0 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R2-Pad1)"))
    (pad 9 smd oval (at 0.5 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /MUTE))
    (pad 10 smd oval (at 1 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /TIP_SW))
    (pad 11 smd oval (at 1.965 1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J3-Pad2)"))
    (pad 12 smd oval (at 1.965 0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R6-Pad2)"))
    (pad 13 smd oval (at 1.965 0) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 14 smd oval (at 1.965 -0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 15 smd oval (at 1.965 -1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J4-Pad2)"))
    (pad 16 smd oval (at 1 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 17 smd oval (at 0.5 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J4-Pad1)"))
    (pad 18 smd oval (at 0 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd oval (at -0.5 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J6-Pad1)"))
    (pad 20 smd oval (at -1 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 21 smd rect (at 0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.18) (zone_connect 2))
    (pad 21 smd rect (at 0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.18) (zone_connect 2))
    (pad 21 smd rect (at -0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.18) (zone_connect 2))
    (pad 21 smd rect (at -0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.18) (zone_connect 2))
    (pad 21 thru_hole circle (at 0 0) (size 0.3 0.3) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 21 thru_hole circle (at -0.625 -0.625) (size 0.3 0.3) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 21 thru_hole circle (at 0.625 -0.625) (size 0.3 0.3) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 21 thru_hole circle (at 0.625 0.625) (size 0.3 0.3) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 21 thru_hole circle (at -0.625 0.625) (size 0.3 0.3) (drill 0.254) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module audio-repair:1bitsy-stub placed (layer F.Cu) (tedit 59F91098)
    (at 73.33 132.62 90)
    (fp_text reference U2 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value 1bitsy-basic-stubby (at 0 -2.54 90) (layer F.Fab))
    (pad 12 thru_hole circle (at 0 27.94) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 0 30.48) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 0 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(U2-Pad14)"))
    (pad 15 thru_hole circle (at 0 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 +3V3))
    (pad 16 thru_hole circle (at 15.24 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 17 thru_hole circle (at 15.24 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(U2-Pad17)"))
    (pad 18 thru_hole circle (at 15.24 30.48) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 15.24 27.94) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at 2.54 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /TIP_SW))
    (pad 32 thru_hole circle (at 2.54 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /VOL_ADC))
    (pad 33 thru_hole circle (at 5.08 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /MUTE))
    (pad 34 thru_hole circle (at 5.08 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /~SHUTDOWN))
    (pad 35 thru_hole circle (at 7.62 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /DAC_L))
    (pad 36 thru_hole circle (at 7.62 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /DAC_R))
    (pad 37 thru_hole circle (at 10.16 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(U2-Pad37)"))
    (pad 38 thru_hole circle (at 10.16 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(U2-Pad38)"))
    (pad 39 thru_hole circle (at 12.7 33.02) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(U2-Pad39)"))
    (pad 40 thru_hole circle (at 12.7 35.56) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(U2-Pad40)"))
    (pad 42 thru_hole circle (at 2.54 27.94) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 43 thru_hole circle (at 2.54 30.48) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 44 thru_hole circle (at 12.7 30.48) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module audio-repair:TerminalBlock_TE_2834016_2 placed (layer F.Cu) (tedit 59F914D0)
    (at 148 138.5 90)
    (fp_text reference Left (at -3.4 -15.3 90) (layer F.SilkS))
    (fp_text value Speaker (at -2.54 -14.6 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -4.18 -10.6 90) (size 2 2.3) (drill 1.15) (layers *.Cu *.Mask)
      (net 16 "Net-(J4-Pad1)"))
    (pad 1 thru_hole oval (at -4.18 -5.52 90) (size 2 2.3) (drill 1.15) (layers *.Cu *.Mask)
      (net 16 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at -1.64 -10.6 90) (size 2 2.3) (drill 1.15) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad2)"))
    (pad 2 thru_hole oval (at -1.64 -5.52 90) (size 2 2.3) (drill 1.15) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad2)"))
  )
  (module audio-repair:TerminalBlock_TE_2834016_2 placed (layer F.Cu) (tedit 59F914FB)
    (at 148.02 129.46 90)
    (fp_text reference Right (at -2.54 -15.32 90) (layer F.SilkS))
    (fp_text value Speaker (at -2.54 -14.6 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -4.18 -10.6 90) (size 2 2.3) (drill 1.15) (layers *.Cu *.Mask)
      (net 20 "Net-(J6-Pad1)"))
    (pad 1 thru_hole oval (at -4.18 -5.52 90) (size 2 2.3) (drill 1.15) (layers *.Cu *.Mask)
      (net 20 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at -1.64 -10.6 90) (size 2 2.3) (drill 1.15) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-Pad2)"))
    (pad 2 thru_hole oval (at -1.64 -5.52 90) (size 2 2.3) (drill 1.15) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-Pad2)"))
  )
  (module audio-repair:R_0603_TH_unpop (layer F.Cu) (tedit 59F907E0)
    (at 111.43 104.68)
    (fp_text reference R4 (at 2 1.5) (layer F.SilkS))
    (fp_text value TBD (at 2 -1.5) (layer F.Fab))
    (pad 1 smd rect (at 1.25 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 2.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 15 "Net-(J3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole circle (at 4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(J3-Pad2)"))
  )
  (module audio-repair:R_0603_TH_unpop (layer F.Cu) (tedit 59F910FB)
    (at 115.43 109.76 180)
    (fp_text reference R5 (at 2 1.5 180) (layer F.SilkS))
    (fp_text value TBD (at 2 1.5 180) (layer F.Fab))
    (pad 1 smd rect (at 1.25 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 15 "Net-(J3-Pad2)"))
    (pad 2 smd rect (at 2.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(J3-Pad2)"))
    (pad 2 thru_hole circle (at 4 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module audio-repair:R_0603_TH_unpop (layer F.Cu) (tedit 59F907E0)
    (at 121.59 104.68)
    (fp_text reference R7 (at 6.41 0.02) (layer F.SilkS))
    (fp_text value TBD (at 2 -1.5) (layer F.Fab))
    (pad 1 smd rect (at 1.25 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 2.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 19 "Net-(J5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 +3V3))
    (pad 2 thru_hole circle (at 4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(J5-Pad2)"))
  )
  (module audio-repair:R_0603_TH_unpop (layer F.Cu) (tedit 59F91057)
    (at 125.59 109.76 180)
    (fp_text reference R8 (at -2.41 -0.04 180) (layer F.SilkS))
    (fp_text value TBD (at 2 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at 1.25 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 19 "Net-(J5-Pad2)"))
    (pad 2 smd rect (at 2.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(J5-Pad2)"))
    (pad 2 thru_hole circle (at 4 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module audio-repair:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 59F9DBB0)
    (at 103.5 103.5)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  )
  (module audio-repair:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 59F9DB9E)
    (at 103.5 146.5)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  )
  (module audio-repair:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 59F9DBA4)
    (at 146.5 146.5)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  )
  (module audio-repair:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 59F9DBAA)
    (at 146.5 103.5)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59FA120D)
    (at 108.89 139.7 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference "3v3 Pwr" (at -2.7 1.2 270) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 100 130.08) (end 100 146.5) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 100 103.5) (end 100 117.38) (layer Edge.Cuts) (width 0.3))
  (gr_arc (start 101.27 117.38) (end 101.27 118.65) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_arc (start 101.27 119.92) (end 101.27 118.65) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_arc (start 103.81 119.92) (end 103.81 121.19) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_arc (start 103.81 122.46) (end 103.81 121.19) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 105.08 127.54) (end 105.08 122.46) (layer Edge.Cuts) (width 0.3))
  (gr_arc (start 103.81 127.54) (end 105.08 127.54) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 101.27 128.81) (end 103.81 128.81) (layer Edge.Cuts) (width 0.3))
  (gr_arc (start 101.27 130.08) (end 100 130.08) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 146.5 150) (end 103.5 150) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 150 103.5) (end 150 146.5) (layer Edge.Cuts) (width 0.3))
  (gr_line (start 103.5 100) (end 146.5 100) (layer Edge.Cuts) (width 0.3))
  (gr_arc (start 103.5 146.5) (end 103.5 150) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_arc (start 146.5 146.5) (end 150 146.5) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_arc (start 146.5 103.5) (end 146.5 100) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_arc (start 103.5 103.5) (end 100 103.5) (angle 90) (layer Edge.Cuts) (width 0.3))
  (gr_text "1Bitsy\nDAC\nAudio" (at 115.9 121.7 90) (layer F.SilkS))
  (gr_text + (at 149 142.68 90) (layer F.SilkS))
  (gr_text - (at 149 140.14 90) (layer F.SilkS))
  (gr_text - (at 149 131.1 90) (layer F.SilkS))
  (gr_text + (at 149 133.64 90) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 98 98) (xy 152 98) (xy 152 152) (xy 98 152)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 99 99) (xy 151 99) (xy 151 151) (xy 99 151)
      )
    )
  )
)
