(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(J1-Pin_1)")
	(net 2 "GND")
	(net 3 "unconnected-(J5-Pin_15-Pad15)")
	(net 4 "Net-(J3-Pin_4)")
	(net 5 "unconnected-(J3-Pin_3-Pad3)")
	(net 6 "Net-(J4-Pin_3)")
	(net 7 "Net-(J4-Pin_2)")
	(net 8 "/A2")
	(net 9 "/A3")
	(net 10 "/A4")
	(net 11 "/FREE")
	(net 12 "/A5")
	(net 13 "/RX")
	(net 14 "/MOSI")
	(net 15 "/A1")
	(net 16 "/SCK")
	(net 17 "/TX")
	(net 18 "/A0")
	(net 19 "/MISO")
	(net 20 "/AREF")
	(net 21 "/~{RST}")
	(net 22 "/SDA")
	(net 23 "/F0")
	(net 24 "/F2")
	(net 25 "/F6")
	(net 26 "/F4")
	(net 27 "/EN")
	(net 28 "/F5")
	(net 29 "/F3")
	(net 30 "/SCL")
	(net 31 "/VBAT")
	(net 32 "/F1")
	(net 33 "/VUSB")
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 64.008 62.23)
		(descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x12 2.54mm single row")
		(property "Reference" "J6"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "feather short"
			(at 0 30.27 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 13.97 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/SDA")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/F0")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/F1")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/F2")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/F3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/F4")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/F5")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/F6")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/VUSB")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/EN")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VBAT")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm"
		(layer "F.Cu")
		(at 103.364 100.076)
		(descr "Soldered wire connection, for 2 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 0.5sqmm")
		(property "Reference" "J9"
			(at 2.808 -6.98 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x02"
			(at 2.3 2.25 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 2.3 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.119048)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.6 0)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/A1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 54.356 107.188)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 117.01 85.78 180)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at -0.338 -3.628 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J4-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J4-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/VUSB")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm"
		(layer "F.Cu")
		(at 113.044 85.852 180)
		(descr "Soldered wire connection, for 2 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 0.5sqmm")
		(property "Reference" "J2"
			(at 2.808 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 2.3 2.54 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 2.3 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.119048)
			(net 33 "/VUSB")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.6 0 180)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 130.556 56.388)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 106.31 74.24)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at -3.524 0.024 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at -6.234 -0.072 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal"
		(layer "F.Cu")
		(at 94.488 77.216 -90)
		(descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
		(tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
		(property "Reference" "R3"
			(at 7.62 -3.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "5k"
			(at 7.62 3.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/A0")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15.24 0 270)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 103.308 78.24)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J3"
			(at -0.254 10.248 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0.324 11.168 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/A0")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J3-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J3-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 130.556 107.188)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm"
		(layer "F.Cu")
		(at 108.36 70.708)
		(descr "Soldered wire connection, for 2 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 0.5sqmm")
		(property "Reference" "J1"
			(at 7.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at -6.76 -0.096 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 2.3 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.119048)
			(net 1 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.6 0)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 54.356 56.388)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x16_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 84.328 62.23)
		(descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x16 2.54mm single row")
		(property "Reference" "J5"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "feather long"
			(at 0 40.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x16_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 19.05 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/FREE")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/TX")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/RX")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/MISO")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/MOSI")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/SCK")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/A5")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/A4")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/A3")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/A2")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/A1")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/A0")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 0 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/AREF")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(J5-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 0 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{RST}")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x16_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
		(layer "F.Cu")
		(at 110.568 79.128)
		(descr "HTSOP, 8 Pin (https://media.digikey.com/pdf/Data%20Sheets/Rohm%20PDFs/BD9G341EFJ.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "HTSOP SO")
		(property "Reference" "U1"
			(at 0.176 -3.436 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0.176 4.184 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.6 -0.8)
			(size 0.97 1.29)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.6 0.8)
			(size 0.97 1.29)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.6 -0.8)
			(size 0.97 1.29)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.6 0.8)
			(size 0.97 1.29)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.65 -1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J1-Pin_1)")
			(pinfunction "vcc")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.65 -0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/A0")
			(pinfunction "CTL")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.65 0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "4" smd roundrect
			(at -2.65 1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(J3-Pin_4)")
			(pinfunction "Ro")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 2.65 1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "gnd")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.65 0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(J4-Pin_2)")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.65 -0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(J4-Pin_3)")
			(pinfunction "CT")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 2.65 -1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/VUSB")
			(pinfunction "Vout")
			(pintype "input")
		)
		(pad "9" smd rect
			(at 0 0)
			(size 2.4 3.2)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal"
		(layer "F.Cu")
		(at 94.488 57.912 -90)
		(descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
		(tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
		(property "Reference" "R1"
			(at 7.62 -3.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 7.62 3.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15.24 0 270)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/A0")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_AMASS:AMASS_XT30UPB-F_1x02_P5.0mm_Vertical"
		(layer "F.Cu")
		(at 112.776 60.452 180)
		(descr "Connector XT30 Vertical PCB Female, https://www.tme.eu/Document/81f11ca924696756331f21b972812074/XT30PB-F.pdf")
		(tags "RC Connector XT30")
		(property "Reference" "J7"
			(at 2.5 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 2.5 4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_AMASS:AMASS_XT30UPB-F_1x02_P5.0mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at 9 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at -4 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 3 3)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 3 3)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J1-Pin_1)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_AMASS.3dshapes/AMASS_XT30UPB-F_1x02_P5.0mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 114.81 74.24)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 3.724 0.024 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 6.094 -0.072 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 33 "/VUSB")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm"
		(layer "B.Cu")
		(at 103.392 95.504)
		(descr "Soldered wire connection, for 2 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 0.5sqmm")
		(property "Reference" "J8"
			(at 2.3 2.25 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x02"
			(at 2.3 -2.25 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "vreg.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 2.3 0 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.119048)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.6 0)
			(size 2.1 2.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/A2")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 48.768 50.292)
		(end 136.144 113.538)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "SCK"
		(at 89.154 75.438 0)
		(layer "F.SilkS")
	)
	(gr_text "NC"
		(at 99.61 84.17 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 104.648 93.472 0)
		(layer "F.SilkS")
	)
	(gr_text "RX"
		(at 88.9 67.564 0)
		(layer "F.SilkS")
	)
	(gr_text "F2"
		(at 61.722 72.644 0)
		(layer "F.SilkS")
	)
	(gr_text "CLK"
		(at 119.042 83.916 0)
		(layer "F.SilkS")
	)
	(gr_text "F1"
		(at 61.722 70.104 0)
		(layer "F.SilkS")
	)
	(gr_text "RST"
		(at 89.154 101.092 0)
		(layer "F.SilkS")
	)
	(gr_text "F6"
		(at 61.722 82.804 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 108.712 74.676 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 89.662 93.472 0)
		(layer "F.SilkS")
	)
	(gr_text "Vcc"
		(at 104.14 68.58 0)
		(layer "F.SilkS")
	)
	(gr_text "MISO"
		(at 89.916 70.358 0)
		(layer "F.SilkS")
	)
	(gr_text "TX"
		(at 88.9 65.024 0)
		(layer "F.SilkS")
	)
	(gr_text "CTL"
		(at 98.736 81.376 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 119.042 86.456 0)
		(layer "F.SilkS")
	)
	(gr_text "MOSI\n"
		(at 89.916 72.898 0)
		(layer "F.SilkS")
	)
	(gr_text "A4"
		(at 88.392 80.518 0)
		(layer "F.SilkS")
	)
	(gr_text "F3"
		(at 61.722 75.184 0)
		(layer "F.SilkS")
	)
	(gr_text "Vout\n"
		(at 119.042 78.836 0)
		(layer "F.SilkS")
	)
	(gr_text "A3"
		(at 88.392 83.058 0)
		(layer "F.SilkS")
	)
	(gr_text "A1"
		(at 109.22 103.124 0)
		(layer "F.SilkS")
	)
	(gr_text "Ro"
		(at 99.61 86.456 0)
		(layer "F.SilkS")
	)
	(gr_text "A5"
		(at 88.392 77.978 0)
		(layer "F.SilkS")
	)
	(gr_text "F4"
		(at 61.722 77.724 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 111.676 68.93 0)
		(layer "F.SilkS")
	)
	(gr_text "F5"
		(at 61.722 80.264 0)
		(layer "F.SilkS")
	)
	(gr_text "VBAT"
		(at 61.722 90.678 0)
		(layer "F.SilkS")
	)
	(gr_text "sda"
		(at 61.976 62.992 0)
		(layer "F.SilkS")
	)
	(gr_text "A2"
		(at 108.712 93.472 0)
		(layer "F.SilkS")
	)
	(gr_text "A0"
		(at 88.392 90.678 0)
		(layer "F.SilkS")
	)
	(gr_text "VUSB"
		(at 61.468 85.852 0)
		(layer "F.SilkS")
	)
	(gr_text "VDD"
		(at 89.154 98.552 0)
		(layer "F.SilkS")
	)
	(gr_text "CT"
		(at 119.042 81.376 0)
		(layer "F.SilkS")
	)
	(gr_text "A2"
		(at 88.392 85.598 0)
		(layer "F.SilkS")
	)
	(gr_text "F0"
		(at 61.722 67.818 0)
		(layer "F.SilkS")
	)
	(gr_text "Vcc"
		(at 98.736 78.836 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 104.648 103.124 0)
		(layer "F.SilkS")
	)
	(gr_text "scl"
		(at 61.722 65.278 0)
		(layer "F.SilkS")
	)
	(gr_text "EN"
		(at 61.722 88.138 0)
		(layer "F.SilkS")
	)
	(gr_text "AREF"
		(at 89.662 96.012 0)
		(layer "F.SilkS")
	)
	(gr_text "FREE"
		(at 89.916 62.484 0)
		(layer "F.SilkS")
	)
	(gr_text "A1"
		(at 88.392 88.138 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 48.768 50.292) (xy 136.144 50.292) (xy 136.144 113.538) (xy 48.768 113.538)
			)
		)
	)
)
