<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="45.72" y2="0" width="0" layer="20"/>
<wire x1="45.72" y1="0" x2="45.72" y2="33.02" width="0" layer="20"/>
<wire x1="45.72" y1="33.02" x2="0" y2="33.02" width="0" layer="20"/>
<wire x1="0" y1="33.02" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.175" y="29.845" drill="3.175"/>
<hole x="42.545" y="29.845" drill="3.175"/>
<hole x="42.545" y="3.175" drill="3.175"/>
<hole x="3.175" y="3.175" drill="3.175"/>
<text>SDA</text>
<text>SCL</text>
<text>02h</text>
<text>01h</text>
<text>SCL</text>
<text>SDA</text>
<text>VCC</text>
<text>GND</text>
<text>I2C - 7 Segment Backpack</text>
<text>0.56 inch LED -  (Rev D)</text>
<text>SET I2C ADDR WITH SJ3 AND SJ4</text>
<text>BOTH OPEN = 03h</text>
<text>SJ4 CLOSED = 02h</text>
<text>SJ3 CLOSED = 01h</text>
<text>DO NOT CLOSE BOTH</text>
<text>I2C 7 SEGMENT BKPK .56" (Rev D)</text>
<text>LED1</text>
<text>LED1</text>
<text>dcity.org</text>
<text>dcity.org</text>
<text>SCL</text>
<text>SDA</text>
<text>VCC</text>
<text>GND</text>
<text>SCL</text>
<text>SDA</text>
<text>VCC</text>
<text>GND</text>
</plain>
<libraries>
<library name="0">
<packages>
<package name="TSSOP-24">
<description>&lt;h3&gt;24-pin TSSOP with Exposed Thermal Pad&lt;/h3&gt;
Used on: &lt;ul&gt;
&lt;li&gt;Allegro A6282 16-bit LED driver&lt;/li&gt;
&lt;/ul&gt;
Last modified: 8/21/10&lt;br&gt;
&lt;b&gt;***Unproven***&lt;/b&gt;&lt;br&gt;</description>
</package>
<package name="7-SEGMENT-4DIGIT-PT6">
</package>
<package name="0805-RES">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="0805-POL">
</package>
<package name="0805-CAP">
</package>
<package name="OSHW-LOGO-S">
</package>
<package name="1X04_LOCK">
</package>
<package name="POT-TC33X">
</package>
<package name="1X02">
</package>
<package name="CREATIVE_COMMONS">
</package>
<package name="JST04_1MM_RA">
<description>&lt;h3&gt;SMD- 4 Pin Right Angle &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="0" package="TSSOP-24" value="AS1115">
<attribute name="NAME"/>
</element>
<element name="DISP1" library="0" package="7-SEGMENT-4DIGIT-PT6" value="LED1"/>
<element name="R1" library="0" package="0805-RES" value="4.7k">
<attribute name="NAME"/>
</element>
<element name="R2" library="0" package="0805-RES" value="4.7k">
<attribute name="NAME"/>
</element>
<element name="R3" library="0" package="0805-RES" value="6.8k">
<attribute name="NAME"/>
</element>
<element name="SJ1" library="0" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="SJ2" library="0" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="SJ3" library="0" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="SJ4" library="0" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="SJ5" library="0" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="SJ6" library="0" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="C1" library="0" package="0805-POL" value="10u">
<attribute name="NAME"/>
</element>
<element name="C2" library="0" package="0805-CAP" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="0" package="0805-RES" value="6.8k">
<attribute name="NAME"/>
</element>
<element name="LOGO1" library="0" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="J2" library="0" package="1X04_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="0" package="POT-TC33X" value="50k">
<attribute name="NAME"/>
</element>
<element name="TP" library="0" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="0" package="CREATIVE_COMMONS" value="CREATIVE_COMMONS"/>
<element name="J1" library="0" package="JST04_1MM_RA" value="QWIIC_RIGHT_ANGLE">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-13694"/>
</element>
<element name="J3" library="0" package="JST04_1MM_RA" value="QWIIC_RIGHT_ANGLE">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-13694"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="15"/>
<contactref element="DISP1" pad="11"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="17"/>
<contactref element="DISP1" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="20"/>
<contactref element="DISP1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="23"/>
<contactref element="DISP1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="21"/>
<contactref element="DISP1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="16"/>
<contactref element="DISP1" pad="10"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="18"/>
<contactref element="DISP1" pad="5"/>
<contactref element="SJ4" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="22"/>
<contactref element="DISP1" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="2"/>
<contactref element="DISP1" pad="12"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="3"/>
<contactref element="DISP1" pad="9"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="4"/>
<contactref element="DISP1" pad="8"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="5"/>
<contactref element="DISP1" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="SJ4" pad="1"/>
<contactref element="SJ3" pad="1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="19"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="R3" pad="2"/>
<contactref element="TP" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R1" pad="1"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="R2" pad="1"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="SJ1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="SJ2" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="4"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="SJ5" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="SJ6" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="3"/>
<contactref element="SJ5" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="13"/>
<contactref element="R5" pad="1"/>
<contactref element="SJ6" pad="1"/>
<contactref element="TP" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
