(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 278)
    (zones 0)
    (modules 67)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (user_trace_width 1.016)
    (user_trace_width 1.524)
    (user_trace_width 2.54)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.7366 0.381)
    (user_via 0.8636 0.381)
    (user_via 0.8636 0.508)
    (uvia_size 0.8)
    (uvia_drill 0.4)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.3048)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 3.3V)
  (net 2 GND)
  (net 3 VCC)
  (net 4 /SDA)
  (net 5 /SCL)
  (net 6 "Net-(D1-PadA)")
  (net 7 "/ADDR(MISO)")
  (net 8 /CLK)
  (net 9 /DO)
  (net 10 /~RST)
  (net 11 "Net-(D3-PadP6)")
  (net 12 "Net-(D3-PadP5)")
  (net 13 /VLED)
  (net 14 "Net-(D4-PadP6)")
  (net 15 "Net-(D4-PadP5)")
  (net 16 "Net-(D5-PadP6)")
  (net 17 "Net-(D5-PadP5)")
  (net 18 "Net-(D6-PadP6)")
  (net 19 "Net-(D6-PadP5)")
  (net 20 "Net-(D7-PadP6)")
  (net 21 "Net-(D7-PadP5)")
  (net 22 "Net-(D8-PadP6)")
  (net 23 "Net-(D8-PadP5)")
  (net 24 "Net-(D10-PadP1)")
  (net 25 "Net-(D10-PadP2)")
  (net 26 "Net-(D10-PadP6)")
  (net 27 "Net-(D10-PadP5)")
  (net 28 "/DO(10)")
  (net 29 "/CO(10)")
  (net 30 "Net-(I2C1-Pad3)")
  (net 31 "Net-(I2C1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.8)
    (uvia_drill 0.4)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net "/ADDR(MISO)")
    (add_net /CLK)
    (add_net "/CO(10)")
    (add_net /DO)
    (add_net "/DO(10)")
    (add_net /SCL)
    (add_net /SDA)
    (add_net /VLED)
    (add_net /~RST)
    (add_net 3.3V)
    (add_net GND)
    (add_net "Net-(D1-PadA)")
    (add_net "Net-(D10-PadP1)")
    (add_net "Net-(D10-PadP2)")
    (add_net "Net-(D10-PadP5)")
    (add_net "Net-(D10-PadP6)")
    (add_net "Net-(D3-PadP5)")
    (add_net "Net-(D3-PadP6)")
    (add_net "Net-(D4-PadP5)")
    (add_net "Net-(D4-PadP6)")
    (add_net "Net-(D5-PadP5)")
    (add_net "Net-(D5-PadP6)")
    (add_net "Net-(D6-PadP5)")
    (add_net "Net-(D6-PadP6)")
    (add_net "Net-(D7-PadP5)")
    (add_net "Net-(D7-PadP6)")
    (add_net "Net-(D8-PadP5)")
    (add_net "Net-(D8-PadP6)")
    (add_net "Net-(I2C1-Pad1)")
    (add_net "Net-(I2C1-Pad3)")
    (add_net VCC)
  )
  (net_class 43V ""
    (clearance 0.1524)
    (trace_width 2.54)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.8)
    (uvia_drill 0.4)
    (diff_pair_width 1.016)
    (diff_pair_gap 0.8636)
  )
  (net_class MustBe6Thou ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.8)
    (uvia_drill 0.4)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
  )
  (net_class Spindle ""
    (clearance 0.6858)
    (trace_width 1.016)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.8)
    (uvia_drill 0.4)
    (diff_pair_width 1.016)
    (diff_pair_gap 0.8636)
  )
  (net_class Stepper ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.7366)
    (via_drill 0.381)
    (uvia_dia 0.7366)
    (uvia_drill 0.381)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
  )
  (module "Qwiic LED Stick:STAND-OFF" (layer F.Cu) (tedit 0)
    (at 105.3211 115.1636 90)
    (descr "<b>Stand Off</b><p>\nThis is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447")
    (fp_text reference JP3 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value STAND-OFF (at 0 0 90) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
  )
  (module "Qwiic LED Stick:STAND-OFF" (layer F.Cu) (tedit 0)
    (at 105.3211 94.8436 90)
    (descr "<b>Stand Off</b><p>\nThis is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447")
    (fp_text reference JP4 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value STAND-OFF (at 0 0 90) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
  )
  (module "Qwiic LED Stick:MICRO-FIDUCIAL" (layer F.Cu) (tedit 0)
    (at 155.2321 93.1926 90)
    (fp_text reference JP2 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value FIDUCIALUFIDUCIAL (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd roundrect (at 0 0 90) (size 0.635 0.635) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:MICRO-FIDUCIAL" (layer F.Cu) (tedit 0)
    (at 103.5431 116.9416 90)
    (fp_text reference JP6 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value FIDUCIALUFIDUCIAL (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd roundrect (at 0 0 90) (size 0.635 0.635) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:0603" (layer F.Cu) (tedit 0)
    (at 110.4011 107.5436 270)
    (descr "<p><b>Generic 1608 (0603) package</b></p>\n<p>0.2mm courtyard excess rounded to nearest 0.05mm.</p>")
    (fp_text reference R4 (at 0 -0.762 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 0.762 270) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(I2C1-Pad3)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /SDA) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:0603" (layer F.Cu) (tedit 0)
    (at 110.4011 102.4636 90)
    (descr "<p><b>Generic 1608 (0603) package</b></p>\n<p>0.2mm courtyard excess rounded to nearest 0.05mm.</p>")
    (fp_text reference R5 (at 0 -0.762 90) (layer F.SilkS))
    (fp_text value 2.2k (at 0 0.762 90) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(I2C1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 90) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCL) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:SMT-JUMPER_3_2-NC_TRACE_SILK" (layer B.Cu) (tedit 0)
    (at 110.9091 105.0036 180)
    (fp_text reference I2C1 (at 0 1.143 180) (layer B.SilkS))
    (fp_text value JUMPER-SMT_3_2-NC_TRACE_SILK (at 0 -1.143 180) (layer B.Fab))
    (pad 3 smd rect (at 1.016 0 180) (size 0.635 1.27) (layers B.Cu B.Mask)
      (net 30 "Net-(I2C1-Pad3)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 0 0 180) (size 0.635 1.27) (layers B.Cu B.Mask)
      (net 1 3.3V) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -1.016 0 180) (size 0.635 1.27) (layers B.Cu B.Mask)
      (net 31 "Net-(I2C1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:1X04_1MM_RA" (layer F.Cu) (tedit 0)
    (at 119.2911 112.6236)
    (descr "<h3>SMD- 4 Pin Right Angle </h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (fp_text reference J2 (at -1.397 2.159) (layer F.SilkS))
    (fp_text value SMD (at -1.651 3.302) (layer F.Fab))
    (pad 4 smd rect (at 1.5 0) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCL) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 0.5 0) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask)
      (net 4 /SDA) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -0.5 0) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 3.3V) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -1.5 0) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad NC1 smd rect (at 2.8 3.675) (size 1.2 2) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad NC2 smd rect (at -2.8 3.675) (size 1.2 2) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:1X04_NO_SILK" (layer F.Cu) (tedit 0)
    (at 104.0511 98.6536 270)
    (descr "<h3>Plated Through Hole - 4 Pin No Silk Outline</h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (fp_text reference J3 (at -1.27 -1.397 270) (layer F.SilkS))
    (fp_text value PTH (at -1.27 2.032 270) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /SCL) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /SDA) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 3.3V) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:CREATIVE_COMMONS" (layer F.Cu) (tedit 0)
    (at 112.9411 126.5936)
    (descr "<h3>Creative Commons License Template</h3>\n<p>CC BY-SA 4.0 License with <a href=\"https://creativecommons.org/licenses/by-sa/4.0/\">link to license</a> and placeholder for designer name.</p>\n<p>Devices using:\n<ul><li>FRAME_LEDGER</li>\n<li>FRAME_LETTER</li></ul></p>")
    (fp_text reference FRAME1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value FRAME-LETTER (at 0 0) (layer F.SilkS) hide)
    (fp_text user "Designed by:" (at 11.43 0) (layer F.Fab))
    (fp_text user " https://creativecommons.org/licenses/by-sa/4.0/" (at 0 -2.54) (layer F.Fab))
    (fp_text user "Released under the Creative Commons Attribution Share-Alike 4.0 License" (at -20.32 -5.08) (layer F.Fab))
  )
  (module "Qwiic LED Stick:SPARKX-MEDIUM" (layer B.Cu) (tedit 0)
    (at 132.7912 93.9546 180)
    (fp_text reference U$2 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value SPARKX-LOGO4 (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:0603" (layer F.Cu) (tedit 0)
    (at 119.2911 109.0676)
    (descr "<p><b>Generic 1608 (0603) package</b></p>\n<p>0.2mm courtyard excess rounded to nearest 0.05mm.</p>")
    (fp_text reference C4 (at 0 -0.762) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.762) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 3.3V) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:1X04_1MM_RA" (layer F.Cu) (tedit 0)
    (at 119.2911 97.3836 180)
    (descr "<h3>SMD- 4 Pin Right Angle </h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (fp_text reference J4 (at -1.397 2.159 180) (layer F.SilkS))
    (fp_text value SMD (at -1.651 3.302 180) (layer F.Fab))
    (pad 4 smd rect (at 1.5 0 180) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCL) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 0.5 0 180) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask)
      (net 4 /SDA) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -0.5 0 180) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 3.3V) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -1.5 0 180) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad NC1 smd rect (at 2.8 3.675 180) (size 1.2 2) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad NC2 smd rect (at -2.8 3.675 180) (size 1.2 2) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:OSHW-LOGO-MINI" (layer B.Cu) (tedit 0)
    (at 109.1311 113.8936 180)
    (descr "<h3>Open-Source Hardware (OSHW) Logo - Mini - Silkscreen</h3>\n<p>Silkscreen logo for open-source hardware designs.</p>\n<p>Devices using:\n<ul><li>OSHW_LOGO</li></ul></p>")
    (fp_text reference LOGO1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-LOGOMINI (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:SPARKX-MEDIUM" (layer B.Cu) (tedit 0)
    (at 134.2136 115.7986 180)
    (fp_text reference U$1 (at 0 0) (layer B.SilkS) hide)
    (fp_text value SPARKX-LOGO4 (at 0 0) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:MICRO-FIDUCIAL" (layer B.Cu) (tedit 0)
    (at 103.5431 116.9416 270)
    (fp_text reference JP1 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value FIDUCIALUFIDUCIAL (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 smd roundrect (at 0 0 270) (size 0.635 0.635) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:MICRO-FIDUCIAL" (layer B.Cu) (tedit 0)
    (at 155.2321 93.1926 270)
    (fp_text reference JP5 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value FIDUCIALUFIDUCIAL (at 0 0 270) (layer B.SilkS) hide)
    (pad 1 smd roundrect (at 0 0 270) (size 0.635 0.635) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:3#3V2" (layer F.Cu) (tedit 0)
    (at 104.3051 101.1936)
    (fp_text reference U$21 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module "Qwiic LED Stick:GND1" (layer F.Cu) (tedit 0)
    (at 104.3051 98.6536)
    (fp_text reference U$22 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module "Qwiic LED Stick:SCL9" (layer F.Cu) (tedit 0)
    (at 104.3051 106.2736)
    (fp_text reference U$26 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module "Qwiic LED Stick:SDA8" (layer F.Cu) (tedit 0)
    (at 104.3051 103.7336)
    (fp_text reference U$27 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module "Qwiic LED Stick:GND1" (layer B.Cu) (tedit 0)
    (at 109.1311 98.6536 180)
    (fp_text reference U$3 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:3#3V2" (layer B.Cu) (tedit 0)
    (at 109.2581 101.1936 180)
    (fp_text reference U$4 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:0603" (layer F.Cu) (tedit 0)
    (at 111.0361 116.6876)
    (descr "<p><b>Generic 1608 (0603) package</b></p>\n<p>0.2mm courtyard excess rounded to nearest 0.05mm.</p>")
    (fp_text reference R3 (at 0 -0.762) (layer F.SilkS))
    (fp_text value 1k (at 0 0.762) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 3.3V) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-PadA)") (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:LED-0603" (layer F.Cu) (tedit 0)
    (at 111.0361 115.2906)
    (descr "<B>LED 0603 SMT</B><p>\n0603, surface mount.\n<p>Specifications:\n<ul><li>Pin count: 2</li>\n<li>Pin pitch:0.075inch </li>\n<li>Area: 0.06\" x 0.03\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>LED - BLUE</li>")
    (fp_text reference D1 (at 0 -0.635) (layer F.SilkS))
    (fp_text value RED (at 0 0.635) (layer F.Fab))
    (pad A smd roundrect (at -0.877 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 6 "Net-(D1-PadA)") (solder_mask_margin 0.1016))
    (pad C smd roundrect (at 0.877 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:(PWR)" (layer F.Cu) (tedit 0)
    (at 108.4961 113.7666)
    (fp_text reference U$10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module "Qwiic LED Stick:(I_SUPER2_C)" (layer B.Cu) (tedit 0)
    (at 112.8141 102.8446 180)
    (fp_text reference U$11 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:SO08-EIAJ_MCU" (layer F.Cu) (tedit 0)
    (at 119.2911 105.0036 90)
    (descr "Fits EIAJ packages (wide version of the SOIC-8).")
    (fp_text reference U1 (at -2.8575 0 180) (layer F.SilkS))
    (fp_text value Tiny85-20-SMT (at 3.4925 0 180) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.3528 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 1 3.3V) (solder_mask_margin 0.1016))
    (pad 7 smd rect (at -0.635 -3.3528 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCL) (solder_mask_margin 0.1016))
    (pad 6 smd rect (at 0.635 -3.3528 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 7 "/ADDR(MISO)") (solder_mask_margin 0.1016))
    (pad 5 smd rect (at 1.905 -3.3528 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 4 /SDA) (solder_mask_margin 0.1016))
    (pad 4 smd rect (at 1.905 3.3782 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 0.635 3.3782 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 8 /CLK) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -0.635 3.3782 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 9 /DO) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -1.905 3.3782 90) (size 0.6096 2.2098) (layers F.Cu F.Paste F.Mask)
      (net 10 /~RST) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:APA102-5050" (layer F.Cu) (tedit 0)
    (at 128.143 112.8649)
    (descr "<h3>APA102C</h3>\n\n<p>Specifications:\n<ul><li>Pin count: 6</li>\n<li>Size: 5.0 x 5.0 mm</li>\n</ul></p>\n<p><b>Datasheet referenced for footprint:</b> <a href=\"https://cdn.sparkfun.com/datasheets/Components/LED/APA102C.pdf\">APA102C</a></p>")
    (fp_text reference D3 (at 0.04 -3.755) (layer F.SilkS))
    (fp_text value APA1025050 (at 0 4.191) (layer F.Fab))
    (pad P3 smd rect (at 1.75 2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad P2 smd rect (at 0 2.1 270) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 8 /CLK) (solder_mask_margin 0.1016))
    (pad P1 smd rect (at -1.75 2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 9 /DO) (solder_mask_margin 0.1016))
    (pad P6 smd rect (at -1.75 -2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 11 "Net-(D3-PadP6)") (solder_mask_margin 0.1016))
    (pad P5 smd rect (at 0 -2.1 270) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 12 "Net-(D3-PadP5)") (solder_mask_margin 0.1016))
    (pad P4 smd rect (at 1.75 -2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 13 /VLED) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:APA102-5050" (layer F.Cu) (tedit 0)
    (at 128.1938 104.9655)
    (descr "<h3>APA102C</h3>\n\n<p>Specifications:\n<ul><li>Pin count: 6</li>\n<li>Size: 5.0 x 5.0 mm</li>\n</ul></p>\n<p><b>Datasheet referenced for footprint:</b> <a href=\"https://cdn.sparkfun.com/datasheets/Components/LED/APA102C.pdf\">APA102C</a></p>")
    (fp_text reference D4 (at 0.04 -3.755) (layer F.SilkS))
    (fp_text value APA1025050 (at 0 4.191) (layer F.Fab))
    (pad P3 smd rect (at 1.75 2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad P2 smd rect (at 0 2.1 270) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 12 "Net-(D3-PadP5)") (solder_mask_margin 0.1016))
    (pad P1 smd rect (at -1.75 2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 11 "Net-(D3-PadP6)") (solder_mask_margin 0.1016))
    (pad P6 smd rect (at -1.75 -2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 14 "Net-(D4-PadP6)") (solder_mask_margin 0.1016))
    (pad P5 smd rect (at 0 -2.1 270) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 15 "Net-(D4-PadP5)") (solder_mask_margin 0.1016))
    (pad P4 smd rect (at 1.75 -2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 13 /VLED) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:APA102-5050" (layer F.Cu) (tedit 0)
    (at 128.1811 97.1296)
    (descr "<h3>APA102C</h3>\n\n<p>Specifications:\n<ul><li>Pin count: 6</li>\n<li>Size: 5.0 x 5.0 mm</li>\n</ul></p>\n<p><b>Datasheet referenced for footprint:</b> <a href=\"https://cdn.sparkfun.com/datasheets/Components/LED/APA102C.pdf\">APA102C</a></p>")
    (fp_text reference D5 (at 0.04 -3.755) (layer F.SilkS))
    (fp_text value APA1025050 (at 0 4.191) (layer F.Fab))
    (pad P3 smd rect (at 1.75 2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad P2 smd rect (at 0 2.1 270) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 15 "Net-(D4-PadP5)") (solder_mask_margin 0.1016))
    (pad P1 smd rect (at -1.75 2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 14 "Net-(D4-PadP6)") (solder_mask_margin 0.1016))
    (pad P6 smd rect (at -1.75 -2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 16 "Net-(D5-PadP6)") (solder_mask_margin 0.1016))
    (pad P5 smd rect (at 0 -2.1 270) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 17 "Net-(D5-PadP5)") (solder_mask_margin 0.1016))
    (pad P4 smd rect (at 1.75 -2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 13 /VLED) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:APA102-5050" (layer F.Cu) (tedit 0)
    (at 134.5311 97.1296 180)
    (descr "<h3>APA102C</h3>\n\n<p>Specifications:\n<ul><li>Pin count: 6</li>\n<li>Size: 5.0 x 5.0 mm</li>\n</ul></p>\n<p><b>Datasheet referenced for footprint:</b> <a href=\"https://cdn.sparkfun.com/datasheets/Components/LED/APA102C.pdf\">APA102C</a></p>")
    (fp_text reference D6 (at 0.04 -3.755) (layer F.SilkS))
    (fp_text value APA1025050 (at 0 4.191) (layer F.Fab))
    (pad P3 smd rect (at 1.75 2.1 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad P2 smd rect (at 0 2.1 90) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 17 "Net-(D5-PadP5)") (solder_mask_margin 0.1016))
    (pad P1 smd rect (at -1.75 2.1 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 16 "Net-(D5-PadP6)") (solder_mask_margin 0.1016))
    (pad P6 smd rect (at -1.75 -2.1 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 18 "Net-(D6-PadP6)") (solder_mask_margin 0.1016))
    (pad P5 smd rect (at 0 -2.1 90) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 19 "Net-(D6-PadP5)") (solder_mask_margin 0.1016))
    (pad P4 smd rect (at 1.75 -2.1 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 13 /VLED) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:APA102-5050" (layer F.Cu) (tedit 0)
    (at 134.5311 105.0036 180)
    (descr "<h3>APA102C</h3>\n\n<p>Specifications:\n<ul><li>Pin count: 6</li>\n<li>Size: 5.0 x 5.0 mm</li>\n</ul></p>\n<p><b>Datasheet referenced for footprint:</b> <a href=\"https://cdn.sparkfun.com/datasheets/Components/LED/APA102C.pdf\">APA102C</a></p>")
    (fp_text reference D7 (at 0.04 -3.755) (layer F.SilkS))
    (fp_text value APA1025050 (at 0 4.191) (layer F.Fab))
    (pad P3 smd rect (at 1.75 2.1 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad P2 smd rect (at 0 2.1 90) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 19 "Net-(D6-PadP5)") (solder_mask_margin 0.1016))
    (pad P1 smd rect (at -1.75 2.1 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 18 "Net-(D6-PadP6)") (solder_mask_margin 0.1016))
    (pad P6 smd rect (at -1.75 -2.1 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 20 "Net-(D7-PadP6)") (solder_mask_margin 0.1016))
    (pad P5 smd rect (at 0 -2.1 90) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 21 "Net-(D7-PadP5)") (solder_mask_margin 0.1016))
    (pad P4 smd rect (at 1.75 -2.1 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 13 /VLED) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:APA102-5050" (layer F.Cu) (tedit 0)
    (at 134.5311 112.8776 180)
    (descr "<h3>APA102C</h3>\n\n<p>Specifications:\n<ul><li>Pin count: 6</li>\n<li>Size: 5.0 x 5.0 mm</li>\n</ul></p>\n<p><b>Datasheet referenced for footprint:</b> <a href=\"https://cdn.sparkfun.com/datasheets/Components/LED/APA102C.pdf\">APA102C</a></p>")
    (fp_text reference D8 (at 0.04 -3.755) (layer F.SilkS))
    (fp_text value APA1025050 (at 0 4.191) (layer F.Fab))
    (pad P3 smd rect (at 1.75 2.1 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad P2 smd rect (at 0 2.1 90) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 21 "Net-(D7-PadP5)") (solder_mask_margin 0.1016))
    (pad P1 smd rect (at -1.75 2.1 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 20 "Net-(D7-PadP6)") (solder_mask_margin 0.1016))
    (pad P6 smd rect (at -1.75 -2.1 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 22 "Net-(D8-PadP6)") (solder_mask_margin 0.1016))
    (pad P5 smd rect (at 0 -2.1 90) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 23 "Net-(D8-PadP5)") (solder_mask_margin 0.1016))
    (pad P4 smd rect (at 1.75 -2.1 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 13 /VLED) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:APA102-5050" (layer F.Cu) (tedit 0)
    (at 140.8811 112.8776)
    (descr "<h3>APA102C</h3>\n\n<p>Specifications:\n<ul><li>Pin count: 6</li>\n<li>Size: 5.0 x 5.0 mm</li>\n</ul></p>\n<p><b>Datasheet referenced for footprint:</b> <a href=\"https://cdn.sparkfun.com/datasheets/Components/LED/APA102C.pdf\">APA102C</a></p>")
    (fp_text reference D9 (at 0.04 -3.755) (layer F.SilkS))
    (fp_text value APA1025050 (at 0 4.191) (layer F.Fab))
    (pad P3 smd rect (at 1.75 2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad P2 smd rect (at 0 2.1 270) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 23 "Net-(D8-PadP5)") (solder_mask_margin 0.1016))
    (pad P1 smd rect (at -1.75 2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 22 "Net-(D8-PadP6)") (solder_mask_margin 0.1016))
    (pad P6 smd rect (at -1.75 -2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 24 "Net-(D10-PadP1)") (solder_mask_margin 0.1016))
    (pad P5 smd rect (at 0 -2.1 270) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 25 "Net-(D10-PadP2)") (solder_mask_margin 0.1016))
    (pad P4 smd rect (at 1.75 -2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 13 /VLED) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:APA102-5050" (layer F.Cu) (tedit 0)
    (at 140.8811 105.0036)
    (descr "<h3>APA102C</h3>\n\n<p>Specifications:\n<ul><li>Pin count: 6</li>\n<li>Size: 5.0 x 5.0 mm</li>\n</ul></p>\n<p><b>Datasheet referenced for footprint:</b> <a href=\"https://cdn.sparkfun.com/datasheets/Components/LED/APA102C.pdf\">APA102C</a></p>")
    (fp_text reference D10 (at 0.04 -3.755) (layer F.SilkS))
    (fp_text value APA1025050 (at 0 4.191) (layer F.Fab))
    (pad P3 smd rect (at 1.75 2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad P2 smd rect (at 0 2.1 270) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 25 "Net-(D10-PadP2)") (solder_mask_margin 0.1016))
    (pad P1 smd rect (at -1.75 2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 24 "Net-(D10-PadP1)") (solder_mask_margin 0.1016))
    (pad P6 smd rect (at -1.75 -2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 26 "Net-(D10-PadP6)") (solder_mask_margin 0.1016))
    (pad P5 smd rect (at 0 -2.1 270) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 27 "Net-(D10-PadP5)") (solder_mask_margin 0.1016))
    (pad P4 smd rect (at 1.75 -2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 13 /VLED) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:APA102-5050" (layer F.Cu) (tedit 0)
    (at 140.8811 97.1296)
    (descr "<h3>APA102C</h3>\n\n<p>Specifications:\n<ul><li>Pin count: 6</li>\n<li>Size: 5.0 x 5.0 mm</li>\n</ul></p>\n<p><b>Datasheet referenced for footprint:</b> <a href=\"https://cdn.sparkfun.com/datasheets/Components/LED/APA102C.pdf\">APA102C</a></p>")
    (fp_text reference D11 (at 0.04 -3.755) (layer F.SilkS))
    (fp_text value APA1025050 (at 0 4.191) (layer F.Fab))
    (pad P3 smd rect (at 1.75 2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad P2 smd rect (at 0 2.1 270) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 27 "Net-(D10-PadP5)") (solder_mask_margin 0.1016))
    (pad P1 smd rect (at -1.75 2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 26 "Net-(D10-PadP6)") (solder_mask_margin 0.1016))
    (pad P6 smd rect (at -1.75 -2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 28 "/DO(10)") (solder_mask_margin 0.1016))
    (pad P5 smd rect (at 0 -2.1 270) (size 2.2 1.1) (layers F.Cu F.Mask)
      (net 29 "/CO(10)") (solder_mask_margin 0.1016))
    (pad P4 smd rect (at 1.75 -2.1 270) (size 2.2 1) (layers F.Cu F.Mask)
      (net 13 /VLED) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:STAND-OFF" (layer F.Cu) (tedit 0)
    (at 153.5811 94.8436)
    (descr "<b>Stand Off</b><p>\nThis is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447")
    (fp_text reference JP7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value STAND-OFF (at 0 0) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
  )
  (module "Qwiic LED Stick:STAND-OFF" (layer F.Cu) (tedit 0)
    (at 153.5811 115.1636)
    (descr "<b>Stand Off</b><p>\nThis is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447")
    (fp_text reference JP8 (at 0 0) (layer F.SilkS) hide)
    (fp_text value STAND-OFF (at 0 0) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
  )
  (module "Qwiic LED Stick:2X3_TEST_POINTS" (layer B.Cu) (tedit 0)
    (at 119.2911 105.0036 270)
    (descr "<h3>Plated Through Hole - 2x3 Test Point Header</h3>\n<p>Specifications:\n<ul><li>Pin count:6</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_03x2</li>\n</ul></p>")
    (fp_text reference J6 (at -3.048 2.032 270) (layer B.SilkS))
    (fp_text value AVR_SPI_PROG_3X2TESTPOINTS (at -3.048 -3.048 270) (layer B.Fab))
    (pad 6 thru_hole circle (at 2.54 1.27 270) (size 0.8636 0.8636) (drill 0.508) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 2.54 -1.27 270) (size 0.8636 0.8636) (drill 0.508) (layers *.Cu *.Mask)
      (net 10 /~RST) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 0 1.27 270) (size 0.8636 0.8636) (drill 0.508) (layers *.Cu *.Mask)
      (net 4 /SDA) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 0 -1.27 270) (size 0.8636 0.8636) (drill 0.508) (layers *.Cu *.Mask)
      (net 5 /SCL) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -2.54 1.27 270) (size 0.8636 0.8636) (drill 0.508) (layers *.Cu *.Mask)
      (net 1 3.3V) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -2.54 -1.27 270) (size 0.8636 0.8636) (drill 0.508) (layers *.Cu *.Mask)
      (net 7 "/ADDR(MISO)") (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:SMT-JUMPER_2_NO_SILK" (layer B.Cu) (tedit 0)
    (at 115.4811 105.0036 180)
    (fp_text reference JP9 (at 0 1.143 180) (layer B.SilkS))
    (fp_text value JUMPER-SMT_2_NO_SILK (at 0 -1.143 180) (layer B.Fab))
    (pad 2 smd rect (at 0.4064 0 180) (size 0.635 1.27) (layers B.Cu B.Mask)
      (net 7 "/ADDR(MISO)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.4064 0 180) (size 0.635 1.27) (layers B.Cu B.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:QWIIC-LOGO-MEDIUM" (layer B.Cu) (tedit 0)
    (at 149.3901 113.5126 180)
    (fp_text reference U$29 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:0603" (layer F.Cu) (tedit 0)
    (at 112.8141 105.0036 270)
    (descr "<p><b>Generic 1608 (0603) package</b></p>\n<p>0.2mm courtyard excess rounded to nearest 0.05mm.</p>")
    (fp_text reference R2 (at 0 -0.762 270) (layer F.SilkS))
    (fp_text value 4.7k (at 0 0.762 270) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 3.3V) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 270) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /~RST) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:SMT-JUMPER_3_1-NC_TRACE_SILK" (layer B.Cu) (tedit 0)
    (at 125.6411 105.0036 90)
    (fp_text reference JP10 (at 0 1.143 90) (layer B.SilkS))
    (fp_text value JUMPER-SMT_3_1-NC_TRACE_SILK (at 0 -1.143 90) (layer B.Fab))
    (pad 3 smd rect (at 1.016 0 90) (size 0.635 1.27) (layers B.Cu B.Mask)
      (net 1 3.3V) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 0 0 90) (size 0.635 1.27) (layers B.Cu B.Mask)
      (net 13 /VLED) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -1.016 0 90) (size 0.635 1.27) (layers B.Cu B.Mask)
      (net 3 VCC) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:1X02_NO_SILK" (layer F.Cu) (tedit 0)
    (at 104.0511 108.8136 270)
    (descr "<h3>Plated Through Hole - No Silk Outline</h3>\n<p>Specifications:\n<ul><li>Pin count:2</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_02</li>\n</ul></p>")
    (fp_text reference J1 (at -1.27 -1.397 270) (layer F.SilkS))
    (fp_text value CONN_021X02_NO_SILK (at -1.27 2.032 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 VCC) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:1X04_NO_SILK" (layer B.Cu) (tedit 0)
    (at 154.8511 101.1936 270)
    (descr "<h3>Plated Through Hole - 4 Pin No Silk Outline</h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (fp_text reference J5 (at -1.27 1.397 270) (layer B.SilkS))
    (fp_text value CONN_041X04_NO_SILK (at -1.27 -2.032 270) (layer B.Fab))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "/DO(10)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "/CO(10)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /VLED) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:VLED4" (layer F.Cu) (tedit 0)
    (at 149.0091 101.1936)
    (fp_text reference U$9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module "Qwiic LED Stick:GND1" (layer F.Cu) (tedit 0)
    (at 149.7711 108.8136)
    (fp_text reference U$12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module "Qwiic LED Stick:DO12" (layer F.Cu) (tedit 0)
    (at 150.6601 106.2736)
    (fp_text reference U$15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module "Qwiic LED Stick:CO9" (layer F.Cu) (tedit 0)
    (at 150.6601 103.7336)
    (fp_text reference U$16 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module "Qwiic LED Stick:SDA0" (layer B.Cu) (tedit 0)
    (at 109.0041 103.7336 180)
    (fp_text reference U$17 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:SCL1" (layer B.Cu) (tedit 0)
    (at 108.7501 106.2736 180)
    (fp_text reference U$18 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:VLED4" (layer B.Cu) (tedit 0)
    (at 154.7241 101.1936 180)
    (fp_text reference U$5 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:DO8" (layer B.Cu) (tedit 0)
    (at 154.5971 106.2736 180)
    (fp_text reference U$6 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:CO5" (layer B.Cu) (tedit 0)
    (at 154.5971 103.7336 180)
    (fp_text reference U$7 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:GND1" (layer B.Cu) (tedit 0)
    (at 154.5971 108.8136 180)
    (fp_text reference U$8 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:VCC1" (layer F.Cu) (tedit 0)
    (at 104.3051 108.8136)
    (fp_text reference U$19 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module "Qwiic LED Stick:VCC1" (layer B.Cu) (tedit 0)
    (at 109.0041 108.8136 180)
    (fp_text reference U$20 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:GND0" (layer B.Cu) (tedit 0)
    (at 109.1311 111.3536 180)
    (fp_text reference U$23 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:GND0" (layer F.Cu) (tedit 0)
    (at 104.3051 111.3536)
    (fp_text reference U$24 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module "Qwiic LED Stick:VLED3" (layer B.Cu) (tedit 0)
    (at 132.4991 105.0036 180)
    (fp_text reference U$25 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:ADDR2" (layer B.Cu) (tedit 0)
    (at 118.4021 107.2896 180)
    (fp_text reference U$28 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:3#3V3" (layer B.Cu) (tedit 0)
    (at 128.1811 102.3366 180)
    (fp_text reference U$30 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:VCC1" (layer B.Cu) (tedit 0)
    (at 128.0541 107.6706 180)
    (fp_text reference U$31 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:0603" (layer F.Cu) (tedit 0)
    (at 122.682 110.3884 180)
    (descr "<p><b>Generic 1608 (0603) package</b></p>\n<p>0.2mm courtyard excess rounded to nearest 0.05mm.</p>")
    (fp_text reference C1 (at 0 -0.762) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 0.762) (layer F.Fab))
    (pad 2 smd rect (at 0.85 0 180) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.85 0 180) (size 1.1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.1016))
  )
  (module "Qwiic LED Stick:QWIIC_LED_STICK1" (layer B.Cu) (tedit 0)
    (at 141.7066 113.1951 180)
    (fp_text reference U$32 (at 0 0) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0) (layer B.SilkS) hide)
  )
  (module "Qwiic LED Stick:QWIIC_LED_STICK1" (layer B.Cu) (tedit 0)
    (at 140.6652 96.2406 180)
    (fp_text reference U$13 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS) hide)
  )
  (gr_line (start 156.1211 117.7036) (end 102.7811 117.7036) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 102.7811 117.7036) (end 102.7811 92.3036) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 102.7811 92.3036) (end 156.1211 92.3036) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 156.1211 92.3036) (end 156.1211 117.7036) (layer Edge.Cuts) (width 0.2032))
  (gr_text X01 (at 109.0041 116.4336) (layer B.Cu))
  (gr_text "Ciara Jekel" (at 143.4211 126.5936) (layer F.Fab))
  (gr_text "Units in Inches" (at 148.5011 84.6836) (layer Dwgs.User))
  (dimension 53.34 (width 0.1) (layer Dwgs.User)
    (gr_text "2.1000 in" (at 129.4511 86.7356) (layer Dwgs.User))
    (feature1 (pts (xy 156.1211 92.3036) (xy 156.1211 87.399179)))
    (feature2 (pts (xy 102.7811 92.3036) (xy 102.7811 87.399179)))
    (crossbar (pts (xy 102.7811 87.9856) (xy 156.1211 87.9856)))
    (arrow1a (pts (xy 156.1211 87.9856) (xy 154.994596 88.572021)))
    (arrow1b (pts (xy 156.1211 87.9856) (xy 154.994596 87.399179)))
    (arrow2a (pts (xy 102.7811 87.9856) (xy 103.907604 88.572021)))
    (arrow2b (pts (xy 102.7811 87.9856) (xy 103.907604 87.399179)))
  )
  (dimension 48.26 (width 0.1) (layer Dwgs.User)
    (gr_text "1.9000 in" (at 129.4511 89.7836) (layer Dwgs.User))
    (feature1 (pts (xy 153.5811 94.8436) (xy 153.5811 90.447179)))
    (feature2 (pts (xy 105.3211 94.8436) (xy 105.3211 90.447179)))
    (crossbar (pts (xy 105.3211 91.0336) (xy 153.5811 91.0336)))
    (arrow1a (pts (xy 153.5811 91.0336) (xy 152.454596 91.620021)))
    (arrow1b (pts (xy 153.5811 91.0336) (xy 152.454596 90.447179)))
    (arrow2a (pts (xy 105.3211 91.0336) (xy 106.447604 91.620021)))
    (arrow2b (pts (xy 105.3211 91.0336) (xy 106.447604 90.447179)))
  )
  (dimension 20.32 (width 0.1) (layer Dwgs.User)
    (gr_text "0.8 in" (at 100.2611 105.0036 90) (layer Dwgs.User))
    (feature1 (pts (xy 105.3211 94.8436) (xy 100.924679 94.8436)))
    (feature2 (pts (xy 105.3211 115.1636) (xy 100.924679 115.1636)))
    (crossbar (pts (xy 101.5111 115.1636) (xy 101.5111 94.8436)))
    (arrow1a (pts (xy 101.5111 94.8436) (xy 102.097521 95.970104)))
    (arrow1b (pts (xy 101.5111 94.8436) (xy 100.924679 95.970104)))
    (arrow2a (pts (xy 101.5111 115.1636) (xy 102.097521 114.037096)))
    (arrow2b (pts (xy 101.5111 115.1636) (xy 100.924679 114.037096)))
  )
  (dimension 25.4 (width 0.1) (layer Dwgs.User)
    (gr_text "1 in" (at 96.4511 105.0036 90) (layer Dwgs.User))
    (feature1 (pts (xy 105.3211 92.3036) (xy 97.114679 92.3036)))
    (feature2 (pts (xy 105.3211 117.7036) (xy 97.114679 117.7036)))
    (crossbar (pts (xy 97.7011 117.7036) (xy 97.7011 92.3036)))
    (arrow1a (pts (xy 97.7011 92.3036) (xy 98.287521 93.430104)))
    (arrow1b (pts (xy 97.7011 92.3036) (xy 97.114679 93.430104)))
    (arrow2a (pts (xy 97.7011 117.7036) (xy 98.287521 116.577096)))
    (arrow2b (pts (xy 97.7011 117.7036) (xy 97.114679 116.577096)))
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy 156.2481 117.8306) (xy 64.5541 117.8306) (xy 64.5541 92.1766) (xy 156.2481 92.1766)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy 156.2481 117.8306) (xy 64.5541 117.8306) (xy 64.5541 92.1766) (xy 156.2481 92.1766)
      )
    )
  )
)
