<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="27.94" y2="0" width="0" layer="20"/>
<wire x1="27.94" y1="0" x2="27.94" y2="53" width="0" layer="20"/>
<wire x1="27.94" y1="53" x2="0" y2="53" width="0" layer="20"/>
<wire x1="0" y1="53" x2="0" y2="0" width="0" layer="20"/>
<text>XBee SMT Breakout 1.0
by Rob Faludi 2014</text>
<text>XBee SMT</text>
<text>XBee SMT Breakout 1.0
by Rob Faludi 2014</text>
<text>GND</text>
<text>VCC</text>
<text>DOUT</text>
<text>DIN</text>
<text>DIO12</text>
<text>RESET</text>
<text>RSSI</text>
<text>DIO11</text>
<text>RES1</text>
<text>DTR</text>
<text>GND2</text>
<text>SPI_ATTN</text>
<text>GND3</text>
<text>SPI_CLK</text>
<text>SPI_SSEL</text>
<text>SPI_MOSI</text>
<text>SPI_MISO</text>
<text>RES2</text>
<text>RES3</text>
<text>n/c</text>
<text>RES8</text>
<text>RF_ANT</text>
<text>GND_RF</text>
<text>RES7</text>
<text>AD0</text>
<text>AD1</text>
<text>AD2</text>
<text>AD3</text>
<text>RTS</text>
<text>ASSC</text>
<text>VREF</text>
<text>ON_SLP</text>
<text>CTS</text>
<text>DIO4</text>
<text>RES6</text>
<text>GND4</text>
<text>RES5</text>
<text>RES4</text>
<text>n/c</text>
<text>n/c</text>
</plain>
<libraries>
<library name="xbee-smt">
<description>Generated from &lt;b&gt;xbee-smt.sch&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="QUBIQ_FLAT-RF">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10_SMD_MALE">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="xbee-smt" package="QUBIQ_FLAT-RF" value="XBEE-SMT"/>
<element name="JP1" library="SparkFun-Connectors" package="1X10_SMD_MALE" value="M10SMD_MALE">
<attribute name="PROD_ID" value="CONN-11291"/>
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X10_SMD_MALE" value="M10SMD_MALE">
<attribute name="PROD_ID" value="CONN-11291"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X10_SMD_MALE" value="M10SMD_MALE">
<attribute name="PROD_ID" value="CONN-11291"/>
<attribute name="NAME"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X10_SMD_MALE" value="M10SMD_MALE">
<attribute name="PROD_ID" value="CONN-11291"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="PIN1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="PIN2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="DOUT">
<contactref element="U$2" pad="PIN3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="DIN">
<contactref element="U$2" pad="PIN4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="DIO12">
<contactref element="U$2" pad="PIN5"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="RESET">
<contactref element="U$2" pad="PIN6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="RSSI">
<contactref element="U$2" pad="PIN7"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="AD0">
<contactref element="U$2" pad="PIN33"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="AD1">
<contactref element="U$2" pad="PIN32"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="AD2">
<contactref element="U$2" pad="PIN31"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="AD3">
<contactref element="U$2" pad="PIN30"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="ASSC">
<contactref element="U$2" pad="PIN28"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="VREF">
<contactref element="U$2" pad="PIN27"/>
<contactref element="JP3" pad="10"/>
</signal>
<signal name="ON_SLP">
<contactref element="U$2" pad="PIN26"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="CTS">
<contactref element="U$2" pad="PIN25"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="DIO4">
<contactref element="U$2" pad="PIN24"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="DIO11">
<contactref element="U$2" pad="PIN8"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="DTR">
<contactref element="U$2" pad="PIN10"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="RTS">
<contactref element="U$2" pad="PIN29"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="SPI_CLK">
<contactref element="U$2" pad="PIN14"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="SPI_ATTN">
<contactref element="U$2" pad="PIN12"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="SPI_SSEL">
<contactref element="U$2" pad="PIN15"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="SPI_MOSI">
<contactref element="U$2" pad="PIN16"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="SPI_MISO">
<contactref element="U$2" pad="PIN17"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="RES2">
<contactref element="U$2" pad="PIN18"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="RES3">
<contactref element="U$2" pad="PIN19"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="RES8">
<contactref element="U$2" pad="PIN37"/>
<contactref element="JP4" pad="10"/>
</signal>
<signal name="RF_ANT">
<contactref element="U$2" pad="PIN36"/>
<contactref element="JP4" pad="9"/>
</signal>
<signal name="GND_RF">
<contactref element="U$2" pad="PIN35"/>
<contactref element="JP4" pad="8"/>
</signal>
<signal name="RES7">
<contactref element="U$2" pad="PIN34"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="RES6">
<contactref element="U$2" pad="PIN23"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="RES5">
<contactref element="U$2" pad="PIN21"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="RES4">
<contactref element="U$2" pad="PIN20"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N/C2">
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N/C3">
<contactref element="JP3" pad="1"/>
</signal>
<signal name="GND2">
<contactref element="U$2" pad="PIN11"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="GND3">
<contactref element="U$2" pad="PIN13"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="RES1">
<contactref element="U$2" pad="PIN9"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="GND4">
<contactref element="U$2" pad="PIN22"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="N/C1">
<contactref element="JP2" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
