(kicad_pcb (version 20171130) (host pcbnew "(5.1.8)-1")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 96)
    (zones 0)
    (modules 22)
    (nets 13)
  )
  (page A)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8 1.8)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 "Net-(D3-Pad1)")
  (net 8 "Net-(J1-Pad1)")
  (net 9 "Net-(J1-Pad3)")
  (net 10 "Net-(Q1-Pad2)")
  (net 11 "Net-(D4-Pad2)")
  (net 12 "Net-(R6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R6-Pad1)")
  )
  (module MountingHole:MountingHole_2.7mm locked (layer F.Cu) (tedit 56D1B4CB)
    (at 92.6465 122.301)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm locked (layer F.Cu) (tedit 56D1B4CB)
    (at 86.741 122.301)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 92.71 116.332)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm locked (layer F.Cu) (tedit 56D1B4CB)
    (at 86.741 116.332)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm_Pad_Via locked (layer F.Cu) (tedit 56DDBDB4)
    (at 79.8195 114.7445)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 -2.625) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.625 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 2.625) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 2.625 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module ESWITCH_DPDT_SLIDE:E-Switch-PBH2UEENAGX-0 (layer F.Cu) (tedit 600F83F1)
    (at 127 121.5)
    (fp_text reference SW1 (at -12.75 -4.65) (layer F.SilkS))
    (fp_text value PBH2UEENAGX (at -6.108 -6.319) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -4.100001 1.25 90) (size 1.8 1.8) (drill 1) (layers *.Cu))
    (pad 2 thru_hole circle (at -6.600001 1.25) (size 1.8 1.8) (drill 1) (layers *.Cu)
      (net 12 "Net-(R6-Pad1)"))
    (pad 3 thru_hole circle (at -9.100001 1.25) (size 1.8 1.8) (drill 1) (layers *.Cu)
      (net 9 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -4.100001 -1.25) (size 1.8 1.8) (drill 1) (layers *.Cu)
      (net 2 GND))
    (pad 5 thru_hole circle (at -6.600001 -1.25) (size 1.8 1.8) (drill 1) (layers *.Cu)
      (net 7 "Net-(D3-Pad1)"))
    (pad 6 thru_hole circle (at -9.100001 -1.25) (size 1.8 1.8) (drill 1) (layers *.Cu)
      (net 9 "Net-(J1-Pad3)"))
    (model D:/projects/KiCAD_projects/MyLibs/3dShapes/eec.models/PBH2UxxNAG1Rxxx.stp
      (offset (xyz 1.651 0 5.08))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 -180 90))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 102.7938 136.652)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 102.6 126.8)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 68k (at 3.65 -2.3) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 125.2 126.8 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value 1.5k (at 4.95 -2.3 90) (layer F.Fab))
    (fp_text user %R (at 5.0244 0.1544 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R6-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 6007D0F5)
    (at 99.314 124.714 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 3.3528 4.953) (layer F.SilkS))
    (fp_text value ".1 4p Header" (at 0 9.95) (layer F.Fab) hide)
    (fp_text user %R (at -1.8542 3.7338 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 95.25 126.75 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 5.25 1.95) (layer F.SilkS))
    (fp_text value 1N4148 (at 5 3.25) (layer F.Fab))
    (fp_text user %R (at 5.38 0) (layer F.Fab))
    (fp_text user K (at 0 -1.8) (layer F.Fab))
    (fp_text user K (at 0.635 2.036) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 90 140.5 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 5.1 -2.2 90) (layer F.SilkS))
    (fp_text value "1N4734 5.6v Zener" (at 5.08 2.47 90) (layer F.Fab))
    (fp_text user %R (at 5.47 0 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user K (at 3.086 2.456 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 102.4 131.6)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D3 (at 5.08 -2.47) (layer F.SilkS))
    (fp_text value 1N5819 (at 5.08 2.47) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.SilkS))
    (fp_text user K (at 0 -2.1) (layer F.Fab))
    (fp_text user %R (at 5.47 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm_Horizontal_O1.27mm_Z3.0mm (layer F.Cu) (tedit 5880A862)
    (at 129.413 139.5095 90)
    (descr "LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins")
    (tags "LED diameter 5.0mm z-position of LED center 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -1.96 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 10.93 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm_Horizontal_O1.27mm_Z3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 85 130.5306 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 4.8694 2.4 90) (layer F.SilkS))
    (fp_text value 8.2k (at 4.9694 3.5 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 96.774 130.302 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value 560 (at 5.2578 2.3876 90) (layer F.Fab))
    (fp_text user %R (at 5.4864 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 120.6 126.8 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value 1k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 4.826 -0.11 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 112.903 140.462 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -3.75) (layer F.SilkS))
    (fp_text value 33uf (at -1.383 -4.534) (layer F.Fab))
    (fp_text user %R (at 3.937 2.667 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.5mm_Pad_Via locked (layer F.Cu) (tedit 56DDBDB4)
    (at 79.8195 146.2405)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 2.625 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 2.625) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.856155 1.856155) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.625 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at -1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 -2.625) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 1.856155 -1.856155) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MountingHole:MountingHole_3.5mm locked (layer F.Cu) (tedit 56D1B4CB)
    (at 132.5245 114.4905)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm locked (layer F.Cu) (tedit 56D1B4CB)
    (at 132.5245 146.4945)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Package_TO_SOT_THT:TO-92L_HandSolder (layer F.Cu) (tedit 5A282C70)
    (at 104.0765 141.0335 180)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm, hand-soldering variant with enlarged pads (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.8) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 2 thru_hole roundrect (at 1.27 -1.27 180) (size 1.1 1.8) (drill 0.75 (offset 0 -0.4)) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole roundrect (at 2.54 0 180) (size 1.1 1.8) (drill 0.75 (offset 0 0.4)) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(J1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.1 1.8) (drill 0.75 (offset 0 0.4)) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92L.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text ESTART (at 104.775 121.92) (layer F.SilkS))
  (gr_text EKEY (at 103.759 124.333) (layer F.SilkS))
  (gr_text 12v/Vcc (at 105.664 119.38) (layer F.SilkS))
  (gr_text GND (at 103.251 116.713) (layer F.SilkS))
  (gr_text 07-Jan-2021 (at 119.38 116.84) (layer B.Mask))
  (gr_text "Sequitur Systems Group ZV" (at 129.54 115.57) (layer B.Mask))
  (dimension 60 (width 0.15) (layer Dwgs.User)
    (gr_text "60.000 mm" (at 106 102.84) (layer Dwgs.User))
    (feature1 (pts (xy 136 115.27) (xy 136 103.553579)))
    (feature2 (pts (xy 76 115.27) (xy 76 103.553579)))
    (crossbar (pts (xy 76 104.14) (xy 136 104.14)))
    (arrow1a (pts (xy 136 104.14) (xy 134.873496 104.726421)))
    (arrow1b (pts (xy 136 104.14) (xy 134.873496 103.553579)))
    (arrow2a (pts (xy 76 104.14) (xy 77.126504 104.726421)))
    (arrow2b (pts (xy 76 104.14) (xy 77.126504 103.553579)))
  )
  (gr_text "TunIcom v 1.1 " (at 120.65 144.78) (layer F.SilkS))
  (gr_arc (start 79 114) (end 79 111) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 79 147) (end 76 147) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 133 114) (end 136 114) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 133 147) (end 133 150) (angle -90) (layer Edge.Cuts) (width 0.1))
  (dimension 39 (width 0.15) (layer Dwgs.User)
    (gr_text "39.000 mm" (at 146.3 130.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 130 111) (xy 145.586421 111)))
    (feature2 (pts (xy 130 150) (xy 145.586421 150)))
    (crossbar (pts (xy 145 150) (xy 145 111)))
    (arrow1a (pts (xy 145 111) (xy 145.586421 112.126504)))
    (arrow1b (pts (xy 145 111) (xy 144.413579 112.126504)))
    (arrow2a (pts (xy 145 150) (xy 145.586421 148.873496)))
    (arrow2b (pts (xy 145 150) (xy 144.413579 148.873496)))
  )
  (gr_line (start 136 114) (end 136 147) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79 111) (end 133 110.998) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 76 147) (end 76 114) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133 150) (end 79 150) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137 151) (xy 74.93 151.13) (xy 75.4 109) (xy 137 109)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.085 152) (xy 73.66 152.4) (xy 73.83 108) (xy 137.915 108)
      )
    )
  )
  (zone (net 1) (net_name "Net-(C1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.01 126.925) (xy 119.197261 126.934519) (xy 119.350968 126.961492) (xy 119.478444 127.003538) (xy 119.587008 127.058278)
        (xy 119.683984 127.123331) (xy 119.776693 127.196317) (xy 119.872456 127.274857) (xy 119.978595 127.356571) (xy 120.102432 127.439078)
        (xy 120.251289 127.52) (xy 121 126.8) (xy 120.251289 126.08) (xy 120.102432 126.160921) (xy 119.978595 126.243428)
        (xy 119.872456 126.325142) (xy 119.776693 126.403682) (xy 119.683984 126.476668) (xy 119.587008 126.541721) (xy 119.478444 126.596461)
        (xy 119.350968 126.638507) (xy 119.197261 126.66548) (xy 119.01 126.675)
      )
    )
  )
  (zone (net 1) (net_name "Net-(C1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.35 126.675) (xy 114.162738 126.66548) (xy 114.009031 126.638507) (xy 113.881555 126.596461) (xy 113.772991 126.541721)
        (xy 113.676015 126.476668) (xy 113.583306 126.403682) (xy 113.487543 126.325142) (xy 113.381404 126.243428) (xy 113.257567 126.160921)
        (xy 113.108711 126.08) (xy 112.36 126.8) (xy 113.108711 127.52) (xy 113.257567 127.439078) (xy 113.381404 127.356571)
        (xy 113.487543 127.274857) (xy 113.583306 127.196317) (xy 113.676015 127.123331) (xy 113.772991 127.058278) (xy 113.881555 127.003538)
        (xy 114.009031 126.961492) (xy 114.162738 126.934519) (xy 114.35 126.925)
      )
    )
  )
  (zone (net 1) (net_name "Net-(C1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.724089 128.012687) (xy 111.863234 127.887004) (xy 111.990994 127.79739) (xy 112.110864 127.736982) (xy 112.226337 127.698922)
        (xy 112.340908 127.676349) (xy 112.458072 127.662404) (xy 112.581323 127.650225) (xy 112.714155 127.632954) (xy 112.860062 127.60373)
        (xy 113.02254 127.555693) (xy 113.042842 126.517158) (xy 112.004307 126.53746) (xy 111.956269 126.699937) (xy 111.927045 126.845844)
        (xy 111.909774 126.978676) (xy 111.897595 127.101927) (xy 111.88365 127.219091) (xy 111.861077 127.333662) (xy 111.823017 127.449135)
        (xy 111.762609 127.569005) (xy 111.672995 127.696765) (xy 111.547313 127.835911)
      )
    )
  )
  (zone (net 1) (net_name "Net-(C1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.3638 136.777) (xy 111.551061 136.786519) (xy 111.704768 136.813492) (xy 111.832244 136.855538) (xy 111.940808 136.910278)
        (xy 112.037784 136.975331) (xy 112.130493 137.048317) (xy 112.226256 137.126857) (xy 112.332395 137.208571) (xy 112.456232 137.291078)
        (xy 112.605089 137.372) (xy 113.3538 136.652) (xy 112.605089 135.932) (xy 112.456232 136.012921) (xy 112.332395 136.095428)
        (xy 112.226256 136.177142) (xy 112.130493 136.255682) (xy 112.037784 136.328668) (xy 111.940808 136.393721) (xy 111.832244 136.448461)
        (xy 111.704768 136.490507) (xy 111.551061 136.51748) (xy 111.3638 136.527)
      )
    )
  )
  (zone (net 1) (net_name "Net-(C1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.0788 138.242) (xy 113.088319 138.054738) (xy 113.115292 137.901031) (xy 113.157338 137.773555) (xy 113.212078 137.664991)
        (xy 113.277131 137.568015) (xy 113.350117 137.475306) (xy 113.428657 137.379543) (xy 113.510371 137.273404) (xy 113.592878 137.149567)
        (xy 113.6738 137.000711) (xy 112.9538 136.252) (xy 112.2338 137.000711) (xy 112.314721 137.149567) (xy 112.397228 137.273404)
        (xy 112.478942 137.379543) (xy 112.557482 137.475306) (xy 112.630468 137.568015) (xy 112.695521 137.664991) (xy 112.750261 137.773555)
        (xy 112.792307 137.901031) (xy 112.81928 138.054738) (xy 112.8288 138.242)
      )
    )
  )
  (zone (net 1) (net_name "Net-(C1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.8288 138.8612) (xy 112.819327 139.045946) (xy 112.792355 139.197485) (xy 112.750049 139.322934) (xy 112.694575 139.42941)
        (xy 112.628099 139.52403) (xy 112.552789 139.613913) (xy 112.47081 139.706174) (xy 112.384328 139.807931) (xy 112.29551 139.926302)
        (xy 112.206522 140.068405) (xy 112.877677 140.861197) (xy 113.643632 140.159571) (xy 113.570489 140.00194) (xy 113.494298 139.870652)
        (xy 113.41759 139.758143) (xy 113.342896 139.656852) (xy 113.272748 139.559216) (xy 113.209677 139.457674) (xy 113.156216 139.344663)
        (xy 113.114894 139.212622) (xy 113.088245 139.053988) (xy 113.0788 138.8612)
      )
    )
  )
  (zone (net 3) (net_name "Net-(D1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.125 125.16) (xy 95.11548 125.347261) (xy 95.088507 125.500968) (xy 95.046461 125.628444) (xy 94.991721 125.737008)
        (xy 94.926668 125.833984) (xy 94.853682 125.926693) (xy 94.775142 126.022456) (xy 94.693428 126.128595) (xy 94.610921 126.252432)
        (xy 94.53 126.401289) (xy 95.25 127.15) (xy 95.97 126.401289) (xy 95.889078 126.252432) (xy 95.806571 126.128595)
        (xy 95.724857 126.022456) (xy 95.646317 125.926693) (xy 95.573331 125.833984) (xy 95.508278 125.737008) (xy 95.453538 125.628444)
        (xy 95.411492 125.500968) (xy 95.384519 125.347261) (xy 95.375 125.16)
      )
    )
  )
  (zone (net 3) (net_name "Net-(D1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.524 122.299) (xy 97.735538 122.310084) (xy 97.908781 122.341455) (xy 98.052108 122.390289) (xy 98.173901 122.453765)
        (xy 98.282537 122.529059) (xy 98.386399 122.613348) (xy 98.493866 122.703809) (xy 98.613319 122.79762) (xy 98.753136 122.891958)
        (xy 98.9217 122.984) (xy 99.764 122.174) (xy 98.9217 121.364) (xy 98.753136 121.456041) (xy 98.613319 121.550379)
        (xy 98.493866 121.64419) (xy 98.386399 121.734651) (xy 98.282537 121.81894) (xy 98.173901 121.894234) (xy 98.052108 121.95771)
        (xy 97.908781 122.006544) (xy 97.735538 122.037915) (xy 97.524 122.049)
      )
    )
  )
  (zone (net 4) (net_name "Net-(D1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.215 128.34) (xy 85.224519 128.152738) (xy 85.251492 127.999031) (xy 85.293538 127.871555) (xy 85.348278 127.762991)
        (xy 85.413331 127.666015) (xy 85.486317 127.573306) (xy 85.564857 127.477543) (xy 85.646571 127.371404) (xy 85.729078 127.247567)
        (xy 85.81 127.098711) (xy 85.09 126.35) (xy 84.37 127.098711) (xy 84.450921 127.247567) (xy 84.533428 127.371404)
        (xy 84.615142 127.477543) (xy 84.693682 127.573306) (xy 84.766668 127.666015) (xy 84.831721 127.762991) (xy 84.886461 127.871555)
        (xy 84.928507 127.999031) (xy 84.95548 128.152738) (xy 84.965 128.34)
      )
    )
  )
  (zone (net 4) (net_name "Net-(D1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.965 128.9306) (xy 84.95553 129.112428) (xy 84.928477 129.261447) (xy 84.88588 129.384584) (xy 84.829773 129.488763)
        (xy 84.762194 129.580911) (xy 84.68518 129.667954) (xy 84.600766 129.756816) (xy 84.51099 129.854425) (xy 84.417889 129.967704)
        (xy 84.323498 130.103582) (xy 84.955283 130.928092) (xy 85.75447 130.264567) (xy 85.688117 130.101303) (xy 85.617381 129.965233)
        (xy 85.544939 129.848647) (xy 85.473469 129.743837) (xy 85.405649 129.643094) (xy 85.344155 129.538711) (xy 85.291666 129.422978)
        (xy 85.250858 129.288188) (xy 85.22441 129.126631) (xy 85.215 128.9306)
      )
    )
  )
  (zone (net 5) (net_name "Net-(D2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.81 140.625) (xy 88.070123 140.639213) (xy 88.282455 140.67938) (xy 88.457495 140.741792) (xy 88.605741 140.82274)
        (xy 88.737693 140.918515) (xy 88.863851 141.02541) (xy 88.994713 141.139714) (xy 89.14078 141.25772) (xy 89.312549 141.375718)
        (xy 89.520522 141.49) (xy 90.55 140.5) (xy 89.520522 139.51) (xy 89.312549 139.624281) (xy 89.14078 139.742279)
        (xy 88.994713 139.860285) (xy 88.863851 139.974589) (xy 88.737693 140.081484) (xy 88.605741 140.177259) (xy 88.457495 140.258207)
        (xy 88.282455 140.320619) (xy 88.070123 140.360786) (xy 87.81 140.375)
      )
    )
  )
  (zone (net 5) (net_name "Net-(D2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.5806 140.375) (xy 86.377601 140.365653) (xy 86.209594 140.339693) (xy 86.068599 140.300241) (xy 85.946642 140.250418)
        (xy 85.835745 140.193343) (xy 85.727931 140.132139) (xy 85.615224 140.069925) (xy 85.489646 140.009822) (xy 85.343221 139.954951)
        (xy 85.167973 139.908434) (xy 84.611416 140.785481) (xy 85.509545 141.307335) (xy 85.627243 141.2016) (xy 85.725671 141.099476)
        (xy 85.811172 141.002734) (xy 85.89009 140.913145) (xy 85.968769 140.83248) (xy 86.053552 140.76251) (xy 86.150783 140.705006)
        (xy 86.266805 140.661738) (xy 86.407963 140.634479) (xy 86.5806 140.625)
      )
    )
  )
  (zone (net 5) (net_name "Net-(D2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.1906 140.5656) (xy 91.943767 140.551508) (xy 91.743006 140.511238) (xy 91.57871 140.447795) (xy 91.441274 140.364185)
        (xy 91.32109 140.263412) (xy 91.208554 140.148484) (xy 91.094058 140.022406) (xy 90.967997 139.888183) (xy 90.820765 139.748821)
        (xy 90.642755 139.607327) (xy 89.458212 140.405314) (xy 90.301884 141.557764) (xy 90.537716 141.476951) (xy 90.733299 141.385713)
        (xy 90.899813 141.288509) (xy 91.048437 141.189799) (xy 91.190353 141.09404) (xy 91.336739 141.005692) (xy 91.498777 140.929216)
        (xy 91.687646 140.869068) (xy 91.914527 140.82971) (xy 92.1906 140.8156)
      )
    )
  )
  (zone (net 5) (net_name "Net-(D2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.204 140.8156) (xy 95.409534 140.824907) (xy 95.579963 140.850631) (xy 95.723328 140.889472) (xy 95.847671 140.938129)
        (xy 95.961034 140.993305) (xy 96.07146 141.051698) (xy 96.18699 141.110011) (xy 96.315666 141.164943) (xy 96.465531 141.213196)
        (xy 96.644626 141.251469) (xy 97.157457 140.348158) (xy 96.234794 139.871022) (xy 96.124371 139.980195) (xy 96.031852 140.085046)
        (xy 95.951133 140.183885) (xy 95.876115 140.275025) (xy 95.800694 140.356775) (xy 95.718769 140.427449) (xy 95.624239 140.485357)
        (xy 95.511002 140.52881) (xy 95.372956 140.556121) (xy 95.204 140.5656)
      )
    )
  )
  (zone (net 6) (net_name "Net-(D3-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119 137.125) (xy 119.191791 137.134457) (xy 119.349532 137.161166) (xy 119.48074 137.202632) (xy 119.592931 137.256359)
        (xy 119.693624 137.319854) (xy 119.790333 137.390621) (xy 119.890576 137.466165) (xy 120.001871 137.543992) (xy 120.131732 137.621607)
        (xy 120.287679 137.696515) (xy 120.9995 136.940025) (xy 120.215769 136.258313) (xy 120.072071 136.345703) (xy 119.952398 136.43326)
        (xy 119.849583 136.518777) (xy 119.756461 136.60005) (xy 119.665867 136.674871) (xy 119.570634 136.741035) (xy 119.463596 136.796335)
        (xy 119.337588 136.838567) (xy 119.185445 136.865524) (xy 119 136.875)
      )
    )
  )
  (zone (net 6) (net_name "Net-(D3-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.75 131.475) (xy 114.489876 131.460786) (xy 114.277544 131.420619) (xy 114.102504 131.358207) (xy 113.954258 131.277259)
        (xy 113.822306 131.181484) (xy 113.696148 131.074589) (xy 113.565286 130.960285) (xy 113.419219 130.842279) (xy 113.24745 130.724281)
        (xy 113.039478 130.61) (xy 112.01 131.6) (xy 113.039478 132.59) (xy 113.24745 132.475718) (xy 113.419219 132.35772)
        (xy 113.565286 132.239714) (xy 113.696148 132.12541) (xy 113.822306 132.018515) (xy 113.954258 131.92274) (xy 114.102504 131.841792)
        (xy 114.277544 131.77938) (xy 114.489876 131.739213) (xy 114.75 131.725)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.525 128.38) (xy 102.534479 128.20798) (xy 102.561752 128.067336) (xy 102.605071 127.951775) (xy 102.662689 127.855005)
        (xy 102.732859 127.770733) (xy 102.813833 127.692667) (xy 102.903864 127.614515) (xy 103.001205 127.529983) (xy 103.104108 127.43278)
        (xy 103.210826 127.316614) (xy 102.69935 126.412535) (xy 101.815951 126.958954) (xy 101.860582 127.135331) (xy 101.913909 127.282763)
        (xy 101.972777 127.409248) (xy 102.034031 127.522784) (xy 102.094516 127.63137) (xy 102.151078 127.743004) (xy 102.200561 127.865685)
        (xy 102.239813 128.007413) (xy 102.265677 128.176185) (xy 102.275 128.38)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.275 129.41) (xy 102.260786 129.670123) (xy 102.220619 129.882455) (xy 102.158207 130.057495) (xy 102.077259 130.205741)
        (xy 101.981484 130.337693) (xy 101.874589 130.463851) (xy 101.760285 130.594713) (xy 101.642279 130.74078) (xy 101.524281 130.912549)
        (xy 101.41 131.120522) (xy 102.4 132.15) (xy 103.39 131.120522) (xy 103.275718 130.912549) (xy 103.15772 130.74078)
        (xy 103.039714 130.594713) (xy 102.92541 130.463851) (xy 102.818515 130.337693) (xy 102.72274 130.205741) (xy 102.641792 130.057495)
        (xy 102.57938 129.882455) (xy 102.539213 129.670123) (xy 102.525 129.41)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.19 126.675) (xy 104.002738 126.66548) (xy 103.849031 126.638507) (xy 103.721555 126.596461) (xy 103.612991 126.541721)
        (xy 103.516015 126.476668) (xy 103.423306 126.403682) (xy 103.327543 126.325142) (xy 103.221404 126.243428) (xy 103.097567 126.160921)
        (xy 102.948711 126.08) (xy 102.2 126.8) (xy 102.948711 127.52) (xy 103.097567 127.439078) (xy 103.221404 127.356571)
        (xy 103.327543 127.274857) (xy 103.423306 127.196317) (xy 103.516015 127.123331) (xy 103.612991 127.058278) (xy 103.721555 127.003538)
        (xy 103.849031 126.961492) (xy 104.002738 126.934519) (xy 104.19 126.925)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.251 121.475044) (xy 119.273433 121.295136) (xy 119.336945 121.178437) (xy 119.435849 121.113252) (xy 119.564463 121.087886)
        (xy 119.717101 121.090642) (xy 119.888079 121.109827) (xy 120.071713 121.133744) (xy 120.262318 121.150698) (xy 120.45421 121.148993)
        (xy 120.641705 121.116936) (xy 120.737441 119.952288) (xy 119.569942 119.902143) (xy 119.484585 120.089269) (xy 119.401061 120.24723)
        (xy 119.321054 120.384477) (xy 119.246249 120.50946) (xy 119.178331 120.63063) (xy 119.118984 120.756437) (xy 119.069893 120.895332)
        (xy 119.032742 121.055764) (xy 119.009216 121.246184) (xy 119.001 121.475044)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.491 125.194) (xy 102.48155 125.382064) (xy 102.454718 125.536514) (xy 102.412776 125.664642) (xy 102.357997 125.773741)
        (xy 102.292656 125.871103) (xy 102.219024 125.964018) (xy 102.139375 126.05978) (xy 102.055983 126.165681) (xy 101.971121 126.289012)
        (xy 101.887063 126.437067) (xy 102.592062 127.199921) (xy 103.326779 126.465647) (xy 103.247707 126.312717) (xy 103.166824 126.185331)
        (xy 103.086516 126.076056) (xy 103.009172 125.977462) (xy 102.937177 125.882115) (xy 102.872919 125.782585) (xy 102.818785 125.671441)
        (xy 102.777162 125.541249) (xy 102.750438 125.384579) (xy 102.741 125.194)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.649 128.712) (xy 96.63948 128.899261) (xy 96.612507 129.052968) (xy 96.570461 129.180444) (xy 96.515721 129.289008)
        (xy 96.450668 129.385984) (xy 96.377682 129.478693) (xy 96.299142 129.574456) (xy 96.217428 129.680595) (xy 96.134921 129.804432)
        (xy 96.054 129.953289) (xy 96.774 130.702) (xy 97.494 129.953289) (xy 97.413078 129.804432) (xy 97.330571 129.680595)
        (xy 97.248857 129.574456) (xy 97.170317 129.478693) (xy 97.097331 129.385984) (xy 97.032278 129.289008) (xy 96.977538 129.180444)
        (xy 96.935492 129.052968) (xy 96.908519 128.899261) (xy 96.899 128.712)
      )
    )
  )
  (zone (net 8) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.677366 140.351143) (xy 100.762963 140.444673) (xy 100.825858 140.530167) (xy 100.87026 140.610034) (xy 100.900381 140.686685)
        (xy 100.92043 140.762529) (xy 100.934617 140.839975) (xy 100.947154 140.921436) (xy 100.962249 141.009319) (xy 100.984115 141.106036)
        (xy 101.016961 141.213996) (xy 101.730954 141.227954) (xy 101.716996 140.513961) (xy 101.609036 140.481115) (xy 101.512319 140.459249)
        (xy 101.424436 140.444154) (xy 101.342975 140.431617) (xy 101.265529 140.41743) (xy 101.189685 140.397381) (xy 101.113034 140.36726)
        (xy 101.033167 140.322858) (xy 100.947673 140.259963) (xy 100.854143 140.174366)
      )
    )
  )
  (zone (net 8) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.439 126.504) (xy 99.450084 126.292461) (xy 99.481455 126.119218) (xy 99.530289 125.975891) (xy 99.593765 125.854098)
        (xy 99.669059 125.745462) (xy 99.753348 125.6416) (xy 99.843809 125.534133) (xy 99.93762 125.41468) (xy 100.031958 125.274863)
        (xy 100.124 125.1063) (xy 99.314 124.264) (xy 98.504 125.1063) (xy 98.596041 125.274863) (xy 98.690379 125.41468)
        (xy 98.78419 125.534133) (xy 98.874651 125.6416) (xy 98.95894 125.745462) (xy 99.034234 125.854098) (xy 99.09771 125.975891)
        (xy 99.146544 126.119218) (xy 99.177915 126.292461) (xy 99.189 126.504)
      )
    )
  )
  (zone (net 9) (net_name "Net-(J1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.491332 118.279891) (xy 100.333914 118.421633) (xy 100.18923 118.521951) (xy 100.053351 118.588768) (xy 99.922347 118.630004)
        (xy 99.792289 118.653581) (xy 99.659246 118.667421) (xy 99.51929 118.679446) (xy 99.36849 118.697577) (xy 99.202918 118.729736)
        (xy 99.018643 118.783845) (xy 98.995802 119.952198) (xy 100.164155 119.929357) (xy 100.218263 119.745081) (xy 100.250422 119.579509)
        (xy 100.268553 119.428709) (xy 100.280578 119.288753) (xy 100.294418 119.15571) (xy 100.317995 119.025652) (xy 100.359231 118.894648)
        (xy 100.426048 118.758769) (xy 100.526366 118.614085) (xy 100.668109 118.456668)
      )
    )
  )
  (zone (net 9) (net_name "Net-(J1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.774999 120.96) (xy 117.763914 121.171538) (xy 117.732543 121.344781) (xy 117.683709 121.488108) (xy 117.620233 121.609901)
        (xy 117.544939 121.718537) (xy 117.46065 121.822399) (xy 117.370189 121.929866) (xy 117.276378 122.049319) (xy 117.18204 122.189136)
        (xy 117.089999 122.3577) (xy 117.899999 123.2) (xy 118.709999 122.3577) (xy 118.617957 122.189136) (xy 118.523619 122.049319)
        (xy 118.429808 121.929866) (xy 118.339347 121.822399) (xy 118.255058 121.718537) (xy 118.179764 121.609901) (xy 118.116288 121.488108)
        (xy 118.067454 121.344781) (xy 118.036083 121.171538) (xy 118.024999 120.96)
      )
    )
  )
  (zone (net 10) (net_name "Net-(Q1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.9188 138.242) (xy 102.928319 138.054738) (xy 102.955292 137.901031) (xy 102.997338 137.773555) (xy 103.052078 137.664991)
        (xy 103.117131 137.568015) (xy 103.190117 137.475306) (xy 103.268657 137.379543) (xy 103.350371 137.273404) (xy 103.432878 137.149567)
        (xy 103.5138 137.000711) (xy 102.7938 136.252) (xy 102.0738 137.000711) (xy 102.154721 137.149567) (xy 102.237228 137.273404)
        (xy 102.318942 137.379543) (xy 102.397482 137.475306) (xy 102.470468 137.568015) (xy 102.535521 137.664991) (xy 102.590261 137.773555)
        (xy 102.632307 137.901031) (xy 102.65928 138.054738) (xy 102.6688 138.242)
      )
    )
  )
  (zone (net 10) (net_name "Net-(Q1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.6688 141.2008) (xy 102.663263 141.330176) (xy 102.647502 141.4375) (xy 102.622789 141.527547) (xy 102.590399 141.605092)
        (xy 102.551604 141.674908) (xy 102.507677 141.741772) (xy 102.459893 141.810458) (xy 102.409524 141.885741) (xy 102.357843 141.972394)
        (xy 102.306124 142.075195) (xy 102.812817 142.578427) (xy 103.295862 142.052453) (xy 103.240335 141.953523) (xy 103.185585 141.870067)
        (xy 103.132806 141.79743) (xy 103.083191 141.730956) (xy 103.037934 141.665988) (xy 102.998229 141.597872) (xy 102.965269 141.52195)
        (xy 102.940248 141.433568) (xy 102.924361 141.32807) (xy 102.9188 141.2008)
      )
    )
  )
  (zone (net 11) (net_name "Net-(D4-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.79 136.835) (xy 126.602738 136.82548) (xy 126.449031 136.798507) (xy 126.321555 136.756461) (xy 126.212991 136.701721)
        (xy 126.116015 136.636668) (xy 126.023306 136.563682) (xy 125.927543 136.485142) (xy 125.821404 136.403428) (xy 125.697567 136.320921)
        (xy 125.548711 136.24) (xy 124.8 136.96) (xy 125.548711 137.68) (xy 125.697567 137.599078) (xy 125.821404 137.516571)
        (xy 125.927543 137.434857) (xy 126.023306 137.356317) (xy 126.116015 137.283331) (xy 126.212991 137.218278) (xy 126.321555 137.163538)
        (xy 126.449031 137.121492) (xy 126.602738 137.094519) (xy 126.79 137.085)
      )
    )
  )
  (zone (net 11) (net_name "Net-(D4-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.6135 137.085) (xy 127.825507 137.096039) (xy 127.999184 137.12732) (xy 128.14289 137.176084) (xy 128.264991 137.239574)
        (xy 128.373847 137.315031) (xy 128.477823 137.399699) (xy 128.58528 137.490818) (xy 128.704581 137.585632) (xy 128.844089 137.681382)
        (xy 129.012167 137.775311) (xy 129.862974 136.974252) (xy 129.029276 136.155403) (xy 128.858282 136.246337) (xy 128.716345 136.339709)
        (xy 128.59502 136.432691) (xy 128.485861 136.522453) (xy 128.380424 136.606166) (xy 128.270264 136.681003) (xy 128.146937 136.744133)
        (xy 128.001997 136.792729) (xy 127.826999 136.82396) (xy 127.6135 136.835)
      )
    )
  )
  (zone (net 12) (net_name "Net-(R6-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.788734 123.88628) (xy 121.642344 123.733174) (xy 121.53774 123.591558) (xy 121.466887 123.457739) (xy 121.42175 123.328028)
        (xy 121.394291 123.198734) (xy 121.376475 123.066165) (xy 121.360268 122.926631) (xy 121.337632 122.776442) (xy 121.300533 122.611906)
        (xy 121.240934 122.429333) (xy 120.072421 122.441468) (xy 120.130216 123.608613) (xy 120.316027 123.657182) (xy 120.482488 123.684372)
        (xy 120.633763 123.697982) (xy 120.774017 123.705812) (xy 120.907414 123.715665) (xy 121.038119 123.735339) (xy 121.170299 123.772636)
        (xy 121.308116 123.835356) (xy 121.455737 123.9313) (xy 121.617327 124.068268)
      )
    )
  )
  (zone (net 12) (net_name "Net-(R6-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.769873 126.095665) (xy 123.918422 126.24813) (xy 124.030641 126.387932) (xy 124.11508 126.517797) (xy 124.180287 126.64045)
        (xy 124.234811 126.758615) (xy 124.287201 126.875019) (xy 124.346006 126.992385) (xy 124.419775 127.11344) (xy 124.517056 127.240909)
        (xy 124.6464 127.377517) (xy 125.580537 126.923252) (xy 125.090111 126.007584) (xy 124.946991 126.03258) (xy 124.817676 126.062548)
        (xy 124.699341 126.092757) (xy 124.589163 126.118478) (xy 124.484319 126.13498) (xy 124.381986 126.137534) (xy 124.279338 126.121411)
        (xy 124.173554 126.08188) (xy 124.061809 126.014212) (xy 123.94128 125.913678)
      )
    )
  )
)
