(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 13)
    (no_connects 0)
    (area 118.918667 90.465 175.507238 117.915)
    (thickness 1.6)
    (drawings 10)
    (tracks 6)
    (zones 0)
    (modules 9)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.27)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 Earth)
  (net 3 "Net-(J2-Pad1)")
  (net 4 "Net-(J3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1.27)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Earth)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
  )
  (module WEA-RF:Manhattan2Pad (layer F.Cu) (tedit 59BAFBA2)
    (at 139.7 99.06 180)
    (fp_text reference J1 (at 0 5.08 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 13.208 -17.78 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -2.54 180) (size 3.81 2.54) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0 2.54 180) (size 3.81 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
  )
  (module WEA-RF:Manhattan2Pad (layer F.Cu) (tedit 59BAFBA7)
    (at 139.192 110.236)
    (fp_text reference J2 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at -15.24 -18.796) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -2.54) (size 3.81 2.54) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 0 2.54) (size 3.81 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
  )
  (module WEA-RF:Manhattan2Pad (layer F.Cu) (tedit 59BAFB97)
    (at 156.972 105.156)
    (fp_text reference J3 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 11.176 -12.192) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -2.54) (size 3.81 2.54) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 0 2.54) (size 3.81 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
  )
  (module WEA-RF:ADE-1+ (layer F.Cu) (tedit 59BAFB9D)
    (at 148.5011 105.0036)
    (fp_text reference U1 (at -1.27 5.08) (layer F.SilkS) hide)
    (fp_text value ADE-1+ (at 23.7109 -9.4996) (layer F.Fab) hide)
    (fp_text user 1 (at -3.81 -4.445) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -2.54) (size 2.54 1.651) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 2 smd rect (at -2.54 0) (size 2.54 1.651) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at -2.54 2.54) (size 2.54 1.651) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 4 smd rect (at 2.54 2.54) (size 2.54 1.651) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 5 smd rect (at 2.54 0) (size 2.54 1.651) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 6 smd rect (at 2.54 -2.54) (size 2.54 1.651) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J3-Pad1)"))
  )
  (module WEA-RF:VIA-0.6 (layer F.Cu) (tedit 59BAFFD7)
    (at 148.59 102.235)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value VIA-0.6 (at 0 -2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 Earth))
  )
  (module WEA-RF:VIA-0.6 (layer F.Cu) (tedit 59BAFFE1)
    (at 148.59 104.775)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value VIA-0.6 (at 0 -2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 Earth))
  )
  (module WEA-RF:VIA-0.6 (layer F.Cu) (tedit 59BAFFEA)
    (at 148.59 107.315)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value VIA-0.6 (at 0 -2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 Earth))
  )
  (module WEA-RF:VIA-0.6 (layer F.Cu) (tedit 59BAFFCD)
    (at 139.7 99.06)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value VIA-0.6 (at 0 -2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 Earth))
  )
  (module WEA-RF:VIA-0.6 (layer F.Cu) (tedit 59BAFFF8)
    (at 156.845 105.41)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value VIA-0.6 (at 0 -2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 Earth))
  )
  (gr_line (start 135.89 115.57) (end 137.16 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.89 93.98) (end 135.89 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.02 93.98) (end 135.89 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.02 115.57) (end 160.02 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.89 115.57) (end 160.02 115.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "WEA 2017" (at 153.035 113.03) (layer F.SilkS))
  (gr_text ADE-1+ (at 149.225 98.425) (layer F.SilkS))
  (gr_text LO (at 156.21 99.06) (layer F.SilkS))
  (gr_text RF (at 142.875 109.855) (layer F.SilkS))
  (gr_text IF (at 142.24 104.14) (layer F.SilkS))
  (zone (net 2) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.385 114.935) (xy 159.385 94.615) (xy 136.525 94.615) (xy 136.525 114.935)
      )
    )
  )
  (zone (net 2) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.525 94.615) (xy 159.385 94.615) (xy 159.385 114.935) (xy 136.525 114.935)
      )
    )
  )
)
