(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (gr_line (start 63.4 -28) (end 0 -28)
    (layer "Edge.Cuts"))
  (gr_line (start 100 0) (end 99.9999 -0.0001)
    (layer "Edge.Cuts"))
  (gr_line (start 29.4 -8) (end 29.4 0)
    (layer "Edge.Cuts"))
  (gr_line (start 0 -28) (end 0 -8)
    (layer "Edge.Cuts"))
  (gr_line (start 99.9999 -0.0001) (end 100 -21)
    (layer "Edge.Cuts"))
  (gr_line (start 29.4 0) (end 100 0)
    (layer "Edge.Cuts"))
  (gr_line (start 100 -21) (end 63.4 -21)
    (layer "Edge.Cuts"))
  (gr_line (start 0 -8) (end 29.4 -8)
    (layer "Edge.Cuts"))
  (gr_line (start 63.4 -21) (end 63.4 -28)
    (layer "Edge.Cuts"))
)
