(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~61~ubuntu18.04.1)
  (general
    (links 10)
    (no_connects 8)
    (area 144.924999 99.924999 156.575001 110.075001)
    (thickness 1.6002)
    (drawings 12)
    (tracks 27)
    (zones 0)
    (modules 5)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu power)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VCC)
  (net 2 /GND)
  (net 3 /PB0)
  (net 4 /PB1)
  (net 5 /PB3)
  (net 6 /PB2)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (net_class 0.25mm ""
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /GND)
    (add_net /PB0)
    (add_net /PB1)
    (add_net /PB2)
    (add_net /PB3)
    (add_net /VCC)
  )
  (net_class 0.2mm ""
    (clearance 0.1524)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (net_class 0.5mm ""
    (clearance 0.1524)
    (trace_width 0.5)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B3EEE63)
    (at 154.6 103)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user PB3 (at -1.88 0.04 90) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (fp_text user VCC (at -1.83 2.5 90) (layer B.SilkS))
    (fp_text user PB2 (at -1.84 5.03 90) (layer F.SilkS))
    (fp_text user PB3 (at -1.88 0.04 90) (layer B.SilkS))
    (fp_text user VCC (at -1.83 2.5 90) (layer F.SilkS))
    (fp_text user PB2 (at -1.84 5.03 90) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /PB3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VCC))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /PB2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B3EEAC2)
    (at 147 103)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user PBO (at 2 0 90) (layer B.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (fp_text user GND (at 2 2.5 90) (layer B.SilkS))
    (fp_text user PB1 (at 2 5 90) (layer F.SilkS))
    (fp_text user PBO (at 2 0 90) (layer F.SilkS))
    (fp_text user GND (at 2 2.5 90) (layer F.SilkS))
    (fp_text user PB1 (at 2 5 90) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /PB0))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /PB1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5B3EE97E)
    (at 150.95 106.5 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at -2.6 0.35 180) (layer F.SilkS))
    (fp_text value ATTINY10-TS (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 /PB0))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /PB1))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 /PB2))
    (pad 6 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /PB3))
    (pad 5 smd rect (at 1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 /VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5B3DB7D4)
    (at 151.65 103.25 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 1.73 0.31 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /VCC))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5B3DB7DD)
    (at 150.33 102.86 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.01 -0.01 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /VCC))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "ATtiny10 BO" (at 150.6 101.1) (layer B.SilkS))
  (gr_text SOT-23 (at 150.9 105.2 90) (layer B.SilkS))
  (gr_arc (start 155 101.5) (end 155 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 155 108.5) (end 156.5 108.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.5 108.5) (end 146.5 110) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.5 101.5) (end 145 101.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 10 (width 0.3) (layer Cmts.User)
    (gr_text "10.000 mm" (at 162.528919 105 270) (layer Cmts.User))
    (feature1 (pts (xy 156.678919 110) (xy 163.878919 110)))
    (feature2 (pts (xy 156.678919 100) (xy 163.878919 100)))
    (crossbar (pts (xy 161.178919 100) (xy 161.178919 110)))
    (arrow1a (pts (xy 161.178919 110) (xy 160.592498 108.873496)))
    (arrow1b (pts (xy 161.178919 110) (xy 161.76534 108.873496)))
    (arrow2a (pts (xy 161.178919 100) (xy 160.592498 101.126504)))
    (arrow2b (pts (xy 161.178919 100) (xy 161.76534 101.126504)))
  )
  (dimension 11.5 (width 0.3) (layer Cmts.User)
    (gr_text "11.500 mm" (at 150.75 91.65) (layer Cmts.User))
    (feature1 (pts (xy 156.5 100) (xy 156.5 90.3)))
    (feature2 (pts (xy 145 100) (xy 145 90.3)))
    (crossbar (pts (xy 145 93) (xy 156.5 93)))
    (arrow1a (pts (xy 156.5 93) (xy 155.373496 93.586421)))
    (arrow1b (pts (xy 156.5 93) (xy 155.373496 92.413579)))
    (arrow2a (pts (xy 145 93) (xy 146.126504 93.586421)))
    (arrow2b (pts (xy 145 93) (xy 146.126504 92.413579)))
  )
  (gr_line (start 155 100) (end 146.5 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.5 108.5) (end 156.5 101.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.5 110) (end 155 110) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145 101.5) (end 145 108.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145 100) (xy 145 110) (xy 156.5 110) (xy 156.5 100)
      )
    )
  )
  (zone (net 2) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145 100) (xy 156.5 100) (xy 156.5 110) (xy 145 110)
      )
    )
  )
)
