(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(DSP1-Vcc)")
	(net 2 "Net-(DSP1-SCL)")
	(net 3 "GND")
	(net 4 "Net-(DSP1-SDA)")
	(net 5 "Net-(U1-GPIO12)")
	(net 6 "unconnected-(U1-GPIO0-Pad1)")
	(net 7 "unconnected-(U1-GPIO3-Pad5)")
	(net 8 "unconnected-(U1-GPIO6-Pad9)")
	(net 9 "unconnected-(U1-GPIO11-Pad15)")
	(net 10 "unconnected-(U1-RUN-Pad30)")
	(net 11 "unconnected-(U1-GPIO22-Pad29)")
	(net 12 "unconnected-(U1-GPIO28_ADC2-Pad34)")
	(net 13 "unconnected-(U1-GPIO10-Pad14)")
	(net 14 "unconnected-(U1-GPIO21-Pad27)")
	(net 15 "unconnected-(U1-ADC_VREF-Pad35)")
	(net 16 "unconnected-(U1-SWCLK-Pad41)")
	(net 17 "unconnected-(U1-GPIO1-Pad2)")
	(net 18 "unconnected-(U1-GPIO9-Pad12)")
	(net 19 "unconnected-(U1-GPIO26_ADC0-Pad31)")
	(net 20 "unconnected-(U1-VBUS-Pad40)")
	(net 21 "unconnected-(U1-GPIO2-Pad4)")
	(net 22 "unconnected-(U1-GPIO7-Pad10)")
	(net 23 "unconnected-(U1-VSYS-Pad39)")
	(net 24 "unconnected-(U1-3V3_EN-Pad37)")
	(net 25 "unconnected-(U1-GPIO27_ADC1-Pad32)")
	(net 26 "unconnected-(U1-GPIO5-Pad7)")
	(net 27 "unconnected-(U1-SWDIO-Pad43)")
	(net 28 "unconnected-(U1-GPIO8-Pad11)")
	(net 29 "unconnected-(U1-GND-Pad42)")
	(net 30 "unconnected-(U1-GPIO4-Pad6)")
	(net 31 "Net-(U1-GPIO19)")
	(net 32 "Net-(U1-GPIO17)")
	(net 33 "Net-(U1-GPIO18)")
	(net 34 "Net-(U1-GPIO16)")
	(net 35 "Net-(U1-GPIO13)")
	(net 36 "Net-(BZ1-+)")
	(footprint "MCU_RaspberryPi_and_Boards:RPi_Pico_SMD_TH"
		(layer "F.Cu")
		(at 148.39 97.51 90)
		(descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x20 2.54mm double row")
		(property "Reference" "U1"
			(at 0 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Pico"
			(at 0 2.159 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "MCU_RaspberryPi_and_Boards:RPi_Pico_SMD_TH"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "GP5"
			(at -12.8 -8.89 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP11"
			(at -13.2 11.43 -45)
			(layer "F.SilkS")
		)
		(fp_text user "3V3"
			(at 12.9 -13.9 -45)
			(layer "F.SilkS")
		)
		(fp_text user "SWDIO"
			(at 5.6 26.2 -90)
			(layer "F.SilkS")
		)
		(fp_text user "GP21"
			(at 13.054 8.9 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP26"
			(at 13.054 -1.27 -45)
			(layer "F.SilkS")
		)
		(fp_text user "SWCLK"
			(at -5.7 26.2 -90)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -12.8 -19.05 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP28"
			(at 13.054 -9.144 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP8"
			(at -12.8 1.27 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP12"
			(at -13.2 13.97 -45)
			(layer "F.SilkS")
		)
		(fp_text user "VSYS"
			(at 13.2 -21.59 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP3"
			(at -12.8 -13.97 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP13"
			(at -13.054 16.51 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 12.8 6.35 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP2"
			(at -12.9 -16.51 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP9"
			(at -12.8 3.81 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP22"
			(at 13.054 3.81 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP19"
			(at 13.054 13.97 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP20"
			(at 13.054 11.43 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP14"
			(at -13.1 21.59 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP17"
			(at 13.054 21.59 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 12.8 -19.05 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP16"
			(at 13.054 24.13 -45)
			(layer "F.SilkS")
		)
		(fp_text user "3V3_EN"
			(at 13.7 -17.2 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP4"
			(at -12.8 -11.43 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -12.8 19.05 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP7"
			(at -12.7 -1.3 -45)
			(layer "F.SilkS")
		)
		(fp_text user "VBUS"
			(at 13.3 -24.2 -45)
			(layer "F.SilkS")
		)
		(fp_text user "ADC_VREF"
			(at 14 -12.5 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 12.8 19.05 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP1"
			(at -12.9 -21.6 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP0"
			(at -12.8 -24.13 -45)
			(layer "F.SilkS")
		)
		(fp_text user "RUN"
			(at 13 1.27 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -12.8 -6.35 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -12.8 6.35 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP18"
			(at 13.054 16.51 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP10"
			(at -13.054 8.89 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP15"
			(at -13.054 24.13 -45)
			(layer "F.SilkS")
		)
		(fp_text user "AGND"
			(at 13.054 -6.35 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP6"
			(at -12.8 -3.81 -45)
			(layer "F.SilkS")
		)
		(fp_text user "GP27"
			(at 13.054 -3.8 -45)
			(layer "F.SilkS")
		)
		(fp_text user "Copper Keepouts shown on Dwgs layer"
			(at 0.1 -30.2 -90)
			(layer "Cmts.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at -2.725 -24 90)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at -2.425 -20.97 90)
			(size 1.5 1.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 2.425 -20.97 90)
			(size 1.5 1.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 2.725 -24 90)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole oval
			(at -8.89 -24.13 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(U1-GPIO0-Pad1)")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "1" smd rect
			(at -8.89 -24.13 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 6 "unconnected-(U1-GPIO0-Pad1)")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole oval
			(at -8.89 -21.59 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(U1-GPIO1-Pad2)")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -8.89 -21.59 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 17 "unconnected-(U1-GPIO1-Pad2)")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole rect
			(at -8.89 -19.05 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -8.89 -19.05 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" thru_hole oval
			(at -8.89 -16.51 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(U1-GPIO2-Pad4)")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -8.89 -16.51 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 21 "unconnected-(U1-GPIO2-Pad4)")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole oval
			(at -8.89 -13.97 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(U1-GPIO3-Pad5)")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -8.89 -13.97 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 7 "unconnected-(U1-GPIO3-Pad5)")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole oval
			(at -8.89 -11.43 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(U1-GPIO4-Pad6)")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -8.89 -11.43 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 30 "unconnected-(U1-GPIO4-Pad6)")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole oval
			(at -8.89 -8.89 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(U1-GPIO5-Pad7)")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -8.89 -8.89 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 26 "unconnected-(U1-GPIO5-Pad7)")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole rect
			(at -8.89 -6.35 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at -8.89 -6.35 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" thru_hole oval
			(at -8.89 -3.81 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(U1-GPIO6-Pad9)")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -8.89 -3.81 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 8 "unconnected-(U1-GPIO6-Pad9)")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole oval
			(at -8.89 -1.27 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(U1-GPIO7-Pad10)")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -8.89 -1.27 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 22 "unconnected-(U1-GPIO7-Pad10)")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole oval
			(at -8.89 1.27 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(U1-GPIO8-Pad11)")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -8.89 1.27 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 28 "unconnected-(U1-GPIO8-Pad11)")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole oval
			(at -8.89 3.81 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(U1-GPIO9-Pad12)")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -8.89 3.81 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 18 "unconnected-(U1-GPIO9-Pad12)")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole rect
			(at -8.89 6.35 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at -8.89 6.35 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" thru_hole oval
			(at -8.89 8.89 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(U1-GPIO10-Pad14)")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -8.89 8.89 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 13 "unconnected-(U1-GPIO10-Pad14)")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole oval
			(at -8.89 11.43 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(U1-GPIO11-Pad15)")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -8.89 11.43 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 9 "unconnected-(U1-GPIO11-Pad15)")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole oval
			(at -8.89 13.97 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-GPIO12)")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at -8.89 13.97 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 5 "Net-(U1-GPIO12)")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole oval
			(at -8.89 16.51 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(U1-GPIO13)")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -8.89 16.51 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 35 "Net-(U1-GPIO13)")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole rect
			(at -8.89 19.05 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "18" smd rect
			(at -8.89 19.05 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "19" thru_hole oval
			(at -8.89 21.59 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(DSP1-SDA)")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at -8.89 21.59 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 4 "Net-(DSP1-SDA)")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole oval
			(at -8.89 24.13 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(DSP1-SCL)")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at -8.89 24.13 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "Net-(DSP1-SCL)")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole oval
			(at 8.89 24.13 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(U1-GPIO16)")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 8.89 24.13 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 34 "Net-(U1-GPIO16)")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 8.89 21.59 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(U1-GPIO17)")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 8.89 21.59 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 32 "Net-(U1-GPIO17)")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole rect
			(at 8.89 19.05 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "23" smd rect
			(at 8.89 19.05 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "24" thru_hole oval
			(at 8.89 16.51 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(U1-GPIO18)")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 8.89 16.51 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 33 "Net-(U1-GPIO18)")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole oval
			(at 8.89 13.97 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(U1-GPIO19)")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 8.89 13.97 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 31 "Net-(U1-GPIO19)")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole oval
			(at 8.89 11.43 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(BZ1-+)")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 8.89 11.43 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 36 "Net-(BZ1-+)")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole oval
			(at 8.89 8.89 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(U1-GPIO21-Pad27)")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 8.89 8.89 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 14 "unconnected-(U1-GPIO21-Pad27)")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole rect
			(at 8.89 6.35 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "28" smd rect
			(at 8.89 6.35 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "29" thru_hole oval
			(at 8.89 3.81 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(U1-GPIO22-Pad29)")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "29" smd rect
			(at 8.89 3.81 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 11 "unconnected-(U1-GPIO22-Pad29)")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole oval
			(at 8.89 1.27 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(U1-RUN-Pad30)")
			(pinfunction "RUN")
			(pintype "input")
		)
		(pad "30" smd rect
			(at 8.89 1.27 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 10 "unconnected-(U1-RUN-Pad30)")
			(pinfunction "RUN")
			(pintype "input")
		)
		(pad "31" thru_hole oval
			(at 8.89 -1.27 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(U1-GPIO26_ADC0-Pad31)")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at 8.89 -1.27 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 19 "unconnected-(U1-GPIO26_ADC0-Pad31)")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole oval
			(at 8.89 -3.81 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(U1-GPIO27_ADC1-Pad32)")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at 8.89 -3.81 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 25 "unconnected-(U1-GPIO27_ADC1-Pad32)")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
		)
		(pad "33" thru_hole rect
			(at 8.89 -6.35 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "33" smd rect
			(at 8.89 -6.35 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "34" thru_hole oval
			(at 8.89 -8.89 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(U1-GPIO28_ADC2-Pad34)")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at 8.89 -8.89 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 12 "unconnected-(U1-GPIO28_ADC2-Pad34)")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
		)
		(pad "35" thru_hole oval
			(at 8.89 -11.43 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(U1-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF")
			(pintype "power_in")
		)
		(pad "35" smd rect
			(at 8.89 -11.43 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 15 "unconnected-(U1-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF")
			(pintype "power_in")
		)
		(pad "36" thru_hole oval
			(at 8.89 -13.97 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(DSP1-Vcc)")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "36" smd rect
			(at 8.89 -13.97 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "Net-(DSP1-Vcc)")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "37" thru_hole oval
			(at 8.89 -16.51 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(U1-3V3_EN-Pad37)")
			(pinfunction "3V3_EN")
			(pintype "input")
		)
		(pad "37" smd rect
			(at 8.89 -16.51 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 24 "unconnected-(U1-3V3_EN-Pad37)")
			(pinfunction "3V3_EN")
			(pintype "input")
		)
		(pad "38" thru_hole rect
			(at 8.89 -19.05 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "38" smd rect
			(at 8.89 -19.05 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "39" thru_hole oval
			(at 8.89 -21.59 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(U1-VSYS-Pad39)")
			(pinfunction "VSYS")
			(pintype "power_in")
		)
		(pad "39" smd rect
			(at 8.89 -21.59 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 23 "unconnected-(U1-VSYS-Pad39)")
			(pinfunction "VSYS")
			(pintype "power_in")
		)
		(pad "40" thru_hole oval
			(at 8.89 -24.13 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(U1-VBUS-Pad40)")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "40" smd rect
			(at 8.89 -24.13 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 20 "unconnected-(U1-VBUS-Pad40)")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "41" thru_hole oval
			(at -2.54 23.9 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(U1-SWCLK-Pad41)")
			(pinfunction "SWCLK")
			(pintype "input")
		)
		(pad "41" smd rect
			(at -2.54 23.9 180)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 16 "unconnected-(U1-SWCLK-Pad41)")
			(pinfunction "SWCLK")
			(pintype "input")
		)
		(pad "42" thru_hole rect
			(at 0 23.9 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(U1-GND-Pad42)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "42" smd rect
			(at 0 23.9 180)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 29 "unconnected-(U1-GND-Pad42)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "43" thru_hole oval
			(at 2.54 23.9 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(U1-SWDIO-Pad43)")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
		)
		(pad "43" smd rect
			(at 2.54 23.9 180)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 27 "unconnected-(U1-SWDIO-Pad43)")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
		)
		(model "C:/Users/ncara/OneDrive/IoT/Tools/KiCad/RP-Pico Libraries/Pico.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/home/robscott/Documents/Electronics/KiCAD/Libraries/KiCad-RP-Pico-main/RP-Pico Libraries/Pico.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 90.39 83.51)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "REF**"
			(at 0 -4.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.5mm"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 180.39 83.51)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "REF**"
			(at 0 -4.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.5mm"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Buzzer_Beeper:Buzzer_12x9.5RM7.6"
		(layer "F.Cu")
		(at 177.39 101.71 -90)
		(descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
		(tags "buzzer")
		(property "Reference" "BZ1"
			(at 3.8 -7.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "Buzzer"
			(at 3.8 7.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Buzzer_Beeper:Buzzer_12x9.5RM7.6"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Buzzer, polarized"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "+"
			(at -0.01 -2.54 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 3.8 -4 90)
			(layer "F.Fab")
		)
		(fp_text user "+"
			(at -0.01 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0.455 0 180)
			(size 3 4)
			(drill 1.02
				(offset 0 1)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(BZ1-+)")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.145 0)
			(size 3 4)
			(drill 1.02
				(offset 0 1)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Buzzer_12x9.5RM7.6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ScottSystemsKiCAD:SH1306 I2C"
		(layer "F.Cu")
		(at 148.39 111.51)
		(property "Reference" "DSP1"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "ScottSystemsKiCAD:SH1306 I2C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "SH1306 I2C"
			(at -4 -7.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 3.81 0)
			(size 1.75 3)
			(drill 1
				(offset 0 0.75)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(DSP1-Vcc)")
			(pinfunction "Vcc")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole oval
			(at 1.27 0)
			(size 1.75 3)
			(drill 1
				(offset 0 0.75)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole oval
			(at -1.27 0)
			(size 1.75 3)
			(drill 1
				(offset 0 0.75)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(DSP1-SCL)")
			(pinfunction "SCL")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole oval
			(at -3.81 0)
			(size 1.75 3)
			(drill 1
				(offset 0 0.75)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(DSP1-SDA)")
			(pinfunction "SDA")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 210.39 109.51)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "REF**"
			(at 0 -4.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.5mm"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 106.39 109.51)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "REF**"
			(at 0 -4.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.5mm"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_3.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "B.Cu")
		(at 192.6 96.8 90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "SW3"
			(at 3.25 2 -90)
			(layer "B.SilkS")
		)
		(property "Value" "Right"
			(at 3.75 -6.7 -90)
			(layer "B.Fab")
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.25 -2.25 -90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 0)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -4.5)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(U1-GPIO18)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 -4.5)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(U1-GPIO18)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "B.Cu")
		(at 204.14 90.26 -90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "SW2"
			(at 3.25 2 90)
			(layer "B.SilkS")
		)
		(property "Value" "Left"
			(at 3.75 -6.7 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.25 -2.25 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(U1-GPIO17)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 -4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(U1-GPIO17)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "B.Cu")
		(at 108.6 91.8 90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "SW6"
			(at 3.25 2 -90)
			(layer "B.SilkS")
		)
		(property "Value" "Button 2"
			(at 3.75 -6.7 -90)
			(layer "B.Fab")
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.25 -2.25 -90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 0)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -4.5)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-GPIO12)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 -4.5)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-GPIO12)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "B.Cu")
		(at 88.14 95.26 -90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "SW5"
			(at 3.25 2 90)
			(layer "B.SilkS")
		)
		(property "Value" "Button 1"
			(at 3.75 -6.7 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.25 -2.25 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(U1-GPIO13)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 -4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(U1-GPIO13)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Symbol:OSHW-Logo_5.7x6mm_SilkScreen"
		(layer "B.Cu")
		(at 88.4 111 180)
		(descr "Open Source Hardware Logo")
		(tags "Logo OSHW")
		(property "Reference" "REF**"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "OSHW-Logo_5.7x6mm_SilkScreen"
			(at 0.75 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Symbol:OSHW-Logo_5.7x6mm_SilkScreen"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "B.Cu")
		(at 196.14 82.26 -90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "SW4"
			(at 3.25 2 90)
			(layer "B.SilkS")
		)
		(property "Value" "Down"
			(at 3.75 -6.7 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.1 -9.05 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(U1-GPIO16)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 -4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(U1-GPIO16)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_THT:SW_PUSH_6mm"
		(layer "B.Cu")
		(at 196.14 98.26 -90)
		(descr "Generic 6mm SW tactile push button")
		(tags "tact sw push 6mm")
		(property "Reference" "SW1"
			(at 3.25 2 90)
			(layer "B.SilkS")
		)
		(property "Value" "UP"
			(at 3.75 -6.7 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Button_Switch_THT:SW_PUSH_6mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.25 -2.25 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(U1-GPIO19)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 -4.5 180)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(U1-GPIO19)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 214.39 82.51)
		(end 214.39 112.51)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 214.39 112.51)
		(mid 212.925534 116.045534)
		(end 209.39 117.51)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.39 112.51)
		(end 82.39 82.51)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 87.39 117.51)
		(mid 83.854466 116.045534)
		(end 82.39 112.51)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 209.39 117.51)
		(end 87.39 117.51)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 209.39 77.51)
		(mid 212.925534 78.974466)
		(end 214.39 82.51)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 82.39 82.51)
		(mid 83.854466 78.974466)
		(end 87.39 77.51)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.39 77.51)
		(end 209.39 77.51)
		(layer "Edge.Cuts")
	)
	(gr_text "PicoCat Game Hat\n20240429"
		(at 194.4 112.8 0)
		(layer "F.Cu" knockout)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 82.39 77.51) (xy 82.39 117.51) (xy 214.39 117.51) (xy 214.39 77.51)
			)
		)
	)
)