(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 33)
    (no_connects 0)
    (area 133.399999 74.399999 164.350001 133.850001)
    (thickness 1.6)
    (drawings 11)
    (tracks 95)
    (zones 0)
    (modules 9)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 133.5 74.5)
    (visible_elements FFFEEFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +12V)
  (net 3 "Net-(P4-Pad2)")
  (net 4 "Net-(P4-Pad3)")
  (net 5 "Net-(D1-Pad1)")
  (net 6 +3V3)
  (net 7 /CS/LWAKE)
  (net 8 /FAULT)
  (net 9 /VBAT_RATIO)
  (net 10 /RXD)
  (net 11 /TXD)
  (net 12 /12V_UNPROTECTED)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net /12V_UNPROTECTED)
    (add_net /CS/LWAKE)
    (add_net /FAULT)
    (add_net /RXD)
    (add_net /TXD)
    (add_net /VBAT_RATIO)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5418A00F)
    (at 144.25 109.25 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /FAULT))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:BL652-SA (layer F.Cu) (tedit 580709F4)
    (at 157.5 102.5 270)
    (fp_text reference U2 (at 0 -3 270) (layer F.SilkS))
    (fp_text value BL652 (at -0.65 -3.3 270) (layer F.Fab))
    (pad 1 smd rect (at 4.9 -4.5 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.9 -3.75 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 4.9 -3 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 4.9 -2.25 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 4.9 -1.5 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P4-Pad2)"))
    (pad 6 smd rect (at 4.9 -0.75 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P4-Pad3)"))
    (pad 7 smd rect (at 4.9 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 4.9 0.75 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 4.9 1.5 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 4.9 2.25 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 4.9 3 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 4.9 3.75 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 4.9 4.5 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 4.9 5.25 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 4.9 6 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 4.9 6.75 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 3.75 7.2 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /FAULT))
    (pad 18 smd rect (at 3 7.2 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 2.25 7.2 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 1.5 7.2 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /VBAT_RATIO))
    (pad 21 smd rect (at 0.75 7.2 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /RXD))
    (pad 22 smd rect (at 0 7.2 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /CS/LWAKE))
    (pad 23 smd rect (at -0.75 7.2 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at -1.5 7.2 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /TXD))
    (pad 25 smd rect (at -2.25 7.2 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at -3 7.2 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 27 smd rect (at -3.75 7.2 180) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at -4.9 6.75 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at -4.9 6 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at -4.9 5.25 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd rect (at -4.9 4.5 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at -4.9 3.75 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at -4.9 3 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at -4.9 2.25 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd rect (at -4.9 1.5 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd rect (at -4.9 0.75 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at -4.9 0 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at -4.9 -0.75 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at -4.9 -1.5 270) (size 1.2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 574D9791)
    (at 144.25 102.5 180)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 5.25 180) (layer F.SilkS))
    (fp_text value MCP2050 (at 0 5.375 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /VBAT_RATIO))
    (pad 2 smd rect (at -2.7 -2.54 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /RXD))
    (pad 3 smd rect (at -2.7 -1.27 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /CS/LWAKE))
    (pad 4 smd rect (at -2.7 0 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 5 smd rect (at -2.7 1.27 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /TXD))
    (pad 6 smd rect (at -2.7 2.54 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.7 3.81 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 2.7 3.81 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 2.7 2.54 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 10 smd rect (at 2.7 1.27 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +12V))
    (pad 11 smd rect (at 2.7 0 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /FAULT))
    (pad 12 smd rect (at 2.7 -1.27 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 2.7 -2.54 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 2.7 -3.81 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 57A875DC)
    (at 136.75 99.25)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0 4.5) (layer F.SilkS))
    (fp_text value RSB36V (at 0.1 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5753A53E)
    (at 136.75 105.5 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value D (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 2 +12V))
    (pad 2 smd rect (at 1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 12 /12V_UNPROTECTED))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.00mm (layer F.Cu) (tedit 56FA75DA)
    (at 162 110 270)
    (descr "Through hole pin header, 1x04, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference P4 (at 0 8.5 270) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(P4-Pad3)"))
    (pad 4 thru_hole circle (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +3V3))
    (model /home/cpriscal/Projets/lin_modules/lin_bluetooth_gateway/Pin_Header_Straight_1x04_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 136.75 102.25)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +12V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Sabre_43160-XX03_03x7.49mm_Angled_BoardLock (layer F.Cu) (tedit 5794C14F)
    (at 156 91 180)
    (descr "Sabre™ Right Angle Header, 43160-XX03, http://www.molex.com/pdm_docs/sd/431601102_sd.pdf")
    (tags "connector molex sabre 43160")
    (fp_text reference P1 (at -5 0 180) (layer F.SilkS))
    (fp_text value MOLEX-0431603103 (at 7.49 17.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 12 /12V_UNPROTECTED))
    (pad 1 thru_hole rect (at 0 -3.18 180) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 12 /12V_UNPROTECTED))
    (pad 2 thru_hole circle (at 7.49 0 180) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 7.49 -3.18 180) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 3 thru_hole circle (at 14.98 0 180) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 14.98 -3.18 180) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -4.75 13.13 180) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 19.73 13.13 180) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (model /home/cpriscal/Projets/lin_modules/lin_bluetooth_gateway/Molex_Sabre_43160-XX03_03x7.49mm_Angled_BoardLock.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Sabre_43160-XX03_03x7.49mm_Angled_BoardLock (layer F.Cu) (tedit 5794C14F)
    (at 141.01 117.18)
    (descr "Sabre™ Right Angle Header, 43160-XX03, http://www.molex.com/pdm_docs/sd/431601102_sd.pdf")
    (tags "connector molex sabre 43160")
    (fp_text reference P2 (at -5 0) (layer F.SilkS))
    (fp_text value MOLEX-0431603103 (at 7.49 17.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 12 /12V_UNPROTECTED))
    (pad 1 thru_hole rect (at 0 -3.18) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 12 /12V_UNPROTECTED))
    (pad 2 thru_hole circle (at 7.49 0) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 7.49 -3.18) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 3 thru_hole circle (at 14.98 0) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 14.98 -3.18) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -4.75 13.13) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 19.73 13.13) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (model /home/cpriscal/Projets/lin_modules/lin_bluetooth_gateway/Molex_Sabre_43160-XX03_03x7.49mm_Angled_BoardLock.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 12V (at 158.5 94.25 270) (layer F.SilkS))
  (gr_text LIN (at 151 94.25 270) (layer F.SilkS))
  (gr_text GND (at 143.5 94.25 270) (layer F.SilkS))
  (gr_line (start 133.5 133.75) (end 133.5 74.5) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 164.25 133.75) (end 133.5 133.75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 164.25 74.5) (end 164.25 133.75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 133.5 74.5) (end 164.25 74.5) (layer Edge.Cuts) (width 0.2))
  (gr_text "LIN<->BLE Gateway\nRev 2, Nov 2016\nCedric Priscal" (at 148.5 102.5 180) (layer B.SilkS))
  (gr_text 12V (at 138.5 114 90) (layer F.SilkS))
  (gr_text GND (at 153.5 114 90) (layer F.SilkS))
  (gr_text LIN (at 146 114 90) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138 88.25) (xy 152 88.25) (xy 152 96.25) (xy 159.75 112) (xy 159.75 120.5)
        (xy 144.75 120.5) (xy 144.75 112) (xy 138 96.25)
      )
    )
  )
  (zone (net 12) (net_name /12V_UNPROTECTED) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.5 74.5) (xy 159.5 74.5) (xy 159.5 106.5) (xy 164.25 106.5) (xy 164.25 133.75)
        (xy 133.5 133.75) (xy 133.5 96.25) (xy 137.25 96.25) (xy 144 112) (xy 144 121.25)
        (xy 160.5 121.25) (xy 160.5 112) (xy 152.75 96.25) (xy 152.75 87.5) (xy 137.25 87.5)
        (xy 137.25 96.25) (xy 133.5 96.25)
      )
    )
  )
)
