(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 35)
    (tracks 110)
    (zones 0)
    (modules 22)
    (nets 97)
  )
  (page A4)
  (title_block
    (date "mar. 31 mars 2015")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.15)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 103.378 121.666)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "/52(SCK)")
  (net 3 "/53(SS)")
  (net 4 "/50(MISO)")
  (net 5 "/51(MOSI)")
  (net 6 /48)
  (net 7 /49)
  (net 8 /46)
  (net 9 /47)
  (net 10 /44)
  (net 11 /45)
  (net 12 /42)
  (net 13 /43)
  (net 14 /40)
  (net 15 /41)
  (net 16 /38)
  (net 17 /39)
  (net 18 /36)
  (net 19 /37)
  (net 20 /34)
  (net 21 /35)
  (net 22 /32)
  (net 23 /33)
  (net 24 /30)
  (net 25 /31)
  (net 26 /28)
  (net 27 /29)
  (net 28 /26)
  (net 29 /27)
  (net 30 /24)
  (net 31 /25)
  (net 32 /22)
  (net 33 /23)
  (net 34 +5V)
  (net 35 /IOREF)
  (net 36 /Reset)
  (net 37 /A0)
  (net 38 /A1)
  (net 39 /A2)
  (net 40 /A3)
  (net 41 /A4)
  (net 42 /A5)
  (net 43 /A6)
  (net 44 /A7)
  (net 45 /A8)
  (net 46 /A9)
  (net 47 /A10)
  (net 48 /A11)
  (net 49 /A12)
  (net 50 /A13)
  (net 51 /A14)
  (net 52 /A15)
  (net 53 /SCL)
  (net 54 /SDA)
  (net 55 /AREF)
  (net 56 "/13(**)")
  (net 57 "/12(**)")
  (net 58 "/20(SDA)")
  (net 59 "/21(SCL)")
  (net 60 "Net-(P8-Pad1)")
  (net 61 "Net-(P9-Pad1)")
  (net 62 "Net-(P10-Pad1)")
  (net 63 "Net-(P11-Pad1)")
  (net 64 "Net-(P12-Pad1)")
  (net 65 "Net-(P13-Pad1)")
  (net 66 "Net-(P2-Pad1)")
  (net 67 +3V3)
  (net 68 "/14(Tx3)")
  (net 69 "/15(Rx3)")
  (net 70 "/16(Tx2)")
  (net 71 "/17(Rx2)")
  (net 72 "/18(Tx1)")
  (net 73 "/19(Rx1)")
  (net 74 MOT1DIR)
  (net 75 +12V)
  (net 76 MOT1STEP)
  (net 77 "Net-(A1-Pad13)")
  (net 78 "Net-(A1-Pad6)")
  (net 79 "Net-(A1-Pad5)")
  (net 80 MS3)
  (net 81 "Net-(A1-Pad4)")
  (net 82 MS2)
  (net 83 "Net-(A1-Pad3)")
  (net 84 MS1)
  (net 85 MOTEN)
  (net 86 MOT2DIR)
  (net 87 MOT2STEP)
  (net 88 "Net-(A2-Pad13)")
  (net 89 "Net-(A2-Pad6)")
  (net 90 "Net-(A2-Pad5)")
  (net 91 "Net-(A2-Pad4)")
  (net 92 "Net-(A2-Pad3)")
  (net 93 BTKEY)
  (net 94 BTTXD)
  (net 95 BTRXD)
  (net 96 BTSTATE)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.381)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net "/12(**)")
    (add_net "/13(**)")
    (add_net "/14(Tx3)")
    (add_net "/15(Rx3)")
    (add_net "/16(Tx2)")
    (add_net "/17(Rx2)")
    (add_net "/18(Tx1)")
    (add_net "/19(Rx1)")
    (add_net "/20(SDA)")
    (add_net "/21(SCL)")
    (add_net /22)
    (add_net /23)
    (add_net /24)
    (add_net /25)
    (add_net /26)
    (add_net /27)
    (add_net /28)
    (add_net /29)
    (add_net /30)
    (add_net /31)
    (add_net /32)
    (add_net /33)
    (add_net /34)
    (add_net /35)
    (add_net /36)
    (add_net /37)
    (add_net /38)
    (add_net /39)
    (add_net /40)
    (add_net /41)
    (add_net /42)
    (add_net /43)
    (add_net /44)
    (add_net /45)
    (add_net /46)
    (add_net /47)
    (add_net /48)
    (add_net /49)
    (add_net "/50(MISO)")
    (add_net "/51(MOSI)")
    (add_net "/52(SCK)")
    (add_net "/53(SS)")
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /AREF)
    (add_net /IOREF)
    (add_net /Reset)
    (add_net /SCL)
    (add_net /SDA)
    (add_net BTKEY)
    (add_net BTRXD)
    (add_net BTSTATE)
    (add_net BTTXD)
    (add_net GND)
    (add_net MOT1DIR)
    (add_net MOT1STEP)
    (add_net MOT2DIR)
    (add_net MOT2STEP)
    (add_net MOTEN)
    (add_net MS1)
    (add_net MS2)
    (add_net MS3)
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A2-Pad13)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P11-Pad1)")
    (add_net "Net-(P12-Pad1)")
    (add_net "Net-(P13-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(P9-Pad1)")
  )
  (net_class +12v ""
    (clearance 0.254)
    (trace_width 1.524)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
  )
  (net_class +5v ""
    (clearance 0.2032)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (net_class Motor ""
    (clearance 0.2032)
    (trace_width 0.762)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad4)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A2-Pad3)")
    (add_net "Net-(A2-Pad4)")
    (add_net "Net-(A2-Pad5)")
    (add_net "Net-(A2-Pad6)")
  )
  (module Symbol:OSHW-Logo2_9.8x8mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 186.182 103.378)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_9.8x8mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A430)
    (at 176.784 76.708 90)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J4 (at 0 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_01x06_Female (at 0 15.47 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 BTKEY))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 BTTXD))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 BTRXD))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 BTSTATE))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_BarrelJack:BarrelJack_Horizontal (layer F.Cu) (tedit 5A1DBF6A)
    (at 113.792 114.046)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J3 (at -8.45 5.75) (layer F.SilkS))
    (fp_text value Barrel_Jack (at -6.2 -5.5) (layer F.Fab))
    (fp_text user %R (at -3 -2.95) (layer F.Fab))
    (pad 3 thru_hole roundrect (at -3 4.7) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (pad 2 thru_hole roundrect (at -6 0) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 75 +12V))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 116.078 94.996 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(A2-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(A2-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(A2-Pad4)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(A2-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 144.018 94.996 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(A1-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(A1-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(A1-Pad4)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(A1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 132.334 90.424)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1 -3.75) (layer F.SilkS))
    (fp_text value 100uF (at 1 3.75) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 +12V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 160.274 90.424)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1 -3.75) (layer F.SilkS))
    (fp_text value 100uF (at 1 3.75) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 +12V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:Pololu_Breakout-16_15.2x20.3mm (layer F.Cu) (tedit 58AB602C)
    (at 110.998 90.424 90)
    (descr "Pololu Breakout 16-pin 15.2x20.3mm 0.6x0.8\\")
    (tags "Pololu Breakout")
    (fp_text reference A2 (at 6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Pololu_Breakout_A4988 (at 6.35 20.17 90) (layer F.Fab))
    (fp_text user %R (at 6.35 0 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 MOT2DIR))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 +12V))
    (pad 15 thru_hole oval (at 12.7 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 MOT2STEP))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 12.7 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(A2-Pad13)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "Net-(A2-Pad6)"))
    (pad 13 thru_hole oval (at 12.7 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(A2-Pad13)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "Net-(A2-Pad5)"))
    (pad 12 thru_hole oval (at 12.7 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 MS3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 "Net-(A2-Pad4)"))
    (pad 11 thru_hole oval (at 12.7 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 MS2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "Net-(A2-Pad3)"))
    (pad 10 thru_hole oval (at 12.7 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 MS1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 +5V))
    (pad 9 thru_hole oval (at 12.7 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 MOTEN))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Module.3dshapes/Pololu_Breakout-16_15.2x20.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:Pololu_Breakout-16_15.2x20.3mm (layer F.Cu) (tedit 58AB602C)
    (at 138.938 90.424 90)
    (descr "Pololu Breakout 16-pin 15.2x20.3mm 0.6x0.8\\")
    (tags "Pololu Breakout")
    (fp_text reference A1 (at 6.35 -2.54 90) (layer F.SilkS))
    (fp_text value Pololu_Breakout_A4988 (at 6.35 20.17 90) (layer F.Fab))
    (fp_text user %R (at 6.35 0 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 MOT1DIR))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 +12V))
    (pad 15 thru_hole oval (at 12.7 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 MOT1STEP))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 12.7 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(A1-Pad13)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(A1-Pad6)"))
    (pad 13 thru_hole oval (at 12.7 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(A1-Pad13)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(A1-Pad5)"))
    (pad 12 thru_hole oval (at 12.7 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 MS3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(A1-Pad4)"))
    (pad 11 thru_hole oval (at 12.7 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 MS2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(A1-Pad3)"))
    (pad 10 thru_hole oval (at 12.7 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 MS1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 +5V))
    (pad 9 thru_hole oval (at 12.7 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 MOTEN))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Module.3dshapes/Pololu_Breakout-16_15.2x20.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Arduino_Mega:Socket_Strip_Arduino_2x18 locked (layer F.Cu) (tedit 55216789)
    (at 197.358 114.046 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 21.59 -2.794 90) (layer F.SilkS))
    (fp_text value Digital (at 21.59 -4.572 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "/52(SCK)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "/53(SS)"))
    (pad 5 thru_hole oval (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "/50(MISO)"))
    (pad 6 thru_hole oval (at 5.08 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "/51(MOSI)"))
    (pad 7 thru_hole oval (at 7.62 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /48))
    (pad 8 thru_hole oval (at 7.62 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /49))
    (pad 9 thru_hole oval (at 10.16 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /46))
    (pad 10 thru_hole oval (at 10.16 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /47))
    (pad 11 thru_hole oval (at 12.7 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /44))
    (pad 12 thru_hole oval (at 12.7 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /45))
    (pad 13 thru_hole oval (at 15.24 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /42))
    (pad 14 thru_hole oval (at 15.24 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /43))
    (pad 15 thru_hole oval (at 17.78 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /40))
    (pad 16 thru_hole oval (at 17.78 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /41))
    (pad 17 thru_hole oval (at 20.32 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /38))
    (pad 18 thru_hole oval (at 20.32 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /39))
    (pad 19 thru_hole oval (at 22.86 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /36))
    (pad 20 thru_hole oval (at 22.86 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /37))
    (pad 21 thru_hole oval (at 25.4 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /34))
    (pad 22 thru_hole oval (at 25.4 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /35))
    (pad 23 thru_hole oval (at 27.94 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /32))
    (pad 24 thru_hole oval (at 27.94 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /33))
    (pad 25 thru_hole oval (at 30.48 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /30))
    (pad 26 thru_hole oval (at 30.48 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /31))
    (pad 27 thru_hole oval (at 33.02 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /28))
    (pad 28 thru_hole oval (at 33.02 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /29))
    (pad 29 thru_hole oval (at 35.56 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /26))
    (pad 30 thru_hole oval (at 35.56 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /27))
    (pad 31 thru_hole oval (at 38.1 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /24))
    (pad 32 thru_hole oval (at 38.1 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /25))
    (pad 33 thru_hole oval (at 40.64 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /22))
    (pad 34 thru_hole oval (at 40.64 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /23))
    (pad 35 thru_hole oval (at 43.18 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 +5V))
    (pad 36 thru_hole oval (at 43.18 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 +5V))
    (model ${KIPRJMOD}/Socket_Arduino_Mega.3dshapes/Socket_header_Arduino_2x18.wrl
      (offset (xyz 21.58999967575073 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Mega:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 55216755)
    (at 131.318 119.126)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 8.89 -2.794) (layer F.SilkS))
    (fp_text value Power (at 8.89 -4.318) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /IOREF))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /Reset))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 +3V3))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 +5V))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 +12V))
    (model ${KIPRJMOD}/Socket_Arduino_Mega.3dshapes/Socket_header_Arduino_1x08.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Mega:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 5521677D)
    (at 154.178 119.126)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 8.89 -2.54) (layer F.SilkS))
    (fp_text value Analog (at 8.89 -4.318) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /A0))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /A1))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /A2))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /A3))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /A4))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /A5))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /A6))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /A7))
    (model ${KIPRJMOD}/Socket_Arduino_Mega.3dshapes/Socket_header_Arduino_1x08.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Mega:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 55216772)
    (at 177.038 119.126)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 8.89 -2.794) (layer F.SilkS))
    (fp_text value Analog (at 8.89 -4.318) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /A8))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /A9))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /A10))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /A11))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /A12))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /A13))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /A14))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /A15))
    (model ${KIPRJMOD}/Socket_Arduino_Mega.3dshapes/Socket_header_Arduino_1x08.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Mega:Socket_Strip_Arduino_1x10 locked (layer F.Cu) (tedit 551AFC9C)
    (at 122.174 70.866)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P5 (at 11.43 2.794) (layer F.SilkS))
    (fp_text value PWM (at 11.43 4.318) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /SCL))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /SDA))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /AREF))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 "/13(**)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 "/12(**)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 86 MOT2DIR))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 87 MOT2STEP))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 MOT1DIR))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 76 MOT1STEP))
    (model ${KIPRJMOD}/Socket_Arduino_Mega.3dshapes/Socket_header_Arduino_1x10.wrl
      (offset (xyz 11.42999982833862 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Mega:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 551AFC7F)
    (at 149.098 70.866)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P6 (at 8.89 2.794) (layer F.SilkS))
    (fp_text value PWM (at 8.89 4.318) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 MS3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 82 MS2))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 84 MS1))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 85 MOTEN))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 93 BTKEY))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 BTSTATE))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 BTRXD))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 94 BTTXD))
    (model ${KIPRJMOD}/Socket_Arduino_Mega.3dshapes/Socket_header_Arduino_1x08.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Mega:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 551AFC73)
    (at 171.958 70.866)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P7 (at 8.89 2.794) (layer F.SilkS))
    (fp_text value Communication (at 8.89 4.064) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 "/14(Tx3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "/15(Rx3)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "/16(Tx2)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 "/17(Rx2)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 "/18(Tx1)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 "/19(Rx1)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 "/20(SDA)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 "/21(SCL)"))
    (model ${KIPRJMOD}/Socket_Arduino_Mega.3dshapes/Socket_header_Arduino_1x08.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Mega:Arduino_1pin locked (layer F.Cu) (tedit 5524FDA7)
    (at 117.348 119.126)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P8 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(P8-Pad1)"))
  )
  (module Socket_Arduino_Mega:Arduino_1pin locked (layer F.Cu) (tedit 5524FDB2)
    (at 169.418 114.046)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P9 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(P9-Pad1)"))
  )
  (module Socket_Arduino_Mega:Arduino_1pin locked (layer F.Cu) (tedit 5524FDBB)
    (at 199.898 119.126)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P10 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(P10-Pad1)"))
  )
  (module Socket_Arduino_Mega:Arduino_1pin locked (layer F.Cu) (tedit 5524FDD2)
    (at 118.618 70.866)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P11 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(P11-Pad1)"))
  )
  (module Socket_Arduino_Mega:Arduino_1pin locked (layer F.Cu) (tedit 5524FDCA)
    (at 169.418 86.106)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P12 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(P12-Pad1)"))
  )
  (module Socket_Arduino_Mega:Arduino_1pin locked (layer F.Cu) (tedit 5524FDC4)
    (at 193.548 70.866)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P13 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(P13-Pad1)"))
  )
  (gr_text "ELV Motor" (at 119.888 97.282) (layer F.SilkS))
  (gr_text "RA Motor" (at 147.828 97.282) (layer F.SilkS))
  (gr_text VMOT (at 156.718 87.122 270) (layer F.SilkS))
  (gr_text VMOT (at 128.778 87.122 270) (layer F.SilkS))
  (gr_text +12V (at 118.11 114.046) (layer F.SilkS))
  (gr_text 100uF (at 161.29 93.98) (layer F.SilkS))
  (gr_text 100uF (at 133.35 93.98) (layer F.SilkS))
  (gr_text "Astrotracker\nMega 2560 shield\nRev 1" (at 185.928 110.236) (layer F.SilkS))
  (gr_text 1 (at 131.318 116.586 90) (layer F.SilkS))
  (gr_line (start 202.438 121.666) (end 103.378 121.666) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 202.438 120.396) (end 202.438 121.666) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.978 117.856) (end 202.438 120.396) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.978 83.566) (end 204.978 117.856) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 202.438 81.026) (end 204.978 83.566) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 202.438 70.866) (end 202.438 81.026) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.898 68.326) (end 202.438 70.866) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.378 68.326) (end 199.898 68.326) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.378 121.666) (end 103.378 68.326) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 202.438 70.866) (xy 202.438 81.026) (xy 204.978 83.566) (xy 204.978 117.856) (xy 202.438 120.396)
        (xy 202.438 121.666) (xy 103.378 121.666) (xy 103.378 68.326) (xy 199.898 68.326)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 202.438 70.866) (xy 202.438 81.026) (xy 204.978 83.566) (xy 204.978 117.856) (xy 202.438 120.396)
        (xy 202.438 121.666) (xy 103.378 121.666) (xy 103.378 68.326) (xy 199.898 68.326)
      )
    )
  )
)
