(kicad_pcb (version 4) (host pcbnew 4.1.0-alpha+201607031448+6962~45~ubuntu15.04.1-product)
  (general
    (links 0)
    (no_connects 0)
    (area 116.122572 34.4675 165.944429 88.983285)
    (thickness 1.6)
    (drawings 20)
    (tracks 159)
    (zones 0)
    (modules 16)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.59918 2.19964)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/donp/osh))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module aalay:aalay-LED1206 (layer F.Cu) (tedit 577AC723)
    (at 134.874 39.37)
    (attr smd)
    (fp_text reference pwr (at -1.27 1.524) (layer F.SilkS))
    (fp_text value >VALUE (at 0.508 2.032) (layer B.SilkS) hide)
    (pad A smd rect (at -1.5875 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask))
    (pad K smd rect (at 1.5875 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask))
  )
  (module aalay:aalay-LED1206 (layer F.Cu) (tedit 57B70DE1)
    (at 151.13 61.722 90)
    (attr smd)
    (fp_text reference status (at 1.016 -1.524 90) (layer F.SilkS))
    (fp_text value >VALUE (at 0.508 2.032 90) (layer B.SilkS) hide)
    (pad A smd rect (at -1.5875 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask))
    (pad K smd rect (at 1.5875 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57A03E1C)
    (at 139.7 78.994 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference NeoPx (at 0.254 -2.286 90) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x03 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57A04201)
    (at 149.9 41)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference TEMP (at 0 -2.3) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x03 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57A04211)
    (at 150 51.4)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference LIGHT (at 0 -2.3) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x03 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module aalay:aalay-SOT223 (layer F.Cu) (tedit 56F70B8E)
    (at 142.5 50.5)
    (descr "SOT223 PACKAGE")
    (tags "SOT223 PACKAGE")
    (attr smd)
    (fp_text reference LM1117 (at 0 -0.5) (layer F.SilkS))
    (fp_text value >VALUE (at 1.27 0.6858) (layer B.SilkS) hide)
    (pad GND smd rect (at -2.30886 3.0988) (size 1.21666 2.23266) (layers F.Cu F.Paste F.Mask))
    (pad OUT smd rect (at 0 3.0988) (size 1.21666 2.23266) (layers F.Cu F.Paste F.Mask))
    (pad IN smd rect (at 2.30886 3.0988) (size 1.21666 2.23266) (layers F.Cu F.Paste F.Mask))
    (pad OUT smd rect (at 0 -3.0988) (size 3.59918 2.19964) (layers F.Cu F.Paste F.Mask))
  )
  (module OPL-Antenna:OPL-Antenna-ANT2-SMD-9.5X2.1X1.0MM (layer F.Cu) (tedit 577AC5CE)
    (at 151.13 71.882 90)
    (attr smd)
    (fp_text reference "WIFI ANT" (at 0.3175 -1.7145 90) (layer F.SilkS))
    (fp_text value >VALUE (at 0.762 2.0955 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -4.7498 0 90) (size 1.39954 2.09804) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 4.7498 0 90) (size 1.39954 2.09804) (layers F.Cu F.Paste F.Mask))
  )
  (module Connect:USB_Micro-B_10103594-0001LF (layer F.Cu) (tedit 56F72406)
    (at 142.3 41.6 180)
    (descr "Micro USB Type B 10103594-0001LF")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference REF** (at -1.5 -4.625 180) (layer F.SilkS) hide)
    (fp_text value USB_Micro-B_10103594-0001LF (at 0 6.175 180) (layer F.Fab) hide)
    (pad +5 smd rect (at -1.3 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad D- smd rect (at -0.65 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad D+ smd rect (at -0.0009 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad ID smd rect (at 0.65 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad GND smd rect (at 1.3 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 thru_hole oval (at -2.425 -1.625 270) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 2.425 -1.625 270) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at -2.725 1.375 270) (size 1.7 1.2) (drill oval 1.2 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 2.725 1.375 270) (size 1.7 1.2) (drill oval 1.2 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 6 smd rect (at -0.9625 1.625 270) (size 2.5 1.425) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.9625 1.625 270) (size 2.5 1.425) (layers F.Cu F.Paste F.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 577AC73E)
    (at 135.128 44.196)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1) (layer F.SilkS))
    (fp_text value Pin_Header_Straight_1x06 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 577AC6FE)
    (at 135.763 41.656)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference "" (at 0 -1.9) (layer F.SilkS))
    (fp_text value R_0603 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57AE431C)
    (at 149.098 64.008 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference "" (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value R_0603 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 577AC7CE)
    (at 133.858 79.502)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 577AC7CA)
    (at 151.384 79.502)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference "" (at 0 -3.2) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module ESP8266:ESP-06 (layer F.Cu) (tedit 57B70D44)
    (at 140.716 67.818 90)
    (fp_text reference ESP-06 (at 0 3.302 90) (layer F.SilkS))
    (fp_text value ESP-06 (at 0 -0.5 90) (layer F.Fab))
    (fp_text user AI (at -5.65 -3.95 90) (layer F.SilkS))
    (fp_text user WIFI (at 4.25 -4.4 90) (layer F.SilkS))
    (fp_text user FCC (at -5.6 4.05 90) (layer F.SilkS))
    (pad GND smd rect (at -7.35 -5.85 90) (size 2 2) (layers F.Cu F.Paste F.Mask))
    (pad GP5 smd rect (at 7.35 -5.85 90) (size 2 2) (layers F.Cu F.Paste F.Mask))
    (pad GP16 smd rect (at -7.35 5.85 90) (size 2 2) (layers F.Cu F.Paste F.Mask))
    (pad GP15 smd rect (at 7.35 5.85 90) (size 2 2) (layers F.Cu F.Paste F.Mask))
    (pad GP14 smd rect (at -2.7 6.15 90) (size 1 1.2) (layers F.Cu F.Paste F.Mask))
    (pad GP12 smd rect (at 0 6.15 90) (size 1 1.2) (layers F.Cu F.Paste F.Mask))
    (pad GP13 smd rect (at 2.7 6.15 90) (size 1 1.2) (layers F.Cu F.Paste F.Mask))
    (pad TX smd rect (at 0 -6.15 90) (size 1 1.2) (layers F.Cu F.Paste F.Mask))
    (pad RST smd rect (at -2.7 -6.15 90) (size 1 1.2) (layers F.Cu F.Paste F.Mask))
    (pad RX smd rect (at 2.7 -6.15 90) (size 1 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 3.3 smd rect (at -7.75 0 90) (size 1.2 1) (layers F.Cu F.Paste F.Mask))
    (pad CHPD smd rect (at -7.75 2.9 90) (size 1.2 1) (layers F.Cu F.Paste F.Mask))
    (pad ANT smd rect (at -7.75 -2.9 90) (size 1.2 1) (layers F.Cu F.Paste F.Mask))
    (pad GP2 smd rect (at 7.75 0 90) (size 1.2 1) (layers F.Cu F.Paste F.Mask))
    (pad GP0 smd rect (at 7.75 -2.9 90) (size 1.2 1) (layers F.Cu F.Paste F.Mask))
    (pad GP4 smd rect (at 7.75 2.9 90) (size 1.2 1) (layers F.Cu F.Paste F.Mask))
    (pad GND smd rect (at -1.3 -1.3 90) (size 2 2) (layers F.Cu F.Paste F.Mask))
    (pad GND smd rect (at 1.3 -1.3 90) (size 2 2) (layers F.Cu F.Paste F.Mask))
    (pad GND smd rect (at -1.3 1.3 90) (size 2 2) (layers F.Cu F.Paste F.Mask))
    (pad GND smd rect (at 1.3 1.3 90) (size 2 2) (layers F.Cu F.Paste F.Mask))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57B7104D)
    (at 148.59 73.025)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -2) (layer F.SilkS))
    (fp_text value Measurement_Point_Round-SMD-Pad_Small (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57B71048)
    (at 132.969 72.39)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -2) (layer F.SilkS))
    (fp_text value Measurement_Point_Round-SMD-Pad_Small (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask))
  )
  (gr_text D (at 142.24 80.518 90) (layer F.SilkS))
  (gr_text G (at 144.78 80.518 90) (layer F.SilkS))
  (gr_text G0 (at 133.096 57.15) (layer F.SilkS))
  (gr_text G2 (at 133 54.3) (layer F.SilkS))
  (gr_text RX (at 133.1 51.8) (layer F.SilkS))
  (gr_text TX (at 133 49.3) (layer F.SilkS))
  (gr_text G (at 133.1 46.4) (layer F.SilkS))
  (gr_text +3 (at 132.9 44.1) (layer F.SilkS))
  (gr_text D (at 151.638 56.642) (layer F.SilkS))
  (gr_text D (at 152 46) (layer F.SilkS))
  (gr_text G (at 151.638 54.102) (layer F.SilkS))
  (gr_text G (at 152 43.6) (layer F.SilkS))
  (gr_text +5 (at 139.446 77.216 90) (layer F.SilkS))
  (gr_text +3 (at 151.892 51.562) (layer F.SilkS))
  (gr_text +3 (at 152.1 40.9) (layer F.SilkS))
  (gr_line (start 132 81) (end 153.3 81) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 132 38) (end 132 81) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 153.3 38) (end 132 38) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 153.3 38) (end 153.3 81) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_text "donp.org\nESP-FTL\n2016 Sep" (at 142.6 73.6) (layer B.SilkS))
)
