<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="48.26" y2="0" width="0" layer="20"/>
<wire x1="48.26" y1="0" x2="48.26" y2="40.64" width="0" layer="20"/>
<wire x1="48.26" y1="40.64" x2="0" y2="40.64" width="0" layer="20"/>
<wire x1="0" y1="40.64" x2="0" y2="0" width="0" layer="20"/>
<hole x="5.08" y="35.56" drill="3.048"/>
<hole x="43.18" y="35.56" drill="3.048"/>
<hole x="5.08" y="5.08" drill="3.048"/>
<hole x="43.18" y="5.08" drill="3.048"/>
<text>IN</text>
<text>OUT</text>
</plain>
<libraries>
<library name="untitled">
<packages>
<package name="DC_DC_5V">
</package>
<package name="DC_DC_6V">
</package>
<package name="MOLEX_2_PIN">
</package>
<package name="MOLEX_6_PIN">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="untitled" package="DC_DC_5V" value="DC_DC_5V"/>
<element name="U$2" library="untitled" package="DC_DC_5V" value="DC_DC_5V"/>
<element name="U$3" library="untitled" package="DC_DC_6V" value="DC_DC_6V"/>
<element name="U$4" library="untitled" package="MOLEX_2_PIN" value="MOLEX_CONNECTOR_2PIN"/>
<element name="U$5" library="untitled" package="MOLEX_6_PIN" value="MOLEX_CONNECTOR_6PIN"/>
</elements>
<signals>
<signal name="N$6">
<contactref element="U$2" pad="P$4"/>
<contactref element="U$5" pad="P$5"/>
</signal>
<signal name="N$7">
<contactref element="U$2" pad="P$3"/>
<contactref element="U$5" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="U$3" pad="P$4"/>
<contactref element="U$5" pad="P$4"/>
</signal>
<signal name="N$9">
<contactref element="U$3" pad="P$3"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="U$4" pad="P$1"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="U$4" pad="P$2"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$3" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$4"/>
<contactref element="U$5" pad="P$6"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="P$3"/>
<contactref element="U$5" pad="P$3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
