(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pin_1)")
  (net 2 "Net-(J1-Pin_2)")
  (net 3 "Net-(J1-Pin_4)")
  (net 4 "Net-(J1-Pin_6)")
  (net 5 "Net-(J1-Pin_8)")
  (net 6 "Net-(J2-Pin_2)")
  (net 7 "Net-(J2-Pin_4)")
  (net 8 "Net-(J2-Pin_6)")
  (net 9 "Net-(J2-Pin_8)")
  (net 10 "Net-(J3-Pin_8)")
  (net 11 "Net-(J3-Pin_6)")
  (net 12 "Net-(R3-Pad2)")
  (net 13 "Net-(R5-Pad2)")
  (net 14 "Net-(R10-Pad1)")
  (net 15 "Net-(R11-Pad2)")
  (net 16 "Net-(R15-Pad2)")
  (net 17 "Net-(R17-Pad2)")
  (net 18 "Net-(R21-Pad2)")
  (net 19 "Net-(R23-Pad2)")
  (net 20 "Net-(R27-Pad2)")
  (net 21 "Net-(R29-Pad2)")
  (net 22 "Net-(J3-Pin_4)")
  (net 23 "Net-(J3-Pin_2)")
  (net 24 "Net-(J4-Pin_2)")
  (net 25 "Net-(J4-Pin_4)")
  (net 26 "Net-(J4-Pin_6)")
  (net 27 "Net-(J4-Pin_8)")
  (net 28 "Net-(J5-Pin_2)")
  (net 29 "Net-(J5-Pin_4)")
  (net 30 "Net-(J5-Pin_6)")
  (net 31 "Net-(J5-Pin_8)")
  (footprint "my_footprints:My_Hole_2.1mm" (layer "F.Cu")
    (at 116.459 98.679)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "My_Hole_2.1mm" (at 0 3.2) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 149.108 90.175 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "1K" (at 1.27 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x04" (at 1.27 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J2-Pin_8)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(J3-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(J3-Pin_2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(J3-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(J3-Pin_4)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J3-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J3-Pin_6)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J3-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 192.405 88.9 -90)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x01, this symbol is compatible with counter-clockwise, top-bottom and odd-even numbering schemes., script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "OUT" (at 1.27 2.54 -90) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x01" (at 1.27 2.33 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(J5-Pin_8)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (at 192.024 93.98)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(J5-Pin_8)"))
  )
  (footprint "my_footprints:My_Hole_2.1mm" (layer "F.Cu")
    (at 160.528 88.519)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "My_Hole_2.1mm" (at 0 3.2) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "my_footprints:My_Hole_2.1mm" (layer "F.Cu")
    (at 192.151 98.679)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "My_Hole_2.1mm" (at 0 3.2) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "my_footprints:My_Hole_2.1mm" (layer "F.Cu")
    (at 145.288 88.519)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "My_Hole_2.1mm" (at 0 3.2) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 118.628 90.175 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "100K" (at 1.27 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x04" (at 1.27 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-Pin_2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J1-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J1-Pin_4)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J1-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J1-Pin_6)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 164.221 90.175 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "100" (at 1.27 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x04" (at 1.27 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J3-Pin_8)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(J4-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(J4-Pin_2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(J4-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(J4-Pin_4)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(J4-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(J4-Pin_6)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(J4-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 133.868 90.175 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "10K" (at 1.27 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x04" (at 1.27 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_8)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J2-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J2-Pin_2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J2-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J2-Pin_4)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J2-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J2-Pin_6)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J2-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 179.334 90.175 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "10" (at 1.27 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x04" (at 1.27 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(J4-Pin_8)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(J5-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(J5-Pin_2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(J5-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(J5-Pin_4)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(J5-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(J5-Pin_6)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(J5-Pin_8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "my_footprints:My_Hole_2.1mm" (layer "F.Cu")
    (at 130.048 88.519)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "My_Hole_2.1mm" (at 0 3.2) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "my_footprints:my_TestPoint" (layer "F.Cu")
    (at 192.024 86.36)
    (descr "Keystone Miniature THM Test Point 5000-5004, http://www.keyelco.com/product-pdf.cfm?p=1309")
    (tags "Through Hole Mount Test Points")
    (attr through_hole)
    (fp_text reference " " (at 0 -2.373) (layer "F.SilkS"))
    (fp_text value "my_TestPoint" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pin_1)"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5000-5004_Miniature.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "my_footprints:My_Hole_2.1mm" (layer "F.Cu")
    (at 175.514 88.519)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "My_Hole_2.1mm" (at 0 3.2) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 168.021 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "1" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 25 "Net-(J4-Pin_4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 18 "Net-(R21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 163.0065 96.012)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 24 "Net-(J4-Pin_2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 25 "Net-(J4-Pin_4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 188.214 96.012 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R29" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 30 "Net-(J5-Pin_6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 21 "Net-(R29-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 157.988 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 17 "Net-(R17-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 10 "Net-(J3-Pin_8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 188.214 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R30" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 21 "Net-(R29-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 31 "Net-(J5-Pin_8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 147.828 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "1" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 9 "Net-(J2-Pin_8)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 23 "Net-(J3-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 183.134 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R27" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "1" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 29 "Net-(J5-Pin_4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 20 "Net-(R27-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 122.428 96.012 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 12 "Net-(R3-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 4 "Net-(J1-Pin_6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 172.974 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 19 "Net-(R23-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 27 "Net-(J4-Pin_8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 137.668 96.012 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 14 "Net-(R10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 8 "Net-(J2-Pin_6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 132.588 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "1" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 5 "Net-(J1-Pin_8)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 6 "Net-(J2-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 117.348 96.012)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 2 "Net-(J1-Pin_2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 3 "Net-(J1-Pin_4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 178.054 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R25" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "1" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 27 "Net-(J4-Pin_8)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 28 "Net-(J5-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 157.988 96.012 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 11 "Net-(J3-Pin_6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 17 "Net-(R17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 172.974 96.012 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 26 "Net-(J4-Pin_6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 19 "Net-(R23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 147.828 96.012)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 23 "Net-(J3-Pin_2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 22 "Net-(J3-Pin_4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 137.668 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "1" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 7 "Net-(J2-Pin_4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 14 "Net-(R10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 122.428 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "1" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 3 "Net-(J1-Pin_4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 12 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 163.0065 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "1" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 10 "Net-(J3-Pin_8)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 24 "Net-(J4-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 142.748 96.012 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 8 "Net-(J2-Pin_6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 15 "Net-(R11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 117.348 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "1" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 1 "Net-(J1-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 2 "Net-(J1-Pin_2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 168.021 96.012 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 18 "Net-(R21-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 26 "Net-(J4-Pin_6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 142.748 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 15 "Net-(R11-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 9 "Net-(J2-Pin_8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 127.508 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0.127 1.778) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 13 "Net-(R5-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 5 "Net-(J1-Pin_8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 178.054 96.012)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R26" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 28 "Net-(J5-Pin_2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 29 "Net-(J5-Pin_4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 152.908 93.345)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "1" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 22 "Net-(J3-Pin_4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 16 "Net-(R15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 127.508 96.012 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 4 "Net-(J1-Pin_6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 13 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 132.588 96.012)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 6 "Net-(J2-Pin_2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 7 "Net-(J2-Pin_4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 183.134 96.012 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R28" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 20 "Net-(R27-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 30 "Net-(J5-Pin_6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 152.908 96.012 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "5_decade_resistor_R2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at 0 1.82) (layer "B.SilkS") hide)
    (fp_text value "2" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 16 "Net-(R15-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 11 "Net-(J3-Pin_6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 194.31 99.664185) (mid 194.086815 100.203) (end 193.548 100.426185)
    (layer "Edge.Cuts"))
  (gr_line (start 193.548 100.426185) (end 115.062 100.426185)
    (layer "Edge.Cuts"))
  (gr_arc (start 114.3 84.709) (mid 114.560382 84.080382) (end 115.189 83.82)
    (layer "Edge.Cuts"))
  (gr_arc (start 193.421 83.82) (mid 194.049618 84.080382) (end 194.31 84.709)
    (layer "Edge.Cuts"))
  (gr_arc (start 115.062 100.426185) (mid 114.523185 100.203) (end 114.3 99.664185)
    (layer "Edge.Cuts"))
  (gr_line (start 114.3 99.664185) (end 114.3 84.709)
    (layer "Edge.Cuts"))
  (gr_line (start 115.189 83.82) (end 193.421 83.82)
    (layer "Edge.Cuts"))
  (gr_line (start 194.31 84.709) (end 194.31 99.664185)
    (layer "Edge.Cuts"))
  (gr_text "jbs" (at 175.768 93.472) (layer "F.Cu"))
  (gr_text "5_decade_resistor_R2.kicad_pcb 4-12-2025" (at 175.387 85.09) (layer "B.Cu"))
  (gr_text "jbs" (at 129.794 85.725) (layer "B.Cu"))
  (gr_text "1" (at 122.428 93.345) (layer "B.SilkS"))
  (gr_text "10K" (at 137.668 97.79) (layer "B.SilkS"))
  (gr_text "1" (at 147.828 93.345) (layer "B.SilkS"))
  (gr_text "1K" (at 152.908 97.79) (layer "B.SilkS"))
  (gr_text "1" (at 168.021 93.345) (layer "B.SilkS"))
  (gr_text "1" (at 137.668 93.345) (layer "B.SilkS"))
  (gr_text "1" (at 132.588 93.345) (layer "B.SilkS"))
  (gr_text "1" (at 162.941 93.345) (layer "B.SilkS"))
  (gr_text "1" (at 152.781 93.345) (layer "B.SilkS"))
  (gr_text "100K" (at 122.555 97.79) (layer "B.SilkS"))
  (gr_text "100" (at 168.021 97.79) (layer "B.SilkS"))
  (gr_text "10" (at 183.134 97.79) (layer "B.SilkS"))
  (gr_text "1" (at 117.348 93.345) (layer "B.SilkS"))
  (gr_text "1" (at 178.054 93.345) (layer "B.SilkS"))
  (gr_text "1" (at 183.134 93.345) (layer "B.SilkS"))
  (gr_text "Resistors: 0.1%, 0.25W, 25 PPM/ C, 200V Max." (at 175.641 85.09) (layer "F.SilkS"))
  (gr_text "5 DECADE RESISTOR: 0 TO 1,111,100 Ohms in 10 Ohm steps" (at 117.348 84.963) (layer "F.SilkS"))
  (gr_text "200" (at 166.751 94.869 90) (layer "F.SilkS"))
  (gr_text "200K" (at 121.158 94.869 90) (layer "F.SilkS"))
  (gr_text "40K" (at 141.478 94.869 90) (layer "F.SilkS"))
  (gr_text "400K" (at 126.238 94.869 90) (layer "F.SilkS"))
  (gr_text "Total Resistance in Ohms = Sum of all values with shunts removed" (at 153.289 98.933) (layer "F.SilkS"))
  (gr_text "10K" (at 133.858 94.869 90) (layer "F.SilkS"))
  (gr_text "2K" (at 151.638 94.869 90) (layer "F.SilkS"))
  (gr_text "100" (at 164.211 94.869 90) (layer "F.SilkS"))
  (gr_text "30K" (at 138.938 94.869 90) (layer "F.SilkS"))
  (gr_text "4K" (at 156.718 94.869 90) (layer "F.SilkS"))
  (gr_text "300K" (at 123.698 94.869 90) (layer "F.SilkS"))
  (gr_text "10" (at 179.324 94.869 90) (layer "F.SilkS"))
  (gr_text "20K" (at 136.398 94.869 90) (layer "F.SilkS"))
  (gr_text "1K" (at 149.098 94.869 90) (layer "F.SilkS"))
  (gr_text "300" (at 169.291 94.869 90) (layer "F.SilkS"))
  (gr_text "30" (at 184.404 94.869 90) (layer "F.SilkS"))
  (gr_text "20" (at 181.864 94.869 90) (layer "F.SilkS"))
  (gr_text "3K" (at 154.178 94.869 90) (layer "F.SilkS"))
  (gr_text "40" (at 186.944 94.869 90) (layer "F.SilkS"))
  (gr_text "100K" (at 118.618 94.869 90) (layer "F.SilkS"))
  (gr_text "400" (at 171.831 94.869 90) (layer "F.SilkS"))
  (gr_text "jbs" (at 129.794 85.725) (layer "B.Mask"))
  (gr_text "jbs" (at 175.768 93.472) (layer "F.Mask"))
)
