(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 14)
    (zones 0)
    (modules 4)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.6 5.6)
    (pad_drill 2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (gerberprecision 5)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber-files/"))
  )
  (net 0 "")
  (net 1 /+input)
  (net 2 /GND)
  (net 3 /+protected)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1.8)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+input)
    (add_net /+protected)
    (add_net /GND)
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5F386838)
    (at 83 52.5)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference J2 (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value gnd (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 2) (layers *.Cu *.Mask)
      (net 2 /GND))
  )
  (module MountingHole:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5DFE13F3)
    (at 94.5 52.5)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference J3 (at 0 -4.5) (layer F.SilkS))
    (fp_text value 105-1102-001 (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 13 13) (layers B.Cu B.Paste B.Mask)
      (net 3 /+protected))
  )
  (module MountingHole:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5F386222)
    (at 94.5 52.5)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference J1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value "spring 11m PAD" (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 13 10) (layers F.Cu F.Paste F.Mask)
      (net 1 /+input))
  )
  (module Package_TO_SOT_SMD:TO-252-3_TabPin4 (layer F.Cu) (tedit 5F362AF3)
    (at 93.5 43)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference Q1 (at 6.8 0) (layer F.SilkS))
    (fp_text value IRLR9343TRPBF (at 1 4) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 3 smd rect (at -4.2 2.28) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /+input))
    (pad 4 smd rect (at 2.1 0) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 3 /+protected))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-252-3_TabPin4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text krbhvee@online.no (at 103 52.5 90) (layer F.SilkS))
  (gr_text "DC -" (at 84 57.5) (layer B.SilkS))
  (gr_text DC+ (at 94.5 60.5) (layer F.SilkS))
  (gr_text IN (at 94 62.5) (layer F.SilkS))
  (gr_text "DC -" (at 84.5 57.5) (layer F.SilkS))
  (gr_text "  DC+ \nOUT" (at 94.5 62.5) (layer B.SilkS))
  (gr_circle (center 94.5 52.5) (end 110 52.5) (layer Edge.Cuts) (width 0.2))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99 37) (xy 104 39.5) (xy 107.5 43) (xy 110 47.5) (xy 110.5 52)
        (xy 110 56.5) (xy 107.5 62.5) (xy 103.5 65.5) (xy 97.5 68.5) (xy 91 68)
        (xy 87 66.5) (xy 84 64.5) (xy 81 61.5) (xy 79 56) (xy 78.5 52)
        (xy 79 47.5) (xy 81 43.5) (xy 84 40.5) (xy 89 37.5) (xy 94 36.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98 37) (xy 101 38) (xy 104.5 40) (xy 107.5 43) (xy 109.5 46.5)
        (xy 110.5 50.5) (xy 110.5 53.5) (xy 110 57) (xy 108.5 60.5) (xy 105.5 64)
        (xy 101.5 67) (xy 97 68.5) (xy 91.5 68.5) (xy 86.5 66.5) (xy 82 62.5)
        (xy 80 59.5) (xy 78.5 54) (xy 79 49) (xy 80.5 45) (xy 83.5 41)
        (xy 89 37.5) (xy 94.5 36.5)
      )
    )
  )
)
