(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 164)
    (no_connects 1)
    (area 17.150001 51.3 89.426191 137.075001)
    (thickness 1.6)
    (drawings 62)
    (tracks 253)
    (zones 0)
    (modules 29)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.5)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /IO0)
  (net 2 /IO1)
  (net 3 /IO2)
  (net 4 /IO3)
  (net 5 /Z0)
  (net 6 /IO4)
  (net 7 /IO5)
  (net 8 /IO6)
  (net 9 /IO7)
  (net 10 /Z1)
  (net 11 /Z2)
  (net 12 /Z3)
  (net 13 /Z4)
  (net 14 /Z5)
  (net 15 /Z6)
  (net 16 /Z7)
  (net 17 /CB0)
  (net 18 /CB1)
  (net 19 /CB2)
  (net 20 /CB3)
  (net 21 /CA3)
  (net 22 /CA2)
  (net 23 /CA1)
  (net 24 /CA0)
  (net 25 /CA7)
  (net 26 /CA6)
  (net 27 /CA5)
  (net 28 /CA4)
  (net 29 /CB4)
  (net 30 /CB5)
  (net 31 /CB6)
  (net 32 /CB7)
  (net 33 /CAH)
  (net 34 /CAL)
  (net 35 /CBH)
  (net 36 /CBL)
  (net 37 "Net-(J1-Pad2)")
  (net 38 "Net-(J2-Pad2)")
  (net 39 "Net-(J3-Pad2)")
  (net 40 "Net-(J4-Pad2)")
  (net 41 "Net-(J5-Pad2)")
  (net 42 "Net-(J6-Pad2)")
  (net 43 "Net-(J7-Pad2)")
  (net 44 "Net-(J8-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CA0)
    (add_net /CA1)
    (add_net /CA2)
    (add_net /CA3)
    (add_net /CA4)
    (add_net /CA5)
    (add_net /CA6)
    (add_net /CA7)
    (add_net /CAH)
    (add_net /CAL)
    (add_net /CB0)
    (add_net /CB1)
    (add_net /CB2)
    (add_net /CB3)
    (add_net /CB4)
    (add_net /CB5)
    (add_net /CB6)
    (add_net /CB7)
    (add_net /CBH)
    (add_net /CBL)
    (add_net /IO0)
    (add_net /IO1)
    (add_net /IO2)
    (add_net /IO3)
    (add_net /IO4)
    (add_net /IO5)
    (add_net /IO6)
    (add_net /IO7)
    (add_net /Z0)
    (add_net /Z1)
    (add_net /Z2)
    (add_net /Z3)
    (add_net /Z4)
    (add_net /Z5)
    (add_net /Z6)
    (add_net /Z7)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J8-Pad2)")
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5A0CAAAB)
    (at 40.64 114.3 180)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference P1 (at -2.54 6.35 270) (layer F.SilkS))
    (fp_text value CONN_6 (at 0 15.03 180) (layer F.Fab) hide)
    (fp_text user %R (at -1.27 -2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /CAH))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /IO0))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /IO1))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /IO2))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /IO3))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /CAL))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5A0CAAB2)
    (at 81.28 114.3 180)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference P6 (at 2.54 6.35 270) (layer F.SilkS))
    (fp_text value CONN_6 (at 0 15.03 180) (layer F.Fab) hide)
    (fp_text user %R (at -1.27 -2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /CAH))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /IO7))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /IO6))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /IO5))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /IO4))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /CAL))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5A0CAA9C)
    (at 63.5 101.6)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference P7 (at 2.54 6.35 270) (layer F.SilkS))
    (fp_text value CONN_6 (at 0 15.03) (layer F.Fab) hide)
    (fp_text user %R (at -1.27 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /CBH))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /CB4))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /CB5))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /CB6))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /CB7))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /CBL))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module "0 My Pins:KF141V-10P" (layer F.Cu) (tedit 5A0CAD4E)
    (at 50.8 73.66)
    (fp_text reference P4 (at -5.08 -1.905 180) (layer F.SilkS))
    (fp_text value CONN_10 (at 10.16 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 /CBL))
    (pad 1 thru_hole circle (at 0 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 /CBL))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad2)"))
    (pad 4 thru_hole circle (at 7.62 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad2)"))
    (pad 4 thru_hole circle (at 7.62 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad2)"))
    (pad 5 thru_hole circle (at 10.16 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 40 "Net-(J4-Pad2)"))
    (pad 5 thru_hole circle (at 10.16 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 40 "Net-(J4-Pad2)"))
    (pad 6 thru_hole circle (at 12.7 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 "Net-(J5-Pad2)"))
    (pad 6 thru_hole circle (at 12.7 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 "Net-(J5-Pad2)"))
    (pad 7 thru_hole circle (at 15.24 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 42 "Net-(J6-Pad2)"))
    (pad 7 thru_hole circle (at 15.24 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 42 "Net-(J6-Pad2)"))
    (pad 8 thru_hole circle (at 17.78 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 43 "Net-(J7-Pad2)"))
    (pad 8 thru_hole circle (at 17.78 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 43 "Net-(J7-Pad2)"))
    (pad 9 thru_hole circle (at 20.32 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 44 "Net-(J8-Pad2)"))
    (pad 9 thru_hole circle (at 20.32 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 44 "Net-(J8-Pad2)"))
    (pad 10 thru_hole circle (at 22.86 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 /CBH))
    (pad 10 thru_hole circle (at 22.86 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 /CBH))
  )
  (module w_conn_pt-1,5:pt_1,5-10-3,5-h (layer F.Cu) (tedit 5A0C939A)
    (at 60.96 78.74 180)
    (descr "10-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P5 (at 19.05 0 360) (layer F.SilkS))
    (fp_text value CONN_10 (at 0 -5 180) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at 8.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J2-Pad2)"))
    (pad 2 thru_hole circle (at 12.25 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at 5.25 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J3-Pad2)"))
    (pad 5 thru_hole circle (at 1.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(J4-Pad2)"))
    (pad 6 thru_hole circle (at -1.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(J5-Pad2)"))
    (pad 7 thru_hole circle (at -5.25 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(J6-Pad2)"))
    (pad 1 thru_hole rect (at 15.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 36 /CBL))
    (pad 8 thru_hole circle (at -8.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(J7-Pad2)"))
    (pad 9 thru_hole circle (at -12.25 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(J8-Pad2)"))
    (pad 10 thru_hole circle (at -15.75 -0.7 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 35 /CBH))
    (model walter/conn_pt-1_5/pt_1,5-10-3,5-h.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5A0C8C3B)
    (at 41 71)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MP1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5A0C8CB6)
    (at 81 71)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MP2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5A0C8CF6)
    (at 41 131)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MP3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5A0C8CDD)
    (at 81 131)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MP4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MECH_NPTH_M3 (at 0 4.2) (layer Eco1.User) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5A0CAA97)
    (at 58.42 101.6)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference P2 (at -2.54 6.35 90) (layer F.SilkS))
    (fp_text value CONN_6 (at 0 15.03) (layer F.Fab) hide)
    (fp_text user %R (at -1.905 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /CBH))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /CB3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /CB2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /CB1))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /CB0))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /CBL))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module w_conn_strip:vasch_strip_5x2 (layer F.Cu) (tedit 5A0DE5CA)
    (at 60.96 130.175 180)
    (descr "Box header 5x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P3 (at 11.96 -0.325 180) (layer F.SilkS))
    (fp_text value CONN_10 (at 0 5.7 180) (layer F.SilkS) hide)
    (pad 9 thru_hole oval (at 5.08 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 24 /CA0))
    (pad 10 thru_hole oval (at 5.08 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 34 /CAL))
    (pad 8 thru_hole oval (at 2.54 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 23 /CA1))
    (pad 7 thru_hole oval (at 2.54 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 22 /CA2))
    (pad 1 thru_hole rect (at -5.08 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 33 /CAH))
    (pad 2 thru_hole oval (at -5.08 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 25 /CA7))
    (pad 3 thru_hole oval (at -2.54 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 26 /CA6))
    (pad 4 thru_hole oval (at -2.54 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 27 /CA5))
    (pad 5 thru_hole oval (at 0 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 28 /CA4))
    (pad 6 thru_hole oval (at 0 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 21 /CA3))
    (model walter/conn_strip/vasch_strip_5x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A0DB7FC)
    (at 43.18 90.17 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value HEADER_2 (at 0 4.87 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /Z0))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A0DB877)
    (at 48.26 90.17 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value HEADER_2 (at 0 4.87 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Z1))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A0DB88E)
    (at 53.34 90.17 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value HEADER_2 (at 0 4.87 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /Z2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A0DB8A5)
    (at 58.42 90.17 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value HEADER_2 (at 0 4.87 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /Z3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A0DB8FF)
    (at 63.5 90.17 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value HEADER_2 (at 0 4.87 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /Z4))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J5-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A0DB915)
    (at 68.58 90.17 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value HEADER_2 (at 0 4.87 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /Z5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J6-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A0DB933)
    (at 73.66 90.17 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value HEADER_2 (at 0 4.87 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /Z6))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J7-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A0DB953)
    (at 78.74 90.17 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value HEADER_2 (at 0 4.87 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Z7))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J8-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen locked (layer B.Cu) (tedit 0)
    (at 78.5 124 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer B.Cu) (tedit 5A118895)
    (at 45.72 116.84)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 0.635 2.54) (layer B.SilkS))
    (fp_text value LTV-845 (at 3.81 -20.11) (layer B.Fab) hide)
    (fp_text user %R (at 3.81 -8.89) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /CA0))
    (pad 9 thru_hole oval (at 7.62 -17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /Z3))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /IO0))
    (pad 10 thru_hole oval (at 7.62 -15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /CB3))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /CA1))
    (pad 11 thru_hole oval (at 7.62 -12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /Z2))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /IO1))
    (pad 12 thru_hole oval (at 7.62 -10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /CB2))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /CA2))
    (pad 13 thru_hole oval (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /Z1))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /IO2))
    (pad 14 thru_hole oval (at 7.62 -5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /CB1))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /CA3))
    (pad 15 thru_hole oval (at 7.62 -2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /Z0))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /IO3))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /CB0))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A118897)
    (at 45.72 99.06)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 0.635 -2.54) (layer F.SilkS))
    (fp_text value LTV-845 (at 3.81 20.11) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /IO3))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /CB0))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /CA3))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /Z0))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /IO2))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /CB1))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /CA2))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /Z1))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /IO1))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /CB2))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /CA1))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /Z2))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /IO0))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /CB3))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /CA0))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /Z3))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer B.Cu) (tedit 5A11881C)
    (at 53.34 99.06 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at -2.54 2.54 180) (layer B.SilkS))
    (fp_text value LTV-845 (at 3.81 -20.11 180) (layer B.Fab) hide)
    (fp_text user %R (at 3.81 -8.89 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /Z3))
    (pad 9 thru_hole oval (at 7.62 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /CA0))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /CB3))
    (pad 10 thru_hole oval (at 7.62 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /IO0))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /Z2))
    (pad 11 thru_hole oval (at 7.62 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /CA1))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /CB2))
    (pad 12 thru_hole oval (at 7.62 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /IO1))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /Z1))
    (pad 13 thru_hole oval (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /CA2))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /CB1))
    (pad 14 thru_hole oval (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /IO2))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /Z0))
    (pad 15 thru_hole oval (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /CA3))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /CB0))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /IO3))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A257703)
    (at 53.34 116.84 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U4 (at 0.635 -2.54 180) (layer F.SilkS))
    (fp_text value LTV-845 (at 3.81 20.11 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /CB0))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /IO3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /Z0))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /CA3))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /CB1))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /IO2))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /Z1))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /CA2))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /CB2))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /IO1))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /Z2))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /CA1))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /CB3))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /IO0))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /Z3))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /CA0))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer B.Cu) (tedit 5A11888A)
    (at 76.835 99.06 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U5 (at 1.27 2.54 180) (layer B.SilkS))
    (fp_text value LTV-845 (at 3.81 -20.11 180) (layer B.Fab) hide)
    (fp_text user %R (at 3.81 -8.89 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /CA4))
    (pad 9 thru_hole oval (at 7.62 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /Z7))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /IO4))
    (pad 10 thru_hole oval (at 7.62 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /CB7))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /CA5))
    (pad 11 thru_hole oval (at 7.62 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /Z6))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /IO5))
    (pad 12 thru_hole oval (at 7.62 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /CB6))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /CA6))
    (pad 13 thru_hole oval (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /Z5))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /IO6))
    (pad 14 thru_hole oval (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /CB5))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /CA7))
    (pad 15 thru_hole oval (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /Z4))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /IO7))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /CB4))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A11888C)
    (at 76.835 116.84 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U6 (at 1.27 -2.54 180) (layer F.SilkS))
    (fp_text value LTV-845 (at 3.81 20.11 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /IO7))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /CB4))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /CA7))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /Z4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /IO6))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /CB5))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /CA6))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /Z5))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /IO5))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /CB6))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /CA5))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /Z6))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /IO4))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /CB7))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /CA4))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /Z7))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer B.Cu) (tedit 5A11888E)
    (at 69.215 116.84)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U7 (at 0 2.54) (layer B.SilkS))
    (fp_text value LTV-845 (at 3.81 -20.11) (layer B.Fab) hide)
    (fp_text user %R (at 3.81 -8.89) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /Z7))
    (pad 9 thru_hole oval (at 7.62 -17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /CA4))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /CB7))
    (pad 10 thru_hole oval (at 7.62 -15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /IO4))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /Z6))
    (pad 11 thru_hole oval (at 7.62 -12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /CA5))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /CB6))
    (pad 12 thru_hole oval (at 7.62 -10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /IO5))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /Z5))
    (pad 13 thru_hole oval (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /CA6))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /CB5))
    (pad 14 thru_hole oval (at 7.62 -5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /IO6))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /Z4))
    (pad 15 thru_hole oval (at 7.62 -2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /CA7))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /CB4))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /IO7))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A118886)
    (at 69.215 99.06)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U8 (at 0 -2.54) (layer F.SilkS))
    (fp_text value LTV-845 (at 3.81 20.11) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /CB4))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /IO7))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /Z4))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /CA7))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /CB5))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /IO6))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /Z5))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /CA6))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /CB6))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /IO5))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /Z6))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /CA5))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /CB7))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /IO4))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /Z7))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /CA4))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_logo:Logo_silk_CC-BY-NC-SA_10x3.6mm (layer F.Cu) (tedit 0)
    (at 44.196 124.46)
    (descr "CC BY-NC-SA logo, 10x3.6mm")
    (fp_text reference LIC1 (at 0.3 -1.4) (layer F.SilkS) hide)
    (fp_text value CC-BY-NC-SA-icon (at 0.3 0.5) (layer F.SilkS) hide)
  )
  (gr_text by (at 78.105 123.19) (layer F.SilkS))
  (dimension 60 (width 0.3) (layer Cmts.User)
    (gr_text "60.000 mm" (at 29.65 101 90) (layer Cmts.User))
    (feature1 (pts (xy 35 71) (xy 28.3 71)))
    (feature2 (pts (xy 35 131) (xy 28.3 131)))
    (crossbar (pts (xy 31 131) (xy 31 71)))
    (arrow1a (pts (xy 31 71) (xy 31.586421 72.126504)))
    (arrow1b (pts (xy 31 71) (xy 30.413579 72.126504)))
    (arrow2a (pts (xy 31 131) (xy 31.586421 129.873496)))
    (arrow2b (pts (xy 31 131) (xy 30.413579 129.873496)))
  )
  (dimension 40 (width 0.3) (layer Cmts.User)
    (gr_text "40.000 mm" (at 61 58.65) (layer Cmts.User))
    (feature1 (pts (xy 81 64) (xy 81 57.3)))
    (feature2 (pts (xy 41 64) (xy 41 57.3)))
    (crossbar (pts (xy 41 60) (xy 81 60)))
    (arrow1a (pts (xy 81 60) (xy 79.873496 60.586421)))
    (arrow1b (pts (xy 81 60) (xy 79.873496 59.413579)))
    (arrow2a (pts (xy 41 60) (xy 42.126504 60.586421)))
    (arrow2b (pts (xy 41 60) (xy 42.126504 59.413579)))
  )
  (dimension 72 (width 0.3) (layer Cmts.User)
    (gr_text "72.000 mm" (at 23.65 101 90) (layer Cmts.User))
    (feature1 (pts (xy 35 65) (xy 22.3 65)))
    (feature2 (pts (xy 35 137) (xy 22.3 137)))
    (crossbar (pts (xy 25 137) (xy 25 65)))
    (arrow1a (pts (xy 25 65) (xy 25.586421 66.126504)))
    (arrow1b (pts (xy 25 65) (xy 24.413579 66.126504)))
    (arrow2a (pts (xy 25 137) (xy 25.586421 135.873496)))
    (arrow2b (pts (xy 25 137) (xy 24.413579 135.873496)))
  )
  (gr_text jeditekunum (at 78.105 125.095) (layer F.SilkS))
  (gr_text v1 (at 69.85 123.19) (layer F.SilkS))
  (gr_text Iso-I/O8 (at 60.96 123.19) (layer F.SilkS))
  (gr_text L (at 63.5 116.84) (layer F.SilkS))
  (gr_text L (at 58.42 116.84) (layer F.SilkS))
  (gr_text L (at 81.28 99.06) (layer F.SilkS))
  (gr_text H (at 81.28 116.84) (layer F.SilkS))
  (gr_text H (at 63.5 99.06) (layer F.SilkS))
  (gr_text H (at 58.42 99.06) (layer F.SilkS))
  (gr_text H (at 40.64 116.84) (layer F.SilkS))
  (gr_text L (at 40.64 99.06) (layer F.SilkS))
  (gr_text L (at 50.8 67.31) (layer F.SilkS))
  (gr_text H (at 73.66 67.31) (layer F.SilkS))
  (gr_text 7 (at 71.12 67.31) (layer F.SilkS))
  (gr_text 6 (at 68.58 67.31) (layer F.SilkS))
  (gr_text 5 (at 66.04 67.31) (layer F.SilkS))
  (gr_text 4 (at 63.5 67.31) (layer F.SilkS))
  (gr_text 3 (at 60.96 67.31) (layer F.SilkS))
  (gr_text 2 (at 58.42 67.31) (layer F.SilkS))
  (gr_text 1 (at 55.88 67.31) (layer F.SilkS))
  (gr_text 0 (at 53.34 67.31) (layer F.SilkS))
  (gr_line (start 37 137) (end 85 137) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 37 65) (end 85 65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 50 (width 0.3) (layer Cmts.User)
    (gr_text "50.000 mm" (at 61 52.65) (layer Cmts.User))
    (feature1 (pts (xy 86 64) (xy 86 51.3)))
    (feature2 (pts (xy 36 64) (xy 36 51.3)))
    (crossbar (pts (xy 36 54) (xy 86 54)))
    (arrow1a (pts (xy 86 54) (xy 84.873496 54.586421)))
    (arrow1b (pts (xy 86 54) (xy 84.873496 53.413579)))
    (arrow2a (pts (xy 36 54) (xy 37.126504 54.586421)))
    (arrow2b (pts (xy 36 54) (xy 37.126504 53.413579)))
  )
  (gr_text 0 (at 43.18 84.455) (layer F.SilkS))
  (gr_text 7 (at 78.74 84.455) (layer F.SilkS))
  (gr_text 6 (at 73.66 84.455) (layer F.SilkS))
  (gr_text 5 (at 68.58 84.455) (layer F.SilkS))
  (gr_text 4 (at 62.865 84.455) (layer F.SilkS))
  (gr_text 3 (at 58.42 84.455) (layer F.SilkS))
  (gr_text 2 (at 53.34 84.455) (layer F.SilkS))
  (gr_text 1 (at 48.26 84.455) (layer F.SilkS))
  (gr_arc (start 37 136) (end 37 137) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 85 136) (end 86 136) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 85 66) (end 85 65) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 37 66) (end 36 66) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86 66) (end 86 136) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 36 66) (end 36 136) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86 65) (xy 86 137) (xy 36 137) (xy 36 136) (xy 36 65)
      )
    )
    (polygon
      (pts        (xy 84 66) (xy 38 66) (xy 38 136) (xy 84 136)
      )
    )
  )
)
