(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 49)
    (zones 0)
    (modules 10)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2 2.2)
    (pad_drill 1.1)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 V12)
  (net 2 GND)
  (net 3 "Net-(Q1-Pad2)")
  (net 4 /V12_RX)
  (net 5 /V12_TX)
  (net 6 PTT_A)
  (net 7 PTT_D)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(Q1-Pad2)")
    (add_net PTT_A)
    (add_net PTT_D)
  )
  (net_class Wide ""
    (clearance 0.254)
    (trace_width 0.762)
    (via_dia 1.016)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /V12_RX)
    (add_net /V12_TX)
    (add_net V12)
  )
  (module Diode_THT:D_DO-34_SOD68_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5AE50CD5)
    (at 172.72 107.95 270)
    (descr "Diode, DO-34_SOD68 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
    (tags "Diode DO-34_SOD68 series Axial Vertical pin pitch 2.54mm  length 3.04mm diameter 1.6mm")
    (fp_text reference D1 (at 1.27 -1.905 270) (layer F.SilkS))
    (fp_text value D (at 1.27 3.14466 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.25566 270) (layer F.Fab))
    (fp_text user A (at 4.29 0 270) (layer F.Fab))
    (fp_text user A (at 4.29 0 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 V12))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 PTT_A))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-34_SOD68_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-6-2.54_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 5C239D10)
    (at 143.51 117.475)
    (descr "Terminal Block Phoenix MPT-0,5-6-2.54, 6 pins, pitch 2.54mm, size 15.7x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-6-2.54 pitch 2.54mm size 15.7x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J2 (at -0.635 -1.905) (layer F.SilkS))
    (fp_text value V12 (at 6.35 4.16) (layer F.Fab) hide)
    (fp_text user %R (at 6.35 2) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 V12))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 V12))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 V12))
    (pad 4 thru_hole circle (at 7.62 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 V12))
    (pad 5 thru_hole circle (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 V12))
    (pad 6 thru_hole circle (at 12.7 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 V12))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-6-2.54_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-6-2.54_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 5C239D09)
    (at 179.07 117.475)
    (descr "Terminal Block Phoenix MPT-0,5-6-2.54, 6 pins, pitch 2.54mm, size 15.7x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-6-2.54 pitch 2.54mm size 15.7x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J3 (at 13.335 -1.905) (layer F.SilkS))
    (fp_text value V12_RX (at 6.35 4.16) (layer F.Fab) hide)
    (fp_text user %R (at 6.35 2) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 12.7 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 /V12_RX))
    (pad 5 thru_hole circle (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 /V12_RX))
    (pad 4 thru_hole circle (at 7.62 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 /V12_RX))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 /V12_RX))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 /V12_RX))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 /V12_RX))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-6-2.54_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-6-2.54_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 5C239D0D)
    (at 161.29 117.475)
    (descr "Terminal Block Phoenix MPT-0,5-6-2.54, 6 pins, pitch 2.54mm, size 15.7x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-6-2.54 pitch 2.54mm size 15.7x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J4 (at -0.635 -1.905) (layer F.SilkS))
    (fp_text value V12_TX (at 6.35 4.16) (layer F.Fab) hide)
    (fp_text user %R (at 6.35 2) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /V12_TX))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /V12_TX))
    (pad 3 thru_hole circle (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /V12_TX))
    (pad 4 thru_hole circle (at 7.62 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /V12_TX))
    (pad 5 thru_hole circle (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /V12_TX))
    (pad 6 thru_hole circle (at 12.7 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /V12_TX))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-6-2.54_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_THT:Relay_SPDT_Omron_G5V-1 (layer F.Cu) (tedit 5C23A2BB)
    (at 186.69 106.68 270)
    (descr "Relay Omron G5V-1, see http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v_1.pdf")
    (tags "Relay Omron G5V-1")
    (fp_text reference K1 (at 2.5 -2.2 270) (layer F.SilkS))
    (fp_text value G5V-1 (at 2.5 12.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 6.35 270) (layer F.Fab))
    (pad 10 thru_hole circle (at 5.08 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /V12_TX))
    (pad 9 thru_hole circle (at 5.08 2.54 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 PTT_A))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 /V12_RX))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 V12))
    (pad 6 thru_hole circle (at 5.08 10.16 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 V12))
    (pad 5 thru_hole circle (at 0 10.16 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 V12))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_Omron_G5V-1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-4-2.54_1x04_P2.54mm_Horizontal (layer F.Cu) (tedit 5C239CF4)
    (at 158.115 109.22 180)
    (descr "Terminal Block Phoenix MPT-0,5-4-2.54, 4 pins, pitch 2.54mm, size 10.6x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-4-2.54 pitch 2.54mm size 10.6x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J1 (at 8.255 -3.81 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x04 (at 3.81 4.16 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 V12))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 PTT_D))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 PTT_A))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-4-2.54_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C239CEF)
    (at 191.77 109.22)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C239CBE)
    (at 143.51 111.125)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Package_TO_SOT_THT:TO-92_Wide (layer F.Cu) (tedit 5C23A064)
    (at 167.64 111.76 90)
    (descr "TO-92 leads molded, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value Q_NPN_EBC (at 2.54 2.79 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 PTT_A))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 161.925 109.22 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at -1.27 1.27 90) (layer F.SilkS))
    (fp_text value 1K (at 1.27 1.92 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -1.92 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 PTT_D))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 2018-12 (at 144.78 107.95) (layer F.SilkS))
  (gr_text 12v:RX (at 179.705 121.285) (layer F.SilkS))
  (gr_text 12v:TX (at 161.925 121.285) (layer F.SilkS))
  (gr_text 12v (at 143.51 121.285) (layer F.SilkS))
  (gr_text KC1FSZ (at 144.145 106.045) (layer F.SilkS))
  (gr_line (start 140.97 104.775) (end 140.97 121.92) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 194.31 104.775) (end 140.97 104.775) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 194.31 121.92) (end 194.31 104.775) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.97 121.92) (end 194.31 121.92) (angle 90) (layer Edge.Cuts) (width 0.15))
)
