(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-1")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 39)
    (zones 0)
    (modules 4)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VIN)
  (net 3 DR)
  (net 4 SS)
  (net 5 MOSI)
  (net 6 MISO)
  (net 7 SCLK)
  (net 8 SYNC)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net DR)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net SCLK)
    (add_net SS)
    (add_net SYNC)
    (add_net VIN)
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 159.512 119.761)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 159.512 100.203)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H1 (at 7.112 4.572) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 152.908 113.792 180)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_02x04_Odd_Even (at 1.27 9.95) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 SCLK))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 SYNC))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 MISO))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 MOSI))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SS))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 DR))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VIN))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KICAD_USER_3D}/901303108.stp
      (offset (xyz 7.62 -3.81 4.826))
      (scale (xyz 1 1 1))
      (rotate (xyz -180 0 -90))
    )
  )
  (module Connector_PinSocket_1.00mm:PinSocket_2x10_P1.00mm_Vertical_SMD (layer F.Cu) (tedit 5A19A41D)
    (at 160.655 109.982)
    (descr "surface-mounted straight socket strip, 2x10, 1.00mm pitch, double cols (https://gct.co/files/drawings/bc085.pdf), script generated")
    (tags "Surface mounted socket strip SMD 2x10 1.00mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 -6.75) (layer F.SilkS) hide)
    (fp_text value Conn_02x10_Odd_Even (at 0 6.75) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 20 smd rect (at -1.525 4.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 1.525 4.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -1.525 3.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 1.525 3.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.525 2.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 1.525 2.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -1.525 1.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 1.525 1.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -1.525 0.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (pad 11 smd rect (at 1.525 0.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (pad 10 smd rect (at -1.525 -0.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (pad 9 smd rect (at 1.525 -0.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -1.525 -1.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 1.525 -1.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 DR))
    (pad 6 smd rect (at -1.525 -2.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 SS))
    (pad 5 smd rect (at 1.525 -2.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 MOSI))
    (pad 4 smd rect (at -1.525 -3.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 MISO))
    (pad 3 smd rect (at 1.525 -3.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 SCLK))
    (pad 2 smd rect (at -1.525 -4.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 SYNC))
    (pad 1 smd rect (at 1.525 -4.5) (size 1.85 0.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_1.00mm.3dshapes/PinSocket_2x10_P1.00mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 139.446 123.444) (end 165.1 123.444) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.446 96.52) (end 139.446 123.444) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.1 96.52) (end 139.446 96.52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.1 123.444) (end 165.1 96.52) (layer Edge.Cuts) (width 0.05))
)
