<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="124.46" y1="55.88" x2="124.46" y2="0" width="0.0254" layer="20"/>
<wire x1="124.46" y1="0" x2="0" y2="0" width="0.0254" layer="20"/>
<text>BoosterPack 1</text>
<text>BoosterPack 2</text>
<text>Target USB</text>
<text>DEBUG</text>
<wire x1="124.46" y1="55.88" x2="0" y2="55.88" width="0.0254" layer="20"/>
<text>POWER</text>
<text>Y1</text>
<text>U14</text>
<text>EK-TM4C1294XL Rev D</text>
<text>http://www.ti.com/launchpad</text>
<text>ICDI</text>
<text>OTG</text>
<text>BoosterPack</text>
<text>CAN</text>
<text>UART</text>
<text>UART</text>
<text>CAN</text>
<text>MCU 3V3</text>
<text>+3v3</text>
<text>U22</text>
<text>Y2</text>
<text>POWER SELECT</text>
<text>+3v3 
PD2 
PP0 
PP1 
See JP4 
See JP5
PQ0
PP4 
PN5 
PN4 
</text>
<text>
+5V 
GND 
PB4 
PB5 
PK0 
PK1 
PK2 
PK3 
PA4 
PA5 
</text>
<text>PG1
PK4
PK5
PM0
PM1
PM2
PH0
PH1
PK6
PK7
</text>
<text>GND
PM7
PP5
PA7
!RESET
PQ2/PA3
PQ3/PA2
PP3
PQ1
PM6
</text>
<text>GND
 PM3
PH2
PH3
!RST
PD1
PD0
PN2
PN3
PP2
</text>
<text> PF1
 PF2
 PF3
 PG0
 PL4
 PL5
PL0
 PL1
 PL2
 PL3
</text>
<text>+5V
GND
PE0
PE1
PE2
PE3
PD7
PA6
PM4
PM5
</text>
<text>+3V3
PE4
PC4
PC5
PC6
PE5
PD3
PC7
PB2
PB3
</text>
<text>TP4</text>
<text>TP5</text>
<text>TP6</text>
<text>TP7</text>
<text>TP9</text>
<text>TP10</text>
<text>TP11</text>
<text>TP13</text>
<text>TP12</text>
<text>TP3</text>
<text>TP8</text>
<text>TP1</text>
<text>TP2</text>
<text>5V
3V3</text>
<text>!WAK
GND</text>
<text>PQ4
!RST</text>
<text>PN3
PM4</text>
<text>PN2
PM5</text>
<text>PN1
PM6</text>
<text>PN0
PM7</text>
<text>PN5
PJ1</text>
<text>PN4
PJ0</text>
<text>PL5
PP5</text>
<text>PK4
PP4</text>
<text>PK5
PA1</text>
<text>PP3
PA0</text>
<text>PP2
PF3</text>
<text>PB3
PF2</text>
<text>PB2
PF1</text>
<text>PL4
PF0</text>
<text>PK6
PF4</text>
<text>GND 
GND</text>
<text>PK7
PB1</text>
<text>PQ3
PB0</text>
<text>PQ2
PP1</text>
<text>PQ1
PP0</text>
<text>PQ0
PD2</text>
<text>PL3
PD0</text>
<text>PL2
PD1</text>
<text>PL1
PD3</text>
<text>PL0
PD6</text>
<text>PM0
PD7</text>
<text>PM1
PD4</text>
<text>PM2
PD5</text>
<text>GND 
GND</text>
<text>PM3
REF</text>
<text>PG0
PK3</text>
<text>PG1
PK2</text>
<text>PA7
PK1</text>
<text>PA6
PK0</text>
<text>PC4
PE5</text>
<text>PC5
PE4</text>
<text>PC6
PE3</text>
<text>PC7
PE2</text>
<text>PH3
PE1</text>
<text>PH2
PE0</text>
<text>PH1
PA5</text>
<text>PH0
PA4</text>
<text>PB5
PA3</text>
<text>PB4
PA2</text>
<text>GND
GND</text>
<text>3V3
5V</text>
<text>BP2_A2.5
PA0</text>
<text>PD4
ICDI RX</text>
<text>BP2_A2.6
PA1</text>
<text>PD5
ICDI_TX</text>
<wire x1="0" y1="55.88" x2="0" y2="0" width="0.0254" layer="20"/>
<text>Layer Stackup
Top silkscreen
Top Solder Mask
Component Side
Layer 2
Layer 3
Solder Side
Bottom Solder Mask
Bottom Silkscreen</text>
<text>File Names
EK-TM4C129EXL.sst
EK-TM4C129EXL.smt
EK-TM4C129EXL.l1
EK-TM4C129EXL.l2
EK-TM4C129EXL.l3
EK-TM4C129EXL.l4
EK-TM4C129EXL.smb
EK-TM4C129EXL.ssb</text>
<text>NOTES: UNLESS OTHERWISE SPECIFIED
1) Manufacture in accordance with IPC-6012, Type 3, Class 2.
2) End Product Features shall not vary more than 20% from artwork originals
3) Material shall be ROHS compliant, copper clad FR-406, NEMA Grade (Tg 170degC)
     Per IPC-4101, Color Natural, or equivalent
4) Construction shall be symetrical multilayer per layer stackup detail
5) Copper weight on inner layers shall be 1 oz per square foot
6) Equivalent copper weight on outler layers shall be 1.0 oz per square foot before plating
7) All plated through holes shall have a minimum of 0.0007 inches of copper
8) Drill hole tolerance after plating shall be +/- 0.003 inches
9) Minimum annular ring shall be 0.001 inches
10) Minmum annular rint at emergent conductors shall be 0.003 inches
11) PCB Thickness shall be 0.062 inches +/- 0.007 inches
12) Warp / Twist shall not exceed 0.010 inches per inch
13) Finish shall be LPI, Gloss RED SMOBC, Both sides balance of exposed copper shall be HASL
14) Silkscreen with nonconductive white epoxy ink
15) Board stack-up should be targetted such that a differential impedance of 90 ohms +/- 10% can 
      be achieved on the top layer with 10.8 mil traces and 6 mil spacing.  Additionally 100 ohm +/- 10% 
      with 8.7 mil traces and 6 mil spacing.  Boards do not need to be impedance controlled.</text>
<text>TXD</text>
<text>RXD</text>
<text>TCK</text>
<text>TMS</text>
<text>TDI</text>
<text>TDO</text>
<text>!RESET</text>
<text>1</text>
<text>15</text>
<text>29</text>
<text>43</text>
<text>57</text>
<text>71</text>
<text>85</text>
<text>EK-TM4C1294XL
REV D</text>
<text>TXD</text>
<text>RXD</text>
<text>TCK</text>
<text>TMS</text>
<text>TDI</text>
<text>TDO</text>
<text>!RESET</text>
<text>Tiva  C Series 
Connected LaunchPad</text>
<text>TM</text>
</plain>
<libraries>
<library name="ek-tm4c129exl">
<packages>
<package name="TC2030-MCP-NL">
<description>&lt;B&gt;TAG-CONNECT ISP Connector&lt;/B&gt;&lt;BR&gt;&lt;BR&gt;&lt;I&gt;Manufacturer:&lt;/I&gt; &lt;a href="www.tag-connect.com"&gt;Tag-Connect&lt;/a&gt;&lt;BR&gt;
&lt;BR&gt;Cable for easy In-Circuit PCB Programming. Designed for Standard JTAG 10 Pin, suitable for many others.&lt;BR&gt;
&lt;BR&gt;Footprint for TC2050 NL &lt;BR&gt;

&lt;TABLE cellspacing=0 cellpadding=0 border=0&gt;
&lt;TR&gt;&lt;TD width=20&gt;&lt;/TD&gt;&lt;TD&gt;
&lt;TABLE cellspacing=0 cellpadding=1 border=1&gt;
&lt;TR bgcolor=silver&gt;&lt;TD align=center&gt;PAD&lt;/TD&gt;&lt;TD align=center&gt;Description&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;1&lt;/TD&gt;&lt;TD&gt;VTREF&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;2&lt;/TD&gt;&lt;TD&gt;nTRST&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;3&lt;/TD&gt;&lt;TD&gt;TDI&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;4&lt;/TD&gt;&lt;TD&gt;TMS&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;5&lt;/TD&gt;&lt;TD&gt;TCK&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;6&lt;/TD&gt;&lt;TD&gt;RTCK&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;7&lt;/TD&gt;&lt;TD&gt;TDO&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;8&lt;/TD&gt;&lt;TD&gt;RESET&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;9&lt;/TD&gt;&lt;TD&gt;GND&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;10&lt;/TD&gt;&lt;TD&gt;NC&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/TD&gt;&lt;/TR&gt;&lt;/TABLE&gt;&lt;BR&gt;&lt;BR&gt;
©2009 ROFA.cz
Modified 7/2011 by Tim McCarthy-Smith 
VIDA Products INC</description>
</package>
<package name="TSW-107-02-S-D">
<description>&lt;b&gt;THROUGH-HOLE .025" SQ POST HEADER&lt;/b&gt;&lt;p&gt;
Source: Samtec TSW.pdf</description>
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="NDK3.2X2.5">
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="DRB8_2P4X1P65">
</package>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="CON_2X5_50MIL">
</package>
<package name="TSW-110-02-S-D">
<description>&lt;b&gt;THROUGH-HOLE .025" SQ POST HEADER&lt;/b&gt;&lt;p&gt;
Source: Samtec TSW.pdf</description>
</package>
<package name="SWITCH_6MM_6MM_TE_CON_SMD">
</package>
<package name="MAG_PULSE_HX1188FNL">
</package>
<package name="D8">
</package>
<package name="RJ45_TE_CON_NOMAG_NOLED">
</package>
<package name="DRY6">
</package>
<package name="LQFP-64-PM">
</package>
<package name="CON_USB_MICRO_B_FCI_10118194">
</package>
<package name="DRV6_1P6X1">
</package>
<package name="C1812">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CON_USB_MICRO_AB_HIROSE_ZX62D-AB-5P8">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
</packages>
</library>
<library name="con-samtec">
<description>&lt;b&gt;Samtec Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TSW-149-02-S-D">
<description>&lt;b&gt;THROUGH-HOLE .025" SQ POST HEADER&lt;/b&gt;&lt;p&gt;
Source: Samtec TSW.pdf</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JUMP">
<description>&lt;b&gt;JUMPER CAB&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="EK-TM4C1294XL REV A">
<packages>
<package name="TQFP-128">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CRYSTAL_32K_SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U21" library="ek-tm4c129exl" package="TC2030-MCP-NL" value="TC2050-NL-MCP-NL">
<attribute name="GNUM"/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="NAME"/>
</element>
<element name="X1" library="ek-tm4c129exl" package="TSW-107-02-S-D" value="TSW-107-02-S-D">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="GNUM" value="G22-THVEU-2X7P-BAB"/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="ek-tm4c129exl" package="R0402" value="10k">
<attribute name="GNUM" value="G11-R0402-1002-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="ek-tm4c129exl" package="C0402" value="1.0uF">
<attribute name="GNUM" value="G10-C0402-C105-GBB"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="ek-tm4c129exl" package="C0402" value="12pF">
<attribute name="GNUM" value="G10-C0402-C120-AAC"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="ek-tm4c129exl" package="C0402" value="12pF">
<attribute name="GNUM" value="G10-C0402-C120-AAC"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y2" library="ek-tm4c129exl" package="NDK3.2X2.5" value="16M">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G15-32X25-1606-AAA"/>
</element>
<element name="C7" library="ek-tm4c129exl" package="C0603" value="2.2uF">
<attribute name="GNUM" value="G10-C0603-C225-HBB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="ek-tm4c129exl" package="R0402" value="5.6k">
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G11-R0402-5601-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="ek-tm4c129exl" package="R0402" value="5.6k">
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G11-R0402-5601-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="ek-tm4c129exl" package="R0402" value="5.6k">
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G11-R0402-5601-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="ek-tm4c129exl" package="R0402" value="10k">
<attribute name="GNUM" value="G11-R0402-1002-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="ek-tm4c129exl" package="R0402" value="10k">
<attribute name="GNUM" value="G11-R0402-1002-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="ek-tm4c129exl" package="R0402" value="10k">
<attribute name="GNUM" value="G11-R0402-1002-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="ek-tm4c129exl" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="GNUM" value="G11-R0402-1002-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="C19" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="ek-tm4c129exl" package="C0603K" value="2.2uF">
<attribute name="DIGIKEY_PARTNUM" value="311-1451-2-ND"/>
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G10-C0603-C225-HBB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D0" library="ek-tm4c129exl" package="CHIPLED_0603" value="">
<attribute name="GNUM" value="G14-D0603-GR00-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="ek-tm4c129exl" package="R0402" value="330">
<attribute name="GNUM" value="G11-R0402-3300-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="ek-tm4c129exl" package="R0402" value="0">
<attribute name="GNUM" value="G11-R0402-0000-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="ek-tm4c129exl" package="R0402" value="0">
<attribute name="GNUM" value="G11-R0402-0000-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="ek-tm4c129exl" package="R0402" value="0">
<attribute name="GNUM" value="G11-R0402-0000-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="ek-tm4c129exl" package="R0402" value="0">
<attribute name="GNUM" value="G11-R0402-0000-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="ek-tm4c129exl" package="R0402" value="0">
<attribute name="GNUM" value="G11-R0402-0000-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="ek-tm4c129exl" package="R0402" value="0">
<attribute name="GNUM" value="G11-R0402-0000-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="ek-tm4c129exl" package="R0402" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="GNUM" value="G11-R0402-0000-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="U6" library="ek-tm4c129exl" package="CON_2X5_50MIL" value="JTAG_ARM_10PIN">
<attribute name="GNUM" value="G22-SMVES-2X5A-BBC"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
</element>
<element name="X6" library="ek-tm4c129exl" package="TSW-110-02-S-D" value="TSW-110-02-S-D">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="GNUM" value="G22-THSTK-2X10-BAC"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X7" library="ek-tm4c129exl" package="TSW-110-02-S-D" value="TSW-110-02-S-D">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="GNUM" value="G22-THSTK-2X10-BAC"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X8" library="ek-tm4c129exl" package="TSW-110-02-S-D" value="TSW-110-02-S-D">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="GNUM" value="G22-THSTK-2X10-BAC"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X9" library="ek-tm4c129exl" package="TSW-110-02-S-D" value="TSW-110-02-S-D">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="GNUM" value="G22-THSTK-2X10-BAC"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="ek-tm4c129exl" package="R0402" value="100k">
<attribute name="GNUM" value="G11-R0402-1003-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="ek-tm4c129exl" package="R0402" value="0">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G11-R0402-0000-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="ek-tm4c129exl" package="R0402" value="0">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G11-R0402-0000-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="ek-tm4c129exl" package="R0402" value="49.9">
<attribute name="GNUM" value="G11-R0402-49R9-ABA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="ek-tm4c129exl" package="R0402" value="49.9">
<attribute name="GNUM" value="G11-R0402-49R9-ABA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="ek-tm4c129exl" package="R0402" value="49.4">
<attribute name="GNUM" value="G11-R0402-49R9-ABA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="ek-tm4c129exl" package="R0402" value="49.9">
<attribute name="GNUM" value="G11-R0402-49R9-ABA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="ek-tm4c129exl" package="R0402" value="4.87k 1%">
<attribute name="GNUM" value="G11-R0402-4871-ABA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="ek-tm4c129exl" package="CHIPLED_0603" value="">
<attribute name="GNUM" value="G14-D0603-GR00-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="ek-tm4c129exl" package="R0402" value="330">
<attribute name="GNUM" value="G11-R0402-3300-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="ek-tm4c129exl" package="CHIPLED_0603" value="">
<attribute name="GNUM" value="G14-D0603-GR00-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="ek-tm4c129exl" package="R0402" value="330">
<attribute name="GNUM" value="G11-R0402-3300-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="ek-tm4c129exl" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="GNUM" value="G14-D0603-GR00-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="R33" library="ek-tm4c129exl" package="R0402" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="GNUM" value="G11-R0402-3300-AAA"/>
</element>
<element name="C16" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="ek-tm4c129exl" package="C0402" value="1.0uF">
<attribute name="GNUM" value="G10-C0402-C105-GBB"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="ek-tm4c129exl" package="C0603K" value="2.2uF">
<attribute name="DIGIKEY_PARTNUM" value="311-1451-2-ND"/>
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G10-C0603-C225-HBB"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP9" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP11" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP12" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="ek-tm4c129exl" package="R0402" value="0">
<attribute name="GNUM" value="G11-R0402-0000-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP13" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="ek-tm4c129exl" package="R0402" value="0">
<attribute name="GNUM" value="G11-R0402-0000-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="ek-tm4c129exl" package="R0402" value="1M">
<attribute name="GNUM" value="G11-R0402-1004-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USR_SW1" library="ek-tm4c129exl" package="SWITCH_6MM_6MM_TE_CON_SMD" value="SWITCH_TACTILE">
<attribute name="NAME"/>
<attribute name="GNUM" value="G21-4P6MM-B3S1-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="USR_SW2" library="ek-tm4c129exl" package="SWITCH_6MM_6MM_TE_CON_SMD" value="SWITCH_TACTILE">
<attribute name="NAME"/>
<attribute name="GNUM" value="G21-4P6MM-B3S1-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="RESET" library="ek-tm4c129exl" package="SWITCH_6MM_6MM_TE_CON_SMD" value="SWITCH_TACTILE">
<attribute name="GNUM" value="G21-4P6MM-B3S1-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
</element>
<element name="C44" library="ek-tm4c129exl" package="C0402" value="12pF">
<attribute name="GNUM" value="G10-C0402-C120-AAC"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="ek-tm4c129exl" package="C0402" value="12pF">
<attribute name="GNUM" value="G10-C0402-C120-AAC"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="ek-tm4c129exl" package="NDK3.2X2.5" value="25Mhz">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G15-32X25-2506-AAA"/>
</element>
<element name="R44" library="ek-tm4c129exl" package="R0402" value="10k">
<attribute name="GNUM" value="G11-R0402-1002-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C47" library="ek-tm4c129exl" package="C0402" value="12pF">
<attribute name="GNUM" value="G10-C0402-C120-AAC"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="ek-tm4c129exl" package="C0402" value="12pF">
<attribute name="GNUM" value="G10-C0402-C120-AAC"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="WAKE" library="ek-tm4c129exl" package="SWITCH_6MM_6MM_TE_CON_SMD" value="SWITCH_TACTILE">
<attribute name="GNUM" value="G21-4P6MM-B3S1-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
</element>
<element name="U10" library="ek-tm4c129exl" package="MAG_PULSE_HX1188FNL" value="MAG_PULSE_HX1188FNL">
<attribute name="GNUM" value="G12-SOI16-1TO1-ZZQ"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
</element>
<element name="U13" library="ek-tm4c129exl" package="D8" value="SLVU2.8-4">
<attribute name="GNUM" value="G14-SOIC8-SLVU-DAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="ek-tm4c129exl" package="R0402" value="75">
<attribute name="GNUM" value="G11-R0402-75R0-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="ek-tm4c129exl" package="R0402" value="75">
<attribute name="GNUM" value="G11-R0402-75R0-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U14" library="ek-tm4c129exl" package="RJ45_TE_CON_NOMAG_NOLED" value="JACK_RJ45_NOMAG_NOLED_TECON">
<attribute name="GNUM" value="G20-8RJ45-ENET-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="R45" library="ek-tm4c129exl" package="R0402" value="75">
<attribute name="GNUM" value="G11-R0402-75R0-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="ek-tm4c129exl" package="R0402" value="75">
<attribute name="GNUM" value="G11-R0402-75R0-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H4" library="holes" package="3,2" value="MOUNT-HOLE3.2">
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G30-62S04-A112-AAA"/>
</element>
<element name="H6" library="holes" package="3,2" value="MOUNT-HOLE3.2">
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G30-62S04-A112-AAA"/>
</element>
<element name="X11" library="con-samtec" package="TSW-149-02-S-D" value="TSW-149-02-S-D">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM1" value="G22-THRE-1x49-AAC"/>
<attribute name="GNUM2" value="G22-THRA-1X49-AAC"/>
</element>
<element name="U4" library="ek-tm4c129exl" package="DRB8_2P4X1P65" value="TPS2052B_DRB_8">
<attribute name="DATASHEETURL" value="http://www.ti.com/lit/gpn/TPS2052B"/>
<attribute name="PIN_COUNT" value="8"/>
<attribute name="GENERIC_PART_NUMBER" value="TPS2052B"/>
<attribute name="DESCRIPTION" value="Current-Limited, Power-Distribution Switches"/>
<attribute name="FAMILY_NAME" value="USB POWER SWITCH"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="INDUSTRY_STD_PKG_TYPE" value="SON"/>
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="tps2052b_drb_8"/>
<attribute name="PACKAGE_DESIGNATOR" value="DRB"/>
<attribute name="GNUM" value="G57-08SON-2052-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="2X03" value="">
<attribute name="GNUM" value="G22-THVEU-2X3P-BAB"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X02" value="">
<attribute name="GNUM" value="G22-THVEU-002P-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X02" value="">
<attribute name="GNUM" value="G22-THVEU-002P-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="ek-tm4c129exl" package="R0402" value="10k">
<attribute name="GNUM" value="G11-R0402-1002-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="ek-tm4c129exl" package="R0402" value="100k">
<attribute name="GNUM" value="G11-R0402-1003-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="ek-tm4c129exl" package="R0402" value="51">
<attribute name="GNUM" value="G11-R0402-51R0-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="ek-tm4c129exl" package="R0402" value="0">
<attribute name="GNUM" value="G11-R0402-0000-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="2X02" value="">
<attribute name="GNUM" value="G22-THVEU-002P-BAB"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="2X02" value="">
<attribute name="GNUM" value="G22-THVEU-002P-BAB"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="ek-tm4c129exl" package="R0402" value="100k">
<attribute name="GNUM" value="G11-R0402-1003-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="ek-tm4c129exl" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="GNUM" value="G14-D0603-GR00-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="R27" library="ek-tm4c129exl" package="R0402" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="GNUM" value="G11-R0402-3300-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="U2" library="ek-tm4c129exl" package="DRY6" value="TPD4S012_DRY_6">
<attribute name="DATASHEETURL" value="http://www.ti.com/lit/gpn/TPD4S012"/>
<attribute name="PIN_COUNT" value="6"/>
<attribute name="GENERIC_PART_NUMBER" value="TPD4S012"/>
<attribute name="DESCRIPTION" value="4-Channel USB ESD Solution with Power Clamp"/>
<attribute name="FAMILY_NAME" value="ESD Solution"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="INDUSTRY_STD_PKG_TYPE" value="SON"/>
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="tpd4s012_dry_6"/>
<attribute name="PACKAGE_DESIGNATOR" value="DRY"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="GNUM" value="G57-SMDRY-S012-AAA "/>
<attribute name="POPOP"/>
</element>
<element name="U20" library="ek-tm4c129exl" package="LQFP-64-PM" value="TM4C123GH6PMI">
<attribute name="GNUM" value="G50-QFP64-F120-EGC"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U22" library="ek-tm4c129exl" package="CON_USB_MICRO_B_FCI_10118194" value="CON_USB_FCI_MICRO_B_10118194">
<attribute name="GNUM" value="G20-USBU-THB-CEB"/>
<attribute name="POPOP"/>
</element>
<element name="U3" library="ek-tm4c129exl" package="DRY6" value="TPD4S012_DRY_6">
<attribute name="DATASHEETURL" value="http://www.ti.com/lit/gpn/TPD4S012"/>
<attribute name="PIN_COUNT" value="6"/>
<attribute name="GENERIC_PART_NUMBER" value="TPD4S012"/>
<attribute name="DESCRIPTION" value="4-Channel USB ESD Solution with Power Clamp"/>
<attribute name="FAMILY_NAME" value="ESD Solution"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="INDUSTRY_STD_PKG_TYPE" value="SON"/>
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="tpd4s012_dry_6"/>
<attribute name="PACKAGE_DESIGNATOR" value="DRY"/>
<attribute name="GNUM" value="G57-SMDRY-S012-AAA "/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="ek-tm4c129exl" package="R0402" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="GNUM" value="G11-R0402-1000-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="R28" library="ek-tm4c129exl" package="R0402" value="5.6k">
<attribute name="GNUM" value="G11-R0402-5601-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="ek-tm4c129exl" package="R0402" value="10k">
<attribute name="GNUM" value="G11-R0402-1002-AAA"/>
<attribute name="POPOP"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="ek-tm4c129exl" package="DRV6_1P6X1" value="TPS73733_DRV_6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="GNUM" value="G51-DRV06-T733-AAA"/>
</element>
<element name="R48" library="ek-tm4c129exl" package="R0402" value="">
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G11-R0402-5232-ABA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="ek-tm4c129exl" package="C0402" value="0.1uF">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G10-C0402-C104-HBA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="jumper" package="JUMP" value="">
<attribute name="GNUM" value="G72-100MI-JMPA-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="J2" library="jumper" package="JUMP" value="">
<attribute name="GNUM" value="G72-100MI-JMPA-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="J3" library="jumper" package="JUMP" value="">
<attribute name="GNUM" value="G72-100MI-JMPA-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="J4" library="jumper" package="JUMP" value="">
<attribute name="GNUM" value="G72-100MI-JMPA-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="J5" library="jumper" package="JUMP" value="">
<attribute name="GNUM" value="G72-100MI-JMPA-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="J6" library="jumper" package="JUMP" value="">
<attribute name="GNUM" value="G72-100MI-JMPA-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="J7" library="jumper" package="JUMP" value="">
<attribute name="GNUM" value="G72-100MI-JMPA-AAA"/>
<attribute name="POPOP"/>
</element>
<element name="R49" library="ek-tm4c129exl" package="R0402" value="2k">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G11-R0402-R202-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="ek-tm4c129exl" package="R0402" value="2k">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G11-R0402-R202-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,2" value="MOUNT-HOLE3.2">
<attribute name="POPOP" value="OMIT"/>
<attribute name="GNUM" value="G30-62S04-A112-AAA"/>
</element>
<element name="U7" library="ek-tm4c129exl" package="CON_USB_MICRO_AB_HIROSE_ZX62D-AB-5P8" value="CON_USB_HIROSE_MICRO_AB_ZX62D_AB_5P8">
<attribute name="NAME"/>
<attribute name="POPOP"/>
<attribute name="GNUM" value="G20-USBU-THAB-CEB"/>
</element>
<element name="R51" library="ek-tm4c129exl" package="R0402" value="100">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G11-R0402-1000-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP14" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="POPOP" value="OMIT"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP15" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="POPOP" value="OMIT"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP16" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="POPOP" value="OMIT"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP17" library="ek-tm4c129exl" package="P1-13" value="TPPAD1-13">
<attribute name="POPOP" value="OMIT"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="GNUM" value="G20-K5000-TP00-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="EK-TM4C1294XL REV A" package="TQFP-128" value="TM4C1294NCPDT">
<attribute name="GNUM" value="G50-QF128-C1294-ALH"/>
</element>
<element name="C31" library="ek-tm4c129exl" package="C1812" value="4700pF">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G10-C1812-C472-ZBA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="EK-TM4C1294XL REV A" package="R1206" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="POPOP"/>
<attribute name="GNUM" value="G11-R1206-R105-CAA"/>
</element>
<element name="R52" library="EK-TM4C1294XL REV A" package="R0603" value="1M">
<attribute name="GNUM" value="G11-R0603-R105-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="EK-TM4C1294XL REV A" package="C0603" value="3300pF">
<attribute name="POPOP"/>
<attribute name="GNUM" value="G10-C0603-C332-ABA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="EK-TM4C1294XL REV A" package="C1210" value="1000pF">
<attribute name="POPOP"/>
<attribute name="GNUM" value="G10-C1210-C102-ZCA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="EK-TM4C1294XL REV A" package="R0603" value="1M">
<attribute name="GNUM" value="G11-R0603-R105-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="EK-TM4C1294XL REV A" package="C0603" value="3300pF">
<attribute name="POPOP" value=""/>
<attribute name="GNUM" value="G10-C0603-C332-ABA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y3" library="EK-TM4C1294XL REV A" package="CRYSTAL_32K_SMD" value="CRYATL_32K_SMD">
<attribute name="POPOP"/>
<attribute name="GNUM" value="G15-CMR2T-3272-AAA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="ICDI_TDI">
<contactref element="U21" pad="8"/>
<contactref element="U20" pad="P$50"/>
</signal>
<signal name="ICDI_TMS">
<contactref element="U21" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="U20" pad="P$51"/>
</signal>
<signal name="ICDI_TCK">
<contactref element="U21" pad="4"/>
<contactref element="R4" pad="2"/>
<contactref element="U20" pad="P$52"/>
</signal>
<signal name="+3V3">
<contactref element="U21" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="D0" pad="A"/>
<contactref element="C13" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="X6" pad="1"/>
<contactref element="X8" pad="1"/>
<contactref element="X11" pad="98"/>
<contactref element="X11" pad="1"/>
<contactref element="U6" pad="P1"/>
<contactref element="U20" pad="P$54"/>
<contactref element="U20" pad="P$42"/>
<contactref element="U20" pad="P$26"/>
<contactref element="U20" pad="P$11"/>
<contactref element="U20" pad="P$2"/>
<contactref element="U20" pad="P$37"/>
<contactref element="C25" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="C27" pad="1"/>
</signal>
<signal name="ICDI_TDO">
<contactref element="U21" pad="6"/>
<contactref element="U20" pad="P$49"/>
</signal>
<signal name="ICDI_RESET">
<contactref element="C2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="U21" pad="10"/>
<contactref element="U20" pad="P$38"/>
</signal>
<signal name="VCP_RXD">
<contactref element="R6" pad="2"/>
<contactref element="X1" pad="13"/>
<contactref element="U20" pad="P$17"/>
</signal>
<signal name="VCP_TXD">
<contactref element="R7" pad="2"/>
<contactref element="X1" pad="11"/>
<contactref element="U20" pad="P$18"/>
</signal>
<signal name="DEBUG_PC1/TMS/SWDIO">
<contactref element="R10" pad="2"/>
<contactref element="X1" pad="7"/>
<contactref element="U6" pad="P2"/>
<contactref element="U20" pad="P$20"/>
<contactref element="U20" pad="P$29"/>
</signal>
<signal name="DEBUG_PC3/TDO/SWO">
<contactref element="X1" pad="3"/>
<contactref element="R15" pad="2"/>
<contactref element="U6" pad="P6"/>
<contactref element="U20" pad="P$21"/>
<contactref element="U20" pad="P$53"/>
</signal>
<signal name="DEBUG_PC2/TDI">
<contactref element="X1" pad="5"/>
<contactref element="R11" pad="2"/>
<contactref element="U6" pad="P8"/>
<contactref element="U20" pad="P$22"/>
</signal>
<signal name="!DEBUG_RESET_OUT">
<contactref element="R16" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="U6" pad="P10"/>
<contactref element="U20" pad="P$23"/>
</signal>
<signal name="!EXTERNAL_DEBUG">
<contactref element="TP2" pad="TP"/>
<contactref element="R40" pad="1"/>
<contactref element="U20" pad="P$24"/>
</signal>
<signal name="N$1">
<contactref element="C9" pad="1"/>
<contactref element="Y2" pad="P$1"/>
<contactref element="U20" pad="P$40"/>
</signal>
<signal name="N$2">
<contactref element="C8" pad="1"/>
<contactref element="Y2" pad="P$3"/>
<contactref element="R50" pad="2"/>
</signal>
<signal name="ICDI_VDDC">
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="U20" pad="P$56"/>
<contactref element="U20" pad="P$25"/>
</signal>
<signal name="VERSION_1">
<contactref element="R13" pad="1"/>
<contactref element="U20" pad="P$47"/>
</signal>
<signal name="VERSION_2">
<contactref element="R14" pad="1"/>
<contactref element="U20" pad="P$48"/>
</signal>
<signal name="VERSION_0">
<contactref element="R12" pad="1"/>
<contactref element="U20" pad="P$61"/>
</signal>
<signal name="DEBUG_ACTIVE">
<contactref element="TP1" pad="TP"/>
<contactref element="U20" pad="P$64"/>
</signal>
<signal name="ICDI_USBD_N">
<contactref element="U20" pad="P$43"/>
<contactref element="U22" pad="P2"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="ICDI_USBD_P">
<contactref element="U20" pad="P$44"/>
<contactref element="U22" pad="P3"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="TARGET_TXD">
<contactref element="R6" pad="1"/>
<contactref element="X1" pad="14"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="TARGET_RXD">
<contactref element="R7" pad="1"/>
<contactref element="X1" pad="12"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="TARGET_TCK/SWCLK">
<contactref element="R8" pad="1"/>
<contactref element="X1" pad="10"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="P$100"/>
</signal>
<signal name="TARGET_TMS/SWDIO">
<contactref element="R10" pad="1"/>
<contactref element="X1" pad="8"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="P$99"/>
</signal>
<signal name="TARGET_TDI">
<contactref element="R11" pad="1"/>
<contactref element="X1" pad="6"/>
<contactref element="U1" pad="P$98"/>
</signal>
<signal name="TARGET_TDO/SWO">
<contactref element="R15" pad="1"/>
<contactref element="X1" pad="4"/>
<contactref element="U1" pad="P$97"/>
</signal>
<signal name="!TARGET_RESET">
<contactref element="R16" pad="1"/>
<contactref element="X1" pad="2"/>
<contactref element="X7" pad="10"/>
<contactref element="X9" pad="10"/>
<contactref element="X11" pad="94"/>
<contactref element="RESET" pad="P$3"/>
<contactref element="RESET" pad="P$4"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="DEBUG_VBUS">
<contactref element="JP1" pad="5"/>
<contactref element="U22" pad="P1"/>
<contactref element="U3" pad="6"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="DEBUG_PC0/TCK/SWCLK">
<contactref element="R8" pad="2"/>
<contactref element="X1" pad="9"/>
<contactref element="U6" pad="P4"/>
<contactref element="U20" pad="P$30"/>
<contactref element="U20" pad="P$19"/>
</signal>
<signal name="+5V">
<contactref element="C21" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="U4" pad="7"/>
<contactref element="X6" pad="2"/>
<contactref element="X8" pad="2"/>
<contactref element="X11" pad="2"/>
<contactref element="X11" pad="97"/>
<contactref element="U5" pad="6"/>
<contactref element="C26" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C28" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C20" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="X6" pad="4"/>
<contactref element="X7" pad="2"/>
<contactref element="X8" pad="4"/>
<contactref element="X9" pad="2"/>
<contactref element="R30" pad="1"/>
<contactref element="R31" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="C18" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="USR_SW1" pad="P$3"/>
<contactref element="USR_SW2" pad="P$4"/>
<contactref element="USR_SW2" pad="P$3"/>
<contactref element="USR_SW1" pad="P$4"/>
<contactref element="WAKE" pad="P$3"/>
<contactref element="WAKE" pad="P$4"/>
<contactref element="C44" pad="2"/>
<contactref element="C47" pad="2"/>
<contactref element="C48" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="RESET" pad="P$1"/>
<contactref element="RESET" pad="P$2"/>
<contactref element="C46" pad="2"/>
<contactref element="U21" pad="3"/>
<contactref element="U21" pad="9"/>
<contactref element="C2" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="U6" pad="P9"/>
<contactref element="U6" pad="P5"/>
<contactref element="C8" pad="2"/>
<contactref element="X11" pad="35"/>
<contactref element="X11" pad="61"/>
<contactref element="X11" pad="62"/>
<contactref element="X11" pad="36"/>
<contactref element="X11" pad="4"/>
<contactref element="X11" pad="3"/>
<contactref element="X11" pad="96"/>
<contactref element="U4" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="U4" pad="9"/>
<contactref element="R27" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="4"/>
<contactref element="U20" pad="P$34"/>
<contactref element="U20" pad="P$35"/>
<contactref element="U20" pad="P$3"/>
<contactref element="U20" pad="P$12"/>
<contactref element="U20" pad="P$27"/>
<contactref element="U20" pad="P$39"/>
<contactref element="U20" pad="P$55"/>
<contactref element="U20" pad="P$32"/>
<contactref element="U21" pad="5"/>
<contactref element="U22" pad="P5"/>
<contactref element="R29" pad="1"/>
<contactref element="U5" pad="3"/>
<contactref element="U5" pad="7"/>
<contactref element="U5" pad="V"/>
<contactref element="U5" pad="V_2"/>
<contactref element="U4" pad="V_6"/>
<contactref element="U4" pad="V"/>
<contactref element="U4" pad="V_2"/>
<contactref element="U4" pad="V_3"/>
<contactref element="U4" pad="V_4"/>
<contactref element="U4" pad="V_5"/>
<contactref element="C26" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="U7" pad="P5"/>
<contactref element="TP14" pad="TP"/>
<contactref element="TP17" pad="TP"/>
<contactref element="TP16" pad="TP"/>
<contactref element="TP15" pad="TP"/>
<contactref element="U1" pad="P$17"/>
<contactref element="U1" pad="P$48"/>
<contactref element="U1" pad="P$55"/>
<contactref element="U1" pad="P$58"/>
<contactref element="U1" pad="P$80"/>
<contactref element="U1" pad="P$114"/>
<contactref element="U1" pad="P$10"/>
<contactref element="C31" pad="2"/>
<contactref element="R47" pad="1"/>
<contactref element="R52" pad="1"/>
<contactref element="C32" pad="2"/>
<contactref element="R34" pad="1"/>
<contactref element="C33" pad="2"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="C19" pad="1"/>
<contactref element="R48" pad="1"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="TARGET_VBUS">
<contactref element="JP1" pad="3"/>
<contactref element="U4" pad="6"/>
<contactref element="TP4" pad="TP"/>
<contactref element="X11" pad="60"/>
<contactref element="U7" pad="P1"/>
<contactref element="U1" pad="P$96"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="D0" pad="C"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="VREG_EN">
<contactref element="TP3" pad="TP"/>
<contactref element="R17" pad="2"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="PA0">
<contactref element="X11" pad="74"/>
<contactref element="JP4" pad="2"/>
<contactref element="U1" pad="P$33"/>
</signal>
<signal name="PA1">
<contactref element="X11" pad="76"/>
<contactref element="JP5" pad="2"/>
<contactref element="U1" pad="P$34"/>
</signal>
<signal name="PA2">
<contactref element="X11" pad="6"/>
<contactref element="R20" pad="2"/>
<contactref element="U1" pad="P$35"/>
</signal>
<signal name="PA3">
<contactref element="X11" pad="8"/>
<contactref element="R19" pad="2"/>
<contactref element="U1" pad="P$36"/>
</signal>
<signal name="PA5">
<contactref element="X11" pad="12"/>
<contactref element="X6" pad="20"/>
<contactref element="U1" pad="P$38"/>
</signal>
<signal name="PA6">
<contactref element="X11" pad="25"/>
<contactref element="X8" pad="16"/>
<contactref element="U1" pad="P$40"/>
</signal>
<signal name="PA7">
<contactref element="X11" pad="27"/>
<contactref element="X7" pad="8"/>
<contactref element="U1" pad="P$41"/>
</signal>
<signal name="PA4">
<contactref element="X11" pad="10"/>
<contactref element="X6" pad="18"/>
<contactref element="U1" pad="P$37"/>
</signal>
<signal name="PB0">
<contactref element="X11" pad="58"/>
<contactref element="R18" pad="1"/>
<contactref element="U1" pad="P$95"/>
</signal>
<signal name="PB2">
<contactref element="X11" pad="67"/>
<contactref element="X8" pad="17"/>
<contactref element="U1" pad="P$91"/>
</signal>
<signal name="PB3">
<contactref element="X11" pad="69"/>
<contactref element="X8" pad="19"/>
<contactref element="U1" pad="P$92"/>
</signal>
<signal name="PB4">
<contactref element="X11" pad="5"/>
<contactref element="X6" pad="6"/>
<contactref element="U1" pad="P$121"/>
</signal>
<signal name="PB5">
<contactref element="X11" pad="7"/>
<contactref element="X6" pad="8"/>
<contactref element="U1" pad="P$120"/>
</signal>
<signal name="PC4">
<contactref element="X11" pad="23"/>
<contactref element="X8" pad="5"/>
<contactref element="U1" pad="P$25"/>
</signal>
<signal name="PC5">
<contactref element="X11" pad="21"/>
<contactref element="X8" pad="7"/>
<contactref element="U1" pad="P$24"/>
</signal>
<signal name="PC6">
<contactref element="X11" pad="19"/>
<contactref element="X8" pad="9"/>
<contactref element="U1" pad="P$23"/>
</signal>
<signal name="PC7">
<contactref element="X11" pad="17"/>
<contactref element="X8" pad="15"/>
<contactref element="U1" pad="P$22"/>
</signal>
<signal name="PD0">
<contactref element="X11" pad="50"/>
<contactref element="X9" pad="14"/>
<contactref element="U1" pad="P$1"/>
</signal>
<signal name="PD1">
<contactref element="X11" pad="48"/>
<contactref element="X9" pad="12"/>
<contactref element="U1" pad="P$2"/>
</signal>
<signal name="PD2">
<contactref element="X11" pad="52"/>
<contactref element="X6" pad="3"/>
<contactref element="U1" pad="P$3"/>
</signal>
<signal name="PD3">
<contactref element="X11" pad="46"/>
<contactref element="X8" pad="13"/>
<contactref element="U1" pad="P$4"/>
</signal>
<signal name="PD4">
<contactref element="X11" pad="40"/>
<contactref element="JP4" pad="3"/>
<contactref element="U1" pad="P$125"/>
</signal>
<signal name="PD5">
<contactref element="X11" pad="38"/>
<contactref element="JP5" pad="3"/>
<contactref element="U1" pad="P$126"/>
</signal>
<signal name="PD6">
<contactref element="X11" pad="44"/>
<contactref element="U4" pad="4"/>
<contactref element="U1" pad="P$127"/>
</signal>
<signal name="PD7">
<contactref element="X11" pad="42"/>
<contactref element="X8" pad="14"/>
<contactref element="U1" pad="P$128"/>
</signal>
<signal name="PF0">
<contactref element="D4" pad="A"/>
<contactref element="X11" pad="66"/>
<contactref element="U1" pad="P$42"/>
</signal>
<signal name="PF1">
<contactref element="X11" pad="68"/>
<contactref element="X9" pad="1"/>
<contactref element="U1" pad="P$43"/>
</signal>
<signal name="PF2">
<contactref element="X11" pad="70"/>
<contactref element="X9" pad="3"/>
<contactref element="U1" pad="P$44"/>
</signal>
<signal name="PF3">
<contactref element="X11" pad="72"/>
<contactref element="X9" pad="5"/>
<contactref element="U1" pad="P$45"/>
</signal>
<signal name="PF4">
<contactref element="D3" pad="A"/>
<contactref element="X11" pad="64"/>
<contactref element="U1" pad="P$46"/>
</signal>
<signal name="PE0">
<contactref element="X11" pad="14"/>
<contactref element="X8" pad="6"/>
<contactref element="U1" pad="P$15"/>
</signal>
<signal name="PE1">
<contactref element="X11" pad="16"/>
<contactref element="X8" pad="8"/>
<contactref element="U1" pad="P$14"/>
</signal>
<signal name="PE2">
<contactref element="X11" pad="18"/>
<contactref element="X8" pad="10"/>
<contactref element="U1" pad="P$13"/>
</signal>
<signal name="PE3">
<contactref element="X11" pad="20"/>
<contactref element="X8" pad="12"/>
<contactref element="U1" pad="P$12"/>
</signal>
<signal name="PE4">
<contactref element="X11" pad="22"/>
<contactref element="X8" pad="3"/>
<contactref element="U1" pad="P$123"/>
</signal>
<signal name="PE5">
<contactref element="X11" pad="24"/>
<contactref element="X8" pad="11"/>
<contactref element="U1" pad="P$124"/>
</signal>
<signal name="PG0">
<contactref element="X11" pad="31"/>
<contactref element="X9" pad="7"/>
<contactref element="U1" pad="P$49"/>
</signal>
<signal name="PG1">
<contactref element="X11" pad="29"/>
<contactref element="X7" pad="1"/>
<contactref element="U1" pad="P$50"/>
</signal>
<signal name="PH0">
<contactref element="X11" pad="9"/>
<contactref element="X7" pad="13"/>
<contactref element="U1" pad="P$29"/>
</signal>
<signal name="PH1">
<contactref element="X11" pad="11"/>
<contactref element="X7" pad="15"/>
<contactref element="U1" pad="P$30"/>
</signal>
<signal name="PH2">
<contactref element="X11" pad="13"/>
<contactref element="X9" pad="6"/>
<contactref element="U1" pad="P$31"/>
</signal>
<signal name="PH3">
<contactref element="X11" pad="15"/>
<contactref element="X9" pad="8"/>
<contactref element="U1" pad="P$32"/>
</signal>
<signal name="PJ0">
<contactref element="X11" pad="82"/>
<contactref element="USR_SW1" pad="P$2"/>
<contactref element="USR_SW1" pad="P$1"/>
<contactref element="U1" pad="P$116"/>
</signal>
<signal name="PJ1">
<contactref element="X11" pad="84"/>
<contactref element="USR_SW2" pad="P$2"/>
<contactref element="USR_SW2" pad="P$1"/>
<contactref element="U1" pad="P$117"/>
</signal>
<signal name="PK0">
<contactref element="X11" pad="26"/>
<contactref element="X6" pad="10"/>
<contactref element="U1" pad="P$18"/>
</signal>
<signal name="PK1">
<contactref element="X11" pad="28"/>
<contactref element="X6" pad="12"/>
<contactref element="U1" pad="P$19"/>
</signal>
<signal name="PK2">
<contactref element="X11" pad="30"/>
<contactref element="X6" pad="14"/>
<contactref element="U1" pad="P$20"/>
</signal>
<signal name="PK3">
<contactref element="X11" pad="32"/>
<contactref element="X6" pad="16"/>
<contactref element="U1" pad="P$21"/>
</signal>
<signal name="PK4">
<contactref element="X11" pad="77"/>
<contactref element="X7" pad="3"/>
<contactref element="U1" pad="P$63"/>
</signal>
<signal name="PK5">
<contactref element="X11" pad="75"/>
<contactref element="X7" pad="5"/>
<contactref element="U1" pad="P$62"/>
</signal>
<signal name="PK6">
<contactref element="X11" pad="63"/>
<contactref element="X7" pad="17"/>
<contactref element="U1" pad="P$61"/>
</signal>
<signal name="PK7">
<contactref element="X11" pad="59"/>
<contactref element="X7" pad="19"/>
<contactref element="U1" pad="P$60"/>
</signal>
<signal name="PL0">
<contactref element="X11" pad="43"/>
<contactref element="X9" pad="13"/>
<contactref element="U1" pad="P$81"/>
</signal>
<signal name="PL1">
<contactref element="X11" pad="45"/>
<contactref element="X9" pad="15"/>
<contactref element="U1" pad="P$82"/>
</signal>
<signal name="PL2">
<contactref element="X11" pad="47"/>
<contactref element="X9" pad="17"/>
<contactref element="U1" pad="P$83"/>
</signal>
<signal name="PL3">
<contactref element="X11" pad="49"/>
<contactref element="X9" pad="19"/>
<contactref element="U1" pad="P$84"/>
</signal>
<signal name="PL4">
<contactref element="X11" pad="65"/>
<contactref element="X9" pad="9"/>
<contactref element="U1" pad="P$85"/>
</signal>
<signal name="PL5">
<contactref element="X11" pad="79"/>
<contactref element="X9" pad="11"/>
<contactref element="U1" pad="P$86"/>
</signal>
<signal name="USBD_P">
<contactref element="TP6" pad="TP"/>
<contactref element="U2" pad="3"/>
<contactref element="U7" pad="P3"/>
<contactref element="U1" pad="P$94"/>
</signal>
<signal name="USBD_N">
<contactref element="TP5" pad="TP"/>
<contactref element="U2" pad="1"/>
<contactref element="U7" pad="P2"/>
<contactref element="U1" pad="P$93"/>
</signal>
<signal name="PM0">
<contactref element="X11" pad="41"/>
<contactref element="X7" pad="7"/>
<contactref element="U1" pad="P$78"/>
</signal>
<signal name="PM1">
<contactref element="X11" pad="39"/>
<contactref element="X7" pad="9"/>
<contactref element="U1" pad="P$77"/>
</signal>
<signal name="PM2">
<contactref element="X11" pad="37"/>
<contactref element="X7" pad="11"/>
<contactref element="U1" pad="P$76"/>
</signal>
<signal name="PM3">
<contactref element="X11" pad="33"/>
<contactref element="X9" pad="4"/>
<contactref element="U1" pad="P$75"/>
</signal>
<signal name="PM4">
<contactref element="X11" pad="92"/>
<contactref element="X8" pad="18"/>
<contactref element="U1" pad="P$74"/>
</signal>
<signal name="PM5">
<contactref element="X11" pad="90"/>
<contactref element="X8" pad="20"/>
<contactref element="U1" pad="P$73"/>
</signal>
<signal name="PM6">
<contactref element="X11" pad="88"/>
<contactref element="X7" pad="20"/>
<contactref element="U1" pad="P$72"/>
</signal>
<signal name="PM7">
<contactref element="X11" pad="86"/>
<contactref element="X7" pad="4"/>
<contactref element="U1" pad="P$71"/>
</signal>
<signal name="PP0">
<contactref element="X11" pad="54"/>
<contactref element="X6" pad="5"/>
<contactref element="U1" pad="P$118"/>
</signal>
<signal name="PP1">
<contactref element="X11" pad="56"/>
<contactref element="X6" pad="7"/>
<contactref element="U1" pad="P$119"/>
</signal>
<signal name="PP2">
<contactref element="X11" pad="71"/>
<contactref element="X9" pad="20"/>
<contactref element="U1" pad="P$103"/>
</signal>
<signal name="PP3">
<contactref element="X11" pad="73"/>
<contactref element="X7" pad="16"/>
<contactref element="U1" pad="P$104"/>
</signal>
<signal name="PP4">
<contactref element="X11" pad="78"/>
<contactref element="X6" pad="15"/>
<contactref element="U1" pad="P$105"/>
</signal>
<signal name="PP5">
<contactref element="X11" pad="80"/>
<contactref element="X7" pad="6"/>
<contactref element="U1" pad="P$106"/>
</signal>
<signal name="PN0">
<contactref element="X11" pad="85"/>
<contactref element="D2" pad="A"/>
<contactref element="U1" pad="P$107"/>
</signal>
<signal name="PN1">
<contactref element="X11" pad="87"/>
<contactref element="D1" pad="A"/>
<contactref element="U1" pad="P$108"/>
</signal>
<signal name="PN2">
<contactref element="X11" pad="89"/>
<contactref element="X9" pad="16"/>
<contactref element="U1" pad="P$109"/>
</signal>
<signal name="PN3">
<contactref element="X11" pad="91"/>
<contactref element="X9" pad="18"/>
<contactref element="U1" pad="P$110"/>
</signal>
<signal name="PN4">
<contactref element="X11" pad="81"/>
<contactref element="X6" pad="19"/>
<contactref element="U1" pad="P$111"/>
</signal>
<signal name="PN5">
<contactref element="X11" pad="83"/>
<contactref element="X6" pad="17"/>
<contactref element="U1" pad="P$112"/>
</signal>
<signal name="PQ0">
<contactref element="X11" pad="51"/>
<contactref element="X6" pad="13"/>
<contactref element="U1" pad="P$5"/>
</signal>
<signal name="PQ1">
<contactref element="X11" pad="53"/>
<contactref element="X7" pad="18"/>
<contactref element="U1" pad="P$6"/>
</signal>
<signal name="PQ2">
<contactref element="X11" pad="55"/>
<contactref element="X7" pad="12"/>
<contactref element="R19" pad="1"/>
<contactref element="U1" pad="P$11"/>
</signal>
<signal name="PQ3">
<contactref element="X11" pad="57"/>
<contactref element="X7" pad="14"/>
<contactref element="R20" pad="1"/>
<contactref element="U1" pad="P$27"/>
</signal>
<signal name="PQ4">
<contactref element="X11" pad="93"/>
<contactref element="U4" pad="5"/>
<contactref element="U1" pad="P$102"/>
</signal>
<signal name="EN0RXI_N">
<contactref element="R21" pad="2"/>
<contactref element="U10" pad="P$8"/>
<contactref element="U1" pad="P$53"/>
</signal>
<signal name="EN0RXI_P">
<contactref element="R22" pad="2"/>
<contactref element="U10" pad="P$6"/>
<contactref element="U1" pad="P$54"/>
</signal>
<signal name="EN0TXO_N">
<contactref element="R23" pad="2"/>
<contactref element="U10" pad="P$3"/>
<contactref element="U1" pad="P$56"/>
</signal>
<signal name="EN0TXO_P">
<contactref element="R24" pad="2"/>
<contactref element="U10" pad="P$1"/>
<contactref element="U1" pad="P$57"/>
</signal>
<signal name="RBIAS">
<contactref element="R25" pad="1"/>
<contactref element="U1" pad="P$59"/>
</signal>
<signal name="N$4">
<contactref element="D4" pad="C"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="D3" pad="C"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="D1" pad="C"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U7" pad="P$1"/>
<contactref element="U7" pad="P$2"/>
<contactref element="U7" pad="P$3"/>
<contactref element="U7" pad="P$4"/>
<contactref element="U7" pad="P$5"/>
<contactref element="U7" pad="P$6"/>
<contactref element="R52" pad="2"/>
<contactref element="C32" pad="1"/>
</signal>
<signal name="TARGET_VDDC">
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="TP12" pad="TP"/>
<contactref element="U1" pad="P$87"/>
<contactref element="U1" pad="P$115"/>
</signal>
<signal name="VBAT">
<contactref element="TP11" pad="TP"/>
<contactref element="R39" pad="1"/>
<contactref element="R42" pad="1"/>
<contactref element="R38" pad="1"/>
</signal>
<signal name="!WAKE">
<contactref element="TP10" pad="TP"/>
<contactref element="R42" pad="2"/>
<contactref element="WAKE" pad="P$1"/>
<contactref element="WAKE" pad="P$2"/>
<contactref element="X11" pad="95"/>
<contactref element="U1" pad="P$64"/>
</signal>
<signal name="!HIB">
<contactref element="TP9" pad="TP"/>
<contactref element="U1" pad="P$65"/>
</signal>
<signal name="VREF+">
<contactref element="TP13" pad="TP"/>
<contactref element="R41" pad="1"/>
<contactref element="X11" pad="34"/>
<contactref element="U1" pad="P$9"/>
</signal>
<signal name="N$29">
<contactref element="C45" pad="1"/>
<contactref element="Y1" pad="P$1"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="Y1" pad="P$3"/>
<contactref element="C44" pad="1"/>
<contactref element="U1" pad="P$88"/>
</signal>
<signal name="N$30">
<contactref element="C47" pad="1"/>
<contactref element="U1" pad="P$67"/>
<contactref element="Y3" pad="P$2"/>
</signal>
<signal name="N$33">
<contactref element="C48" pad="1"/>
<contactref element="U1" pad="P$66"/>
<contactref element="Y3" pad="P$1"/>
</signal>
<signal name="BP2_A2.5">
<contactref element="X6" pad="9"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="BP2_A2.6">
<contactref element="X6" pad="11"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="N$32">
<contactref element="R32" pad="2"/>
<contactref element="U10" pad="P$15"/>
</signal>
<signal name="N$34">
<contactref element="R43" pad="2"/>
<contactref element="U10" pad="P$10"/>
</signal>
<signal name="N$36">
<contactref element="R32" pad="1"/>
<contactref element="R43" pad="1"/>
<contactref element="R46" pad="1"/>
<contactref element="R45" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="JACK_TX_P">
<contactref element="U14" pad="1"/>
<contactref element="U13" pad="8"/>
<contactref element="U13" pad="1"/>
<contactref element="U10" pad="P$16"/>
</signal>
<signal name="JACK_TX_N">
<contactref element="U14" pad="2"/>
<contactref element="U13" pad="7"/>
<contactref element="U10" pad="P$14"/>
<contactref element="U13" pad="2"/>
</signal>
<signal name="JACK_RX_P">
<contactref element="U14" pad="3"/>
<contactref element="U13" pad="6"/>
<contactref element="U13" pad="3"/>
<contactref element="U10" pad="P$11"/>
</signal>
<signal name="JACK_RX_N">
<contactref element="U14" pad="6"/>
<contactref element="U13" pad="5"/>
<contactref element="U13" pad="4"/>
<contactref element="U10" pad="P$9"/>
</signal>
<signal name="N$44">
<contactref element="U14" pad="4"/>
<contactref element="U14" pad="5"/>
<contactref element="R45" pad="2"/>
</signal>
<signal name="N$45">
<contactref element="U14" pad="7"/>
<contactref element="U14" pad="8"/>
<contactref element="R46" pad="2"/>
</signal>
<signal name="MCU_3V3">
<contactref element="C40" pad="1"/>
<contactref element="C43" pad="1"/>
<contactref element="C42" pad="1"/>
<contactref element="C41" pad="1"/>
<contactref element="R41" pad="2"/>
<contactref element="R39" pad="2"/>
<contactref element="R44" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="U10" pad="P$2"/>
<contactref element="U10" pad="P$7"/>
<contactref element="U1" pad="P$7"/>
<contactref element="U1" pad="P$16"/>
<contactref element="U1" pad="P$26"/>
<contactref element="U1" pad="P$28"/>
<contactref element="U1" pad="P$39"/>
<contactref element="U1" pad="P$47"/>
<contactref element="U1" pad="P$51"/>
<contactref element="U1" pad="P$52"/>
<contactref element="U1" pad="P$69"/>
<contactref element="U1" pad="P$79"/>
<contactref element="U1" pad="P$90"/>
<contactref element="U1" pad="P$101"/>
<contactref element="U1" pad="P$113"/>
<contactref element="U1" pad="P$122"/>
<contactref element="U1" pad="P$8"/>
</signal>
<signal name="VBUS">
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="4"/>
<contactref element="U4" pad="2"/>
<contactref element="R35" pad="1"/>
<contactref element="R36" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U4" pad="3"/>
<contactref element="R35" pad="2"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R36" pad="1"/>
<contactref element="U4" pad="8"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="N$11">
<contactref element="R38" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="P$68"/>
</signal>
<signal name="N$12">
<contactref element="R40" pad="2"/>
<contactref element="U6" pad="P3"/>
</signal>
<signal name="N$13">
<contactref element="C20" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="U5" pad="1"/>
<contactref element="R48" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="D2" pad="C"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="TARGET_ID">
<contactref element="R18" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="TP7" pad="TP"/>
<contactref element="U7" pad="P4"/>
</signal>
<signal name="N$15">
<contactref element="U20" pad="P$46"/>
<contactref element="R28" pad="1"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R49" pad="2"/>
<contactref element="U1" pad="P$89"/>
</signal>
<signal name="N$17">
<contactref element="U20" pad="P$41"/>
<contactref element="R50" pad="1"/>
</signal>
<signal name="!TARGET_RESET_FILTERED">
<contactref element="R44" pad="2"/>
<contactref element="C46" pad="1"/>
<contactref element="R51" pad="2"/>
<contactref element="U1" pad="P$70"/>
</signal>
<signal name="CHASSIS">
<contactref element="U14" pad="9"/>
<contactref element="U14" pad="10"/>
<contactref element="C31" pad="1"/>
<contactref element="R47" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="C33" pad="1"/>
<contactref element="U22" pad="P6"/>
<contactref element="U22" pad="P7"/>
<contactref element="U22" pad="P8"/>
<contactref element="U22" pad="P9"/>
<contactref element="U22" pad="P10"/>
<contactref element="U22" pad="P11"/>
<contactref element="R34" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
