(kicad_pcb (version 20171130) (host pcbnew 5.0.1)
  (general
    (thickness 1.6002)
    (drawings 41)
    (tracks 917)
    (zones 0)
    (modules 24)
    (nets 113)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /DROK_MC_IN2)
  (net 4 /DROK_MC_IN1)
  (net 5 /DROK_MC_ENA1)
  (net 6 /DROK_MC_ENA2)
  (net 7 /DROK_MC_IN3)
  (net 8 /DROK_MC_IN4)
  (net 9 /EXTRA_OUT1)
  (net 10 /EXTRA_OUT2)
  (net 11 +24V)
  (net 12 /SCL)
  (net 13 /SDA)
  (net 14 +3V3)
  (net 15 /Relays/RELAY_1)
  (net 16 /Relays/RELAY_2)
  (net 17 /Relays/RELAY_3)
  (net 18 /Relays/RELAY_4)
  (net 19 /Relays/RELAY_5)
  (net 20 /Relays/RELAY_6)
  (net 21 /Relays/RELAY_7)
  (net 22 /Relays/RELAY_8)
  (net 23 /Relays/RELAY_9)
  (net 24 /Relays/RELAY_10)
  (net 25 /Relays/RELAY_11)
  (net 26 /Relays/RELAY_12)
  (net 27 /Relays/RELAY_13)
  (net 28 /Relays/RELAY_14)
  (net 29 /Relays/RELAY_15)
  (net 30 /Relays/RELAY_16)
  (net 31 /Hall_Encoder)
  (net 32 /Hall_Stop)
  (net 33 /PIN_PUMP_O1)
  (net 34 /PIN_PUMP_O2)
  (net 35 /EXTRA_OUT_BUF1)
  (net 36 /EXTRA_OUT_BUF2)
  (net 37 /PIN_PUMP_ENA)
  (net 38 /PIN_REEL_O2)
  (net 39 /PIN_REEL_O1)
  (net 40 /PIN_REEL_ENA)
  (net 41 "Net-(U5-Pad15)")
  (net 42 "Net-(U5-Pad25)")
  (net 43 "Net-(U5-Pad26)")
  (net 44 "Net-(U5-Pad28)")
  (net 45 "Net-(U5-Pad29)")
  (net 46 "Net-(U5-Pad37)")
  (net 47 "Net-(U5-Pad10)")
  (net 48 "Net-(U5-Pad9)")
  (net 49 "Net-(U5-Pad8)")
  (net 50 "Net-(U5-Pad7)")
  (net 51 "Net-(U5-Pad38)")
  (net 52 "Net-(U5-Pad39)")
  (net 53 "Net-(U5-Pad40)")
  (net 54 "Net-(U5-Pad41)")
  (net 55 "Net-(U5-Pad42)")
  (net 56 "Net-(U5-Pad43)")
  (net 57 "Net-(U5-Pad44)")
  (net 58 "Net-(U5-Pad54)")
  (net 59 "Net-(U5-Pad56)")
  (net 60 "Net-(U5-Pad57)")
  (net 61 "Net-(U5-Pad63)")
  (net 62 "Net-(U5-Pad64)")
  (net 63 "Net-(U5-Pad65)")
  (net 64 "Net-(U5-Pad66)")
  (net 65 "Net-(U5-Pad67)")
  (net 66 "Net-(U5-Pad68)")
  (net 67 "Net-(U5-Pad69)")
  (net 68 "Net-(U5-Pad70)")
  (net 69 "Net-(U5-Pad71)")
  (net 70 "Net-(U5-Pad72)")
  (net 71 "Net-(U5-Pad73)")
  (net 72 "Net-(U5-Pad74)")
  (net 73 "Net-(U5-Pad75)")
  (net 74 "Net-(U5-Pad76)")
  (net 75 "Net-(U5-Pad77)")
  (net 76 "Net-(U5-Pad78)")
  (net 77 "Net-(U5-Pad79)")
  (net 78 "Net-(U5-Pad80)")
  (net 79 "Net-(U5-Pad81)")
  (net 80 "Net-(U5-Pad82)")
  (net 81 "Net-(U5-Pad83)")
  (net 82 "Net-(U5-Pad84)")
  (net 83 "Net-(U5-Pad85)")
  (net 84 "Net-(U5-Pad86)")
  (net 85 "Net-(U5-Pad58)")
  (net 86 "Net-(U5-Pad59)")
  (net 87 "Net-(U5-Pad60)")
  (net 88 "Net-(U5-Pad61)")
  (net 89 "Net-(U5-Pad62)")
  (net 90 VALVE_PIN_7)
  (net 91 VALVE_PIN_6)
  (net 92 VALVE_PIN_5)
  (net 93 VALVE_PIN_4)
  (net 94 VALVE_PIN_8)
  (net 95 VALVE_PIN_3)
  (net 96 VALVE_PIN_2)
  (net 97 VALVE_PIN_1)
  (net 98 VALVE_PIN_16)
  (net 99 VALVE_PIN_9)
  (net 100 VALVE_PIN_10)
  (net 101 VALVE_PIN_11)
  (net 102 VALVE_PIN_12)
  (net 103 VALVE_PIN_13)
  (net 104 VALVE_PIN_14)
  (net 105 VALVE_PIN_15)
  (net 106 /PPM_DEPTH)
  (net 107 /PPM_GO)
  (net 108 /PPM_BOTL_SEL)
  (net 109 /+24V_SW)
  (net 110 "Net-(U5-Pad55)")
  (net 111 "Net-(U5-Pad52)")
  (net 112 "Net-(U5-Pad27)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_gap 0.1524)
    (diff_pair_width 0.1524)
    (add_net /DROK_MC_ENA1)
    (add_net /DROK_MC_ENA2)
    (add_net /DROK_MC_IN1)
    (add_net /DROK_MC_IN2)
    (add_net /DROK_MC_IN3)
    (add_net /DROK_MC_IN4)
    (add_net /EXTRA_OUT1)
    (add_net /EXTRA_OUT2)
    (add_net /EXTRA_OUT_BUF1)
    (add_net /EXTRA_OUT_BUF2)
    (add_net /Hall_Encoder)
    (add_net /Hall_Stop)
    (add_net /PIN_PUMP_ENA)
    (add_net /PIN_PUMP_O1)
    (add_net /PIN_PUMP_O2)
    (add_net /PIN_REEL_ENA)
    (add_net /PIN_REEL_O1)
    (add_net /PIN_REEL_O2)
    (add_net /PPM_BOTL_SEL)
    (add_net /PPM_DEPTH)
    (add_net /PPM_GO)
    (add_net /Relays/RELAY_1)
    (add_net /Relays/RELAY_10)
    (add_net /Relays/RELAY_11)
    (add_net /Relays/RELAY_12)
    (add_net /Relays/RELAY_13)
    (add_net /Relays/RELAY_14)
    (add_net /Relays/RELAY_15)
    (add_net /Relays/RELAY_16)
    (add_net /Relays/RELAY_2)
    (add_net /Relays/RELAY_3)
    (add_net /Relays/RELAY_4)
    (add_net /Relays/RELAY_5)
    (add_net /Relays/RELAY_6)
    (add_net /Relays/RELAY_7)
    (add_net /Relays/RELAY_8)
    (add_net /Relays/RELAY_9)
    (add_net /SCL)
    (add_net /SDA)
    (add_net "Net-(U5-Pad10)")
    (add_net "Net-(U5-Pad15)")
    (add_net "Net-(U5-Pad25)")
    (add_net "Net-(U5-Pad26)")
    (add_net "Net-(U5-Pad27)")
    (add_net "Net-(U5-Pad28)")
    (add_net "Net-(U5-Pad29)")
    (add_net "Net-(U5-Pad37)")
    (add_net "Net-(U5-Pad38)")
    (add_net "Net-(U5-Pad39)")
    (add_net "Net-(U5-Pad40)")
    (add_net "Net-(U5-Pad41)")
    (add_net "Net-(U5-Pad42)")
    (add_net "Net-(U5-Pad43)")
    (add_net "Net-(U5-Pad44)")
    (add_net "Net-(U5-Pad52)")
    (add_net "Net-(U5-Pad54)")
    (add_net "Net-(U5-Pad55)")
    (add_net "Net-(U5-Pad56)")
    (add_net "Net-(U5-Pad57)")
    (add_net "Net-(U5-Pad58)")
    (add_net "Net-(U5-Pad59)")
    (add_net "Net-(U5-Pad60)")
    (add_net "Net-(U5-Pad61)")
    (add_net "Net-(U5-Pad62)")
    (add_net "Net-(U5-Pad63)")
    (add_net "Net-(U5-Pad64)")
    (add_net "Net-(U5-Pad65)")
    (add_net "Net-(U5-Pad66)")
    (add_net "Net-(U5-Pad67)")
    (add_net "Net-(U5-Pad68)")
    (add_net "Net-(U5-Pad69)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad70)")
    (add_net "Net-(U5-Pad71)")
    (add_net "Net-(U5-Pad72)")
    (add_net "Net-(U5-Pad73)")
    (add_net "Net-(U5-Pad74)")
    (add_net "Net-(U5-Pad75)")
    (add_net "Net-(U5-Pad76)")
    (add_net "Net-(U5-Pad77)")
    (add_net "Net-(U5-Pad78)")
    (add_net "Net-(U5-Pad79)")
    (add_net "Net-(U5-Pad8)")
    (add_net "Net-(U5-Pad80)")
    (add_net "Net-(U5-Pad81)")
    (add_net "Net-(U5-Pad82)")
    (add_net "Net-(U5-Pad83)")
    (add_net "Net-(U5-Pad84)")
    (add_net "Net-(U5-Pad85)")
    (add_net "Net-(U5-Pad86)")
    (add_net "Net-(U5-Pad9)")
    (add_net VALVE_PIN_1)
    (add_net VALVE_PIN_10)
    (add_net VALVE_PIN_11)
    (add_net VALVE_PIN_12)
    (add_net VALVE_PIN_13)
    (add_net VALVE_PIN_14)
    (add_net VALVE_PIN_15)
    (add_net VALVE_PIN_16)
    (add_net VALVE_PIN_2)
    (add_net VALVE_PIN_3)
    (add_net VALVE_PIN_4)
    (add_net VALVE_PIN_5)
    (add_net VALVE_PIN_6)
    (add_net VALVE_PIN_7)
    (add_net VALVE_PIN_8)
    (add_net VALVE_PIN_9)
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 1.016)
    (via_drill 0.508)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_gap 0.1524)
    (diff_pair_width 0.1524)
    (add_net +24V)
    (add_net +3V3)
    (add_net +5V)
    (add_net /+24V_SW)
    (add_net GND)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5C2CDD23)
    (at 148.59 78.74 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "PPM Inputs" (at -2.794 4.953 180) (layer F.SilkS))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 /PPM_GO))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 /PPM_DEPTH))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 /PPM_BOTL_SEL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C2CDCF5)
    (at 138.43 57.15 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value +24V (at 0 4.87 180) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +24V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_8x10 (layer F.Cu) (tedit 5C2CDE78)
    (at 184.15 62.23 270)
    (descr "SMT capacitor, aluminium electrolytic, 8x10, Nichicon ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference 100u1 (at 0 -5.2 270) (layer F.SilkS))
    (fp_text value CP1 (at 0 5.2 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -3.25 0 270) (size 3.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 3.25 0 270) (size 3.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5C2CDD44)
    (at 180.34 92.71 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at -2.54 -1.524 180) (layer F.SilkS))
    (fp_text value DROK_REEL (at -2.413 4.318 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /DROK_MC_IN2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /DROK_MC_IN1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /DROK_MC_ENA1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5C2CDD3B)
    (at 180.34 111.76 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value DROK_PUMP (at -3.683 2.286 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /DROK_MC_ENA2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /DROK_MC_IN3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /DROK_MC_IN4))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5C2CDD40)
    (at 179.07 99.06 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J3 (at -2.159 -0.254 180) (layer F.SilkS))
    (fp_text value "Extra Out" (at -2.032 5.207 180) (layer F.SilkS))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /EXTRA_OUT1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /EXTRA_OUT2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C2CDCFF)
    (at 143.51 54.61)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Switch (at 0 4.87) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 /+24V_SW))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +24V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C2CDD4B)
    (at 181.61 77.47 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J5 (at -2.413 -2.794 180) (layer F.SilkS))
    (fp_text value "DROK Pwr" (at -2.413 2.413 180) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5C2CDD5C)
    (at 179.07 69.85 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J6 (at -2.159 -1.397 180) (layer F.SilkS))
    (fp_text value "External I2C" (at -2.159 4.445 180) (layer F.SilkS))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SCL))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /SDA))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x09_P2.54mm_Vertical (layer F.Cu) (tedit 5C2CDD30)
    (at 135.89 97.79 90)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J7 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value "Relay Board" (at 4.953 11.049 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 10.16 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /Relays/RELAY_1))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Relays/RELAY_2))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /Relays/RELAY_3))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /Relays/RELAY_4))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /Relays/RELAY_5))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /Relays/RELAY_6))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /Relays/RELAY_7))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /Relays/RELAY_8))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /Relays/RELAY_9))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /Relays/RELAY_10))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /Relays/RELAY_11))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /Relays/RELAY_12))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /Relays/RELAY_13))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /Relays/RELAY_14))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /Relays/RELAY_15))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /Relays/RELAY_16))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5C2CDD07)
    (at 156.21 60.96 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at -1.27 8.128) (layer F.SilkS))
    (fp_text value Hall_Encoder (at 1.27 12.065 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /Hall_Encoder))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5C2CDD1E)
    (at 156.21 71.12 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J9 (at -1.143 8.255) (layer F.SilkS))
    (fp_text value Hall_Stop (at 1.016 10.414) (layer F.SilkS))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /Hall_Stop))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5C2CDD56)
    (at 185.42 73.66)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -1.016 1.778) (layer F.SilkS))
    (fp_text value 4.7k (at 1.778 1.82) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 +3V3))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 /SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5C2CDD52)
    (at 180.34 73.66)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.54 1.778) (layer F.SilkS))
    (fp_text value 4,7k (at 0.635 1.905) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 /SDA))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5C2CDD0D)
    (at 156.21 64.77)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -6.604 0.508) (layer F.SilkS))
    (fp_text value 10k (at -3.937 0.508) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 31 /Hall_Encoder))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5C2CDD13)
    (at 156.21 67.31)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -6.604 0.381) (layer F.SilkS))
    (fp_text value 10k (at -3.81 0.381) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 +3V3))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 32 /Hall_Stop))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 154.94 54.61 180)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U1 (at -2.54 2.159 180) (layer F.SilkS))
    (fp_text value OKI-78SR (at 2.54 2.5 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 109 /+24V_SW))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 182.88 105.41 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -5.375 90) (layer F.SilkS))
    (fp_text value 74LS125 (at 0 5.375 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.015001 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /PIN_PUMP_O1))
    (pad 2 smd rect (at -2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /DROK_MC_IN3))
    (pad 4 smd rect (at -2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /PIN_PUMP_O2))
    (pad 5 smd rect (at -2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /DROK_MC_IN4))
    (pad 7 smd rect (at -2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /EXTRA_OUT1))
    (pad 9 smd rect (at 2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /EXTRA_OUT_BUF1))
    (pad 11 smd rect (at 2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /EXTRA_OUT2))
    (pad 12 smd rect (at 2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /EXTRA_OUT_BUF2))
    (pad 14 smd rect (at 2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 182.88 85.09 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at -2.667 -5.334 90) (layer F.SilkS))
    (fp_text value 74LS125 (at 0 5.375 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 14 smd rect (at 2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 13 smd rect (at 2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /PIN_PUMP_ENA))
    (pad 12 smd rect (at 2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /DROK_MC_ENA2))
    (pad 10 smd rect (at 2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /PIN_REEL_O2))
    (pad 9 smd rect (at 2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /DROK_MC_IN2))
    (pad 7 smd rect (at -2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /DROK_MC_IN1))
    (pad 5 smd rect (at -2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /PIN_REEL_O1))
    (pad 3 smd rect (at -2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /DROK_MC_ENA1))
    (pad 2 smd rect (at -2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /PIN_REEL_ENA))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 140.97 87.63 270)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 -5.375 270) (layer F.SilkS))
    (fp_text value 74LS125 (at 0 5.375 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 97 VALVE_PIN_1))
    (pad 2 smd rect (at -2.7 -2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 -1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /Relays/RELAY_1))
    (pad 4 smd rect (at -2.7 0 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 96 VALVE_PIN_2))
    (pad 5 smd rect (at -2.7 1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.7 2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /Relays/RELAY_2))
    (pad 7 smd rect (at -2.7 3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /Relays/RELAY_3))
    (pad 9 smd rect (at 2.7 2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 2.7 1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 VALVE_PIN_3))
    (pad 11 smd rect (at 2.7 0 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /Relays/RELAY_4))
    (pad 12 smd rect (at 2.7 -1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 2.7 -2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 VALVE_PIN_4))
    (pad 14 smd rect (at 2.7 -3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module teensy:Teensy35_36 (layer F.Cu) (tedit 58E3CF68)
    (at 167.64 83.82 270)
    (fp_text reference U5 (at 31.877 -9.525 270) (layer F.SilkS))
    (fp_text value Teensy3.6 (at -0.127 -0.127 270) (layer F.Fab))
    (pad 17 thru_hole circle (at 11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 90 VALVE_PIN_7))
    (pad 18 thru_hole circle (at 13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 91 VALVE_PIN_6))
    (pad 19 thru_hole circle (at 16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 92 VALVE_PIN_5))
    (pad 20 thru_hole circle (at 19.05 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 93 VALVE_PIN_4))
    (pad 16 thru_hole circle (at 8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 94 VALVE_PIN_8))
    (pad 15 thru_hole circle (at 6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 "Net-(U5-Pad15)"))
    (pad 14 thru_hole circle (at 3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 /PIN_PUMP_O2))
    (pad 21 thru_hole circle (at 21.59 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 95 VALVE_PIN_3))
    (pad 22 thru_hole circle (at 24.13 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 96 VALVE_PIN_2))
    (pad 23 thru_hole circle (at 26.67 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 97 VALVE_PIN_1))
    (pad 24 thru_hole circle (at 29.21 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 98 VALVE_PIN_16))
    (pad 25 thru_hole circle (at 16.51 5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 42 "Net-(U5-Pad25)"))
    (pad 26 thru_hole circle (at 16.51 2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 "Net-(U5-Pad26)"))
    (pad 27 thru_hole circle (at 16.51 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 112 "Net-(U5-Pad27)"))
    (pad 28 thru_hole circle (at 16.51 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 "Net-(U5-Pad28)"))
    (pad 29 thru_hole circle (at 16.51 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 "Net-(U5-Pad29)"))
    (pad 30 thru_hole circle (at 29.21 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 99 VALVE_PIN_9))
    (pad 31 thru_hole circle (at 26.67 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 100 VALVE_PIN_10))
    (pad 32 thru_hole circle (at 24.13 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 101 VALVE_PIN_11))
    (pad 33 thru_hole circle (at 21.59 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 102 VALVE_PIN_12))
    (pad 34 thru_hole circle (at 19.05 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 103 VALVE_PIN_13))
    (pad 35 thru_hole circle (at 16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 104 VALVE_PIN_14))
    (pad 36 thru_hole circle (at 13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 105 VALVE_PIN_15))
    (pad 37 thru_hole circle (at 11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 "Net-(U5-Pad37)"))
    (pad 13 thru_hole circle (at 1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 /PIN_PUMP_O1))
    (pad 12 thru_hole circle (at -1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 106 /PPM_DEPTH))
    (pad 11 thru_hole circle (at -3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 107 /PPM_GO))
    (pad 10 thru_hole circle (at -6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 "Net-(U5-Pad10)"))
    (pad 9 thru_hole circle (at -8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 48 "Net-(U5-Pad9)"))
    (pad 8 thru_hole circle (at -11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 "Net-(U5-Pad8)"))
    (pad 7 thru_hole circle (at -13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 "Net-(U5-Pad7)"))
    (pad 6 thru_hole circle (at -16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 /Hall_Stop))
    (pad 5 thru_hole circle (at -19.05 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 /Hall_Encoder))
    (pad 4 thru_hole circle (at -21.59 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 /PIN_PUMP_ENA))
    (pad 3 thru_hole circle (at -24.13 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 /EXTRA_OUT_BUF2))
    (pad 2 thru_hole circle (at -26.67 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 /EXTRA_OUT_BUF1))
    (pad 1 thru_hole rect (at -29.21 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 38 thru_hole circle (at 8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "Net-(U5-Pad38)"))
    (pad 39 thru_hole circle (at 6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 "Net-(U5-Pad39)"))
    (pad 40 thru_hole circle (at 3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 "Net-(U5-Pad40)"))
    (pad 41 thru_hole circle (at 1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 54 "Net-(U5-Pad41)"))
    (pad 42 thru_hole circle (at -1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 55 "Net-(U5-Pad42)"))
    (pad 43 thru_hole circle (at -3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 56 "Net-(U5-Pad43)"))
    (pad 44 thru_hole circle (at -6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 57 "Net-(U5-Pad44)"))
    (pad 45 thru_hole circle (at -8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 /SDA))
    (pad 46 thru_hole circle (at -11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 /SCL))
    (pad 47 thru_hole circle (at -13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 108 /PPM_BOTL_SEL))
    (pad 48 thru_hole circle (at -16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 /PIN_REEL_O2))
    (pad 49 thru_hole circle (at -19.05 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 39 /PIN_REEL_O1))
    (pad 50 thru_hole circle (at -21.59 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 40 /PIN_REEL_ENA))
    (pad 51 thru_hole circle (at -24.13 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (pad 52 thru_hole circle (at -26.67 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 111 "Net-(U5-Pad52)"))
    (pad 53 thru_hole circle (at -29.21 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 54 thru_hole circle (at -26.67 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 "Net-(U5-Pad54)"))
    (pad 55 thru_hole circle (at -21.59 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 110 "Net-(U5-Pad55)"))
    (pad 56 thru_hole circle (at -19.05 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 59 "Net-(U5-Pad56)"))
    (pad 57 thru_hole circle (at -16.51 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 60 "Net-(U5-Pad57)"))
    (pad 63 thru_hole circle (at -13.97 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 61 "Net-(U5-Pad63)"))
    (pad 64 thru_hole circle (at -11.43 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 "Net-(U5-Pad64)"))
    (pad 65 thru_hole circle (at -8.89 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 "Net-(U5-Pad65)"))
    (pad 66 thru_hole circle (at -6.35 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 "Net-(U5-Pad66)"))
    (pad 67 thru_hole circle (at 8.89 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 "Net-(U5-Pad67)"))
    (pad 68 thru_hole circle (at 11.43 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 "Net-(U5-Pad68)"))
    (pad 69 thru_hole circle (at 13.97 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 "Net-(U5-Pad69)"))
    (pad 70 thru_hole circle (at 19.05 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 68 "Net-(U5-Pad70)"))
    (pad 71 thru_hole circle (at 21.59 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 69 "Net-(U5-Pad71)"))
    (pad 72 thru_hole circle (at 24.13 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 "Net-(U5-Pad72)"))
    (pad 73 thru_hole circle (at 26.67 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 71 "Net-(U5-Pad73)"))
    (pad 74 thru_hole circle (at 29.21 0 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 72 "Net-(U5-Pad74)"))
    (pad 75 thru_hole circle (at 29.21 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 73 "Net-(U5-Pad75)"))
    (pad 76 thru_hole circle (at 26.67 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 "Net-(U5-Pad76)"))
    (pad 77 thru_hole circle (at 24.13 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 "Net-(U5-Pad77)"))
    (pad 78 thru_hole circle (at 21.59 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 76 "Net-(U5-Pad78)"))
    (pad 79 thru_hole circle (at 19.05 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 77 "Net-(U5-Pad79)"))
    (pad 80 thru_hole circle (at 13.97 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 78 "Net-(U5-Pad80)"))
    (pad 81 thru_hole circle (at 11.43 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 79 "Net-(U5-Pad81)"))
    (pad 82 thru_hole circle (at 8.89 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 80 "Net-(U5-Pad82)"))
    (pad 83 thru_hole circle (at -6.35 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 81 "Net-(U5-Pad83)"))
    (pad 84 thru_hole circle (at -8.89 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 82 "Net-(U5-Pad84)"))
    (pad 85 thru_hole circle (at -11.43 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 83 "Net-(U5-Pad85)"))
    (pad 86 thru_hole circle (at -13.97 -2.54 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 84 "Net-(U5-Pad86)"))
    (pad 58 thru_hole circle (at -22.86 4.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 85 "Net-(U5-Pad58)"))
    (pad 59 thru_hole circle (at -20.32 4.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 86 "Net-(U5-Pad59)"))
    (pad 60 thru_hole circle (at -17.78 4.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 87 "Net-(U5-Pad60)"))
    (pad 61 thru_hole circle (at -15.24 4.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 88 "Net-(U5-Pad61)"))
    (pad 62 thru_hole circle (at -12.7 4.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 89 "Net-(U5-Pad62)"))
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 139.7 104.14 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at 0 -5.375 90) (layer F.SilkS))
    (fp_text value 74LS125 (at 0 5.375 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 14 smd rect (at 2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 13 smd rect (at 2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 VALVE_PIN_8))
    (pad 12 smd rect (at 2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /Relays/RELAY_8))
    (pad 10 smd rect (at 2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 VALVE_PIN_7))
    (pad 9 smd rect (at 2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /Relays/RELAY_7))
    (pad 7 smd rect (at -2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /Relays/RELAY_6))
    (pad 5 smd rect (at -2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 91 VALVE_PIN_6))
    (pad 3 smd rect (at -2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /Relays/RELAY_5))
    (pad 2 smd rect (at -2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 VALVE_PIN_5))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 152.4 87.63 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U7 (at 0 -5.375 90) (layer F.SilkS))
    (fp_text value 74LS125 (at 0 5.375 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 14 smd rect (at 2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 13 smd rect (at 2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 102 VALVE_PIN_12))
    (pad 12 smd rect (at 2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /Relays/RELAY_12))
    (pad 10 smd rect (at 2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 101 VALVE_PIN_11))
    (pad 9 smd rect (at 2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /Relays/RELAY_11))
    (pad 7 smd rect (at -2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /Relays/RELAY_10))
    (pad 5 smd rect (at -2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 100 VALVE_PIN_10))
    (pad 3 smd rect (at -2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /Relays/RELAY_9))
    (pad 2 smd rect (at -2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 99 VALVE_PIN_9))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 152.4 104.14 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U8 (at 0 -5.375 90) (layer F.SilkS))
    (fp_text value 74LS125 (at 0 5.375 90) (layer F.Fab))
    (fp_text user %R (at -1.035001 2.674999 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 103 VALVE_PIN_13))
    (pad 2 smd rect (at -2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /Relays/RELAY_13))
    (pad 4 smd rect (at -2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 104 VALVE_PIN_14))
    (pad 5 smd rect (at -2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /Relays/RELAY_14))
    (pad 7 smd rect (at -2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /Relays/RELAY_15))
    (pad 9 smd rect (at 2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 105 VALVE_PIN_15))
    (pad 11 smd rect (at 2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /Relays/RELAY_16))
    (pad 12 smd rect (at 2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 98 VALVE_PIN_16))
    (pad 14 smd rect (at 2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "WaterSampler v1.0\nSimpleUnmanned, LLC\nAndy Vaselaar\n2019-01-02" (at 136.525 71.12 90) (layer F.SilkS))
  (gr_line (start 130.81 117.602) (end 130.81 96.266) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 190.754 117.602) (end 130.81 117.602) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 190.754 50.8) (end 190.754 117.602) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 50.8) (end 190.754 50.8) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 96.266) (end 130.81 50.8) (layer Edge.Cuts) (width 0.1))
  (gr_text GO (at 148.59 76.454) (layer F.SilkS))
  (gr_text DEP (at 151.13 76.454) (layer F.SilkS))
  (gr_text BOT (at 153.543 76.454) (layer F.SilkS))
  (gr_text SIG (at 153.67 73.66) (layer F.SilkS))
  (gr_text "3.3\n" (at 156.21 73.66) (layer F.SilkS))
  (gr_text SIG (at 153.797 58.674) (layer F.SilkS))
  (gr_text "3.3\n" (at 156.21 58.674) (layer F.SilkS))
  (gr_text +5V (at 149.733 52.705) (layer F.SilkS))
  (gr_text +24V (at 154.813 52.705) (layer F.SilkS))
  (gr_text GND (at 152.4 52.705) (layer F.SilkS))
  (gr_text GND (at 151.003 58.674) (layer F.SilkS))
  (gr_text GND (at 151.003 73.66) (layer F.SilkS))
  (gr_text GND (at 156.21 76.454) (layer F.SilkS))
  (gr_text GND (at 156.21 100.076) (layer F.SilkS))
  (gr_text GND (at 156.337 92.964) (layer F.SilkS))
  (gr_text "15\n" (at 153.67 100.076) (layer F.SilkS))
  (gr_text 16 (at 153.67 92.964) (layer F.SilkS))
  (gr_text 2 (at 136.017 92.964) (layer F.SilkS))
  (gr_text 1 (at 136.017 100.076) (layer F.SilkS))
  (gr_text "IN4\n" (at 185.42 114.3) (layer F.SilkS))
  (gr_text ENA2 (at 180.086 114.173) (layer F.SilkS))
  (gr_text IN3 (at 183.007 114.173) (layer F.SilkS))
  (gr_text 2 (at 184.277 96.774) (layer F.SilkS))
  (gr_text 1 (at 181.737 96.774) (layer F.SilkS))
  (gr_text GND (at 186.944 96.774) (layer F.SilkS))
  (gr_text "+5V\n" (at 178.816 96.774) (layer F.SilkS))
  (gr_text IN2 (at 185.42 90.424) (layer F.SilkS))
  (gr_text IN1 (at 182.88 90.424) (layer F.SilkS))
  (gr_text ENA1 (at 180.467 90.424) (layer F.SilkS))
  (gr_text GND (at 186.69 67.945) (layer F.SilkS))
  (gr_text SCL (at 184.15 67.945) (layer F.SilkS))
  (gr_text SDA (at 181.61 67.945) (layer F.SilkS))
  (gr_text "3.3\n" (at 179.07 67.945) (layer F.SilkS))
  (gr_text GND (at 178.816 77.597) (layer F.SilkS))
  (gr_text "+5V\n" (at 187.071 77.724) (layer F.SilkS))
)
