(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 29)
    (tracks 322)
    (zones 0)
    (modules 30)
    (nets 20)
  )
  (page A4)
  (title_block
    (title "DMX Demonstrator - Analog IO PWM (DMX-IO4)")
    (date 2023-12-19)
    (rev 1.5)
    (company "Sparky Bobo Designs")
    (comment 2 "Designed by: SparkyBobo")
    (comment 3 https://creativecommons.org/licenses/by-sa/4.0/)
    (comment 4 "Released under the Creative Commons Attribution Share-Alike 4.0m License")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.15)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "grb"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /AO1)
  (net 3 /AO0)
  (net 4 /AO3)
  (net 5 /AO2)
  (net 6 "Net-(J2-Pad2)")
  (net 7 "Net-(J2-Pad3)")
  (net 8 "Net-(J2-Pad4)")
  (net 9 "Net-(J2-Pad5)")
  (net 10 "Net-(R1-Pad2)")
  (net 11 +5V)
  (net 12 "Net-(C5-Pad1)")
  (net 13 "Net-(C4-Pad2)")
  (net 14 "Net-(RV1-Pad1)")
  (net 15 "Net-(C3-Pad2)")
  (net 16 "Net-(R4-Pad1)")
  (net 17 "Net-(C7-Pad1)")
  (net 18 "Net-(D1-Pad2)")
  (net 19 VDC)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net /AO0)
    (add_net /AO1)
    (add_net /AO2)
    (add_net /AO3)
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(RV1-Pad1)")
    (add_net VDC)
  )
  (net_class Power ""
    (clearance 0.25)
    (trace_width 0.75)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 1.27)
    (uvia_drill 0.635)
    (diff_pair_width 0.75)
    (diff_pair_gap 0.25)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
  )
  (module Package_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 153.6065 90.7415)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 7.62 -2.286) (layer F.SilkS))
    (fp_text value LM339 (at 3.81 17.57) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad4)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /AO3))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C5-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /AO1))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /AO0))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C5-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 VDC))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /AO2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C5-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad5)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 164.2745 87.122 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad4)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 VDC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 167.386 110.109 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at -1.8415 0 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 VDC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 164.2745 110.109 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at -1.8415 0 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 VDC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 167.386 87.122 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at -1.778 -0.0635 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad5)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 VDC))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3299P_Horizontal (layer F.Cu) (tedit 5A3D4994)
    (at 147.701 119.507 90)
    (descr "Potentiometer, horizontal, Bourns 3299P, https://www.bourns.com/pdfs/3299.pdf")
    (tags "Potentiometer horizontal Bourns 3299P")
    (fp_text reference RV1 (at -6.096 3.175 180) (layer F.SilkS))
    (fp_text value 10k (at -0.76 8.555 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(RV1-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3299P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MC:PhoenixContact_MC_1,5_2-G-3.81_1x02_P3.81mm_Horizontal (layer F.Cu) (tedit 5A00FA1A)
    (at 133.7945 75.1205 180)
    (descr "Generic Phoenix Contact connector footprint for: MC_1,5/2-G-3.81; number of pins: 02; pin pitch: 3.81mm; Angled || order number: 1803277 8A 160V")
    (tags "phoenix_contact connector MC_01x02_G_3.81mm")
    (fp_text reference J4 (at -3.7465 0 180) (layer F.SilkS))
    (fp_text value Power (at 1.905 9 180) (layer F.Fab))
    (fp_text user %R (at 2.905 3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 3.81 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_2-G-3.81_1x02_P3.81mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MC:PhoenixContact_MC_1,5_5-G-3.81_1x05_P3.81mm_Horizontal (layer F.Cu) (tedit 5A00FA1A)
    (at 161.163 75.057 180)
    (descr "Generic Phoenix Contact connector footprint for: MC_1,5/5-G-3.81; number of pins: 05; pin pitch: 3.81mm; Angled || order number: 1803303 8A 160V")
    (tags "phoenix_contact connector MC_01x05_G_3.81mm")
    (fp_text reference J2 (at -1.9685 -3.175 180) (layer F.SilkS))
    (fp_text value Output (at 7.62 9 180) (layer F.Fab))
    (fp_text user %R (at 7.62 3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 3.81 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 7.62 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 11.43 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 15.24 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad5)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_5-G-3.81_1x05_P3.81mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 131.064 108.0135)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C6 (at 1.27 3.7465) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 3.75) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 VDC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 120.8405 80.3275)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C7 (at 1.25 -3.75) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 3.75) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 120.8405 86.614)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at -2.413 0) (layer F.SilkS))
    (fp_text value 1N5819 (at 5.08 2.47) (layer F.Fab))
    (fp_text user %R (at 5.47 0) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown (layer F.Cu) (tedit 5AC8BA0D)
    (at 125.9205 91.1225 180)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference U3 (at 2.54 -20.58 180) (layer F.SilkS))
    (fp_text value LM317T (at 2.54 2 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -20.58 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 VDC))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(R4-Pad1)"))
    (pad "" np_thru_hole oval (at 2.54 -16.66 180) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 130.556 91.1225 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -1.8415 0 180) (layer F.SilkS))
    (fp_text value "392 1%" (at 5.08 2.37 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 VDC))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 133.9215 101.2825 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 12.0015 0 180) (layer F.SilkS))
    (fp_text value "2.74k 1%" (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 5AE50EF0)
    (at 141.097 118.491)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (fp_text reference C3 (at -2.413 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 5AE50EF0)
    (at 141.097 115.57)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (fp_text reference C4 (at -2.4765 0) (layer F.SilkS))
    (fp_text value 0.68uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(C4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 5AE50EF0)
    (at 143.5735 121.3485 180)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (fp_text reference C5 (at 4.8895 0 180) (layer F.SilkS))
    (fp_text value 0.68uF (at 1.25 2.25 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 148.1455 111.4425 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 330 (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 144.7165 101.2825 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 12.065 0) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.37 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 141.2875 111.4425 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 171.7675 105.7275 180)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J1 (at -2.8575 0 180) (layer F.SilkS))
    (fp_text value "Analog Extension" (at -2.794 9.779 270) (layer F.Fab))
    (fp_text user %R (at 0 8.89 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /AO3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /AO2))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /AO1))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /AO0))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 140.9065 90.7415)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 0 -2.286) (layer F.SilkS))
    (fp_text value NE555 (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C3-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C4-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(RV1-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 5AE50EF0)
    (at 153.837 87.5665)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (fp_text reference C2 (at 5.1035 -0.6985) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 VDC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 5AE50EF0)
    (at 148.2725 87.5665 180)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (fp_text reference C1 (at 5.08 0.635 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.25 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 63EF0484)
    (at 171.864 71.2775)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 63F18A57)
    (at 120.429 122.9665)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 63EF0607)
    (at 171.864 122.7125)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 63EF048B)
    (at 120.556 71.1505)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MH1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module footprints:OSHW-LOGO-S locked (layer F.Cu) (tedit 200000)
    (at 126.1745 125.095)
    (descr "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (tags "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (attr virtual)
    (fp_text reference "" (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 0) (layer F.SilkS))
  )
  (module footprints:logo_cr_5x5 locked (layer B.Cu) (tedit 0)
    (at 127 122.4915 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text 10k (at 167.3225 92.7735 270) (layer F.SilkS))
  (gr_text 10k (at 164.211 92.7735 270) (layer F.SilkS))
  (gr_text 10k (at 167.3225 105.156 270) (layer F.SilkS))
  (gr_text 10k (at 164.211 105.156 270) (layer F.SilkS))
  (gr_text 10k (at 150.876 119.253 270) (layer F.SilkS))
  (gr_text 0.68uF/ (at 134.4295 121.3485) (layer F.SilkS))
  (gr_text 0.68uF/ (at 134.4295 115.57) (layer F.SilkS))
  (gr_text 0.1uF/ (at 134.9375 118.491) (layer F.SilkS))
  (gr_text 2.74k (at 133.7945 96.139 270) (layer F.SilkS))
  (gr_text 392 (at 130.556 96.393 270) (layer F.SilkS))
  (gr_text 330 (at 148.1455 106.3625 270) (layer F.SilkS))
  (gr_text 10k (at 144.7165 106.3625 270) (layer F.SilkS))
  (gr_text 10k (at 141.2875 106.3625 270) (layer F.SilkS))
  (gr_text LM339 (at 157.353 98.3615 270) (layer F.SilkS))
  (gr_text 555 (at 144.5895 94.6785 270) (layer F.SilkS))
  (gr_arc (start 175.49874 126.182) (end 175.51654 126.9365) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "PWM Output" (at 162.8775 124.841) (layer F.SilkS))
  (gr_text " -    +\nPower In" (at 132.2705 79.756 180) (layer F.SilkS))
  (gr_text "Analog Extention" (at 174.6885 95.9485 90) (layer F.SilkS))
  (gr_line (start 116.9949 66.9595) (end 175.43526 66.95948) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.2507 67.7775) (end 176.25324 126.1642) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 175.4327 67.7775) (end 176.2507 67.7775) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 116.9949 67.7215) (end 116.9949 66.9595) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 117 126.1745) (end 116.2329 126.1975) (angle -88.28261211) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117 126.941945) (end 175.514 126.9365) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.2329 126.1975) (end 116.2329 67.7215) (layer Edge.Cuts) (width 0.15))
  (gr_text "DMX-IO4, Rev 1.5\nSparky Bobo Designs\n\n" (at 137.541 124.968) (layer B.SilkS))
  (gr_text DMX-IO4 (at 133.223 125.1585) (layer F.SilkS))
  (gr_text "G   1   2   3   4\nPWM Out" (at 153.6065 79.883 180) (layer F.SilkS))
  (zone (net 11) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.176 126.8095) (xy 138.176 86.0425) (xy 149.7965 86.0425) (xy 149.7965 89.8525) (xy 151.003 91.694)
        (xy 151.003 108.458) (xy 156.718 108.458) (xy 156.718 116.5225) (xy 169.672 116.5225) (xy 169.672 86.1695)
        (xy 176.149 86.1695) (xy 176.149 126.0475) (xy 175.387 126.8095)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.149 126.0475) (xy 175.387 126.8095) (xy 116.967 126.8095) (xy 116.332 126.1745) (xy 116.332 119.38)
        (xy 129.032 119.38) (xy 129.032 89.3445) (xy 116.332 89.3445) (xy 116.332 67.691) (xy 116.9035 67.056)
        (xy 175.4505 67.056) (xy 176.149 67.691)
      )
    )
  )
  (zone (net 19) (net_name VDC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 89.789) (xy 128.651 89.8525) (xy 128.651 118.999) (xy 116.332 118.999)
      )
    )
  )
  (zone (net 19) (net_name VDC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.6045 126.8095) (xy 116.967 126.8095) (xy 116.332 126.1745) (xy 116.332 67.691) (xy 116.9035 67.056)
        (xy 175.4505 67.056) (xy 176.149 67.691) (xy 176.149 85.6615) (xy 169.037 85.62975) (xy 169.037 115.91925)
        (xy 157.2895 115.951) (xy 157.2895 107.95) (xy 151.5745 107.95) (xy 151.5745 91.44) (xy 150.3045 89.535)
        (xy 150.3045 85.471) (xy 137.6045 85.471)
      )
    )
  )
)
