(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 64)
    (zones 0)
    (modules 3)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.7 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad8)")
  (net 2 "Net-(J1-Pad7)")
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad4)")
  (net 6 "Net-(J1-Pad3)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
  )
  (module sub:sub2 (layer F.Cu) (tedit 0)
    (at 134.5 113.45 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 144.56 130.11 270)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J1 (at -0.03 -2.74 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x08_MountingPin (at 0 20.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sub:nmcard (layer F.Cu) (tedit 61F4B8CB)
    (at 134.694999 94.444999)
    (fp_text reference J2 (at 0 7.4) (layer F.SilkS) hide)
    (fp_text value Micro_SD_Card (at 0.03 -7.5) (layer F.Fab) hide)
    (pad 8 smd custom (at 2.2 5.1) (size 2 0.725) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 8 smd custom (at 3.4 3) (size 1 5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 7 smd rect (at 2 2.5) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 6 smd rect (at -0.3 3) (size 2 5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 5 smd rect (at -2.9 3) (size 2 5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 4 smd custom (at 2.2 -5.4) (size 2 0.725) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad5)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 4 smd custom (at 3.4 -3.3) (size 1 5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad5)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 3 smd rect (at 2 -2.9) (size 1.5 4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 2 smd rect (at -0.3 -3.3) (size 2 5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad7)"))
    (pad 1 smd rect (at -2.9 -3.3) (size 2 5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad8)"))
  )
  (gr_text "JT\nVer 1.2" (at 134.75 119.2 90) (layer B.SilkS))
  (gr_line (start 124.7 124.7) (end 130.3 124.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.7 132.3) (end 124.7 124.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 146.85 132.3) (end 124.7 132.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 146.85 124.8) (end 146.85 132.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139 124.8) (end 146.85 124.8) (layer Edge.Cuts) (width 0.05))
  (gr_text TCK (at 129.36 127.3 90) (layer F.SilkS))
  (gr_text VCC (at 131.9 127.25 90) (layer F.SilkS))
  (gr_text TDO (at 134.5 127.3 90) (layer F.SilkS))
  (gr_text RST (at 144.44 127.39 90) (layer F.SilkS))
  (gr_text GND (at 141.9 127.2 90) (layer F.SilkS))
  (gr_text TMS (at 139.45 127.25 90) (layer F.SilkS))
  (gr_text TDI (at 136.82 127.3 90) (layer F.SilkS))
  (gr_line (start 139 124.8) (end 139 88.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 130.3 88.3) (end 130.3 124.7) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139 88.3) (end 130.3 88.3) (layer Edge.Cuts) (width 0.05))
)
