<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="101.0412" y2="0" width="0" layer="20"/>
<wire x1="101.0412" y1="0" x2="101.0412" y2="57.785" width="0" layer="20"/>
<wire x1="101.0412" y1="57.785" x2="0" y2="57.785" width="0" layer="20"/>
<wire x1="0" y1="57.785" x2="0" y2="0" width="0" layer="20"/>
<text>RX</text>
<text>TX</text>
<text>VCC</text>
<text>GND</text>
<text>FTDI 3.3V ONLY!</text>
<text>VCC</text>
<text>I2C HEADER</text>
<text>-</text>
<text>10k</text>
<text>100k Ω</text>
<text>100k Ω</text>
<text>ICSP
HEADER</text>
<text>RST</text>
<text>0.1µF</text>
<text>CR1220</text>
<text>GREEN</text>
<text>BLACK</text>
<text>POWER</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>GND</text>
<text>TX</text>
<text>RX</text>
<text>DTR</text>
<text>SDA</text>
<text>SDA</text>
<text>SCL</text>
<text>SCL</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>POWER</text>
<text>New Molex 
microSD
502774-0891</text>
<hole x="72.644" y="0.381" drill="0.381"/>
<hole x="72.644" y="1.016" drill="0.381"/>
<hole x="72.644" y="1.651" drill="0.381"/>
<hole x="72.644" y="2.286" drill="0.381"/>
<hole x="72.644" y="2.921" drill="0.381"/>
<hole x="72.644" y="3.556" drill="0.381"/>
<hole x="72.644" y="4.191" drill="0.381"/>
<hole x="72.644" y="4.826" drill="0.381"/>
<hole x="72.644" y="5.461" drill="0.381"/>
<hole x="72.644" y="6.096" drill="0.381"/>
<hole x="72.644" y="6.731" drill="0.381"/>
<hole x="72.644" y="7.366" drill="0.381"/>
<hole x="72.644" y="8.001" drill="0.381"/>
<hole x="72.644" y="8.636" drill="0.381"/>
<hole x="72.644" y="9.271" drill="0.381"/>
<hole x="72.644" y="9.906" drill="0.381"/>
<hole x="72.644" y="10.541" drill="0.381"/>
<hole x="72.644" y="11.176" drill="0.381"/>
<hole x="72.644" y="11.811" drill="0.381"/>
<hole x="72.644" y="12.446" drill="0.381"/>
<hole x="72.644" y="13.081" drill="0.381"/>
<hole x="72.644" y="13.716" drill="0.381"/>
<hole x="72.644" y="14.351" drill="0.381"/>
<hole x="72.644" y="14.986" drill="0.381"/>
<hole x="72.644" y="15.621" drill="0.381"/>
<hole x="72.644" y="16.256" drill="0.381"/>
<hole x="72.644" y="16.891" drill="0.381"/>
<hole x="72.644" y="17.526" drill="0.381"/>
<hole x="72.644" y="18.161" drill="0.381"/>
<hole x="72.644" y="18.796" drill="0.381"/>
<hole x="72.644" y="19.431" drill="0.381"/>
<hole x="72.644" y="20.066" drill="0.381"/>
<hole x="72.644" y="20.701" drill="0.381"/>
<hole x="72.644" y="21.336" drill="0.381"/>
<hole x="72.644" y="21.971" drill="0.381"/>
<hole x="72.644" y="22.606" drill="0.381"/>
<hole x="72.644" y="23.241" drill="0.381"/>
<hole x="72.644" y="23.876" drill="0.381"/>
<hole x="72.644" y="24.511" drill="0.381"/>
<hole x="72.644" y="25.146" drill="0.381"/>
<hole x="72.644" y="25.781" drill="0.381"/>
<hole x="72.644" y="26.416" drill="0.381"/>
<hole x="72.644" y="27.051" drill="0.381"/>
<hole x="72.644" y="27.686" drill="0.381"/>
<hole x="72.644" y="28.321" drill="0.381"/>
<hole x="72.644" y="28.956" drill="0.381"/>
<hole x="72.644" y="29.591" drill="0.381"/>
<hole x="72.644" y="30.226" drill="0.381"/>
<hole x="72.644" y="30.861" drill="0.381"/>
<hole x="72.644" y="31.496" drill="0.381"/>
<hole x="72.644" y="32.131" drill="0.381"/>
<hole x="72.644" y="32.766" drill="0.381"/>
<hole x="72.644" y="33.401" drill="0.381"/>
<hole x="72.644" y="34.036" drill="0.381"/>
<hole x="72.644" y="34.671" drill="0.381"/>
<hole x="72.644" y="35.306" drill="0.381"/>
<hole x="72.644" y="35.941" drill="0.381"/>
<hole x="72.644" y="36.576" drill="0.381"/>
<hole x="72.644" y="37.211" drill="0.381"/>
<hole x="72.644" y="37.846" drill="0.381"/>
<hole x="72.644" y="38.481" drill="0.381"/>
<hole x="72.644" y="39.116" drill="0.381"/>
<hole x="72.644" y="39.751" drill="0.381"/>
<hole x="72.644" y="40.386" drill="0.381"/>
<hole x="72.644" y="41.021" drill="0.381"/>
<hole x="72.644" y="41.656" drill="0.381"/>
<hole x="72.644" y="42.291" drill="0.381"/>
<hole x="72.644" y="42.926" drill="0.381"/>
<hole x="72.644" y="43.561" drill="0.381"/>
<hole x="72.644" y="44.196" drill="0.381"/>
<hole x="72.644" y="44.831" drill="0.381"/>
<hole x="72.644" y="45.466" drill="0.381"/>
<hole x="78.994" y="32.004" drill="0.381"/>
<hole x="78.359" y="32.004" drill="0.381"/>
<hole x="77.724" y="32.004" drill="0.381"/>
<hole x="77.089" y="32.004" drill="0.381"/>
<hole x="76.454" y="32.004" drill="0.381"/>
<hole x="75.819" y="32.004" drill="0.381"/>
<hole x="75.184" y="32.004" drill="0.381"/>
<hole x="74.549" y="32.004" drill="0.381"/>
<hole x="73.914" y="32.004" drill="0.381"/>
<hole x="73.279" y="32.004" drill="0.381"/>
<hole x="73.279" y="10.668" drill="0.381"/>
<hole x="73.914" y="10.668" drill="0.381"/>
<hole x="74.549" y="10.668" drill="0.381"/>
<hole x="75.184" y="10.668" drill="0.381"/>
<hole x="75.819" y="10.668" drill="0.381"/>
<hole x="76.454" y="10.668" drill="0.381"/>
<hole x="77.089" y="10.668" drill="0.381"/>
<hole x="77.724" y="10.668" drill="0.381"/>
<hole x="73.3044" y="21.336" drill="0.381"/>
<hole x="73.9394" y="21.336" drill="0.381"/>
<hole x="74.5744" y="21.336" drill="0.381"/>
<hole x="75.2094" y="21.336" drill="0.381"/>
<hole x="75.8444" y="21.336" drill="0.381"/>
<hole x="76.4794" y="21.336" drill="0.381"/>
<hole x="77.1144" y="21.336" drill="0.381"/>
<hole x="77.7494" y="21.336" drill="0.381"/>
<hole x="78.3844" y="21.336" drill="0.381"/>
<hole x="79.0194" y="21.336" drill="0.381"/>
<hole x="78.359" y="10.668" drill="0.381"/>
<hole x="78.994" y="10.668" drill="0.381"/>
<text>VCC</text>
<text>VCC</text>
<text>SLP</text>
<text>SLP</text>
<text>GND</text>
<text>GND</text>
<text>VOUT</text>
<text>VOUT</text>
<text>GND</text>
<text>GND</text>
<text>SLP</text>
<text>VCC</text>
<text>GND</text>
<text>VOUT</text>
<text>VCC</text>
<text>SLP</text>
<text>GND</text>
<text>VOUT</text>
<hole x="79.756" y="0.381" drill="0.381"/>
<hole x="79.756" y="1.016" drill="0.381"/>
<hole x="79.756" y="1.651" drill="0.381"/>
<hole x="79.756" y="2.286" drill="0.381"/>
<hole x="79.756" y="2.921" drill="0.381"/>
<hole x="79.756" y="3.556" drill="0.381"/>
<hole x="79.756" y="4.191" drill="0.381"/>
<hole x="79.756" y="4.826" drill="0.381"/>
<hole x="79.756" y="5.461" drill="0.381"/>
<hole x="79.756" y="6.096" drill="0.381"/>
<hole x="79.756" y="6.731" drill="0.381"/>
<hole x="79.756" y="7.366" drill="0.381"/>
<hole x="79.756" y="8.001" drill="0.381"/>
<hole x="79.756" y="8.636" drill="0.381"/>
<hole x="79.756" y="9.271" drill="0.381"/>
<hole x="79.756" y="9.906" drill="0.381"/>
<hole x="79.756" y="10.541" drill="0.381"/>
<hole x="79.756" y="11.176" drill="0.381"/>
<hole x="79.756" y="11.811" drill="0.381"/>
<hole x="79.756" y="12.446" drill="0.381"/>
<hole x="79.756" y="13.081" drill="0.381"/>
<hole x="79.756" y="13.716" drill="0.381"/>
<hole x="79.756" y="14.351" drill="0.381"/>
<hole x="79.756" y="14.986" drill="0.381"/>
<hole x="79.756" y="15.621" drill="0.381"/>
<hole x="79.756" y="16.256" drill="0.381"/>
<hole x="79.756" y="16.891" drill="0.381"/>
<hole x="79.756" y="17.526" drill="0.381"/>
<hole x="79.756" y="18.161" drill="0.381"/>
<hole x="79.756" y="18.796" drill="0.381"/>
<hole x="79.756" y="19.431" drill="0.381"/>
<hole x="79.756" y="20.066" drill="0.381"/>
<hole x="79.756" y="20.701" drill="0.381"/>
<hole x="79.756" y="21.336" drill="0.381"/>
<hole x="79.756" y="21.971" drill="0.381"/>
<hole x="79.756" y="22.606" drill="0.381"/>
<hole x="79.756" y="23.241" drill="0.381"/>
<hole x="79.756" y="23.876" drill="0.381"/>
<hole x="79.756" y="24.511" drill="0.381"/>
<hole x="79.756" y="25.146" drill="0.381"/>
<hole x="79.756" y="25.781" drill="0.381"/>
<hole x="79.756" y="26.416" drill="0.381"/>
<hole x="79.756" y="27.051" drill="0.381"/>
<hole x="79.756" y="27.686" drill="0.381"/>
<hole x="79.756" y="28.321" drill="0.381"/>
<hole x="79.756" y="28.956" drill="0.381"/>
<hole x="79.756" y="29.591" drill="0.381"/>
<hole x="79.756" y="30.226" drill="0.381"/>
<hole x="79.756" y="30.861" drill="0.381"/>
<hole x="79.756" y="31.496" drill="0.381"/>
<hole x="79.756" y="32.131" drill="0.381"/>
<hole x="79.756" y="32.766" drill="0.381"/>
<hole x="79.756" y="33.401" drill="0.381"/>
<hole x="79.756" y="34.036" drill="0.381"/>
<hole x="79.756" y="34.671" drill="0.381"/>
<hole x="79.756" y="35.306" drill="0.381"/>
<hole x="79.756" y="35.941" drill="0.381"/>
<hole x="79.756" y="36.576" drill="0.381"/>
<hole x="79.756" y="37.211" drill="0.381"/>
<hole x="79.756" y="37.846" drill="0.381"/>
<hole x="79.756" y="38.481" drill="0.381"/>
<hole x="79.756" y="39.116" drill="0.381"/>
<hole x="79.756" y="39.751" drill="0.381"/>
<hole x="79.756" y="40.386" drill="0.381"/>
<hole x="79.756" y="41.021" drill="0.381"/>
<hole x="79.756" y="41.656" drill="0.381"/>
<hole x="79.756" y="42.291" drill="0.381"/>
<hole x="79.756" y="42.926" drill="0.381"/>
<hole x="79.756" y="43.561" drill="0.381"/>
<hole x="79.756" y="44.196" drill="0.381"/>
<hole x="79.756" y="44.831" drill="0.381"/>
<hole x="79.756" y="45.466" drill="0.381"/>
<hole x="80.518" y="10.668" drill="0.381"/>
<hole x="81.153" y="10.668" drill="0.381"/>
<hole x="81.788" y="10.668" drill="0.381"/>
<hole x="82.423" y="10.668" drill="0.381"/>
<hole x="83.058" y="10.668" drill="0.381"/>
<hole x="83.693" y="10.668" drill="0.381"/>
<hole x="84.328" y="10.668" drill="0.381"/>
<hole x="84.963" y="10.668" drill="0.381"/>
<hole x="85.598" y="10.668" drill="0.381"/>
<hole x="86.233" y="10.668" drill="0.381"/>
<hole x="80.391" y="21.336" drill="0.381"/>
<hole x="81.026" y="21.336" drill="0.381"/>
<hole x="81.661" y="21.336" drill="0.381"/>
<hole x="82.296" y="21.336" drill="0.381"/>
<hole x="82.931" y="21.336" drill="0.381"/>
<hole x="83.566" y="21.336" drill="0.381"/>
<hole x="84.201" y="21.336" drill="0.381"/>
<hole x="84.836" y="21.336" drill="0.381"/>
<hole x="85.471" y="21.336" drill="0.381"/>
<hole x="86.106" y="21.336" drill="0.381"/>
<hole x="86.233" y="32.004" drill="0.381"/>
<hole x="85.598" y="32.004" drill="0.381"/>
<hole x="84.963" y="32.004" drill="0.381"/>
<hole x="84.328" y="32.004" drill="0.381"/>
<hole x="83.693" y="32.004" drill="0.381"/>
<hole x="83.058" y="32.004" drill="0.381"/>
<hole x="82.423" y="32.004" drill="0.381"/>
<hole x="81.788" y="32.004" drill="0.381"/>
<hole x="81.153" y="32.004" drill="0.381"/>
<hole x="80.518" y="32.004" drill="0.381"/>
<hole x="86.868" y="0.381" drill="0.381"/>
<hole x="86.868" y="1.016" drill="0.381"/>
<hole x="86.868" y="1.651" drill="0.381"/>
<hole x="86.868" y="2.286" drill="0.381"/>
<hole x="86.868" y="2.921" drill="0.381"/>
<hole x="86.868" y="3.556" drill="0.381"/>
<hole x="86.868" y="4.191" drill="0.381"/>
<hole x="86.868" y="4.826" drill="0.381"/>
<hole x="86.868" y="5.461" drill="0.381"/>
<hole x="86.868" y="6.096" drill="0.381"/>
<hole x="86.868" y="6.731" drill="0.381"/>
<hole x="86.868" y="7.366" drill="0.381"/>
<hole x="86.868" y="8.001" drill="0.381"/>
<hole x="86.868" y="8.636" drill="0.381"/>
<hole x="86.868" y="9.271" drill="0.381"/>
<hole x="86.868" y="9.906" drill="0.381"/>
<hole x="86.868" y="10.541" drill="0.381"/>
<hole x="86.868" y="11.176" drill="0.381"/>
<hole x="86.868" y="11.811" drill="0.381"/>
<hole x="86.868" y="12.446" drill="0.381"/>
<hole x="86.868" y="13.081" drill="0.381"/>
<hole x="86.868" y="13.716" drill="0.381"/>
<hole x="86.868" y="14.351" drill="0.381"/>
<hole x="86.868" y="14.986" drill="0.381"/>
<hole x="86.868" y="15.621" drill="0.381"/>
<hole x="86.868" y="16.256" drill="0.381"/>
<hole x="86.868" y="16.891" drill="0.381"/>
<hole x="86.868" y="17.526" drill="0.381"/>
<hole x="86.868" y="18.161" drill="0.381"/>
<hole x="86.868" y="18.796" drill="0.381"/>
<hole x="86.868" y="19.431" drill="0.381"/>
<hole x="86.868" y="20.066" drill="0.381"/>
<hole x="86.868" y="20.701" drill="0.381"/>
<hole x="86.868" y="21.336" drill="0.381"/>
<hole x="86.868" y="21.971" drill="0.381"/>
<hole x="86.868" y="22.606" drill="0.381"/>
<hole x="86.868" y="23.241" drill="0.381"/>
<hole x="86.868" y="23.876" drill="0.381"/>
<hole x="86.868" y="24.511" drill="0.381"/>
<hole x="86.868" y="25.146" drill="0.381"/>
<hole x="86.868" y="25.781" drill="0.381"/>
<hole x="86.868" y="26.416" drill="0.381"/>
<hole x="86.868" y="27.051" drill="0.381"/>
<hole x="86.868" y="27.686" drill="0.381"/>
<hole x="86.868" y="28.321" drill="0.381"/>
<hole x="86.868" y="28.956" drill="0.381"/>
<hole x="86.868" y="29.591" drill="0.381"/>
<hole x="86.868" y="30.226" drill="0.381"/>
<hole x="86.868" y="30.861" drill="0.381"/>
<hole x="86.868" y="31.496" drill="0.381"/>
<hole x="86.868" y="32.131" drill="0.381"/>
<hole x="86.868" y="32.766" drill="0.381"/>
<hole x="86.868" y="33.401" drill="0.381"/>
<hole x="86.868" y="34.036" drill="0.381"/>
<hole x="86.868" y="34.671" drill="0.381"/>
<hole x="86.868" y="35.306" drill="0.381"/>
<hole x="86.868" y="35.941" drill="0.381"/>
<hole x="86.868" y="36.576" drill="0.381"/>
<hole x="86.868" y="37.211" drill="0.381"/>
<hole x="86.868" y="37.846" drill="0.381"/>
<hole x="86.868" y="38.481" drill="0.381"/>
<hole x="86.868" y="39.116" drill="0.381"/>
<hole x="86.868" y="39.751" drill="0.381"/>
<hole x="86.868" y="40.386" drill="0.381"/>
<hole x="86.868" y="41.021" drill="0.381"/>
<hole x="86.868" y="41.656" drill="0.381"/>
<hole x="86.868" y="42.291" drill="0.381"/>
<hole x="86.868" y="42.926" drill="0.381"/>
<hole x="86.868" y="43.561" drill="0.381"/>
<hole x="86.868" y="44.196" drill="0.381"/>
<hole x="86.868" y="44.831" drill="0.381"/>
<hole x="86.868" y="45.466" drill="0.381"/>
<hole x="93.345" y="32.004" drill="0.381"/>
<hole x="92.71" y="32.004" drill="0.381"/>
<hole x="92.075" y="32.004" drill="0.381"/>
<hole x="91.44" y="32.004" drill="0.381"/>
<hole x="90.805" y="32.004" drill="0.381"/>
<hole x="90.17" y="32.004" drill="0.381"/>
<hole x="89.535" y="32.004" drill="0.381"/>
<hole x="88.9" y="32.004" drill="0.381"/>
<hole x="88.265" y="32.004" drill="0.381"/>
<hole x="87.6046" y="32.004" drill="0.381"/>
<hole x="87.6046" y="10.668" drill="0.381"/>
<hole x="88.265" y="10.668" drill="0.381"/>
<hole x="88.9" y="10.668" drill="0.381"/>
<hole x="89.535" y="10.668" drill="0.381"/>
<hole x="90.17" y="10.668" drill="0.381"/>
<hole x="90.805" y="10.668" drill="0.381"/>
<hole x="91.44" y="10.668" drill="0.381"/>
<hole x="92.075" y="10.668" drill="0.381"/>
<hole x="87.6046" y="21.336" drill="0.381"/>
<hole x="88.265" y="21.336" drill="0.381"/>
<hole x="88.9" y="21.336" drill="0.381"/>
<hole x="89.535" y="21.336" drill="0.381"/>
<hole x="90.17" y="21.336" drill="0.381"/>
<hole x="90.805" y="21.336" drill="0.381"/>
<hole x="91.44" y="21.336" drill="0.381"/>
<hole x="92.075" y="21.336" drill="0.381"/>
<hole x="92.71" y="21.336" drill="0.381"/>
<hole x="93.345" y="21.336" drill="0.381"/>
<hole x="92.71" y="10.668" drill="0.381"/>
<hole x="93.345" y="10.668" drill="0.381"/>
<hole x="93.98" y="0.381" drill="0.381"/>
<hole x="93.98" y="1.016" drill="0.381"/>
<hole x="93.98" y="1.651" drill="0.381"/>
<hole x="93.98" y="2.286" drill="0.381"/>
<hole x="93.98" y="2.921" drill="0.381"/>
<hole x="93.98" y="3.556" drill="0.381"/>
<hole x="93.98" y="4.191" drill="0.381"/>
<hole x="93.98" y="4.826" drill="0.381"/>
<hole x="93.98" y="5.461" drill="0.381"/>
<hole x="93.98" y="6.096" drill="0.381"/>
<hole x="93.98" y="6.731" drill="0.381"/>
<hole x="93.98" y="7.366" drill="0.381"/>
<hole x="93.98" y="8.001" drill="0.381"/>
<hole x="93.98" y="8.636" drill="0.381"/>
<hole x="93.98" y="9.271" drill="0.381"/>
<hole x="93.98" y="9.906" drill="0.381"/>
<hole x="93.98" y="10.541" drill="0.381"/>
<hole x="93.98" y="11.176" drill="0.381"/>
<hole x="93.98" y="11.811" drill="0.381"/>
<hole x="93.98" y="12.446" drill="0.381"/>
<hole x="93.98" y="13.081" drill="0.381"/>
<hole x="93.98" y="13.716" drill="0.381"/>
<hole x="93.98" y="14.351" drill="0.381"/>
<hole x="93.98" y="14.986" drill="0.381"/>
<hole x="93.98" y="15.621" drill="0.381"/>
<hole x="93.98" y="16.256" drill="0.381"/>
<hole x="93.98" y="16.891" drill="0.381"/>
<hole x="93.98" y="17.526" drill="0.381"/>
<hole x="93.98" y="18.161" drill="0.381"/>
<hole x="93.98" y="18.796" drill="0.381"/>
<hole x="93.98" y="19.431" drill="0.381"/>
<hole x="93.98" y="20.066" drill="0.381"/>
<hole x="93.98" y="20.701" drill="0.381"/>
<hole x="93.98" y="21.336" drill="0.381"/>
<hole x="93.98" y="21.971" drill="0.381"/>
<hole x="93.98" y="22.606" drill="0.381"/>
<hole x="93.98" y="23.241" drill="0.381"/>
<hole x="93.98" y="23.876" drill="0.381"/>
<hole x="93.98" y="24.511" drill="0.381"/>
<hole x="93.98" y="25.146" drill="0.381"/>
<hole x="93.98" y="25.781" drill="0.381"/>
<hole x="93.98" y="26.416" drill="0.381"/>
<hole x="93.98" y="27.051" drill="0.381"/>
<hole x="93.98" y="27.686" drill="0.381"/>
<hole x="93.98" y="28.321" drill="0.381"/>
<hole x="93.98" y="28.956" drill="0.381"/>
<hole x="93.98" y="29.591" drill="0.381"/>
<hole x="93.98" y="30.226" drill="0.381"/>
<hole x="93.98" y="30.861" drill="0.381"/>
<hole x="93.98" y="31.496" drill="0.381"/>
<hole x="93.98" y="32.131" drill="0.381"/>
<hole x="93.98" y="32.766" drill="0.381"/>
<hole x="93.98" y="33.401" drill="0.381"/>
<hole x="93.98" y="34.036" drill="0.381"/>
<hole x="93.98" y="34.671" drill="0.381"/>
<hole x="93.98" y="35.306" drill="0.381"/>
<hole x="93.98" y="35.941" drill="0.381"/>
<hole x="93.98" y="36.576" drill="0.381"/>
<hole x="93.98" y="37.211" drill="0.381"/>
<hole x="93.98" y="37.846" drill="0.381"/>
<hole x="93.98" y="38.481" drill="0.381"/>
<hole x="93.98" y="39.116" drill="0.381"/>
<hole x="93.98" y="39.751" drill="0.381"/>
<hole x="93.98" y="40.386" drill="0.381"/>
<hole x="93.98" y="41.021" drill="0.381"/>
<hole x="93.98" y="41.656" drill="0.381"/>
<hole x="93.98" y="42.291" drill="0.381"/>
<hole x="93.98" y="42.926" drill="0.381"/>
<hole x="93.98" y="43.561" drill="0.381"/>
<hole x="93.98" y="44.196" drill="0.381"/>
<hole x="93.98" y="44.831" drill="0.381"/>
<hole x="93.98" y="45.466" drill="0.381"/>
<hole x="94.615" y="10.668" drill="0.381"/>
<hole x="95.25" y="10.668" drill="0.381"/>
<hole x="95.885" y="10.668" drill="0.381"/>
<hole x="96.52" y="10.668" drill="0.381"/>
<hole x="97.155" y="10.668" drill="0.381"/>
<hole x="97.79" y="10.668" drill="0.381"/>
<hole x="98.425" y="10.668" drill="0.381"/>
<hole x="99.06" y="10.668" drill="0.381"/>
<hole x="99.695" y="10.668" drill="0.381"/>
<hole x="100.33" y="10.668" drill="0.381"/>
<hole x="94.615" y="21.336" drill="0.381"/>
<hole x="95.25" y="21.336" drill="0.381"/>
<hole x="95.885" y="21.336" drill="0.381"/>
<hole x="96.52" y="21.336" drill="0.381"/>
<hole x="97.155" y="21.336" drill="0.381"/>
<hole x="97.79" y="21.336" drill="0.381"/>
<hole x="98.425" y="21.336" drill="0.381"/>
<hole x="99.06" y="21.336" drill="0.381"/>
<hole x="99.695" y="21.336" drill="0.381"/>
<hole x="100.33" y="21.336" drill="0.381"/>
<hole x="100.33" y="32.004" drill="0.381"/>
<hole x="99.695" y="32.004" drill="0.381"/>
<hole x="99.06" y="32.004" drill="0.381"/>
<hole x="98.425" y="32.004" drill="0.381"/>
<hole x="97.79" y="32.004" drill="0.381"/>
<hole x="97.155" y="32.004" drill="0.381"/>
<hole x="96.52" y="32.004" drill="0.381"/>
<hole x="95.885" y="32.004" drill="0.381"/>
<hole x="95.25" y="32.004" drill="0.381"/>
<hole x="94.615" y="32.004" drill="0.381"/>
<text>10k </text>
<text>0.1µF</text>
<text>10k </text>
<text>VCC</text>
<text>SLP</text>
<text>GND</text>
<text>VOUT</text>
<text>SLP</text>
<text>VCC</text>
<text>GND</text>
<text>VOUT</text>
<text>VCC</text>
<text>SLP</text>
<text>GND</text>
<text>VOUT</text>
<text>SLP</text>
<text>VCC</text>
<text>GND</text>
<text>VOUT</text>
<text>VCC</text>
<text>SLP</text>
<text>GND</text>
<text>VOUT</text>
<text>SLP</text>
<text>VCC</text>
<text>GND</text>
<text>VOUT</text>
<text>VCC</text>
<text>SLP</text>
<text>GND</text>
<text>VOUT</text>
<text>SLP</text>
<text>VCC</text>
<text>GND</text>
<text>VOUT</text>
<text>VCC</text>
<text>SLP</text>
<text>GND</text>
<text>VOUT</text>
<text>SLP</text>
<text>VCC</text>
<text>GND</text>
<text>VOUT</text>
<text>VCC</text>
<text>SLP</text>
<text>GND</text>
<text>VOUT</text>
<text>SLP</text>
<text>VCC</text>
<text>GND</text>
<text>VOUT</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>RED</text>
<text>GRN</text>
<text>+</text>
<text>+</text>
<text>0.1µF</text>
<text>VREG</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>OUT</text>
<text>Mussel
Gape
Tracker
RevC</text>
<text>L P MILLER
2017</text>
<text>millerlp@gmail.com</text>
<text>RX</text>
<text>TX</text>
<text>100Ω</text>
<text>100Ω</text>
<text>HALL0</text>
<text>HALL1</text>
<text>HALL2</text>
<text>HALL3</text>
<text>HALL4</text>
<text>HALL5</text>
<text>HALL6</text>
<text>HALL7</text>
<text>HALL8</text>
<text>HALL9</text>
<text>HALL10</text>
<text>HALL11</text>
<text>HALL12</text>
<text>HALL13</text>
<text>HALL14</text>
<text>HALL15</text>
<text>HALL14</text>
<text>HALL 0</text>
<text>VCC</text>
<text>MISO</text>
<text>SCK</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>10k</text>
<text>4.7k</text>
<text>4.7k</text>
<text>RESET</text>
<text>GND</text>
<text>RESET</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>BUTTON2</text>
<text>BUTTON1</text>
<text>GND</text>
<text>B1</text>
<text>B2</text>
<text>RTC</text>
<text>RST</text>
<text>SCK</text>
<text>MISO</text>
<text>VCC</text>
<text>VCC</text>
<text>ADC7</text>
<text>AREF</text>
<text>ADC6</text>
<text>MOSI</text>
<text>AGND</text>
<text>GND</text>
<text>0.1µF</text>
<text>VBAT</text>
<text>GND</text>
<hole x="72.644" y="46.101" drill="0.381"/>
<hole x="72.644" y="46.736" drill="0.381"/>
<hole x="72.644" y="47.371" drill="0.381"/>
<hole x="72.644" y="48.006" drill="0.381"/>
<hole x="72.644" y="48.641" drill="0.381"/>
<hole x="72.644" y="49.276" drill="0.381"/>
<hole x="72.644" y="49.911" drill="0.381"/>
<hole x="72.644" y="50.546" drill="0.381"/>
<hole x="72.644" y="51.181" drill="0.381"/>
<hole x="72.644" y="51.816" drill="0.381"/>
<hole x="72.644" y="52.451" drill="0.381"/>
<hole x="72.644" y="53.086" drill="0.381"/>
<hole x="72.644" y="53.721" drill="0.381"/>
<hole x="72.644" y="54.356" drill="0.381"/>
<hole x="72.644" y="54.991" drill="0.381"/>
<hole x="72.644" y="55.626" drill="0.381"/>
<hole x="72.644" y="56.261" drill="0.381"/>
<hole x="72.644" y="56.896" drill="0.381"/>
<hole x="78.994" y="42.672" drill="0.381"/>
<hole x="78.359" y="42.672" drill="0.381"/>
<hole x="77.724" y="42.672" drill="0.381"/>
<hole x="77.089" y="42.672" drill="0.381"/>
<hole x="76.454" y="42.672" drill="0.381"/>
<hole x="75.819" y="42.672" drill="0.381"/>
<hole x="75.184" y="42.672" drill="0.381"/>
<hole x="74.549" y="42.672" drill="0.381"/>
<hole x="73.914" y="42.672" drill="0.381"/>
<hole x="73.279" y="42.672" drill="0.381"/>
<hole x="79.756" y="46.101" drill="0.381"/>
<hole x="79.756" y="46.736" drill="0.381"/>
<hole x="79.756" y="47.371" drill="0.381"/>
<hole x="79.756" y="48.006" drill="0.381"/>
<hole x="79.756" y="48.641" drill="0.381"/>
<hole x="79.756" y="49.276" drill="0.381"/>
<hole x="79.756" y="49.911" drill="0.381"/>
<hole x="79.756" y="50.546" drill="0.381"/>
<hole x="79.756" y="51.181" drill="0.381"/>
<hole x="79.756" y="51.816" drill="0.381"/>
<hole x="79.756" y="52.451" drill="0.381"/>
<hole x="79.756" y="53.086" drill="0.381"/>
<hole x="79.756" y="53.721" drill="0.381"/>
<hole x="79.756" y="54.356" drill="0.381"/>
<hole x="79.756" y="54.991" drill="0.381"/>
<hole x="79.756" y="55.626" drill="0.381"/>
<hole x="79.756" y="56.261" drill="0.381"/>
<hole x="79.756" y="56.896" drill="0.381"/>
<hole x="86.233" y="42.672" drill="0.381"/>
<hole x="85.598" y="42.672" drill="0.381"/>
<hole x="84.963" y="42.672" drill="0.381"/>
<hole x="84.328" y="42.672" drill="0.381"/>
<hole x="83.693" y="42.672" drill="0.381"/>
<hole x="83.058" y="42.672" drill="0.381"/>
<hole x="82.423" y="42.672" drill="0.381"/>
<hole x="81.788" y="42.672" drill="0.381"/>
<hole x="81.153" y="42.672" drill="0.381"/>
<hole x="80.518" y="42.672" drill="0.381"/>
<hole x="86.868" y="46.101" drill="0.381"/>
<hole x="86.868" y="46.736" drill="0.381"/>
<hole x="86.868" y="47.371" drill="0.381"/>
<hole x="86.868" y="48.006" drill="0.381"/>
<hole x="86.868" y="48.641" drill="0.381"/>
<hole x="86.868" y="49.276" drill="0.381"/>
<hole x="86.868" y="49.911" drill="0.381"/>
<hole x="86.868" y="50.546" drill="0.381"/>
<hole x="86.868" y="51.181" drill="0.381"/>
<hole x="86.868" y="51.816" drill="0.381"/>
<hole x="86.868" y="52.451" drill="0.381"/>
<hole x="86.868" y="53.086" drill="0.381"/>
<hole x="86.868" y="53.721" drill="0.381"/>
<hole x="86.868" y="54.356" drill="0.381"/>
<hole x="86.868" y="54.991" drill="0.381"/>
<hole x="86.868" y="55.626" drill="0.381"/>
<hole x="86.868" y="56.261" drill="0.381"/>
<hole x="86.868" y="56.896" drill="0.381"/>
<hole x="93.345" y="42.672" drill="0.381"/>
<hole x="92.71" y="42.672" drill="0.381"/>
<hole x="92.075" y="42.672" drill="0.381"/>
<hole x="91.44" y="42.672" drill="0.381"/>
<hole x="90.805" y="42.672" drill="0.381"/>
<hole x="90.17" y="42.672" drill="0.381"/>
<hole x="89.535" y="42.672" drill="0.381"/>
<hole x="88.9" y="42.672" drill="0.381"/>
<hole x="88.265" y="42.672" drill="0.381"/>
<hole x="87.6046" y="42.672" drill="0.381"/>
<hole x="93.98" y="46.101" drill="0.381"/>
<hole x="93.98" y="46.736" drill="0.381"/>
<hole x="93.98" y="47.371" drill="0.381"/>
<hole x="93.98" y="48.006" drill="0.381"/>
<hole x="93.98" y="48.641" drill="0.381"/>
<hole x="93.98" y="49.276" drill="0.381"/>
<hole x="93.98" y="49.911" drill="0.381"/>
<hole x="93.98" y="50.546" drill="0.381"/>
<hole x="93.98" y="51.181" drill="0.381"/>
<hole x="93.98" y="51.816" drill="0.381"/>
<hole x="93.98" y="52.451" drill="0.381"/>
<hole x="93.98" y="53.086" drill="0.381"/>
<hole x="93.98" y="53.721" drill="0.381"/>
<hole x="93.98" y="54.356" drill="0.381"/>
<hole x="93.98" y="54.991" drill="0.381"/>
<hole x="93.98" y="55.626" drill="0.381"/>
<hole x="93.98" y="56.261" drill="0.381"/>
<hole x="93.98" y="56.896" drill="0.381"/>
<hole x="100.33" y="42.672" drill="0.381"/>
<hole x="99.695" y="42.672" drill="0.381"/>
<hole x="99.06" y="42.672" drill="0.381"/>
<hole x="98.425" y="42.672" drill="0.381"/>
<hole x="97.79" y="42.672" drill="0.381"/>
<hole x="97.155" y="42.672" drill="0.381"/>
<hole x="96.52" y="42.672" drill="0.381"/>
<hole x="95.885" y="42.672" drill="0.381"/>
<hole x="95.25" y="42.672" drill="0.381"/>
<hole x="94.615" y="42.672" drill="0.381"/>
<hole x="78.994" y="53.34" drill="0.381"/>
<hole x="78.359" y="53.34" drill="0.381"/>
<hole x="77.724" y="53.34" drill="0.381"/>
<hole x="77.089" y="53.34" drill="0.381"/>
<hole x="76.454" y="53.34" drill="0.381"/>
<hole x="75.819" y="53.34" drill="0.381"/>
<hole x="75.184" y="53.34" drill="0.381"/>
<hole x="74.549" y="53.34" drill="0.381"/>
<hole x="73.914" y="53.34" drill="0.381"/>
<hole x="73.279" y="53.34" drill="0.381"/>
<hole x="86.1314" y="53.34" drill="0.381"/>
<hole x="85.4964" y="53.34" drill="0.381"/>
<hole x="84.8614" y="53.34" drill="0.381"/>
<hole x="84.2264" y="53.34" drill="0.381"/>
<hole x="83.5914" y="53.34" drill="0.381"/>
<hole x="82.9564" y="53.34" drill="0.381"/>
<hole x="82.3214" y="53.34" drill="0.381"/>
<hole x="81.6864" y="53.34" drill="0.381"/>
<hole x="81.0514" y="53.34" drill="0.381"/>
<hole x="80.4164" y="53.34" drill="0.381"/>
<hole x="93.2942" y="53.34" drill="0.381"/>
<hole x="92.6592" y="53.34" drill="0.381"/>
<hole x="92.0242" y="53.34" drill="0.381"/>
<hole x="91.3892" y="53.34" drill="0.381"/>
<hole x="90.7542" y="53.34" drill="0.381"/>
<hole x="90.1192" y="53.34" drill="0.381"/>
<hole x="89.4842" y="53.34" drill="0.381"/>
<hole x="88.8492" y="53.34" drill="0.381"/>
<hole x="88.2142" y="53.34" drill="0.381"/>
<hole x="87.5538" y="53.34" drill="0.381"/>
<hole x="100.3808" y="53.34" drill="0.381"/>
<hole x="99.7458" y="53.34" drill="0.381"/>
<hole x="99.1108" y="53.34" drill="0.381"/>
<hole x="98.4758" y="53.34" drill="0.381"/>
<hole x="97.8408" y="53.34" drill="0.381"/>
<hole x="97.2058" y="53.34" drill="0.381"/>
<hole x="96.5708" y="53.34" drill="0.381"/>
<hole x="95.9358" y="53.34" drill="0.381"/>
<hole x="95.3008" y="53.34" drill="0.381"/>
<hole x="94.6658" y="53.34" drill="0.381"/>
<hole x="72.644" y="57.4548" drill="0.381"/>
<hole x="79.756" y="57.4548" drill="0.381"/>
<hole x="86.868" y="57.4548" drill="0.381"/>
<hole x="93.98" y="57.4548" drill="0.381"/>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>SLP</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VCC</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>VOUT</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>HALL
EFFECT
A139x</text>
<text>1</text>
<text>2</text>
<text>DTR</text>
<text>LP MILLER
2017</text>
<text>Mussel
Gape
Tracker
RevC</text>
<text>PWR JMPR</text>
<text>CUT TRACE
TO USE
PWR JMPR</text>
</plain>
<libraries>
<library name="miller">
<packages>
<package name="PUSHBUTTON_DPST_SMD">
<description>PUSHBUTTON Omron B3S-1000 SMD DPST</description>
</package>
<package name="PANASONIC_B">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B&lt;/b&gt;</description>
</package>
<package name="0603">
<description>0603 surface mount part</description>
</package>
<package name="2X3">
<description>ISP programming header for Arduino&lt;br&gt;
Keepout area gives approximate footprint of connector from AVR MKII ISP</description>
</package>
<package name="1X06-RIGHT_ANGLE">
<description>1x06 0.1" spacing right angle header&lt;p&gt;
Example: Sullins PPPC061LGBN-RC, Digikey PN S5481-ND</description>
</package>
<package name="CHIPLED_0805">
<description>Surface mount LED 0805 footprint with marker for positive (anode) terminal</description>
</package>
<package name="MICROSD_SOCKET_MOLEX_REVERSEMOUNT">
<description>&lt;b&gt;Molex micro SD card slot, push-push spring-loaded style "reverse mount"&lt;/b&gt;&lt;br&gt;
Molex PN 5027740891&lt;br&gt;
Digikey PN WM24066CT-ND&lt;br&gt;
This version has the surface mount pins easily accessible at the rear of the housing rather than underneath it like most other sockets.</description>
</package>
<package name="CR1220_BATTERY_HOLDER_SMD">
<description>CR1220 Battery Holder, SMD
Keystone Part # 3000</description>
</package>
<package name="SOT95P237X112-3N">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="DS3231M_SOIC8">
<description>Maxim DS3231M real time clock pattern&lt;br&gt;
This is the smaller cheaper DS3231M model, vs S model. This version does not have as many square wave output frequencies (just 32.768 kHz and 1Hz).</description>
</package>
<package name="22-23-2021">
<description>.100" (2.54mm) Center Headers - 2 Pin</description>
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447
Outer keepout is 0.127" radius (0.254" diameter).</description>
</package>
<package name="STAND-OFF_M2">
<description>M2 stand-off hole&lt;p&gt;
Drill diam = 2.2mm &lt;br&gt;
Outer keepout diameter = 3.175mm (0.125")</description>
</package>
<package name="A139*_HALL_EFFECT">
<description>Allegro A193* series hall effect sensors&lt;br&gt;
6-pin MLP/DFN package&lt;br&gt;

Example Digikey PN 620-1031-1-ND</description>
</package>
<package name="2X2_1.5MM">
<description>2X2 header 1.5mm pitch&lt;p&gt;
0.8mm drill</description>
</package>
<package name="1X01_SMALL">
<description>0.35" diameter drill, 0.55" copper diameter&lt;br&gt;
This hole should be barely large enough for standard 0.1" pitch header pins.</description>
</package>
<package name="JST-PH-4-THM">
<description>&lt;b&gt;JST PH series 4-pin male header, shrouded&lt;br&gt;&lt;/b&gt;
JST PN B4B-PH-K-S</description>
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="SSOP24">
<description>TSSOP-24 or SSOP-24&lt;p&gt;
0.65mm between pad centers, 0.348mm pad width x 1.397mm pad length&lt;br&gt;
7.312mm between pad centers across body &lt;br&gt;(appropriate for body width of 5.03mm/0.209")</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SOT23-3">
<description>SOT23-3 package&lt;br&gt;
Pad size 0.8 x 0.9mm</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip 0603 size</description>
</package>
<package name="DO214AC">
<description>DO-214AC footprint</description>
</package>
<package name="POWER_JACK_DC_2,1MM">
<description>2.1 mm DC power jack. Digikey PN CP-202AH-ND</description>
</package>
<package name="TSOT-23_5-LEAD">
</package>
<package name="BATTERY_4XAA_PTH">
<description>Keystone PN 2477&lt;p&gt;
4xAA battery holder, plastic housing, through-hole mount.</description>
</package>
<package name="1X04_LOCK">
<description>0.035" drills, 0.056" pad width&lt;br&gt;
Staggered holes to help hold header in position while soldering.</description>
</package>
<package name="1X02_NOSILK">
<description>1x2 header, 0.1" pitch</description>
</package>
</packages>
</library>
<library name="Felicia_force_logger">
<packages>
<package name="I_0805">
<description>&lt;b&gt;0805 (2012) Inductor footprint&lt;br&gt;&lt;/b&gt;
Example:
Taiyo Yuden inductor # LBR2012T100K&lt;br&gt;
Digikey PN 587-2045-1-ND</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="1" library="miller" package="PUSHBUTTON_DPST_SMD" value="PUSHBUTTON_DPST_SMDSTANDARD">
<attribute name="NAME"/>
</element>
<element name="C1" library="miller" package="PANASONIC_B" value="1µF">
<attribute name="NAME"/>
</element>
<element name="C2" library="miller" package="PANASONIC_B" value="1µF">
<attribute name="NAME"/>
</element>
<element name="C5" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="J1" library="miller" package="2X3" value="AVR_SPI_PRG_6PTH"/>
<element name="JP1" library="miller" package="1X06-RIGHT_ANGLE" value="FTDI_HEADER"/>
<element name="LED2" library="miller" package="CHIPLED_0805" value="GREEN_LED"/>
<element name="R1" library="miller" package="R0603" value="100 Ω">
<attribute name="NAME"/>
</element>
<element name="R2" library="miller" package="R0603" value="100 Ω">
<attribute name="NAME"/>
</element>
<element name="R8" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
</element>
<element name="R7" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
</element>
<element name="R5" library="miller" package="R0603" value="100k Ω">
<attribute name="NAME"/>
</element>
<element name="R4" library="miller" package="R0603" value="100k Ω">
<attribute name="NAME"/>
</element>
<element name="RESET" library="miller" package="PUSHBUTTON_DPST_SMD" value="PUSHBUTTON_DPST_SMDSTANDARD">
<attribute name="NAME"/>
</element>
<element name="U$1" library="miller" package="MICROSD_SOCKET_MOLEX_REVERSEMOUNT" value="MICROSD_MOLEX_REVERSECURRENT"/>
<element name="CR1220_BATTERY" library="miller" package="CR1220_BATTERY_HOLDER_SMD" value="CR1220_BATTERY_HOLDERSMD"/>
<element name="MCP1700T-3302" library="miller" package="SOT95P237X112-3N" value="MCP1700T-3302E/TT">
<attribute name="PACKAGE" value="SOT23-3"/>
<attribute name="OC_NEWARK" value="88H9817"/>
<attribute name="MPN" value="MCP1700T-3302E/TT"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="OC_FARNELL" value="1296592"/>
</element>
<element name="U1" library="miller" package="TQFP32-08" value="ATMEGA328P">
<attribute name="VALUE"/>
</element>
<element name="R6" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
</element>
<element name="C3" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C4" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="LED1" library="miller" package="CHIPLED_0805" value="RED_LED"/>
<element name="DS3231M" library="miller" package="DS3231M_SOIC8" value="DS3231MSOIC-8">
<attribute name="NAME"/>
</element>
<element name="MOLEX_KK" library="miller" package="22-23-2021" value="22-23-2021">
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462926"/>
</element>
<element name="C7" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STANDOFF2" library="miller" package="STAND-OFF" value="STAND-OFF4-40"/>
<element name="A139_HALL1" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL1_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R51" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL2" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL2_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R52" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C52" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$17" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL"/>
<element name="HALL0" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL1" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="GROUND_CON" library="miller" package="SJ_2S-TRACE" value="SOLDER_JUMPER_TRACESTANDARD"/>
<element name="C23" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="INDUCTOR" library="Felicia_force_logger" package="I_0805" value="10µH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STANDOFF1" library="miller" package="STAND-OFF" value="STAND-OFF4-40"/>
<element name="STANDOFF3" library="miller" package="STAND-OFF" value="STAND-OFF4-40"/>
<element name="A139_HALL3" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL3_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R53" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
</element>
<element name="C53" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL4" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL4_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R54" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
</element>
<element name="C54" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="R9" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
</element>
<element name="2" library="miller" package="PUSHBUTTON_DPST_SMD" value="PUSHBUTTON_DPST_SMDSTANDARD">
<attribute name="NAME"/>
</element>
<element name="R3" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SHIFT_0" library="miller" package="SO16" value="74HC595D">
<attribute name="VALUE"/>
</element>
<element name="SHIFT_1" library="miller" package="SO16" value="74HC595D">
<attribute name="VALUE"/>
</element>
<element name="R14" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="miller" package="SSOP24" value="74HC4067SM96">
<attribute name="VALUE"/>
</element>
<element name="C6" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="miller" package="R0603" value="100k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HALL2" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL3" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL4" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL5" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL6" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL7" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="A139_HALL0" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL0_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R50" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL5" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL5_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R55" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C55" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL6" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL6_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R56" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C56" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL7" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL7_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R57" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C57" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HALL8" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL9" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL10" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL11" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL12" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL13" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL14" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="HALL15" library="miller" package="JST-PH-4-THM" value="JST-4PINTH_STRAIGHT">
<attribute name="NAME"/>
</element>
<element name="A139_HALL9" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL9_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R59" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C59" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL10" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL10_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R60" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C60" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL11" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL11_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R61" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C61" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL12" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL12_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R62" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C62" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL8" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL8_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R58" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C58" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL13" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL13_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R63" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C63" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL14" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL14_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R64" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C64" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL15" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL15_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R65" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C65" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BJT" library="miller" package="SOT23" value="KSC1623_BJT_TRANSISTOR">
<attribute name="NAME"/>
</element>
<element name="P-FET" library="miller" package="SOT23-3" value="MOSFET-PCHANNELBSH203">
<attribute name="PROD_ID" value="TRANS-08285"/>
<attribute name="NAME"/>
</element>
<element name="R29" library="miller" package="R0603" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="miller" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL"/>
<element name="U$4" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL"/>
<element name="U$6" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL"/>
<element name="U$7" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL"/>
<element name="U$8" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL"/>
<element name="U$9" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL"/>
<element name="U$10" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL"/>
<element name="U$11" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL"/>
<element name="SCHOTTKY" library="miller" package="DO214AC" value="SCHOTTKY_DIODE_DO-214AC">
<attribute name="NAME"/>
</element>
<element name="2,1MM_JACK" library="miller" package="POWER_JACK_DC_2,1MM" value="POWER_JACK_2,1MM"/>
<element name="LTC4411" library="miller" package="TSOT-23_5-LEAD" value="LTC4411TSOT-23_5-LEAD">
<attribute name="SPICEMODEL" value="LTC4411.sub"/>
<attribute name="VALUE2" value=" LTC4411"/>
<attribute name="NAME"/>
</element>
<element name="R34" library="miller" package="R0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="miller" package="0603" value="4.7µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PRIMARY_BATTERY" library="miller" package="BATTERY_4XAA_PTH" value="BATTERY_4XAA"/>
<element name="OLED" library="miller" package="1X04_LOCK" value="PINHD-1X4LOCK">
<attribute name="NAME"/>
</element>
<element name="STANDOFF4_M2" library="miller" package="STAND-OFF_M2" value="STAND-OFFM2"/>
<element name="STANDOFF5_M2" library="miller" package="STAND-OFF_M2" value="STAND-OFFM2"/>
<element name="A139_HALL16" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL16_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R66" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C66" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL17" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL17_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R67" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C67" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL18" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL18_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R68" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C68" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A139_HALL19" library="miller" package="A139*_HALL_EFFECT" value="HALL_EFFECT_ALLEGRO_A139MLP/DFN-6"/>
<element name="HALL19_HEADER" library="miller" package="2X2_1.5MM" value="PINHD-2X21.5MM_SILK"/>
<element name="R69" library="miller" package="R0603" value="10k Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C69" library="miller" package="0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR_JUMPER" library="miller" package="1X02_NOSILK" value="PWR_JMPR"/>
<element name="PWR_PASSTHRU" library="miller" package="SJ_2S-TRACE" value="PWR"/>
</elements>
<signals>
<signal name="GND">
<contactref element="RESET" pad="P$1"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="U$1" pad="GND6"/>
<contactref element="C4" pad="2"/>
<contactref element="U$1" pad="MNT4"/>
<contactref element="U$1" pad="MNT3"/>
<contactref element="U$1" pad="MNT2"/>
<contactref element="U$1" pad="MNT1"/>
<contactref element="1" pad="S$1"/>
<contactref element="MCP1700T-3302" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="CR1220_BATTERY" pad="GND"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="J1" pad="6"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="DS3231M" pad="5"/>
<contactref element="C7" pad="2"/>
<contactref element="GROUND_CON" pad="1"/>
<contactref element="2" pad="S$1"/>
<contactref element="R3" pad="1"/>
<contactref element="SHIFT_0" pad="13"/>
<contactref element="SHIFT_0" pad="8"/>
<contactref element="SHIFT_1" pad="13"/>
<contactref element="SHIFT_1" pad="8"/>
<contactref element="U$2" pad="12"/>
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R32" pad="1"/>
<contactref element="BJT" pad="2"/>
<contactref element="R29" pad="1"/>
<contactref element="U$4" pad="1"/>
<contactref element="U$7" pad="1"/>
<contactref element="U$9" pad="1"/>
<contactref element="LTC4411" pad="2"/>
<contactref element="MOLEX_KK" pad="1"/>
<contactref element="2,1MM_JACK" pad="P$2"/>
<contactref element="LTC4411" pad="3"/>
<contactref element="C25" pad="2"/>
<contactref element="PRIMARY_BATTERY" pad="GND"/>
<contactref element="OLED" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R6" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="DS3231M" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="MCP1700T-3302" pad="2"/>
<contactref element="C2" pad="+"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U$1" pad="VDD4"/>
<contactref element="HALL0" pad="1"/>
<contactref element="HALL1" pad="1"/>
<contactref element="INDUCTOR" pad="P$2"/>
<contactref element="R9" pad="2"/>
<contactref element="SHIFT_1" pad="16"/>
<contactref element="SHIFT_0" pad="16"/>
<contactref element="R14" pad="2"/>
<contactref element="U$2" pad="24"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="HALL2" pad="1"/>
<contactref element="HALL3" pad="1"/>
<contactref element="HALL4" pad="1"/>
<contactref element="HALL5" pad="1"/>
<contactref element="HALL6" pad="1"/>
<contactref element="HALL7" pad="1"/>
<contactref element="HALL8" pad="1"/>
<contactref element="HALL9" pad="1"/>
<contactref element="HALL10" pad="1"/>
<contactref element="HALL11" pad="1"/>
<contactref element="HALL12" pad="1"/>
<contactref element="HALL13" pad="1"/>
<contactref element="HALL14" pad="1"/>
<contactref element="HALL15" pad="1"/>
<contactref element="R28" pad="2"/>
<contactref element="R34" pad="2"/>
<contactref element="OLED" pad="1"/>
</signal>
<signal name="DTR">
<contactref element="C5" pad="1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="17"/>
<contactref element="U$1" pad="SCK5"/>
<contactref element="J1" pad="3"/>
<contactref element="SHIFT_0" pad="11"/>
<contactref element="SHIFT_1" pad="11"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="16"/>
<contactref element="U$1" pad="MISO7"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="15"/>
<contactref element="U$1" pad="MOSI3"/>
<contactref element="J1" pad="4"/>
<contactref element="SHIFT_0" pad="14"/>
</signal>
<signal name="CS_SD">
<contactref element="U1" pad="14"/>
<contactref element="U$1" pad="CS2"/>
</signal>
<signal name="NC1">
<contactref element="U$1" pad="NC1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="RES8">
<contactref element="U$1" pad="RES8"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="LED_RED">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="TO_FTDI_TX">
<contactref element="U1" pad="30"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="TO_FTDI_RX">
<contactref element="U1" pad="31"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="BUTTON2">
<contactref element="2" pad="P$1"/>
<contactref element="U1" pad="1"/>
<contactref element="U$8" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="27"/>
<contactref element="R8" pad="1"/>
<contactref element="DS3231M" pad="7"/>
<contactref element="OLED" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="28"/>
<contactref element="R7" pad="1"/>
<contactref element="DS3231M" pad="8"/>
<contactref element="OLED" pad="3"/>
</signal>
<signal name="VBAT">
<contactref element="CR1220_BATTERY" pad="P$1"/>
<contactref element="CR1220_BATTERY" pad="P$2"/>
<contactref element="DS3231M" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="LED_GRN">
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="HALL0_OUTPUT">
<contactref element="HALL0" pad="4"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="RESET">
<contactref element="J1" pad="5"/>
<contactref element="U1" pad="29"/>
<contactref element="R6" pad="1"/>
<contactref element="RESET" pad="S$1"/>
<contactref element="C5" pad="2"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="VRAW">
<contactref element="P-FET" pad="2"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="32KHZ">
<contactref element="U1" pad="7"/>
<contactref element="DS3231M" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="HALL1_GND">
<contactref element="HALL1_HEADER" pad="P$1"/>
<contactref element="A139_HALL1" pad="P$3_4"/>
<contactref element="C51" pad="2"/>
</signal>
<signal name="HALL1_VCC">
<contactref element="A139_HALL1" pad="P$6"/>
<contactref element="A139_HALL1" pad="P$1"/>
<contactref element="HALL1_HEADER" pad="P$2"/>
<contactref element="C51" pad="1"/>
</signal>
<signal name="!SLEEP1">
<contactref element="R51" pad="2"/>
<contactref element="A139_HALL1" pad="P$5"/>
</signal>
<signal name="HALL2_GND">
<contactref element="HALL2_HEADER" pad="P$1"/>
<contactref element="A139_HALL2" pad="P$3_4"/>
<contactref element="C52" pad="2"/>
</signal>
<signal name="HALL2_VOUT">
<contactref element="HALL2_HEADER" pad="P$3"/>
<contactref element="A139_HALL2" pad="P$2"/>
</signal>
<signal name="HALL2_VCC">
<contactref element="HALL2_HEADER" pad="P$2"/>
<contactref element="C52" pad="1"/>
<contactref element="A139_HALL2" pad="P$1"/>
<contactref element="A139_HALL2" pad="P$6"/>
</signal>
<signal name="!SLEEP2">
<contactref element="R52" pad="2"/>
<contactref element="A139_HALL2" pad="P$5"/>
</signal>
<signal name="AREF">
<contactref element="U1" pad="20"/>
<contactref element="U$17" pad="1"/>
</signal>
<signal name="HALL0_!SLEEP">
<contactref element="HALL0" pad="3"/>
<contactref element="SHIFT_0" pad="15"/>
</signal>
<signal name="HALL1_VOUT">
<contactref element="A139_HALL1" pad="P$2"/>
<contactref element="HALL1_HEADER" pad="P$3"/>
</signal>
<signal name="HALL1_!SLEEP_IN">
<contactref element="R51" pad="1"/>
<contactref element="HALL1_HEADER" pad="P$4"/>
</signal>
<signal name="HALL2_!SLEEP_IN">
<contactref element="R52" pad="1"/>
<contactref element="HALL2_HEADER" pad="P$4"/>
</signal>
<signal name="HALL1_OUTPUT">
<contactref element="HALL1" pad="4"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="HALL1_!SLEEP">
<contactref element="HALL1" pad="3"/>
<contactref element="SHIFT_0" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="GROUND_CON" pad="2"/>
<contactref element="HALL0" pad="2"/>
<contactref element="HALL1" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="U1" pad="21"/>
<contactref element="HALL2" pad="2"/>
<contactref element="HALL3" pad="2"/>
<contactref element="HALL4" pad="2"/>
<contactref element="HALL5" pad="2"/>
<contactref element="HALL6" pad="2"/>
<contactref element="HALL7" pad="2"/>
<contactref element="HALL8" pad="2"/>
<contactref element="HALL9" pad="2"/>
<contactref element="HALL10" pad="2"/>
<contactref element="HALL11" pad="2"/>
<contactref element="HALL12" pad="2"/>
<contactref element="HALL13" pad="2"/>
<contactref element="HALL14" pad="2"/>
<contactref element="HALL15" pad="2"/>
<contactref element="U$11" pad="1"/>
</signal>
<signal name="AVCC">
<contactref element="U1" pad="18"/>
<contactref element="INDUCTOR" pad="P$1"/>
<contactref element="C23" pad="1"/>
</signal>
<signal name="HALL3_GND">
<contactref element="HALL3_HEADER" pad="P$1"/>
<contactref element="C53" pad="2"/>
<contactref element="A139_HALL3" pad="P$3_4"/>
</signal>
<signal name="HALL3_VOUT">
<contactref element="HALL3_HEADER" pad="P$3"/>
<contactref element="A139_HALL3" pad="P$2"/>
</signal>
<signal name="HALL3_VCC">
<contactref element="HALL3_HEADER" pad="P$2"/>
<contactref element="C53" pad="1"/>
<contactref element="A139_HALL3" pad="P$6"/>
<contactref element="A139_HALL3" pad="P$1"/>
</signal>
<signal name="HALL3_!SLEEP_IN">
<contactref element="HALL3_HEADER" pad="P$4"/>
<contactref element="R53" pad="1"/>
</signal>
<signal name="!SLEEP3">
<contactref element="R53" pad="2"/>
<contactref element="A139_HALL3" pad="P$5"/>
</signal>
<signal name="HALL4_GND">
<contactref element="HALL4_HEADER" pad="P$1"/>
<contactref element="C54" pad="2"/>
<contactref element="A139_HALL4" pad="P$3_4"/>
</signal>
<signal name="HALL4_VOUT">
<contactref element="HALL4_HEADER" pad="P$3"/>
<contactref element="A139_HALL4" pad="P$2"/>
</signal>
<signal name="HALL4_VCC">
<contactref element="HALL4_HEADER" pad="P$2"/>
<contactref element="A139_HALL4" pad="P$1"/>
<contactref element="C54" pad="1"/>
<contactref element="A139_HALL4" pad="P$6"/>
</signal>
<signal name="HALL4_!SLEEP_IN">
<contactref element="HALL4_HEADER" pad="P$4"/>
<contactref element="R54" pad="1"/>
</signal>
<signal name="!SLEEP4">
<contactref element="A139_HALL4" pad="P$5"/>
<contactref element="R54" pad="2"/>
</signal>
<signal name="BUTTON1">
<contactref element="1" pad="P$1"/>
<contactref element="U1" pad="32"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="CS_SHIFT_REG">
<contactref element="SHIFT_0" pad="12"/>
<contactref element="SHIFT_1" pad="12"/>
<contactref element="U1" pad="25"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="QH*">
<contactref element="SHIFT_0" pad="9"/>
<contactref element="SHIFT_1" pad="14"/>
</signal>
<signal name="SHIFT_CLEAR">
<contactref element="U1" pad="24"/>
<contactref element="SHIFT_0" pad="10"/>
<contactref element="SHIFT_1" pad="10"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="MUX_S0">
<contactref element="U$2" pad="10"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="MUX_S1">
<contactref element="U1" pad="9"/>
<contactref element="U$2" pad="11"/>
</signal>
<signal name="MUX_S2">
<contactref element="U1" pad="10"/>
<contactref element="U$2" pad="14"/>
</signal>
<signal name="MUX_S3">
<contactref element="U1" pad="11"/>
<contactref element="U$2" pad="13"/>
</signal>
<signal name="ANALOG_0">
<contactref element="U$2" pad="1"/>
<contactref element="U1" pad="22"/>
<contactref element="R15" pad="1"/>
<contactref element="U$10" pad="1"/>
</signal>
<signal name="HALL2_!SLEEP">
<contactref element="SHIFT_0" pad="2"/>
<contactref element="HALL2" pad="3"/>
</signal>
<signal name="HALL3_!SLEEP">
<contactref element="SHIFT_0" pad="3"/>
<contactref element="HALL3" pad="3"/>
</signal>
<signal name="HALL4_!SLEEP">
<contactref element="SHIFT_0" pad="4"/>
<contactref element="HALL4" pad="3"/>
</signal>
<signal name="HALL5_!SLEEP">
<contactref element="SHIFT_0" pad="5"/>
<contactref element="HALL5" pad="3"/>
</signal>
<signal name="HALL6_!SLEEP">
<contactref element="SHIFT_0" pad="6"/>
<contactref element="HALL6" pad="3"/>
</signal>
<signal name="HALL7_!SLEEP">
<contactref element="SHIFT_0" pad="7"/>
<contactref element="HALL7" pad="3"/>
</signal>
<signal name="HALL8_!SLEEP">
<contactref element="SHIFT_1" pad="15"/>
<contactref element="HALL8" pad="3"/>
</signal>
<signal name="HALL9_!SLEEP">
<contactref element="SHIFT_1" pad="1"/>
<contactref element="HALL9" pad="3"/>
</signal>
<signal name="HALL10_!SLEEP">
<contactref element="SHIFT_1" pad="2"/>
<contactref element="HALL10" pad="3"/>
</signal>
<signal name="HALL11_!SLEEP">
<contactref element="SHIFT_1" pad="3"/>
<contactref element="HALL11" pad="3"/>
</signal>
<signal name="HALL12_!SLEEP">
<contactref element="SHIFT_1" pad="4"/>
<contactref element="HALL12" pad="3"/>
</signal>
<signal name="HALL13_!SLEEP">
<contactref element="SHIFT_1" pad="5"/>
<contactref element="HALL13" pad="3"/>
</signal>
<signal name="HALL14_!SLEEP">
<contactref element="SHIFT_1" pad="6"/>
<contactref element="HALL14" pad="3"/>
</signal>
<signal name="HALL15_!SLEEP">
<contactref element="SHIFT_1" pad="7"/>
<contactref element="HALL15" pad="3"/>
</signal>
<signal name="HALL2_OUTPUT">
<contactref element="U$2" pad="7"/>
<contactref element="HALL2" pad="4"/>
</signal>
<signal name="HALL3_OUTPUT">
<contactref element="U$2" pad="6"/>
<contactref element="HALL3" pad="4"/>
</signal>
<signal name="HALL4_OUTPUT">
<contactref element="U$2" pad="5"/>
<contactref element="HALL4" pad="4"/>
</signal>
<signal name="HALL5_OUTPUT">
<contactref element="U$2" pad="4"/>
<contactref element="HALL5" pad="4"/>
</signal>
<signal name="HALL6_OUTPUT">
<contactref element="U$2" pad="3"/>
<contactref element="HALL6" pad="4"/>
</signal>
<signal name="HALL7_OUTPUT">
<contactref element="U$2" pad="2"/>
<contactref element="HALL7" pad="4"/>
</signal>
<signal name="HALL8_OUTPUT">
<contactref element="U$2" pad="23"/>
<contactref element="HALL8" pad="4"/>
</signal>
<signal name="HALL9_OUTPUT">
<contactref element="U$2" pad="22"/>
<contactref element="HALL9" pad="4"/>
</signal>
<signal name="HALL10_OUTPUT">
<contactref element="U$2" pad="21"/>
<contactref element="HALL10" pad="4"/>
</signal>
<signal name="HALL11_OUTPUT">
<contactref element="U$2" pad="20"/>
<contactref element="HALL11" pad="4"/>
</signal>
<signal name="HALL12_OUTPUT">
<contactref element="U$2" pad="19"/>
<contactref element="HALL12" pad="4"/>
</signal>
<signal name="HALL13_OUTPUT">
<contactref element="U$2" pad="18"/>
<contactref element="HALL13" pad="4"/>
</signal>
<signal name="HALL14_OUTPUT">
<contactref element="U$2" pad="17"/>
<contactref element="HALL14" pad="4"/>
</signal>
<signal name="HALL15_OUTPUT">
<contactref element="U$2" pad="16"/>
<contactref element="HALL15" pad="4"/>
</signal>
<signal name="HALL0_GND">
<contactref element="HALL0_HEADER" pad="P$1"/>
<contactref element="C50" pad="2"/>
<contactref element="A139_HALL0" pad="P$3_4"/>
</signal>
<signal name="HALL0_VOUT">
<contactref element="HALL0_HEADER" pad="P$3"/>
<contactref element="A139_HALL0" pad="P$2"/>
</signal>
<signal name="HALL0_VCC">
<contactref element="HALL0_HEADER" pad="P$2"/>
<contactref element="C50" pad="1"/>
<contactref element="A139_HALL0" pad="P$1"/>
<contactref element="A139_HALL0" pad="P$6"/>
</signal>
<signal name="HALL0_!SLEEP_IN">
<contactref element="HALL0_HEADER" pad="P$4"/>
<contactref element="R50" pad="1"/>
</signal>
<signal name="!SLEEP0">
<contactref element="R50" pad="2"/>
<contactref element="A139_HALL0" pad="P$5"/>
</signal>
<signal name="HALL5_GND">
<contactref element="HALL5_HEADER" pad="P$1"/>
<contactref element="A139_HALL5" pad="P$3_4"/>
<contactref element="C55" pad="2"/>
</signal>
<signal name="HALL5_VOUT">
<contactref element="HALL5_HEADER" pad="P$3"/>
<contactref element="A139_HALL5" pad="P$2"/>
</signal>
<signal name="HALL5_VCC">
<contactref element="HALL5_HEADER" pad="P$2"/>
<contactref element="A139_HALL5" pad="P$6"/>
<contactref element="A139_HALL5" pad="P$1"/>
<contactref element="C55" pad="1"/>
</signal>
<signal name="HALL5_!SLEEP_IN">
<contactref element="HALL5_HEADER" pad="P$4"/>
<contactref element="R55" pad="1"/>
</signal>
<signal name="!SLEEP5">
<contactref element="R55" pad="2"/>
<contactref element="A139_HALL5" pad="P$5"/>
</signal>
<signal name="HALL6_VCC">
<contactref element="C56" pad="1"/>
<contactref element="A139_HALL6" pad="P$6"/>
<contactref element="A139_HALL6" pad="P$1"/>
<contactref element="HALL6_HEADER" pad="P$2"/>
</signal>
<signal name="HALL6_VOUT">
<contactref element="A139_HALL6" pad="P$2"/>
<contactref element="HALL6_HEADER" pad="P$3"/>
</signal>
<signal name="HALL6_GND">
<contactref element="A139_HALL6" pad="P$3_4"/>
<contactref element="C56" pad="2"/>
<contactref element="HALL6_HEADER" pad="P$1"/>
</signal>
<signal name="!SLEEP6">
<contactref element="R56" pad="2"/>
<contactref element="A139_HALL6" pad="P$5"/>
</signal>
<signal name="HALL6_!SLEEP_IN">
<contactref element="R56" pad="1"/>
<contactref element="HALL6_HEADER" pad="P$4"/>
</signal>
<signal name="HALL7_GND">
<contactref element="HALL7_HEADER" pad="P$1"/>
<contactref element="A139_HALL7" pad="P$3_4"/>
<contactref element="C57" pad="2"/>
</signal>
<signal name="HALL7_VOUT">
<contactref element="HALL7_HEADER" pad="P$3"/>
<contactref element="A139_HALL7" pad="P$2"/>
</signal>
<signal name="HALL7_VCC">
<contactref element="HALL7_HEADER" pad="P$2"/>
<contactref element="A139_HALL7" pad="P$6"/>
<contactref element="A139_HALL7" pad="P$1"/>
<contactref element="C57" pad="1"/>
</signal>
<signal name="HALL7_!SLEEP_IN">
<contactref element="HALL7_HEADER" pad="P$4"/>
<contactref element="R57" pad="1"/>
</signal>
<signal name="!SLEEP7">
<contactref element="A139_HALL7" pad="P$5"/>
<contactref element="R57" pad="2"/>
</signal>
<signal name="HALL8_VCC">
<contactref element="C58" pad="1"/>
<contactref element="A139_HALL8" pad="P$1"/>
<contactref element="A139_HALL8" pad="P$6"/>
<contactref element="HALL8_HEADER" pad="P$2"/>
</signal>
<signal name="HALL8_VOUT">
<contactref element="A139_HALL8" pad="P$2"/>
<contactref element="HALL8_HEADER" pad="P$3"/>
</signal>
<signal name="HALL8_GND">
<contactref element="A139_HALL8" pad="P$3_4"/>
<contactref element="C58" pad="2"/>
<contactref element="HALL8_HEADER" pad="P$1"/>
</signal>
<signal name="!SLEEP8">
<contactref element="R58" pad="2"/>
<contactref element="A139_HALL8" pad="P$5"/>
</signal>
<signal name="HALL8_!SLEEP_IN">
<contactref element="R58" pad="1"/>
<contactref element="HALL8_HEADER" pad="P$4"/>
</signal>
<signal name="HALL9_GND">
<contactref element="HALL9_HEADER" pad="P$1"/>
<contactref element="C59" pad="2"/>
<contactref element="A139_HALL9" pad="P$3_4"/>
</signal>
<signal name="HALL9_VOUT">
<contactref element="HALL9_HEADER" pad="P$3"/>
<contactref element="A139_HALL9" pad="P$2"/>
</signal>
<signal name="HALL9_VCC">
<contactref element="HALL9_HEADER" pad="P$2"/>
<contactref element="A139_HALL9" pad="P$1"/>
<contactref element="A139_HALL9" pad="P$6"/>
<contactref element="C59" pad="1"/>
</signal>
<signal name="HALL9_!SLEEP_IN">
<contactref element="HALL9_HEADER" pad="P$4"/>
<contactref element="R59" pad="1"/>
</signal>
<signal name="!SLEEP9">
<contactref element="A139_HALL9" pad="P$5"/>
<contactref element="R59" pad="2"/>
</signal>
<signal name="HALL10_!SLEEP_IN">
<contactref element="R60" pad="1"/>
<contactref element="HALL10_HEADER" pad="P$4"/>
</signal>
<signal name="!SLEEP10">
<contactref element="R60" pad="2"/>
<contactref element="A139_HALL10" pad="P$5"/>
</signal>
<signal name="HALL10_GND">
<contactref element="A139_HALL10" pad="P$3_4"/>
<contactref element="C60" pad="2"/>
<contactref element="HALL10_HEADER" pad="P$1"/>
</signal>
<signal name="HALL10_VOUT">
<contactref element="A139_HALL10" pad="P$2"/>
<contactref element="HALL10_HEADER" pad="P$3"/>
</signal>
<signal name="HALL10_VCC">
<contactref element="A139_HALL10" pad="P$1"/>
<contactref element="A139_HALL10" pad="P$6"/>
<contactref element="C60" pad="1"/>
<contactref element="HALL10_HEADER" pad="P$2"/>
</signal>
<signal name="HALL11_GND">
<contactref element="A139_HALL11" pad="P$3_4"/>
<contactref element="C61" pad="2"/>
<contactref element="HALL11_HEADER" pad="P$1"/>
</signal>
<signal name="HALL11_VOUT">
<contactref element="A139_HALL11" pad="P$2"/>
<contactref element="HALL11_HEADER" pad="P$3"/>
</signal>
<signal name="HALL11_VCC">
<contactref element="C61" pad="1"/>
<contactref element="A139_HALL11" pad="P$1"/>
<contactref element="A139_HALL11" pad="P$6"/>
<contactref element="HALL11_HEADER" pad="P$2"/>
</signal>
<signal name="!SLEEP11">
<contactref element="A139_HALL11" pad="P$5"/>
<contactref element="R61" pad="2"/>
</signal>
<signal name="HALL11_!SLEEP_IN">
<contactref element="R61" pad="1"/>
<contactref element="HALL11_HEADER" pad="P$4"/>
</signal>
<signal name="HALL15_!SLEEP_IN">
<contactref element="R65" pad="1"/>
<contactref element="HALL15_HEADER" pad="P$4"/>
</signal>
<signal name="!SLEEP15">
<contactref element="A139_HALL15" pad="P$5"/>
<contactref element="R65" pad="2"/>
</signal>
<signal name="HALL15_GND">
<contactref element="A139_HALL15" pad="P$3_4"/>
<contactref element="C65" pad="2"/>
<contactref element="HALL15_HEADER" pad="P$1"/>
</signal>
<signal name="HALL15_VOUT">
<contactref element="A139_HALL15" pad="P$2"/>
<contactref element="HALL15_HEADER" pad="P$3"/>
</signal>
<signal name="HALL15_VCC">
<contactref element="A139_HALL15" pad="P$1"/>
<contactref element="A139_HALL15" pad="P$6"/>
<contactref element="C65" pad="1"/>
<contactref element="HALL15_HEADER" pad="P$2"/>
</signal>
<signal name="HALL14_!SLEEP_IN">
<contactref element="R64" pad="1"/>
<contactref element="HALL14_HEADER" pad="P$4"/>
</signal>
<signal name="!SLEEP14">
<contactref element="R64" pad="2"/>
<contactref element="A139_HALL14" pad="P$5"/>
</signal>
<signal name="HALL14_GND">
<contactref element="A139_HALL14" pad="P$3_4"/>
<contactref element="C64" pad="2"/>
<contactref element="HALL14_HEADER" pad="P$1"/>
</signal>
<signal name="HALL14_VOUT">
<contactref element="A139_HALL14" pad="P$2"/>
<contactref element="HALL14_HEADER" pad="P$3"/>
</signal>
<signal name="HALL14_VCC">
<contactref element="A139_HALL14" pad="P$6"/>
<contactref element="C64" pad="1"/>
<contactref element="A139_HALL14" pad="P$1"/>
<contactref element="HALL14_HEADER" pad="P$2"/>
</signal>
<signal name="HALL13_!SLEEP_IN">
<contactref element="R63" pad="1"/>
<contactref element="HALL13_HEADER" pad="P$4"/>
</signal>
<signal name="!SLEEP13">
<contactref element="R63" pad="2"/>
<contactref element="A139_HALL13" pad="P$5"/>
</signal>
<signal name="HALL13_GND">
<contactref element="A139_HALL13" pad="P$3_4"/>
<contactref element="C63" pad="2"/>
<contactref element="HALL13_HEADER" pad="P$1"/>
</signal>
<signal name="HALL13_VOUT">
<contactref element="A139_HALL13" pad="P$2"/>
<contactref element="HALL13_HEADER" pad="P$3"/>
</signal>
<signal name="HALL13_VCC">
<contactref element="C63" pad="1"/>
<contactref element="A139_HALL13" pad="P$6"/>
<contactref element="A139_HALL13" pad="P$1"/>
<contactref element="HALL13_HEADER" pad="P$2"/>
</signal>
<signal name="HALL12_!SLEEP_IN">
<contactref element="R62" pad="1"/>
<contactref element="HALL12_HEADER" pad="P$4"/>
</signal>
<signal name="!SLEEP12">
<contactref element="R62" pad="2"/>
<contactref element="A139_HALL12" pad="P$5"/>
</signal>
<signal name="HALL12_GND">
<contactref element="C62" pad="2"/>
<contactref element="A139_HALL12" pad="P$3_4"/>
<contactref element="HALL12_HEADER" pad="P$1"/>
</signal>
<signal name="HALL12_VOUT">
<contactref element="A139_HALL12" pad="P$2"/>
<contactref element="HALL12_HEADER" pad="P$3"/>
</signal>
<signal name="HALL12_VCC">
<contactref element="A139_HALL12" pad="P$1"/>
<contactref element="C62" pad="1"/>
<contactref element="A139_HALL12" pad="P$6"/>
<contactref element="HALL12_HEADER" pad="P$2"/>
</signal>
<signal name="MUX_!EN">
<contactref element="U1" pad="12"/>
<contactref element="U$2" pad="15"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R31" pad="2"/>
<contactref element="BJT" pad="1"/>
</signal>
<signal name="GATE">
<contactref element="R33" pad="1"/>
<contactref element="P-FET" pad="1"/>
<contactref element="BJT" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="P-FET" pad="3"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="BATT_MONITOR">
<contactref element="U1" pad="19"/>
<contactref element="R29" pad="2"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="BATT_MONITOR_EN">
<contactref element="R32" pad="2"/>
<contactref element="R31" pad="1"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="V_JACK">
<contactref element="2,1MM_JACK" pad="P$1"/>
<contactref element="SCHOTTKY" pad="A"/>
</signal>
<signal name="VBATTERY">
<contactref element="LTC4411" pad="1"/>
<contactref element="MOLEX_KK" pad="2"/>
<contactref element="PRIMARY_BATTERY" pad="VBAT"/>
</signal>
<signal name="N$1">
<contactref element="LTC4411" pad="4"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="HALL16_GND">
<contactref element="HALL16_HEADER" pad="P$1"/>
<contactref element="C66" pad="2"/>
<contactref element="A139_HALL16" pad="P$3_4"/>
</signal>
<signal name="HALL16_VOUT">
<contactref element="HALL16_HEADER" pad="P$3"/>
<contactref element="A139_HALL16" pad="P$2"/>
</signal>
<signal name="HALL16_VCC">
<contactref element="HALL16_HEADER" pad="P$2"/>
<contactref element="C66" pad="1"/>
<contactref element="A139_HALL16" pad="P$1"/>
<contactref element="A139_HALL16" pad="P$6"/>
</signal>
<signal name="HALL16_!SLEEP_IN">
<contactref element="HALL16_HEADER" pad="P$4"/>
<contactref element="R66" pad="1"/>
</signal>
<signal name="!SLEEP16">
<contactref element="A139_HALL16" pad="P$5"/>
<contactref element="R66" pad="2"/>
</signal>
<signal name="HALL17_GND">
<contactref element="HALL17_HEADER" pad="P$1"/>
<contactref element="C67" pad="2"/>
<contactref element="A139_HALL17" pad="P$3_4"/>
</signal>
<signal name="HALL17_VCC">
<contactref element="HALL17_HEADER" pad="P$2"/>
<contactref element="C67" pad="1"/>
<contactref element="A139_HALL17" pad="P$1"/>
<contactref element="A139_HALL17" pad="P$6"/>
</signal>
<signal name="HALL17_!SLEEP_IN">
<contactref element="HALL17_HEADER" pad="P$4"/>
<contactref element="R67" pad="1"/>
</signal>
<signal name="HALL17_VOUT">
<contactref element="HALL17_HEADER" pad="P$3"/>
<contactref element="A139_HALL17" pad="P$2"/>
</signal>
<signal name="!SLEEP17">
<contactref element="A139_HALL17" pad="P$5"/>
<contactref element="R67" pad="2"/>
</signal>
<signal name="HALL18_!SLEEP_IN">
<contactref element="R68" pad="1"/>
<contactref element="HALL18_HEADER" pad="P$4"/>
</signal>
<signal name="!SLEEP18">
<contactref element="A139_HALL18" pad="P$5"/>
<contactref element="R68" pad="2"/>
</signal>
<signal name="HALL18_GND">
<contactref element="C68" pad="2"/>
<contactref element="A139_HALL18" pad="P$3_4"/>
<contactref element="HALL18_HEADER" pad="P$1"/>
</signal>
<signal name="HALL18_VOUT">
<contactref element="A139_HALL18" pad="P$2"/>
<contactref element="HALL18_HEADER" pad="P$3"/>
</signal>
<signal name="HALL18_VCC">
<contactref element="A139_HALL18" pad="P$6"/>
<contactref element="A139_HALL18" pad="P$1"/>
<contactref element="C68" pad="1"/>
<contactref element="HALL18_HEADER" pad="P$2"/>
</signal>
<signal name="HALL19_GND">
<contactref element="HALL19_HEADER" pad="P$1"/>
<contactref element="A139_HALL19" pad="P$3_4"/>
<contactref element="C69" pad="2"/>
</signal>
<signal name="HALL19_VOUT">
<contactref element="HALL19_HEADER" pad="P$3"/>
<contactref element="A139_HALL19" pad="P$2"/>
</signal>
<signal name="HALL19_VCC">
<contactref element="HALL19_HEADER" pad="P$2"/>
<contactref element="C69" pad="1"/>
<contactref element="A139_HALL19" pad="P$6"/>
<contactref element="A139_HALL19" pad="P$1"/>
</signal>
<signal name="HALL19_!SLEEP_IN">
<contactref element="HALL19_HEADER" pad="P$4"/>
<contactref element="R69" pad="1"/>
</signal>
<signal name="!SLEEP19">
<contactref element="R69" pad="2"/>
<contactref element="A139_HALL19" pad="P$5"/>
</signal>
<signal name="VRAW2">
<contactref element="MCP1700T-3302" pad="3"/>
<contactref element="C1" pad="+"/>
<contactref element="PWR_JUMPER" pad="1"/>
<contactref element="PWR_PASSTHRU" pad="1"/>
</signal>
<signal name="VRAW1">
<contactref element="SCHOTTKY" pad="C"/>
<contactref element="LTC4411" pad="5"/>
<contactref element="C25" pad="1"/>
<contactref element="PWR_PASSTHRU" pad="2"/>
<contactref element="PWR_JUMPER" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
