(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+3V3")
  (net 2 "/SCL")
  (net 3 "/SDA")
  (net 4 "GND")
  (net 5 "/AX")
  (net 6 "/AY")
  (net 7 "unconnected-(U1-ALERT{slash}RDY-Pad2)")
  (net 8 "unconnected-(U1-AIN2-Pad6)")
  (net 9 "unconnected-(U1-AIN3-Pad7)")
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x04_P1.27mm_Vertical" (layer "F.Cu")
    (at 184.5 73.46)
    (descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x04 1.27mm single row")
    (property "Sheetfile" "psp_2ndstick_pcb.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -1.695) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04" (at 0 5.505) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.905 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 1 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 2 "/SCL") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 3 "/SDA") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x04_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-10_3x3mm_P0.5mm" (layer "F.Cu")
    (at 180 74.5)
    (descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
    (tags "SSOP 0.5")
    (property "Sheetfile" "psp_2ndstick_pcb.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ultra-Small, Low-Power, I2C-Compatible, 860-SPS, 16-Bit ADCs With Internal Reference, Oscillator, and Programmable Comparator, VSSOP-10")
    (property "ki_keywords" "16 bit 4 channel I2C ADC")
    (attr smd)
    (fp_text reference "U1" (at 0 0) (layer "F.SilkS"))
    (fp_text value "ADS1115IDGS" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.15 -1) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "ADDR") (pintype "input"))
    (pad "2" smd rect (at -2.15 -0.5) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "unconnected-(U1-ALERT{slash}RDY-Pad2)") (pinfunction "ALERT/RDY") (pintype "output+no_connect"))
    (pad "3" smd rect (at -2.15 0) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at -2.15 0.5) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/AX") (pinfunction "AIN0") (pintype "input"))
    (pad "5" smd rect (at -2.15 1) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/AY") (pinfunction "AIN1") (pintype "input"))
    (pad "6" smd rect (at 2.15 1) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "unconnected-(U1-AIN2-Pad6)") (pinfunction "AIN2") (pintype "input+no_connect"))
    (pad "7" smd rect (at 2.15 0.5) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "unconnected-(U1-AIN3-Pad7)") (pinfunction "AIN3") (pintype "input+no_connect"))
    (pad "8" smd rect (at 2.15 0) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "9" smd rect (at 2.15 -0.5) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "10" smd rect (at 2.15 -1) (size 1.1 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/SCL") (pinfunction "SCL") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-10_3x3mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "F.Cu")
    (at 180.0675 77.5 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "psp_2ndstick_pcb.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "0.1uf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x04_P1.27mm_Vertical" (layer "F.Cu")
    (at 175.5 73.46)
    (descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x04 1.27mm single row")
    (property "Sheetfile" "psp_2ndstick_pcb.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -1.695) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04" (at 0 5.505) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.905 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 1 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 5 "/AX") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 6 "/AY") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x04_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 174.5 71.95) (end 185.5 78.75)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Y" (at 176.5 76.5) (layer "B.SilkS"))
  (gr_text "VCC" (at 176.5 74) (layer "B.SilkS"))
  (gr_text "SCL" (at 183.5 75.25) (layer "B.SilkS"))
  (gr_text "GND" (at 176.5 77.75) (layer "B.SilkS"))
  (gr_text "VCC" (at 183.5 74) (layer "B.SilkS"))
  (gr_text "SDA" (at 183.5 76.5) (layer "B.SilkS"))
  (gr_text "X" (at 176.5 75.25) (layer "B.SilkS"))
  (gr_text "GND" (at 183.5 77.75) (layer "B.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 174.5 78.75) (xy 174.5 71.95))
    (height -2)
    (gr_text "6.8000 mm" (at 171.35 75.35 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 174.5 71.95) (xy 185.5 71.95))
    (height -1.2)
    (gr_text "11.0000 mm" (at 180 69.6) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 4) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 174.7 72.45)
        (xy 185.3 72.45)
        (xy 185.3 78.25)
        (xy 174.7 78.25)
      )
    )
  )
)
