<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="14.5" x2="0" y2="1.5" width="0.3048" layer="20"/>
<wire x1="0" y1="1.5" x2="1.5" y2="0" width="0.3048" layer="20" curve="90"/>
<wire x1="1.5" y1="0" x2="7.5" y2="0" width="0.3048" layer="20"/>
<wire x1="7.5" y1="0" x2="7.5" y2="16" width="0.3048" layer="20"/>
<wire x1="7.5" y1="16" x2="1.5" y2="16" width="0.3048" layer="20"/>
<wire x1="1.5" y1="16" x2="0" y2="14.5" width="0.3048" layer="20" curve="90"/>
<text>PROG ADAPTER</text>
</plain>
<libraries>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP14SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TX" library="testpad" package="TP14SQ" value="TPSQTP14SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="RX" library="testpad" package="TP14SQ" value="TPSQTP14SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="VCC" library="testpad" package="TP14SQ" value="TPSQTP14SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="RST" library="testpad" package="TP14SQ" value="TPSQTP14SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="GND" library="testpad" package="TP14SQ" value="TPSQTP14SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TX1" library="testpad" package="TP14SQ" value="TPSQTP14SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="RX1" library="testpad" package="TP14SQ" value="TPSQTP14SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="VCC1" library="testpad" package="TP14SQ" value="TPSQTP14SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="RST1" library="testpad" package="TP14SQ" value="TPSQTP14SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="GND1" library="testpad" package="TP14SQ" value="TPSQTP14SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="TX1" pad="TP"/>
<contactref element="TX" pad="TP"/>
</signal>
<signal name="N$2">
<contactref element="RX1" pad="TP"/>
<contactref element="RX" pad="TP"/>
</signal>
<signal name="N$3">
<contactref element="VCC1" pad="TP"/>
<contactref element="VCC" pad="TP"/>
</signal>
<signal name="N$4">
<contactref element="RST1" pad="TP"/>
<contactref element="RST" pad="TP"/>
</signal>
<signal name="GND">
<contactref element="GND1" pad="TP"/>
<contactref element="GND" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
