(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "SMuFF Connector Board PCB")
    (date "2023-03-26")
    (rev "1")
    (company "Technik Gegg")
    (comment 4 "AISLER Project ID: BNDRXJJP")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "unconnected-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "unconnected-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J2-Pad1)")
  (net 8 "unconnected-(J2-Pad2)")
  (net 9 "Net-(J2-Pad3)")
  (net 10 "Net-(J2-Pad4)")
  (net 11 "unconnected-(J2-Pad5)")
  (net 12 "Net-(J2-Pad6)")
  (net 13 "GND")
  (net 14 "+5V")
  (net 15 "/SCL")
  (net 16 "/SDA")
  (net 17 "/NeoPixel")
  (net 18 "/Feeder")
  (net 19 "/Selector")
  (net 20 "Net-(J6-Pad1)")
  (net 21 "Net-(J6-Pad2)")
  (net 22 "Net-(J6-Pad3)")
  (net 23 "Net-(J6-Pad4)")
  (net 24 "Net-(J6-Pad5)")
  (net 25 "Net-(J6-Pad6)")
  (net 26 "Net-(J6-Pad7)")
  (net 27 "Net-(J6-Pad8)")
  (net 28 "Net-(J6-Pad11)")
  (net 29 "Net-(J6-Pad13)")
  (net 30 "Net-(J10-Pad2)")
  (net 31 "Net-(J12-Pad3)")
  (net 32 "Net-(J12-Pad4)")
  (net 33 "/VCC-IN")
  (footprint "Connector_JST:JST_PH_B6B-PH-K_1x06_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5B7745C2)
    (at 90.7708 113.9228 -90)
    (descr "JST PH series connector, B6B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -2.0358 0.0928 90) (layer "B.SilkS"))
    (fp_text value "Selector Stepper" (at 5 4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5 1.5 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.2083333333)
      (net 1 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "unconnected-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval (at 4 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 6 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 8 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "unconnected-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval (at 10 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B6B-PH-K_1x06_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 108.807 102.0064)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 108.807 119.9134)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (footprint "Connector_JST:JST_PH_B6B-PH-K_1x06_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5B7745C2)
    (at 83.862 113.872 -90)
    (descr "JST PH series connector, B6B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -2.112 -0.1612 90) (layer "B.SilkS"))
    (fp_text value "Feeder Stepper" (at 5 4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5 1.5 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.2083333333)
      (net 7 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 "unconnected-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval (at 4 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 6 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 8 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 "unconnected-(J2-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval (at 10 0 270) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B6B-PH-K_1x06_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 164.814 110.8964)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (footprint "Symbol:KiCad-Logo2_5mm_SilkScreen" (layer "F.Cu")
    (tedit 0)
    (at 162.401 119.634 90)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.08 90) (layer "F.SilkS") hide)
    (fp_text value "KiCad-Logo2_5mm_SilkScreen" (at 0 5.08 90) (layer "F.Fab") hide)
  )
  (footprint "Connector_JST:JST_XH_B5B-XH-A_1x05_P2.50mm_Vertical" (layer "F.Cu")
    (tedit 5C28146C)
    (at 90.6442 98.0224 -90)
    (descr "JST XH series connector, B5B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -2.0104 0.0932 90) (layer "B.SilkS"))
    (fp_text value "Signals" (at 5 4.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5 2.7 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 15 "/SCL") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 "/SDA") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 17 "/NeoPixel") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 18 "/Feeder") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 19 "/Selector") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B5B-XH-A_1x05_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical" (layer "F.Cu")
    (tedit 5C28146C)
    (at 82.948 98.0224 -90)
    (descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -2.1374 -0.1016 90) (layer "B.SilkS"))
    (fp_text value "Power" (at 3.75 4.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 2.7 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 13 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 13 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 33 "/VCC-IN") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 33 "/VCC-IN") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:Logo-5mm" (layer "B.Cu")
    (tedit 0)
    (at 142.716 123.19)
    (descr "TechnikGegg")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at -0.323379 2.357953) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.581121 -2.322276) (layer "B.SilkS") hide)
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 123.539 105.664 -90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J13" (at 0.254 2.667) (layer "F.SilkS"))
    (fp_text value "(Lid Servo)" (at 0 -7.41 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J12-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical" (layer "B.Cu")
    (tedit 5C28146C)
    (at 115.919 99.7204 -90)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J10" (at -2.1844 -0.127) (layer "F.SilkS"))
    (fp_text value "Feeder Sensor" (at 2.5 -4.6 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 -2.7 90) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 13 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 30 "Net-(J10-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical" (layer "B.Cu")
    (tedit 5C28146C)
    (at 138.508 103.9714 -90)
    (descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 3.8008 -2.2014) (layer "F.SilkS"))
    (fp_text value "Feeder Motor" (at 3.75 -4.6 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 -2.7 90) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 27 "Net-(J6-Pad8)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 26 "Net-(J6-Pad7)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 25 "Net-(J6-Pad6)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 24 "Net-(J6-Pad5)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical" (layer "B.Cu")
    (tedit 5C28146C)
    (at 123.472 116.8824)
    (descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at 3.75 -2.2014) (layer "F.SilkS"))
    (fp_text value "Selector Motor" (at 3.75 -4.6) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 -2.7) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 23 "Net-(J6-Pad4)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 22 "Net-(J6-Pad3)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-Pad2)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 20 "Net-(J6-Pad1)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x20_P1.27mm_Vertical" (layer "B.Cu")
    (tedit 59FED6E3)
    (at 102.5 123.2154)
    (descr "Through hole straight pin header, 1x20, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x20 1.27mm single row")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at -0.043 2.1336 90) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x16" (at 0 -25.825) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -12.065 90) (layer "B.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 20 "Net-(J6-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 21 "Net-(J6-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 22 "Net-(J6-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 23 "Net-(J6-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 "Net-(J6-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -6.35) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 25 "Net-(J6-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 26 "Net-(J6-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -8.89) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 27 "Net-(J6-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -11.43) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 "GND") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -12.7) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 28 "Net-(J6-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 -13.97) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 30 "Net-(J10-Pad2)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -15.24) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 29 "Net-(J6-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 -16.51) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 31 "Net-(J12-Pad3)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -17.78) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 32 "Net-(J12-Pad4)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 -19.05) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -20.32) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 -21.59) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 "GND") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -22.86) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 -24.13) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 "GND") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x20_P1.27mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical" (layer "B.Cu")
    (tedit 5C28146C)
    (at 115.902 112.0286 -90)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at -1.9196 -0.271) (layer "F.SilkS"))
    (fp_text value "Selector Endstop" (at 2.5 -4.6 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 -2.7 90) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 13 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 28 "Net-(J6-Pad11)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical" (layer "B.Cu")
    (tedit 5C28146C)
    (at 148.7104 118.3132)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J11" (at 2.5254 -2.176) (layer "F.SilkS"))
    (fp_text value "NeoPixels" (at 2.5 -4.6) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 -2.7) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 13 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 29 "Net-(J6-Pad13)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x20_P1.27mm_Horizontal" (layer "B.Cu")
    (tedit 59FED6E3)
    (at 94.9452 123.1392)
    (descr "Through hole angled pin header, 1x20, 1.27mm pitch, 4.0mm pin length, single row")
    (tags "Through hole angled pin header THT 1x20 1.27mm single row")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0.0508 2.0828 270) (layer "B.SilkS"))
    (fp_text value "Connector 1x20" (at 2.4325 -25.765 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1 -12.065 270) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad6)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -6.35) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad4)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad3)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -8.89) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 33 "/VCC-IN") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -11.43) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 "GND") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -12.7) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 19 "/Selector") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 -13.97) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 "/Feeder") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -15.24) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 "/NeoPixel") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 -16.51) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 "/SDA") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -17.78) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 "/SCL") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 -19.05) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 33 "/VCC-IN") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -20.32) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 33 "/VCC-IN") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 -21.59) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 "GND") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -22.86) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 -24.13) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 "GND") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x20_P1.27mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical" (layer "B.Cu")
    (tedit 5C28146C)
    (at 123.472 100.6264)
    (descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J12" (at -2.6 -0.0424) (layer "F.SilkS"))
    (fp_text value "I2C" (at 3.75 -4.6) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 -2.7) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 13 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 31 "Net-(J12-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.5 0) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 32 "Net-(J12-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 136.239 98.552 -90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J14" (at -1.905 -2.54) (layer "F.SilkS"))
    (fp_text value "(Cutter Servo)" (at 0 -7.41 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J12-Pad4)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical" (layer "B.Cu")
    (tedit 5C28146C)
    (at 162.511 100.096 -90)
    (descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (property "Sheetfile" "SMuFF Connector.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J15" (at -3.81 -0.381) (layer "F.SilkS"))
    (fp_text value "SPARE" (at 1.25 -4.6 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 -2.7 90) (layer "B.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 13 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.5 0 270) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 118.01562 122.91782) (end 118.0018 126.873) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 99.78938 108.79916) (mid 99.4918 109.51758) (end 98.77338 109.81516) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 137.22898 121.90182) (mid 137.9474 122.1994) (end 138.24498 122.91782) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 98.755202 110.4392) (mid 99.473622 110.73678) (end 99.771202 111.4552) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.59589 94.8436) (end 78.867 94.8436) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 143.524742 100.130629) (mid 143.8372 99.376287) (end 144.591542 99.063829) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 99.78938 121.15078) (mid 99.4918 121.8692) (end 98.77338 122.16678) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.76398 114.97858) (end 99.771202 111.4552) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 157.901142 99.056171) (mid 158.655484 99.368629) (end 158.967942 100.122971) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.5962 126.873) (end 78.867 126.873) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 99.76398 114.97858) (mid 99.4664 115.697) (end 98.74798 115.99458) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 98.76647 98.96749) (end 97.61251 98.96749) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 96.60342 123.80682) (mid 96.901 123.0884) (end 97.61942 122.79082) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.79 94.869) (end 168.116 94.869) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 98.773378 101.066598) (mid 99.491798 101.364178) (end 99.789378 102.082598) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.57802 114.97858) (end 96.585242 111.4552) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 97.61942 122.16678) (mid 96.901 121.8692) (end 96.60342 121.15078) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.78247 97.95149) (end 99.79 94.869) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 97.61942 109.81516) (mid 96.901 109.51758) (end 96.60342 108.79916) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 97.61251 98.96749) (mid 96.89409 98.66991) (end 96.59651 97.95149) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 98.780602 116.6114) (mid 99.499022 116.90898) (end 99.796602 117.6274) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 144.5992 110.548459) (mid 143.844861 110.236) (end 143.5324 109.481659) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 98.77338 122.16678) (end 97.61942 122.16678) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.78938 121.15078) (end 99.796602 117.6274) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 99.78247 97.95149) (mid 99.48489 98.66991) (end 98.76647 98.96749) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 96.603418 102.082598) (mid 96.900998 101.364178) (end 97.619418 101.066598) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 97.619418 101.066598) (end 98.773378 101.066598) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 97.59402 115.99458) (mid 96.8756 115.697) (end 96.57802 114.97858) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 158.9756 109.481658) (end 158.967942 100.122971) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.78938 123.80682) (end 99.79 126.873) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 118.01562 122.91782) (mid 118.3132 122.1994) (end 119.03162 121.90182) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 168.116 126.873) (end 138.2268 126.873) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 143.524742 100.130629) (end 143.5324 109.481659) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 97.61942 122.79082) (end 98.77338 122.79082) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 144.591542 99.063829) (end 157.901142 99.056171) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.60342 121.15078) (end 96.610642 117.6274) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.60342 123.80682) (end 96.5962 126.873) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 158.9756 109.481658) (mid 158.663142 110.236) (end 157.9088 110.548458) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 96.585242 111.4552) (mid 96.882822 110.73678) (end 97.601242 110.4392) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 97.601242 110.4392) (end 98.755202 110.4392) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 78.867 126.873) (end 78.867 94.8436) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138.2268 126.873) (end 138.24498 122.91782) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.60342 108.79916) (end 96.603418 102.082598) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 144.5992 110.548459) (end 157.9088 110.548458) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 97.626642 116.6114) (end 98.780602 116.6114) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 98.77338 122.79082) (mid 99.4918 123.0884) (end 99.78938 123.80682) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 98.77338 109.81516) (end 97.61942 109.81516) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 96.610642 117.6274) (mid 96.908222 116.90898) (end 97.626642 116.6114) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 98.74798 115.99458) (end 97.59402 115.99458) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.78938 108.79916) (end 99.789378 102.082598) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.79 126.873) (end 118.0018 126.873) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 168.116 94.869) (end 168.116 126.873) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.59651 97.95149) (end 96.59589 94.8436) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 119.03162 121.90182) (end 137.22898 121.90182) (layer "Edge.Cuts") (width 0.1))
  (gr_text "SELECTOR" (at 127.222 112.1664 180) (layer "B.SilkS"))
  (gr_text "I2C" (at 132.175 104.14 180) (layer "B.SilkS"))
  (gr_text "FED" (at 87.884 105.41) (layer "B.SilkS"))
  (gr_text "(LID SERVO)" (at 126.079 108.331 180) (layer "B.SilkS"))
  (gr_text "REV: 1" (at 158.464 117.475 180) (layer "B.SilkS"))
  (gr_text "SPARE PWR" (at 163.29 106.426 180) (layer "B.SilkS"))
  (gr_text "GND" (at 80.518 99.314) (layer "B.SilkS"))
  (gr_text "(CUTTER SERVO)" (at 149.447 97.79 180) (layer "B.SilkS"))
  (gr_text "+5V" (at 80.899 104.394) (layer "B.SilkS"))
  (gr_text "NEOPIXEL" (at 151.2758 113.3094 180) (layer "B.SilkS"))
  (gr_text "SELECTOR" (at 112.109 115.316 270) (layer "B.SilkS"))
  (gr_text "SDA" (at 87.884 100.584) (layer "B.SilkS"))
  (gr_text "FEEDER" (at 134.715 107.7214 -90) (layer "B.SilkS"))
  (gr_text "NPX" (at 87.757 103.124) (layer "B.SilkS"))
  (gr_text "SMuFF Connector Board\n2023 Technik Gegg" (at 145.891 123.698 180) (layer "B.SilkS"))
  (gr_text "FEEDER" (at 112.1344 102.235 270) (layer "B.SilkS"))
  (gr_text "SEL" (at 87.884 108.077) (layer "B.SilkS"))
  (gr_text "SCL" (at 87.884 98.044) (layer "B.SilkS"))
  (gr_text "SIG" (at 113.125 114.554) (layer "F.SilkS"))
  (gr_text "VCC" (at 165.449 102.616) (layer "F.SilkS"))
  (gr_text "GND" (at 165.195 100.076) (layer "F.SilkS"))
  (gr_text "SDA" (at 128.492 98.171 270) (layer "F.SilkS"))
  (gr_text "POWER" (at 82.931 109.347) (layer "F.SilkS"))
  (gr_text "FEEDER" (at 79.756 118.8212 270) (layer "F.SilkS"))
  (gr_text "GND" (at 123.412 103.378 270) (layer "F.SilkS"))
  (gr_text "VCC" (at 138.779 100.965 270) (layer "F.SilkS"))
  (gr_text "VCC" (at 113.125 104.775) (layer "F.SilkS"))
  (gr_text "SIG" (at 128.619 107.823 270) (layer "F.SilkS"))
  (gr_text "SIG" (at 113.125 102.235) (layer "F.SilkS"))
  (gr_text "GND" (at 148.685 121.031 270) (layer "F.SilkS"))
  (gr_text "VCC" (at 153.765 121.158 270) (layer "F.SilkS"))
  (gr_text "SIG" (at 151.098 120.904 270) (layer "F.SilkS"))
  (gr_text "SELECTOR" (at 86.741 118.872 270) (layer "F.SilkS"))
  (gr_text "GND" (at 113.125 99.695) (layer "F.SilkS"))
  (gr_text "VCC" (at 125.952 103.251 270) (layer "F.SilkS"))
  (gr_text "SIG" (at 141.319 100.711 270) (layer "F.SilkS"))
  (gr_text "GND" (at 136.239 100.965 270) (layer "F.SilkS"))
  (gr_text "GND" (at 112.998 112.141) (layer "F.SilkS"))
  (gr_text "SCL" (at 131.032 98.044 270) (layer "F.SilkS"))
  (gr_text "SIGNALS" (at 86.233 103.0732 270) (layer "F.SilkS"))
  (gr_text "VCC" (at 112.998 117.094) (layer "F.SilkS"))
  (zone (net 13) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 168.148 94.8944)
        (xy 168.148 126.873)
        (xy 138.2522 126.873)
        (xy 138.25231 121.8946)
        (xy 118.027756 121.904218)
        (xy 118.002246 126.873)
        (xy 78.8416 126.873)
        (xy 78.8416 94.869)
      )
    )
  )
)
