<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="-50.927" y1="-114.046" x2="-50.927" y2="-88.138" width="0" layer="20"/>
<wire x1="-50.927" y1="-88.138" x2="-49.022" y2="-85.852" width="0" layer="20"/>
<wire x1="-49.022" y1="-85.852" x2="-49.022" y2="-59.944" width="0" layer="20"/>
<wire x1="-49.022" y1="-59.944" x2="-60.452" y2="-48.514" width="0" layer="20"/>
<wire x1="-60.452" y1="-48.514" x2="-65.278" y2="-48.514" width="0" layer="20"/>
<wire x1="-65.278" y1="-48.514" x2="-65.278" y2="-86.487" width="0" layer="20"/>
<wire x1="-65.278" y1="-86.487" x2="-63.373" y2="-88.392" width="0" layer="20"/>
<wire x1="-63.373" y1="-88.392" x2="-63.373" y2="-114.046" width="0" layer="20"/>
<hole x="-57.15" y="-57.15" drill="3.175"/>
<hole x="-57.15" y="-93.98" drill="3.175"/>
<hole x="-57.15" y="-104.14" drill="3.175"/>
<text>RGBMarker</text>
<text>J008534C</text>
<text>20230411</text>
<text>S</text>
<text>S</text>
<wire x1="-50.927" y1="-114.046" x2="-63.373" y2="-114.046" width="0" layer="20" curve="-183.50681"/>
<text>MOLEX</text>
<text>533980471</text>
<text>For use with pre-
made Molex cable:
0151340403
ends are reversed</text>
<text>Countersink
out to line</text>
</plain>
<libraries>
<library name="STEVES_BU">
<packages>
<package name="LED_THRU_VSMY">
</package>
<package name="LOGO_BMP_OP">
</package>
<package name="533980471">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R" library="STEVES_BU" package="LED_THRU_VSMY" value="VSMY2850RGX01"/>
<element name="G" library="STEVES_BU" package="LED_THRU_VSMY" value="VSMY2850RGX01"/>
<element name="B" library="STEVES_BU" package="LED_THRU_VSMY" value="VSMY2850RGX01"/>
<element name="TP1" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="U$1" library="STEVES_BU" package="LOGO_BMP_OP" value="JFRC-LOGOLOGO_OP"/>
<element name="J2" library="STEVES_BU" package="533980471" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="R">
<contactref element="R" pad="A"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="B">
<contactref element="B" pad="A"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="TP1" pad="TP"/>
<contactref element="R" pad="C"/>
<contactref element="G" pad="C"/>
<contactref element="B" pad="C"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J2" pad="3"/>
<contactref element="G" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
