(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.646)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Purple") (thickness 0.0254))
      (layer "F.Cu" (type "copper") (thickness 0.0356))
      (layer "dielectric 1" (type "core") (thickness 1.524) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.0356))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Purple") (thickness 0.0254))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "ENIG")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 167 100)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+4V")
  (net 2 "GND")
  (net 3 "Net-(C103-Pad1)")
  (net 4 "Net-(C107-Pad1)")
  (net 5 "Net-(C108-Pad1)")
  (net 6 "Net-(C108-Pad2)")
  (net 7 "Net-(C109-Pad1)")
  (net 8 "Net-(C110-Pad1)")
  (net 9 "Net-(D101-Pad1)")
  (net 10 "Net-(D102-Pad1)")
  (net 11 "Net-(D104-Pad1)")
  (net 12 "Net-(D105-Pad1)")
  (net 13 "Net-(D106-Pad1)")
  (net 14 "Net-(D107-Pad1)")
  (net 15 "Net-(D108-Pad1)")
  (net 16 "Net-(D109-Pad1)")
  (net 17 "Net-(Q101-Pad2)")
  (net 18 "Net-(Q102-Pad2)")
  (net 19 "Net-(Q102-Pad3)")
  (net 20 "Net-(Q103-Pad2)")
  (net 21 "Net-(Q103-Pad3)")
  (net 22 "unconnected-(Q104-Pad1)")
  (net 23 "Net-(R101-Pad2)")
  (net 24 "Net-(R109-Pad2)")
  (net 25 "Net-(R110-Pad2)")
  (net 26 "Net-(R121-Pad2)")
  (net 27 "Net-(R122-Pad2)")
  (net 28 "Net-(R129-Pad2)")
  (net 29 "Net-(R130-Pad2)")
  (net 30 "Net-(R141-Pad1)")
  (net 31 "Net-(R142-Pad2)")
  (net 32 "Net-(R143-Pad2)")
  (net 33 "+5V")
  (net 34 "Net-(D110-Pad2)")
  (net 35 "Net-(C112-Pad1)")
  (net 36 "Net-(C114-Pad1)")
  (net 37 "Net-(C116-Pad1)")
  (net 38 "/Sample")
  (net 39 "Net-(Q106-Pad3)")
  (net 40 "Net-(R139-Pad1)")
  (net 41 "Net-(RV101-Pad1)")
  (net 42 "/Four_Fifths_Ref.")
  (net 43 "/Three_Fifths_Ref.")
  (net 44 "/Two_Fifths_Ref.")
  (net 45 "/One_Fifth_Ref.")
  (net 46 "/Ref.")
  (net 47 "/Random")
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 153.1 78.695 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R111" (at -1.345 1.6 90 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 0.95 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.005 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "Net-(Q101-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(Q102-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 155.5 102.7)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U106" (at -2.45 -1.1 unlocked) (layer "F.SilkS"))
    (fp_text value "LM358" (at 3.81 9.95) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 3.81 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(Q106-Pad3)") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(Q106-Pad3)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(RV101-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C116-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/Random") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/Random") (pintype "output"))
    (pad "8" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+4V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 211.1 86.34 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R121" (at -2.01 0 90 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 2.54 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "/Random") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 26 "Net-(R121-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 207.4 120.84 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R145" (at 6.89 1.1 90 unlocked) (layer "F.SilkS"))
    (fp_text value "470R" (at 2.54 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 "Net-(R143-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(D109-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "parts:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 201.5 87.7)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J104" (at 0 -3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+4V") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Vishay_T73YP_Vertical" (layer "F.Cu")
    (tedit 5A3D4993)
    (at 119.175 110.375 -90)
    (descr "Potentiometer, vertical, Vishay T73YP, http://www.vishay.com/docs/51016/t73.pdf")
    (tags "Potentiometer vertical Vishay T73YP")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV102" (at -2.425 1.725 90 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Potentiometer_Small" (at -0.06 2.01 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -2.56 -2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C108-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C108-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -5.08 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Vishay_T73YP_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 161 88.195 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R146" (at 0.855 -1.45 -270 unlocked) (layer "F.SilkS"))
    (fp_text value "470k" (at 0.95 1.92 -270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.95 0 -270 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 "Net-(C114-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 40 "Net-(R139-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 210.1 119.54 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R132" (at 7.04 0.75 90 unlocked) (layer "F.SilkS"))
    (fp_text value "470R" (at 2.54 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "Net-(R130-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(D107-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 176.4 108.075 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D102" (at 1.27 -2.96 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Red" (at 1.27 2.96 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D102-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 217.8 95.64 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R112" (at 1.69 1.65 90 unlocked) (layer "F.SilkS"))
    (fp_text value "470R" (at 2.54 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(D101-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 "Net-(R109-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 170.1 98.9)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R105" (at 2.5 -5.95 unlocked) (layer "F.SilkS"))
    (fp_text value "100k" (at 2.54 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 43 "/Three_Fifths_Ref.") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 44 "/Two_Fifths_Ref.") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 215.6 94.84 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R123" (at 3.64 -1.6 90 unlocked) (layer "F.SilkS"))
    (fp_text value "470R" (at 2.54 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(D104-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 26 "Net-(R121-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 149.4 83.295 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R108" (at 4.105 0.6 90 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 0.95 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.855 -0.1 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 33 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(Q102-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 204.5 79.35 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C101" (at -2.25 -0.05 90 unlocked) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.25 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+4V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 213.3 87.84 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R109" (at 1.79 1.7 90 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 2.54 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "/Random") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 "Net-(R109-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 204.6 119.15 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C102" (at 4.7 0.8 90 unlocked) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.25 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+4V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "parts:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 124.4 91.7)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J103" (at 0 -3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 123.1 100.5)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R120" (at -3.95 3.55 unlocked) (layer "F.SilkS"))
    (fp_text value "470R" (at 0.95 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.95 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Net-(Q103-Pad3)") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 175.1 103.3 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R115" (at 2.5 8.35 unlocked) (layer "F.SilkS"))
    (fp_text value "100k" (at 2.54 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 45 "/One_Fifth_Ref.") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 200.8 113.075 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D109" (at 1.27 -2.96 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Green" (at 1.27 2.96 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D109-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92L_Inline" (layer "F.Cu")
    (tedit 5A279A44)
    (at 151.97 119.95 180)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "TO-92L Inline Wide transistor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q104" (at -3.03 -0.9 90 unlocked) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 1.19 2.79) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.19 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 22 "unconnected-(Q104-Pad1)") (pinfunction "E") (pintype "passive+no_connect"))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(C108-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 208.275 95.7 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D104" (at 1.27 -2.96 unlocked) (layer "F.SilkS"))
    (fp_text value "Red" (at 1.27 2.96) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D104-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 133.3 117.9 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C106" (at 4.7 0.6 -270 unlocked) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.25 -270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 -270 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+4V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 140.3 78.7 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D110" (at 2.55 1.85 90 unlocked) (layer "F.SilkS"))
    (fp_text value "1N4004" (at 1.27 3.639635 90) (layer "F.Fab") hide)
    (fp_text user "A" (at 4.64 0 90) (layer "F.SilkS") hide)
    (fp_text user "A" (at 4.64 0 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 0.1 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(D110-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "parts:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 132.7 87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J109" (at 0 -3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+4V") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 154.75 118.2)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C110" (at 0 -1.9 unlocked) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C110-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 158.75 87.3 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C112" (at 1.25 1.85 unlocked) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C112-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Vishay_T73YP_Vertical" (layer "F.Cu")
    (tedit 5A3D4993)
    (at 130.825 118.425 90)
    (descr "Potentiometer, vertical, Vishay T73YP, http://www.vishay.com/docs/51016/t73.pdf")
    (tags "Potentiometer vertical Vishay T73YP")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV101" (at 2.375 -6.625 90 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Potentiometer_Small" (at -0.06 2.01 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -2.56 -2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(RV101-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(RV101-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -5.08 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R141-Pad1)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Vishay_T73YP_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 165.6 98.65 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C115" (at 5.3 0.45 90 unlocked) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.25 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+4V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 118.7 98.1 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C105" (at 3.25 -2.2 90 unlocked) (layer "F.SilkS"))
    (fp_text value "10uF" (at 2.5 2.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.5 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+4V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "parts:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 205.8 92.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J112" (at 0 -3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 214.7 109.96 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R130" (at 2.44 -1.7 90 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 2.54 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "/Random") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "Net-(R130-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 146.7 119.15 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C108" (at 1.75 -7.25 -270 unlocked) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.25 -270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 -270 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C108-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C108-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 151.66 82.8)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R101" (at 2.59 1.7 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 2.54 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 33 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 "Net-(R101-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 186 112.905 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R124" (at 0.705 1.7 90 unlocked) (layer "F.SilkS"))
    (fp_text value "470R" (at 0.95 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.95 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 "Net-(R122-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(D105-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 175.14 101.1 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R106" (at 2.54 7.15 unlocked) (layer "F.SilkS"))
    (fp_text value "100k" (at 2.54 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 44 "/Two_Fifths_Ref.") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 45 "/One_Fifth_Ref.") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 210.8 109.575 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D107" (at 4.925 0.05 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Amber" (at 1.27 2.96 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D107-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "parts:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 128.2 92.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J107" (at 0 -3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 181.9 91.725 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D106" (at 4.975 -0.1 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Amber" (at 1.27 2.96 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(D106-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tedit 5A1DD157)
    (at 121.43 86.1)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q105" (at 5.42 -1.6 unlocked) (layer "F.SilkS"))
    (fp_text value "2N7000" (at 1.27 2.79) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "S") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 "+4V") (pinfunction "G") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 34 "Net-(D110-Pad2)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "parts:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 218.3 102.3)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J106" (at 0 -3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/Ref.") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92L_Inline" (layer "F.Cu")
    (tedit 5A279A44)
    (at 144.1 84.845)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "TO-92L Inline Wide transistor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q102" (at 1.1 2.455 unlocked) (layer "F.SilkS"))
    (fp_text value "2N3906" (at 1.19 2.79) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.19 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 18 "Net-(Q102-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 19 "Net-(Q102-Pad3)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 147.8 114.8 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C107" (at 0 2.05 90 unlocked) (layer "F.SilkS"))
    (fp_text value "10uF" (at 2.5 2.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.5 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C107-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "parts:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 218.7 98.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J105" (at 0 -3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/Random") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 127.1 104.1 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R114" (at -2.2 0.1 90 unlocked) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 "Net-(Q103-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(Q102-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 137.725 84.7 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J101" (at 0 -2.33 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02" (at 0 4.87 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.27 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 118.9 100.3 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R119" (at 0.45 1.35 90 unlocked) (layer "F.SilkS"))
    (fp_text value "220R" (at 0.95 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.95 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "+4V") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Net-(Q103-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 212.4 112.36 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R143" (at -2.01 -0.75 90 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 2.54 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "/Random") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 "Net-(R143-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 151.49 117 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R134" (at -0.21 1.55 unlocked) (layer "F.SilkS"))
    (fp_text value "100k" (at 2.54 1.92 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C107-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C108-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 138.15 114.1 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C111" (at 1.3 2 unlocked) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "/Ref.") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 146.595 123.9)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R141" (at -0.045 1.45 unlocked) (layer "F.SilkS"))
    (fp_text value "100k" (at 0.95 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.95 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 30 "Net-(R141-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(C110-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 158.5 89.8 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R139" (at 4.05 -0.75 unlocked) (layer "F.SilkS"))
    (fp_text value "47k" (at 0.95 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.95 -1.92 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 40 "Net-(R139-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "+4V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 152.1 94.65 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C114" (at 4.85 0.4 90 unlocked) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.25 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C114-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 177.66 83.5)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R144" (at 2.54 -1.92 unlocked) (layer "F.SilkS"))
    (fp_text value "470R" (at 2.54 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(D108-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 31 "Net-(R142-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 208.705 81.6 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R129" (at 1.005 1.65 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 0.95 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.95 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "/Random") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 28 "Net-(R129-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92L_Inline" (layer "F.Cu")
    (tedit 5A279A44)
    (at 124.3 103.55 180)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "TO-92L Inline Wide transistor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q103" (at 5.15 -1.6 unlocked) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 1.19 2.79) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.19 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 20 "Net-(Q103-Pad2)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 21 "Net-(Q103-Pad3)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 130.15 76.75)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW101" (at 3.55 -1.75 unlocked) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.25 2.25 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(R101-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(R101-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 201.625 116 -90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U102" (at 3.8 17.525 90 unlocked) (layer "F.SilkS"))
    (fp_text value "LM2901" (at 3.81 17.57 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 7.62 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R122-Pad2)") (pintype "open_collector"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R110-Pad2)") (pintype "open_collector"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+4V") (pinfunction "V+") (pintype "power_in"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "/One_Fifth_Ref.") (pinfunction "-") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/Random") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "/Three_Fifths_Ref.") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/Random") (pinfunction "+") (pintype "input"))
    (pad "8" thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "/Four_Fifths_Ref.") (pinfunction "-") (pintype "input"))
    (pad "9" thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/Random") (pinfunction "+") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "/Two_Fifths_Ref.") (pinfunction "-") (pintype "input"))
    (pad "11" thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/Random") (pinfunction "+") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "13" thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R130-Pad2)") (pintype "open_collector"))
    (pad "14" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R143-Pad2)") (pintype "open_collector"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 201.625 77.1 -90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U101" (at 3.65 17.425 90 unlocked) (layer "F.SilkS"))
    (fp_text value "LM2901" (at 3.81 17.57 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 7.62 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R121-Pad2)") (pintype "open_collector"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R109-Pad2)") (pintype "open_collector"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+4V") (pinfunction "V+") (pintype "power_in"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "/Three_Fifths_Ref.") (pinfunction "-") (pintype "input"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/Random") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "/Two_Fifths_Ref.") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/Random") (pinfunction "+") (pintype "input"))
    (pad "8" thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "/One_Fifth_Ref.") (pinfunction "-") (pintype "input"))
    (pad "9" thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/Random") (pinfunction "+") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "/One_Fifth_Ref.") (pinfunction "-") (pintype "input"))
    (pad "11" thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "/Random") (pinfunction "+") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "13" thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R129-Pad2)") (pintype "open_collector"))
    (pad "14" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R142-Pad2)") (pintype "open_collector"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "parts:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 115.7 102.3)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J110" (at 0 -3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/Ref.") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 178.4 91.64 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R131" (at -0.86 -1.65 90 unlocked) (layer "F.SilkS"))
    (fp_text value "470R" (at 2.54 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(D106-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 28 "Net-(R129-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "parts:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 115.3 98.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J111" (at 0 -3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/Random") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 152.7 108.3 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C116" (at 2.15 -2.05 90 unlocked) (layer "F.SilkS"))
    (fp_text value "10uF" (at 2.5 2.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.5 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C116-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 214.3 105.695 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R122" (at 0.95 -1.92 90 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 0.95 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.95 -1.92 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "/Random") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 "Net-(R122-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 173.56 110.4)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R113" (at 2.49 1.7 unlocked) (layer "F.SilkS"))
    (fp_text value "470R" (at 2.54 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(D102-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 "Net-(R110-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 149.75 92.2)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C113" (at -1 -1.75 unlocked) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+4V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 175.24 96.7 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R104" (at 2.64 4.8 unlocked) (layer "F.SilkS"))
    (fp_text value "100k" (at 2.54 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 43 "/Three_Fifths_Ref.") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 "/Four_Fifths_Ref.") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 146.1 80.695 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C103" (at -1.65 1.495 unlocked) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C103-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 179 94.46 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R103" (at 2.74 1.6 90 unlocked) (layer "F.SilkS"))
    (fp_text value "100k" (at 2.54 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 46 "/Ref.") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 42 "/Four_Fifths_Ref.") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92L_Inline" (layer "F.Cu")
    (tedit 5A279A44)
    (at 146.4 76.45 180)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "TO-92L Inline Wide transistor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q101" (at 2.05 2.35 unlocked) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 1.19 2.79) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.19 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 17 "Net-(Q101-Pad2)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 0 180) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(C103-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 124.025 81.3 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J102" (at -1.3 -2.975 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0 4.87 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.27 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(D110-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 124 95.428234 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D103" (at -2.278234 2.1 -270 unlocked) (layer "F.SilkS"))
    (fp_text value "1N4004" (at 1.27 3.639635 -270) (layer "F.Fab") hide)
    (fp_text user "A" (at 4.64 0 -270) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 1.35 0.05 -270 unlocked) (layer "F.Fab"))
    (fp_text user "A" (at 4.64 0 -270) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "+4V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 142.85 114.1 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C109" (at 1.3 1.85 unlocked) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.25) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C109-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 180.46 107)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D105" (at 1.44 -3.5 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Red" (at 1.27 2.96) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(D105-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 208.7 83.8 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R142" (at 4.15 0 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 0.95 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.95 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "/Random") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 31 "Net-(R142-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 139.295 75.9)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R102" (at 0.95 -1.92 unlocked) (layer "F.SilkS"))
    (fp_text value "1k" (at 0.95 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.95 -1.92 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 "Net-(R101-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "Net-(Q101-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "parts:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 209.6 91.4)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J108" (at 0 -3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "F.Cu")
    (tedit 5A02FF81)
    (at 160.54 114.13 180)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q106" (at -1.51 0.58 90 unlocked) (layer "F.SilkS"))
    (fp_text value "2N7000" (at 2.54 2.79 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.54 0 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C116-Pad1)") (pinfunction "S") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "/Sample") (pinfunction "G") (pintype "input"))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(Q106-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 121.3 90.3 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C104" (at 2.85 2 unlocked) (layer "F.SilkS"))
    (fp_text value "10uF" (at 2.5 2.5) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.5 0 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 145.1 114.305 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R133" (at 3.305 0.15 unlocked) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0.95 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.8 0.05 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "+4V") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C107-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 204.4 116.905 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R110" (at 0.855 1.45 90 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 0.95 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.8 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "/Random") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 "Net-(R110-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 150.1 80.6 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R107" (at -0.35 1.45 unlocked) (layer "F.SilkS"))
    (fp_text value "R_Small" (at 0.95 1.92) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1 0.1 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(Q102-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C103-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 133.3 115.705 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R140" (at 4.355 -0.2 90 unlocked) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0.95 1.92 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.95 0 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "+4V") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(C109-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 155 99.9 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U105" (at 0.5 -2.05 90 unlocked) (layer "F.SilkS"))
    (fp_text value "NE555P" (at 3.81 9.95 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 3.81 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C114-Pad1)") (pinfunction "TR") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "/Sample") (pinfunction "Q") (pintype "output"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+4V") (pinfunction "R") (pintype "input"))
    (pad "5" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C112-Pad1)") (pinfunction "CV") (pintype "input"))
    (pad "6" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C114-Pad1)") (pinfunction "THR") (pintype "input"))
    (pad "7" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(R139-Pad1)") (pinfunction "DIS") (pintype "input"))
    (pad "8" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+4V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 207.2 101.825 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D101" (at 4.925 1 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Red" (at 1.27 2.96 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D101-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 174.9 87.26 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D108" (at 1.29 2.8 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Amber" (at 1.27 2.96 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D108-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 136.2 124.2 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U104" (at 0.3 -2.1 90 unlocked) (layer "F.SilkS"))
    (fp_text value "LM358" (at 3.81 9.95 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 3.81 3.81 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(RV101-Pad1)") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R141-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C108-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C109-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "/Ref.") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "/Ref.") (pintype "output"))
    (pad "8" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+4V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 188.2 108.25 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 128.4 102.9 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 118.18233 90.640379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 124.7 117.55 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 177.818529 110.142567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 181.05 75 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 169.45 89.3 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 213.85 89.65 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 180.8 99.5 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 134.55 84.15 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 189.8 87.55 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 121.818529 90.942567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 218.15 93.7 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 137.2 121.5 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 131.818529 123.792567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 179.85 77.75 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 147.9 87.55 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 220 100.8 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 162.18233 92.440379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 150.95 77.75 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 120.85 115.4 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 138.25 118.6 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 148.8 76.7 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 183.7 73.7 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 175.7 110.6 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 117.3 96.9 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 197.85 88.7 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 146.85 88.25 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 178 98.75 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 131.9 122.7 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 220.668529 111.842567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 189.7 79.7 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 202.2 82.2 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 193.2 87.05 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 163.75 94.45 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 116.95 88.7 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 146.95 86.8 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 207.93233 74.590379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 210.768529 121.842567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 149.03233 73.290379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 125 84.4 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 211.28233 84.440379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 172.7 92.45 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 208.968529 110.292567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 145.35 120.45 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 149.75 109.5 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 123.05 118.05 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 125.93233 111.340379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 208 78.15 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 171.8 99.95 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 126.65 102 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 135.68233 82.990379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 132.2 81.85 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 173.25 106.15 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 202.18233 74.340379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:pi-fan" locked (layer "B.Cu")
    (tedit 0)
    (at 194 99.5 180)
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "M102" (at 0 0.5 unlocked) (layer "B.SilkS"))
    (fp_text value "Fan" (at 0 -1 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab"))
    (fp_circle (center -11.9 11.9) (end -10 11.9) (layer "Edge.Cuts") (width 0.12) (fill none))
    (fp_circle (center 11.9 11.9) (end 13.8 11.9) (layer "Edge.Cuts") (width 0.12) (fill none))
    (fp_circle (center 11.9 -11.9) (end 13.8 -11.9) (layer "Edge.Cuts") (width 0.12) (fill none))
    (fp_circle (center -11.9 -11.9) (end -10 -11.9) (layer "Edge.Cuts") (width 0.12) (fill none))
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 206.418529 93.742567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 183.45 111.35 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 163.25 95.95 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 114.6 95.5 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 158.7 94.5 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 210.4 112.05 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 134.6 81.3 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:rocket" (layer "B.Cu")
    (tedit 0)
    (at 185.85 81.1 -90)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "rocket" (at 0 -1 90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 90 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 218.918529 115.692567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 218.5 92.45 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 173.218529 109.092567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 160.268529 99.342567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 215.88233 101.790379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 216.28233 87.640379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 140.368529 122.692567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:rocket" (layer "B.Cu")
    (tedit 0)
    (at 158.95 96.8 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "rocket" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "B.Cu")
    (tedit 5AC8BA0D)
    (at 121.055 100.54 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U103" (at 8.39 0.445 180 unlocked) (layer "B.SilkS"))
    (fp_text value "TLV1117-ADJ" (at 2.54 -2.5 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.64 -0.005 90 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(Q103-Pad3)") (pinfunction "ADJ") (pintype "input"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "+4V") (pinfunction "VO") (pintype "power_out"))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "+5V") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 200.218529 90.792567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 210.73233 79.140379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 143.05 119.4 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 127.28233 95.690379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 186.5 83.35 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 115.9 106.9 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 199.5 118.6 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 210.15 104.95 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 217.068529 88.692567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 209.15 117.1 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 142.5 122.6 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 204.818529 124.092567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 153.25 121.9 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 116.43233 100.540379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 171.75 92.95 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 157.35 104 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 118.98432 105.125343 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 217.6 104.85 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:rocket" (layer "B.Cu")
    (tedit 0)
    (at 183.05 119.85 -90)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "rocket" (at 0 -1 90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 90 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 187.68233 81.740379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 176.05 94.85 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 206.15 117.4 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 183.55 80.9 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 171.6 85.2 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 186.518529 125.292567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 153.65 105.55 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 209.918529 81.392567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 219.218529 104.842567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 212.9 114.85 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:rocket" (layer "B.Cu")
    (tedit 0)
    (at 112.6 107.55 -90)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "rocket" (at 0 -1 90 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 90 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 132.8 78.55 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 173.4 89.2 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 154.2 82.65 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 187.6 121.55 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 212.85 109.6 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 177.55 96.85 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 153.43233 111.990379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 144.9 122.8 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 126.15 78.85 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 161.7 96.2 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 143.518529 121.742567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 155.85 94.6 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 216.418529 93.942567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 175.85 87.85 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 137.218529 85.842567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 148.5 118.1 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 147.75 78.75 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 117.35 94.45 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 155.85 119.9 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 185.375588 121.035645 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 123.45 114.35 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 148.118529 121.892567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 162.05 95.1 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 134.73233 73.890379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 153.15 106.7 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 195.43233 107.890379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 155.15 83.4 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 174.6 79.7 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 212.03233 100.140379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 119.568529 98.642567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 126.5 99.1 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 122.1 111.15 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 217.3 100.2 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 134.15 77.3 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 155.3 116.25 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 133.43233 118.340379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 181.9 77.85 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 161.3 101.8 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 126.018529 119.192567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 161.7 102.95 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 180.7 116.35 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 210.768529 101.842567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 164.25 96.9 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 188.93233 77.640379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 211.65 90.9 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:pi-fan" locked (layer "B.Cu")
    (tedit 0)
    (at 140 100 180)
    (property "Sheetfile" "light_blower.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "M101" (at 0 0.5 unlocked) (layer "B.SilkS"))
    (fp_text value "Fan" (at 0 -1 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab"))
    (fp_circle (center 11.9 11.9) (end 13.8 11.9) (layer "Edge.Cuts") (width 0.12) (fill none))
    (fp_circle (center 11.9 -11.9) (end 13.8 -11.9) (layer "Edge.Cuts") (width 0.12) (fill none))
    (fp_circle (center -11.9 11.9) (end -10 11.9) (layer "Edge.Cuts") (width 0.12) (fill none))
    (fp_circle (center -11.9 -11.9) (end -10 -11.9) (layer "Edge.Cuts") (width 0.12) (fill none))
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 144.98233 82.640379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 215.95 103.65 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 129.85 120.6 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 213.518529 91.542567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 155.168529 108.842567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 137 79.2 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 174.868529 113.042567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 163.868529 97.892567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 215.25 86.55 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 171.5 102.1 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 144.468529 124.592567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 157.45 98.1 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 134.1 80.05 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 139.4 120.55 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 132.45 83.6 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 143.48233 116.590379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 219.768529 101.292567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 119.1 89.75 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 159.35 96.35 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 204.4 77.45 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 153.3 115.6 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 142.5 120.4 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 194.8 86.75 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 122.55 83.6 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 132.08233 75.240379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 177.1 99.75 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 129.95 122.7 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 135.05 122.2 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 143.25 118.25 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:rocket" (layer "B.Cu")
    (tedit 0)
    (at 169.155272 108.633611 -135)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 45 unlocked) (layer "B.SilkS") hide)
    (fp_text value "rocket" (at 0 -1 45 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 45 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 171.95 95.4 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 173 101.95 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 157.718529 123.642567 45)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 225 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 225 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 225 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 174.35 92.2 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 185.7 119 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 175.83432 112.375343 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 127.6 118 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 115.05 96.75 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:little_star" (layer "B.Cu")
    (tedit 0)
    (at 172.7 99.85 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "little_star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (footprint "parts:star" (layer "B.Cu")
    (tedit 0)
    (at 149.88233 103.340379 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 0.5 unlocked) (layer "B.SilkS") hide)
    (fp_text value "star" (at 0 -1 unlocked) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab") hide)
  )
  (gr_circle (center 140 100) (end 167 100) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 140 100) (end 151 100) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_circle (center 194 100) (end 221 100) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_rect (start 214.5 92.7) (end 210.025 103.3) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_circle (center 194 100) (end 204.9 100) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_text "FAN" (at 135.05 84.25) (layer "F.SilkS"))
  (gr_text "POWER\n" (at 125.1 79.35) (layer "F.SilkS"))
  (zone locked (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.18))
    (min_thickness 0.18) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 221.05 127)
        (xy 112.9 127)
        (xy 112.9 72.9)
        (xy 221.05 72.9)
      )
    )
  )
)
