(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 120)
    (zones 0)
    (modules 160)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (user_trace_width 1.016)
    (user_trace_width 1.524)
    (user_trace_width 2.54)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.7366 0.381)
    (user_via 0.8636 0.50038)
    (user_via 0.8636 0.508)
    (uvia_size 0.8)
    (uvia_drill 0.4)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.8)
    (uvia_drill 0.4)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
  )
  (net_class 43V ""
    (clearance 0.1524)
    (trace_width 2.54)
    (via_dia 0.70104)
    (via_drill 0.59944)
    (uvia_dia 0.70104)
    (uvia_drill 0.59944)
    (diff_pair_width 1.016)
    (diff_pair_gap 0.8636)
  )
  (net_class Spindle ""
    (clearance 0.6858)
    (trace_width 1.016)
    (via_dia 0.70104)
    (via_drill 0.59944)
    (uvia_dia 0.70104)
    (uvia_drill 0.59944)
    (diff_pair_width 1.016)
    (diff_pair_gap 0.8636)
  )
  (net_class Stepper ""
    (clearance 0.2286)
    (trace_width 0.6096)
    (via_dia 0.7366)
    (via_drill 0.381)
    (uvia_dia 0.7366)
    (uvia_drill 0.381)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 41.91 39.37)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 1.524) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 29.21 26.67)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 0.508) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 39.37 24.13)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 0.288) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 24.13 39.37)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 24.13 36.83)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 41.91 24.13)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 1.524) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 31.75 36.83)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 29.21 24.13)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 0.508) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 26.67 26.67)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 -0.728) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 39.37 39.37)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 0.288) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 26.67 24.13)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 -0.728) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 39.37 26.67)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 0.288) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 24.13 34.29)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 39.37 36.83)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 0.288) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 41.91 36.83)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 1.524) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 31.75 34.29)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 41.91 26.67)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 1.524) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 24.13 41.91)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 44.45 26.67)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 26.67 21.59)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -6.096 1.05) (layer B.SilkS) hide)
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 31.75 26.67)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 36.83 36.83)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 44.45 34.29)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 41.91 21.59)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 1.524) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 24.13 26.67)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 44.45 21.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 44.45 39.37)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 39.37 34.29)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 0.288) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 24.13 24.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 31.75 21.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 29.21 21.59)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 0.508) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 36.83 24.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 41.91 34.29)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 1.524) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 36.83 26.67)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 39.37 21.59)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 0.288) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 36.83 39.37)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 26.67 39.37)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 -0.728) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 29.21 36.83)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 0.508) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 29.21 34.29)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 0.508) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 26.67 41.91)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 -0.728) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 29.21 39.37)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 0.508) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 29.21 41.91)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 0.508) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 26.67 36.83)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 -0.728) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 31.75 39.37)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 26.67 34.29)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 -0.728) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 31.75 41.91)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 34.29 24.13 270)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 0.288 270) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05 270) (layer B.Fab))
    (fp_text user %R (at 0 0.68 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 34.29 34.29 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0 270) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 44.45 31.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 31.75 31.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 24.13 31.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 34.29 26.67 270)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 1.524 270) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05 270) (layer B.Fab))
    (fp_text user %R (at 0 0.68 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 41.91 31.75)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 1.524) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 36.83 31.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 34.29 29.21 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0 270) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 39.37 31.75)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 0.288) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 34.29 21.59 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0 270) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 34.29 39.37 270)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 1.524 270) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05 270) (layer B.Fab))
    (fp_text user %R (at 0 0.68 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 34.29 41.91 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0 270) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 34.29 36.83 270)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 0.288 270) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05 270) (layer B.Fab))
    (fp_text user %R (at 0 0.68 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 26.67 31.75)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 -0.728) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 29.21 31.75)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 0.508) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 26.67 29.21)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 -0.728) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 39.37 41.91)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 0.288) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 31.75 24.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 24.13 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 44.45 36.83)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 41.91 29.21)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 1.524) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 39.37 29.21)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 0.288) (layer B.SilkS))
    (fp_text value R_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 44.45 24.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 36.83 21.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 36.83 41.91)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 36.83 34.29)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 44.45 41.91)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 24.13 21.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 36.83 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 31.75 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer B.Cu) (tedit 5D3A7A41)
    (at 44.45 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 29.21 29.21)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 0.508) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 41.91 41.91)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 1.524) (layer B.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 -1.05) (layer B.Fab))
    (fp_text user %R (at 0 0.68) (layer B.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 34.29 29.21 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0 90) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 34.29 26.67 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 -0.288 90) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.68 90) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 34.29 21.59 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0 90) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 34.29 24.13 90)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 -1.524 90) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.68 90) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 34.29 41.91 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0 90) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 34.29 39.37 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 -0.288 90) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.68 90) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 34.29 34.29 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0 90) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 34.29 36.83 90)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 -1.524 90) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.68 90) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 39.37 31.75)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 -0.288) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 36.83 31.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41.91 31.75)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 -1.524) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 44.45 31.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 24.13 31.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 31.75 31.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26.67 31.75)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 0.728) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.21 31.75)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 -0.508) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 39.37 34.29)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 -0.288) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26.67 34.29)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 0.728) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 39.37 21.59)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 -0.288) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41.91 34.29)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 -1.524) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.21 34.29)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 -0.508) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41.91 21.59)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 -1.524) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 44.45 39.37)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 31.75 39.37)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 44.45 26.67)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 44.45 34.29)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 31.75 34.29)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 44.45 21.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 36.83 34.29)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 24.13 34.29)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 36.83 21.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 36.83 41.91)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 24.13 41.91)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 36.83 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 44.45 41.91)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 31.75 41.91)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 44.45 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 36.83 39.37)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 24.13 39.37)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 36.83 26.67)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 36.83 36.83)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 24.13 36.83)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 36.83 24.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 44.45 36.83)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 31.75 36.83)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 44.45 24.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 39.37 41.91)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 -0.288) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26.67 41.91)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -6.096 -1.05) (layer F.SilkS) hide)
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 39.37 29.21)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 -0.288) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41.91 41.91)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 -1.524) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.21 41.91)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 -0.508) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41.91 29.21)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 -1.524) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41.91 39.37)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 -1.524) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.21 39.37)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 -0.508) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41.91 26.67)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 -1.524) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 39.37 39.37)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 -0.288) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26.67 39.37)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 0.728) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 39.37 26.67)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 -0.288) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41.91 36.83)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 -1.524) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.21 36.83)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 -0.508) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 41.91 24.13)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -26.924 -1.524) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 39.37 36.83)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 -0.288) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26.67 36.83)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 0.728) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 39.37 24.13)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -23.622 -0.288) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 24.13 21.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 31.75 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 31.75 26.67)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 24.13 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 24.13 26.67)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 24.13 24.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 31.75 21.59)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module TestPoints:TestPoint_0303_0603 (layer F.Cu) (tedit 5D3A7A41)
    (at 31.75 24.13)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference T (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0303_TestPad (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at 0 0) (size 0.95 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.21 29.21)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 -0.508) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.21 26.67)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 -0.508) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26.67 29.21)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 0.728) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26.67 26.67)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 0.728) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.21 21.59)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 -0.508) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26.67 21.59)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 0.728) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 29.21 24.13)
    (descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference REF** (at -14.478 -0.508) (layer F.SilkS))
    (fp_text value LED_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26.67 24.13)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference REF** (at -11.176 0.728) (layer F.SilkS))
    (fp_text value R_0201_0603Metric (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Billy Bogardus 7/25/2019" (at 33.274 20.066 180) (layer B.SilkS))
  (gr_text "0201 Practice Board " (at 34.036 43.434 180) (layer B.SilkS))
  (gr_text "Billy Bogardus 7/25/2019" (at 35.306 43.434) (layer F.SilkS))
  (gr_text "0201 Practice Board " (at 34.544 20.066) (layer F.SilkS))
  (gr_line (start 46.99 19.05) (end 21.59 19.05) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 46.99 44.45) (end 46.99 19.05) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 21.59 44.45) (end 46.99 44.45) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 21.59 19.05) (end 21.59 44.45) (layer Edge.Cuts) (width 0.12))
)
