(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~61~ubuntu18.04.1)
  (general
    (links 41)
    (no_connects 0)
    (area 132.558999 51.740999 160.349001 173.0674)
    (thickness 1.6)
    (drawings 17)
    (tracks 46)
    (zones 0)
    (modules 17)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /B-BY)
  (net 3 /HD-CS)
  (net 4 /G-Y)
  (net 5 /R-RY)
  (net 6 /VD)
  (net 7 /AUDIO)
  (net 8 "Net-(L1-Pad1)")
  (net 9 "Net-(R1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /AUDIO)
    (add_net /B-BY)
    (add_net /G-Y)
    (add_net /HD-CS)
    (add_net /R-RY)
    (add_net /VD)
    (add_net GND)
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(R1-Pad1)")
  )
  (module RCA:RCJ-02 (layer F.Cu) (tedit 5AE60EEB)
    (at 148.4884 146.9644)
    (fp_text reference L1 (at 4.95 4.9) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -4.15 -2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at -5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.7) (layers *.Cu *.Mask)
      (net 8 "Net-(L1-Pad1)"))
  )
  (module Molex_FPC:52852-1472 (layer F.Cu) (tedit 5AE60F8B)
    (at 138.684 95.1484 270)
    (fp_text reference J1 (at 14.986 -0.4064 270) (layer F.SilkS))
    (fp_text value Conn_01x14 (at 6.45 3.5 270) (layer F.Fab))
    (pad "" smd rect (at 16.15 2.35 270) (size 2.1 2.8) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /G-Y))
    (pad 2 smd rect (at 1 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 /B-BY))
    (pad 4 smd rect (at 3 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 4 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /R-RY))
    (pad 6 smd rect (at 5 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 6 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /HD-CS))
    (pad 8 smd rect (at 7 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 8 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /VD))
    (pad 10 smd rect (at 9 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 10 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /AUDIO))
    (pad 12 smd rect (at 11 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 12 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 13 0 270) (size 0.6 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad "" smd rect (at -3.15 2.35 270) (size 2.1 2.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Molex_BNC:73171-1900 (layer F.Cu) (tedit 5AE6029D)
    (at 148.4884 135.0772)
    (fp_text reference VD1 (at 0 6.95) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -6.25) (layer F.Fab))
    (pad 2 thru_hole circle (at -3.43 3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.43 3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.43 -3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.32 2.32) (drill 1.32) (layers *.Cu *.Mask)
      (net 6 /VD))
    (pad 2 thru_hole circle (at -3.43 -3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Molex_BNC:73171-1900 (layer F.Cu) (tedit 5AE6029D)
    (at 148.4884 99.1108)
    (fp_text reference R-RY1 (at 0 6.95) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -6.25) (layer F.Fab))
    (pad 2 thru_hole circle (at -3.43 3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.43 3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.43 -3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.32 2.32) (drill 1.32) (layers *.Cu *.Mask)
      (net 5 /R-RY))
    (pad 2 thru_hole circle (at -3.43 -3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Molex_BNC:73171-1900 (layer F.Cu) (tedit 5AE6029D)
    (at 148.4884 63.1444)
    (fp_text reference GY1 (at 0 6.95) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -6.25) (layer F.Fab))
    (pad 2 thru_hole circle (at -3.43 3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.43 3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.43 -3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.32 2.32) (drill 1.32) (layers *.Cu *.Mask)
      (net 4 /G-Y))
    (pad 2 thru_hole circle (at -3.43 -3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Molex_BNC:73171-1900 (layer F.Cu) (tedit 5AE6029D)
    (at 148.4884 117.094)
    (fp_text reference CS1 (at 0 6.95) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -6.25) (layer F.Fab))
    (pad 2 thru_hole circle (at -3.43 3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.43 3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.43 -3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.32 2.32) (drill 1.32) (layers *.Cu *.Mask)
      (net 3 /HD-CS))
    (pad 2 thru_hole circle (at -3.43 -3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Molex_BNC:73171-1900 (layer F.Cu) (tedit 5AE6029D)
    (at 148.4884 81.1276)
    (fp_text reference B-BY1 (at 0 6.95) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -6.25) (layer F.Fab))
    (pad 2 thru_hole circle (at -3.43 3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.43 3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.43 -3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.32 2.32) (drill 1.32) (layers *.Cu *.Mask)
      (net 2 /B-BY))
    (pad 2 thru_hole circle (at -3.43 -3.43) (size 3.16 3.16) (drill 2.16) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AE61870)
    (at 156.6672 55.6768)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J2 (at -4.6228 0) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AE6186B)
    (at 140.4112 55.6768)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J3 (at 4.6736 0) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AE6187A)
    (at 140.462 167.7924)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J4 (at 4.4704 0) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AE6187C)
    (at 156.6164 167.7924)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J5 (at -4.2672 0 180) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5AE60FC8)
    (at 156.6164 108.1532)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J6 (at 1.8796 4.318) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 140.4112 126.0856)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference J7 (at 0 -4.2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module RCA:RCJ-02 (layer F.Cu) (tedit 5AE60EEB)
    (at 148.4884 158.9532)
    (fp_text reference R1 (at 4.95 4.9) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -4.15 -2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at -5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.7) (layers *.Cu *.Mask)
      (net 9 "Net-(R1-Pad1)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 141.3256 141.2494 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 20K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 /AUDIO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 148.3614 142.875 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 475R (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 /AUDIO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 148.3614 154.6606 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 475R (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 /AUDIO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 136.4488 51.816) (end 136.4488 90.0176) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.274 51.816) (end 136.4488 51.816) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.274 171.5516) (end 160.274 51.816) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.2232 171.5516) (end 160.274 171.5516) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.8044 171.5516) (end 160.2232 171.5516) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.8044 113.284) (end 136.8044 171.5516) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "JVC IF-C01COMG Clone BNC Input Rev. B\n2018 Martin Hejnfelt (martin@hejnfelt.com)" (at 140.208 87.884 90) (layer B.SilkS))
  (gr_text RIGHT (at 157.48 160.6296 90) (layer F.SilkS))
  (gr_text LEFT (at 157.3784 148.4884 90) (layer F.SilkS))
  (gr_text VD (at 156.4132 135.0264 90) (layer F.SilkS))
  (gr_text HD/CS (at 156.3624 117.094 90) (layer F.SilkS))
  (gr_text R/R-Y (at 156.1084 98.7552 90) (layer F.SilkS))
  (gr_text B/B-Y (at 156.0068 81.4324 90) (layer F.SilkS))
  (gr_text G/Y (at 156.21 63.754 90) (layer F.SilkS))
  (gr_line (start 132.842 90.0176) (end 132.842 113.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.4488 90.0176) (end 132.842 90.0176) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.8044 113.284) (end 132.842 113.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.1216 171.3992) (xy 136.9568 171.3992) (xy 136.9568 113.1316) (xy 132.9944 113.1316) (xy 132.9944 90.17)
        (xy 136.6012 90.17) (xy 136.6012 51.9684) (xy 160.1216 51.9684)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.1216 171.3992) (xy 136.9568 171.3992) (xy 136.9568 113.1316) (xy 132.9944 113.1316) (xy 132.9944 90.17)
        (xy 136.6012 90.17) (xy 136.6012 51.9684) (xy 160.1216 51.9684)
      )
    )
  )
)
