(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 6)
    (no_connects 0)
    (area 36.84236 88.75 77.250001 123.41596)
    (thickness 1.6)
    (drawings 22)
    (tracks 16)
    (zones 0)
    (modules 6)
    (nets 5)
  )
  (page A4)
  (title_block
    (title "Micro USB Battery Power Supply")
    (date 2018-03-06)
    (rev v01)
    (company "Marston Air & Space Administration")
    (comment 1 "Designer: Steve Hyde")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 5v)
  (net 3 Drain)
  (net 4 Source)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5v)
    (add_net Drain)
    (add_net GND)
    (add_net Source)
  )
  (module Connectors_Mini-Universal:MiniUniversalMate-N-LokSocket_2PinHorizontal (layer F.Cu) (tedit 5AB6F368)
    (at 53.75 104.5)
    (descr "Mini Universal Mate-N-Lok Socket, 2 Pin, Horizontal,")
    (tags "Mini Universal Mate-N-Lok Socket, 2 Pin, Horizontal,")
    (fp_text reference J1 (at 0 -3) (layer F.SilkS) hide)
    (fp_text value Mini-Universal_MATE-N-LOK_Right_Angle_2 (at -0.16002 17.84096) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.0701 0 90) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 0 7.3406) (size 4.0005 4.0005) (drill 4.0005) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.0701 0.01016 90) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.Mask)
      (net 3 Drain))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5AB6EDB5)
    (at 60 92.5)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference U1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value BoostBuck (at 3 2 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 Source))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 5v))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 5AB6ECEA)
    (at 72.75 103.25 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 12.49 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 5.08 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 5v))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SuperSOT-3 (layer F.Cu) (tedit 5AB6F225)
    (at 52.5 98.25 180)
    (descr "3-pin SuperSOT package https://www.fairchildsemi.com/package-drawings/MA/MA03B.pdf")
    (tags "SuperSOT-3 SSOT-3")
    (attr smd)
    (fp_text reference Q1 (at 0 -2.35 180) (layer F.SilkS) hide)
    (fp_text value Q_PMOS_GSD (at 0 2.4 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.4 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.1 0.95 180) (size 1.4 1) (layers F.Cu F.Paste F.Mask)
      (net 4 Source))
    (pad 3 smd rect (at 1.1 0 180) (size 1.4 1) (layers F.Cu F.Paste F.Mask)
      (net 3 Drain))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SuperSOT-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5AB9888B)
    (at 49.5 92.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference 3mm (at 3 0 90) (layer F.SilkS))
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5AB98899)
    (at 73.5 92.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference 3mm (at 0 3) (layer F.SilkS))
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text "Marston Air & Space Agency\nReward If Found\n07986877951" (at 64.25 109.5) (layer B.SilkS))
  (gr_text "Made In Marston - Sent Into Space" (at 61.5 118) (layer B.SilkS))
  (gr_text "Reward If Found 07986877951" (at 75.5 109 270) (layer F.SilkS))
  (gr_text "Mini Mate-N-Lok" (at 53.75 108) (layer F.SilkS))
  (gr_text G (at 55.25 99.25) (layer F.SilkS))
  (gr_text S (at 55.25 97.25) (layer F.SilkS))
  (gr_text D (at 49.75 97.25) (layer F.SilkS))
  (gr_text FDN304PZ (at 48.25 100 90) (layer F.SilkS))
  (gr_line (start 76.5 119.5) (end 46.5 119.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.5 89.5) (end 76.5 119.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 46.5 89.5) (end 76.5 89.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "5v GND In\nBuck/Boost\n" (at 63.25 95 90) (layer F.SilkS))
  (gr_text "5v  Micro USB  GND" (at 68 106) (layer F.SilkS))
  (gr_text "MASA Micro USB Battery Power v02" (at 61.5 116) (layer B.SilkS))
  (gr_line (start 46.5 89.5) (end 46.5 119.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 120) (xy 46 120) (xy 46 89) (xy 77 89)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.25 120.25) (xy 45.75 120.25) (xy 45.75 88.75) (xy 77.25 88.75)
      )
    )
  )
)
