(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 6)
    (no_connects 6)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 18)
    (tracks 24)
    (zones 0)
    (modules 2)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VCC)
  (net 2 /SWDIO)
  (net 3 /RESET)
  (net 4 /SWCLK)
  (net 5 /GND)
  (net 6 /SWO)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GND)
    (add_net /RESET)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /SWO)
    (add_net /VCC)
  )
  (module Socket_Strips:Socket_Strip_Angled_1x06 (layer F.Cu) (tedit 0)
    (at 121.92 108.712)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 12.7 9.017) (layer F.SilkS))
    (fp_text value PPPC061LGBN-RC (at 0 -2.75) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /VCC))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /SWDIO))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SWCLK))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SWO))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_1x06.wrl
      (at (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x03 (layer F.Cu) (tedit 54E9F9C7)
    (at 125.73 95.25)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 7.747 3.302) (layer F.SilkS))
    (fp_text value 75867-131LF (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /SWDIO))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SWCLK))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /GND))
    (pad 6 thru_hole oval (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SWO))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x03.wrl
      (at (xyz 0.1 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_line (start 123.698 93.472) (end 128.27 93.472) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 95.25) (end 123.698 93.472) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 100.33) (end 121.92 95.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.38 102.87) (end 121.92 100.33) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.38 118.999) (end 119.38 102.87) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 118.999) (end 119.38 118.999) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 102.87) (end 137.16 118.999) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 100.33) (end 137.16 102.87) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 95.25) (end 134.62 100.33) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.842 93.472) (end 134.62 95.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.588 93.472) (end 132.842 93.472) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 93.472) (end 132.588 93.472) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 134.62 105.537 90) (layer F.SilkS))
  (gr_text RESET (at 132.207 104.775 90) (layer F.SilkS))
  (gr_text SWO (at 129.54 105.537 90) (layer F.SilkS))
  (gr_text "SWCLK\n" (at 127 104.648 90) (layer F.SilkS))
  (gr_text SWDIO (at 124.46 104.775 90) (layer F.SilkS))
  (gr_text VCC (at 122.047 105.537 90) (layer F.SilkS))
)
