(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 221)
    (zones 0)
    (modules 26)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1.27)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (user_trace_width 2.032)
    (user_trace_width 2.54)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.397 0.7112)
    (user_via 1.778 0.889)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.57 1.57)
    (pad_drill 1.57)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 VCC)
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 /TCK)
  (net 7 /TDO)
  (net 8 /TMS)
  (net 9 /TDI)
  (net 10 +BATT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net /TCK)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 121.92 99.06 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -2.86 0) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 114.3 125.73 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.048 0 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 129.56 111.76 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 3.175 0) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 134.874 115.57 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 1.27 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 147.32 129.225 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 1.905 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.25 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 116.86 132.08)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 3.048 0) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 129.54 145.415)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -3.302 0) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MAX7128_JTAG_Tester:284-5756-00-1102 (layer F.Cu) (tedit 5E28DA85)
    (at 124.46 121.92 90)
    (descr "3M Textool PLCC84 Test Socket")
    (tags PLCC)
    (fp_text reference U2 (at 0 0) (layer F.SilkS))
    (fp_text value EPM7128SLC84-10 (at 0 3.81 90) (layer F.Fab))
    (fp_text user LATCH (at -27 0 180) (layer F.Fab) hide)
    (fp_text user HINGE (at 23 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0 90) (size 6.35 6.35) (drill 6.35) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -17.78 17.78 90) (size 1.57 1.57) (drill 1.57) (layers *.Cu *.Mask)
      (clearance 2.032))
    (pad "" np_thru_hole circle (at 17.78 -17.78 90) (size 1.57 1.57) (drill 1.57) (layers *.Cu *.Mask)
      (clearance 2.032))
    (pad "" np_thru_hole circle (at -17.78 -17.78 90) (size 1.57 1.57) (drill 1.57) (layers *.Cu *.Mask)
      (clearance 2.032))
    (pad "" np_thru_hole circle (at 17.78 17.78 90) (size 1.57 1.57) (drill 1.57) (layers *.Cu *.Mask)
      (clearance 2.032))
    (pad 1 thru_hole rect (at -19.43 0 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -14.35 1.27 90) (size 2.1 1.8) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at -19.43 2.54 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 4 thru_hole oval (at -14.35 3.81 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at -19.43 5.08 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -14.35 6.35 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at -19.43 7.62 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at -14.35 8.89 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at -19.43 10.16 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at -14.35 11.43 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at -19.43 12.7 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at -12.7 14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at -11.43 19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 14 thru_hole oval (at -10.16 14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 9 /TDI))
    (pad 15 thru_hole oval (at -8.83 19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at -7.62 14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at -6.35 19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at -5.08 14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at -3.81 19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 20 thru_hole oval (at -2.54 14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at -1.27 19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 0 14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 1.27 19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 8 /TMS))
    (pad 24 thru_hole oval (at 2.54 14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 3.81 19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 26 thru_hole oval (at 5.08 14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 27 thru_hole oval (at 6.35 19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at 7.62 14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 29 thru_hole oval (at 8.83 19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at 10.16 14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 31 thru_hole oval (at 11.43 19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at 12.7 14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 33 thru_hole oval (at 19.43 12.7 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 34 thru_hole oval (at 14.35 11.43 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 35 thru_hole oval (at 19.43 10.16 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at 14.35 8.89 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 19.43 7.62 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 14.35 6.35 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 39 thru_hole oval (at 19.43 5.08 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 40 thru_hole oval (at 14.35 3.81 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 41 thru_hole oval (at 19.43 2.54 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 42 thru_hole oval (at 14.35 1.27 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 43 thru_hole oval (at 19.43 0 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 44 thru_hole oval (at 14.35 -1.27 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 45 thru_hole oval (at 19.43 -2.54 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 46 thru_hole oval (at 14.35 -3.81 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 47 thru_hole oval (at 19.43 -5.08 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 48 thru_hole oval (at 14.35 -6.35 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 49 thru_hole oval (at 19.43 -7.62 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 50 thru_hole oval (at 14.35 -8.89 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 51 thru_hole oval (at 19.43 -10.16 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 52 thru_hole oval (at 14.35 -11.43 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 53 thru_hole oval (at 19.43 -12.7 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 54 thru_hole oval (at 12.7 -14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 55 thru_hole oval (at 11.43 -19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 56 thru_hole oval (at 10.16 -14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 57 thru_hole oval (at 8.89 -19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 58 thru_hole oval (at 7.62 -14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 59 thru_hole oval (at 6.35 -19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 60 thru_hole oval (at 5.08 -14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 61 thru_hole oval (at 3.81 -19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 62 thru_hole oval (at 2.54 -14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 6 /TCK))
    (pad 63 thru_hole oval (at 1.27 -19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 64 thru_hole oval (at 0 -14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 65 thru_hole oval (at -1.27 -19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 66 thru_hole oval (at -2.54 -14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 67 thru_hole oval (at -3.81 -19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 68 thru_hole oval (at -5.08 -14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 69 thru_hole oval (at -6.35 -19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 70 thru_hole oval (at -7.62 -14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 71 thru_hole oval (at -8.89 -19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /TDO))
    (pad 72 thru_hole oval (at -10.16 -14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 73 thru_hole oval (at -11.43 -19.43 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 74 thru_hole oval (at -12.7 -14.35 90) (size 1.75 2.2) (drill 1) (layers *.Cu *.Mask))
    (pad 75 thru_hole oval (at -19.43 -12.7 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 76 thru_hole oval (at -14.35 -11.43 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 77 thru_hole oval (at -19.43 -10.16 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 78 thru_hole oval (at -14.35 -8.89 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 79 thru_hole oval (at -19.43 -7.62 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 80 thru_hole oval (at -14.35 -6.35 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 81 thru_hole oval (at -19.43 -5.08 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 82 thru_hole oval (at -14.35 -3.81 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 83 thru_hole oval (at -19.43 -2.54 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (pad 84 thru_hole oval (at -14.35 -1.27 90) (size 2.2 1.75) (drill 1) (layers *.Cu *.Mask))
    (model Sockets.3dshapes/PLCC84.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 80.01 134.62)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference TP6 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value VBAT (at -2.54 1.27 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +BATT))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +BATT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MAX7128_JTAG_Tester:TE_2-1761606-3 (layer F.Cu) (tedit 5E28B9CD)
    (at 85.09 99.695 270)
    (fp_text reference J2 (at -3.175 -1.27 180) (layer F.SilkS))
    (fp_text value JTAG (at 1.27 -2.54 270) (layer F.SilkS) hide)
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 10 thru_hole circle (at 10.16 -2.54 270) (size 1.778 1.778) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole circle (at 10.16 0 270) (size 1.778 1.778) (drill 0.89) (layers *.Cu *.Mask)
      (net 9 /TDI))
    (pad 8 thru_hole circle (at 7.62 -2.54 270) (size 1.778 1.778) (drill 0.89) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.778 1.778) (drill 0.89) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 5.08 -2.54 270) (size 1.778 1.778) (drill 0.89) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.778 1.778) (drill 0.89) (layers *.Cu *.Mask)
      (net 8 /TMS))
    (pad 4 thru_hole circle (at 2.54 -2.54 270) (size 1.778 1.778) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.778 1.778) (drill 0.89) (layers *.Cu *.Mask)
      (net 7 /TDO))
    (pad 2 thru_hole circle (at 0 -2.54 270) (size 1.778 1.778) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.778 1.778) (drill 0.89) (layers *.Cu *.Mask)
      (net 6 /TCK))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 80.01 141.605)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference TP5 (at 0 5.08) (layer F.SilkS) hide)
    (fp_text value GND (at -2.54 1.143 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Big (layer B.Cu) (tedit 5E28B73C)
    (at 82.55 109.855)
    (descr "Mesurement Point, Square, SMD Pad,  3mm x 3mm,")
    (tags "Mesurement Point Square SMD Pad 3x3mm")
    (attr virtual)
    (fp_text reference TP4 (at -2.54 -0.635) (layer B.SilkS))
    (fp_text value TDI (at -2.54 0.635) (layer B.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.032 2.032) (layers B.Cu B.Mask)
      (net 9 /TDI))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Big (layer B.Cu) (tedit 5E28B737)
    (at 82.55 104.775)
    (descr "Mesurement Point, Square, SMD Pad,  3mm x 3mm,")
    (tags "Mesurement Point Square SMD Pad 3x3mm")
    (attr virtual)
    (fp_text reference TP3 (at -2.54 0) (layer B.SilkS))
    (fp_text value TMS (at -2.54 1.27) (layer B.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.032 2.032) (layers B.Cu B.Mask)
      (net 8 /TMS))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Big (layer B.Cu) (tedit 5E28B730)
    (at 82.55 102.235)
    (descr "Mesurement Point, Square, SMD Pad,  3mm x 3mm,")
    (tags "Mesurement Point Square SMD Pad 3x3mm")
    (attr virtual)
    (fp_text reference TP2 (at -2.54 -0.635) (layer B.SilkS))
    (fp_text value TDO (at -2.54 0.635) (layer B.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.032 2.032) (layers B.Cu B.Mask)
      (net 7 /TDO))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Big (layer B.Cu) (tedit 5E28B727)
    (at 82.55 99.695)
    (descr "Mesurement Point, Square, SMD Pad,  3mm x 3mm,")
    (tags "Mesurement Point Square SMD Pad 3x3mm")
    (attr virtual)
    (fp_text reference TP1 (at -2.54 -1.27) (layer B.SilkS))
    (fp_text value TCK (at -2.54 0) (layer B.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.032 2.032) (layers B.Cu B.Mask)
      (net 6 /TCK))
  )
  (module TO_SOT_Packages_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 58CE4E7E)
    (at 85.725 129.54 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -4.318 180) (layer F.SilkS))
    (fp_text value AP1117-50 (at 0.914 0.24 270) (layer F.Fab))
    (fp_text user %R (at -0.61 0 90) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 93.345 99.775 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 2.921 0) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /TCK))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 93.345 109.935 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.001 0 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /TDI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 95.25 102.155 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -2.921 0) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /TDO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 95.25 107.315 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.001 0) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /TMS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 92.71 117.475)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.001 0 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 80.01 120.65 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 0 -3.048 90) (layer F.SilkS) hide)
    (fp_text value CURRENT (at 2.54 1.016 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Barrel_Jack_CUI_PJ-102AH (layer F.Cu) (tedit 59BC552D)
    (at 89.535 138.43)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (fp_text reference J1 (at 0.127 11.176 90) (layer F.SilkS))
    (fp_text value "DC INPUT" (at -5.5 6.2 90) (layer F.Fab))
    (fp_text user %R (at 0 6.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 10 +BATT))
    (pad 2 thru_hole circle (at 0 6) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.7 3) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Barrel_Jack_CUI_PJ-102AH.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 595FCA25)
    (at 86.44 117.475 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D2 (at 2.841 0 270) (layer F.SilkS))
    (fp_text value POWER (at 0 1.27) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 93.345 130.175 270)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D1 (at -0.127 -2.667 90) (layer F.SilkS))
    (fp_text value GF1A (at 3.048 2.6 90) (layer F.Fab))
    (fp_text user %R (at -3.556 2.54 90) (layer F.Fab))
    (pad 1 smd rect (at -2.5 0 270) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2.5 0 270) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 10 +BATT))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_6.3x4.5 (layer F.Cu) (tedit 58AA8B18)
    (at 89.535 121.92)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x4.5")
    (attr smd)
    (fp_text reference C1 (at -4.191 -2.413 270) (layer F.SilkS))
    (fp_text value 47u (at 0 -1.016 90) (layer F.Fab))
    (fp_text user + (at -1.73 -0.08) (layer F.Fab))
    (fp_text user + (at -4.28 2.96) (layer F.SilkS))
    (fp_text user %R (at 0 2.032 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x4.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text "PIN #1" (at 80.01 104.775 270) (layer F.SilkS))
  (gr_text "PLCC PIN #1" (at 111.76 150.495) (layer F.SilkS))
  (gr_text "USB BLASTER" (at 77.47 104.775 270) (layer F.SilkS))
  (gr_text "TomCircuit \nJAN-2020" (at 87.63 149.225) (layer B.SilkS))
  (gr_text "EPM7128S\nEPM7160S\nJTAG TESTER" (at 87.63 127.635) (layer B.SilkS))
  (gr_line (start 76.2 93.98) (end 76.2 152.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.4 93.98) (end 76.2 93.98) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.4 152.4) (end 152.4 93.98) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.2 152.4) (end 152.4 152.4) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.33 134.62) (xy 102.235 132.715) (xy 102.235 102.87) (xy 104.775 100.33) (xy 125.73 100.33)
        (xy 135.89 100.33) (xy 147.32 100.33) (xy 147.32 143.51) (xy 123.698 143.51) (xy 121.285 145.415)
        (xy 100.33 145.415)
      )
    )
  )
)
