(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 57)
    (no_connects 1)
    (area 111.584761 81.78057 213.87543 152.729001)
    (thickness 1.6002)
    (drawings 39)
    (tracks 132)
    (zones 0)
    (modules 34)
    (nets 81)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /RD)
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad9)")
  (net 8 "Net-(J1-Pad10)")
  (net 9 "Net-(J1-Pad11)")
  (net 10 "Net-(J1-Pad12)")
  (net 11 "Net-(J1-Pad13)")
  (net 12 "Net-(J1-Pad14)")
  (net 13 "Net-(J1-Pad15)")
  (net 14 "Net-(J1-Pad16)")
  (net 15 "Net-(J1-Pad17)")
  (net 16 "Net-(J1-Pad18)")
  (net 17 +3V3)
  (net 18 /SPI_CLK)
  (net 19 /SPI_MISO)
  (net 20 "Net-(J2-Pad7)")
  (net 21 /SPI_MOSI)
  (net 22 "Net-(J2-Pad9)")
  (net 23 /CS)
  (net 24 "Net-(J2-Pad11)")
  (net 25 /RST)
  (net 26 "Net-(J2-Pad13)")
  (net 27 /SPI_DC)
  (net 28 "Net-(J2-Pad15)")
  (net 29 "Net-(J2-Pad16)")
  (net 30 "Net-(J2-Pad17)")
  (net 31 "Net-(J2-Pad18)")
  (net 32 "Net-(J2-Pad19)")
  (net 33 "Net-(J2-Pad20)")
  (net 34 "Net-(J2-Pad21)")
  (net 35 "Net-(J2-Pad22)")
  (net 36 VCC)
  (net 37 /R1IN)
  (net 38 /T1OUT)
  (net 39 /R1OUT)
  (net 40 /T1IN)
  (net 41 /SW_UP)
  (net 42 /MCU_LED)
  (net 43 /SW_DOWN)
  (net 44 "Net-(J10-Pad4)")
  (net 45 "Net-(J10-Pad6)")
  (net 46 "Net-(J10-Pad25)")
  (net 47 "Net-(J10-Pad26)")
  (net 48 "Net-(J10-Pad27)")
  (net 49 "Net-(J10-Pad28)")
  (net 50 "Net-(J10-Pad29)")
  (net 51 "Net-(J10-Pad30)")
  (net 52 "Net-(J10-Pad7)")
  (net 53 "Net-(J10-Pad8)")
  (net 54 "Net-(J10-Pad32)")
  (net 55 "Net-(J10-Pad9)")
  (net 56 "Net-(J10-Pad33)")
  (net 57 "Net-(J10-Pad10)")
  (net 58 "Net-(J10-Pad11)")
  (net 59 "Net-(J10-Pad35)")
  (net 60 "Net-(J10-Pad12)")
  (net 61 "Net-(J10-Pad13)")
  (net 62 "Net-(J10-Pad14)")
  (net 63 "Net-(J10-Pad38)")
  (net 64 "Net-(J10-Pad39)")
  (net 65 "Net-(J10-Pad16)")
  (net 66 "Net-(J10-Pad40)")
  (net 67 "Net-(J10-Pad17)")
  (net 68 "Net-(J10-Pad41)")
  (net 69 "Net-(J10-Pad18)")
  (net 70 "Net-(J10-Pad19)")
  (net 71 "Net-(J10-Pad21)")
  (net 72 "Net-(J10-Pad22)")
  (net 73 "Net-(J10-Pad23)")
  (net 74 "Net-(J10-Pad47)")
  (net 75 "Net-(J10-Pad24)")
  (net 76 "Net-(D1-Pad2)")
  (net 77 "Net-(J5-Pad2)")
  (net 78 "Net-(J5-Pad4)")
  (net 79 "Net-(J5-Pad8)")
  (net 80 "Net-(J5-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CS)
    (add_net /MCU_LED)
    (add_net /R1IN)
    (add_net /R1OUT)
    (add_net /RD)
    (add_net /RST)
    (add_net /SPI_CLK)
    (add_net /SPI_DC)
    (add_net /SPI_MISO)
    (add_net /SPI_MOSI)
    (add_net /SW_DOWN)
    (add_net /SW_UP)
    (add_net /T1IN)
    (add_net /T1OUT)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J10-Pad10)")
    (add_net "Net-(J10-Pad11)")
    (add_net "Net-(J10-Pad12)")
    (add_net "Net-(J10-Pad13)")
    (add_net "Net-(J10-Pad14)")
    (add_net "Net-(J10-Pad16)")
    (add_net "Net-(J10-Pad17)")
    (add_net "Net-(J10-Pad18)")
    (add_net "Net-(J10-Pad19)")
    (add_net "Net-(J10-Pad21)")
    (add_net "Net-(J10-Pad22)")
    (add_net "Net-(J10-Pad23)")
    (add_net "Net-(J10-Pad24)")
    (add_net "Net-(J10-Pad25)")
    (add_net "Net-(J10-Pad26)")
    (add_net "Net-(J10-Pad27)")
    (add_net "Net-(J10-Pad28)")
    (add_net "Net-(J10-Pad29)")
    (add_net "Net-(J10-Pad30)")
    (add_net "Net-(J10-Pad32)")
    (add_net "Net-(J10-Pad33)")
    (add_net "Net-(J10-Pad35)")
    (add_net "Net-(J10-Pad38)")
    (add_net "Net-(J10-Pad39)")
    (add_net "Net-(J10-Pad4)")
    (add_net "Net-(J10-Pad40)")
    (add_net "Net-(J10-Pad41)")
    (add_net "Net-(J10-Pad47)")
    (add_net "Net-(J10-Pad6)")
    (add_net "Net-(J10-Pad7)")
    (add_net "Net-(J10-Pad8)")
    (add_net "Net-(J10-Pad9)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad8)")
  )
  (net_class Power ""
    (clearance 0.15)
    (trace_width 0.5)
    (via_dia 0.7)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net VCC)
  )
  (module Terminal_Blocks:TerminalBlock_Altech_AK300-2_P5.00mm (layer F.Cu) (tedit 5A89CD8C)
    (at 170.688 143.002 180)
    (descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
    (tags "Altech AK300 terminal block pitch 5.0mm")
    (fp_text reference J3 (at -1.92 -6.99 180) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_01x02 (at 2.78 7.75 180) (layer F.Fab))
    (fp_text user %R (at 2.5 -2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 36 VCC))
    (pad 2 thru_hole oval (at 5 0 180) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_Altech_AK300-2_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Altech_AK300-3_P5.00mm (layer F.Cu) (tedit 5A89CD58)
    (at 149.86 143.002 180)
    (descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
    (tags "Altech AK300 terminal block pitch 5.0mm")
    (fp_text reference J4 (at 5 -7.1 180) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_01x03 (at 4.95 7.3 180) (layer F.Fab))
    (fp_text user %R (at 5 -2 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5 0 180) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 37 /R1IN))
    (pad 3 thru_hole oval (at 10 0 180) (size 1.98 3.96) (drill 1.32) (layers *.Cu *.Mask)
      (net 38 /T1OUT))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_Altech_AK300-3_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x10_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 119.38 124.46)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x10_Female (at 0 25.19) (layer F.Fab))
    (fp_text user %R (at 0 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /T1OUT))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /R1IN))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(J5-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 +3V3))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /T1IN))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(J5-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /R1OUT))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(J5-Pad10)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x10_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 167.64 92.202)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Conn_02x10_Odd_Even (at 1.27 25.19) (layer F.Fab))
    (fp_text user %R (at 1.27 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 +3V3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x11_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 127 92.202)
    (descr "Through hole straight pin header, 2x11, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x11 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Conn_02x11_Odd_Even (at 1.27 27.73) (layer F.Fab))
    (fp_text user %R (at 1.27 12.7 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 +3V3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /SPI_CLK))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /RD))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /SPI_MISO))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /SPI_MOSI))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /CS))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /RST))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /SPI_DC))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad22)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x11_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:GS3 (layer B.Cu) (tedit 58613494)
    (at 119.38 92.202 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J6 (at -1.7 0 360) (layer B.SilkS))
    (fp_text value GS3 (at 1.8 0 360) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers B.Cu B.Mask)
      (net 44 "Net-(J10-Pad4)"))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers B.Cu B.Mask)
      (net 17 +3V3))
    (pad 3 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers B.Cu B.Mask)
      (net 17 +3V3))
  )
  (module Connect:GS3 (layer B.Cu) (tedit 58613494)
    (at 119.38 99.822 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J7 (at -1.7 0 360) (layer B.SilkS))
    (fp_text value GS3 (at 1.8 0 360) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers B.Cu B.Mask)
      (net 2 /RD))
    (pad 3 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers B.Cu B.Mask)
      (net 45 "Net-(J10-Pad6)"))
  )
  (module Housings_DIP:DIP-48_W15.24mm_LongPads (layer F.Cu) (tedit 59C78D6C)
    (at 193.294 146.812 180)
    (descr "48-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil LongPads")
    (fp_text reference J10 (at 7.62 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_02x24_Counter_Clockwise (at 7.62 60.75 180) (layer F.Fab))
    (fp_text user %R (at 7.62 29.21 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole oval (at 15.24 58.42 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(J10-Pad25)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /R1OUT))
    (pad 26 thru_hole oval (at 15.24 55.88 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(J10-Pad26)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /T1IN))
    (pad 27 thru_hole oval (at 15.24 53.34 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(J10-Pad27)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(J10-Pad4)"))
    (pad 28 thru_hole oval (at 15.24 50.8 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(J10-Pad28)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /MCU_LED))
    (pad 29 thru_hole oval (at 15.24 48.26 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(J10-Pad29)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(J10-Pad6)"))
    (pad 30 thru_hole oval (at 15.24 45.72 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(J10-Pad30)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(J10-Pad7)"))
    (pad 31 thru_hole oval (at 15.24 43.18 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /SPI_MISO))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(J10-Pad8)"))
    (pad 32 thru_hole oval (at 15.24 40.64 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(J10-Pad32)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(J10-Pad9)"))
    (pad 33 thru_hole oval (at 15.24 38.1 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(J10-Pad33)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(J10-Pad10)"))
    (pad 34 thru_hole oval (at 15.24 35.56 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(J10-Pad11)"))
    (pad 35 thru_hole oval (at 15.24 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(J10-Pad35)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(J10-Pad12)"))
    (pad 36 thru_hole oval (at 15.24 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /SPI_CLK))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(J10-Pad13)"))
    (pad 37 thru_hole oval (at 15.24 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /CS))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(J10-Pad14)"))
    (pad 38 thru_hole oval (at 15.24 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(J10-Pad38)"))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 +3V3))
    (pad 39 thru_hole oval (at 15.24 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(J10-Pad39)"))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(J10-Pad16)"))
    (pad 40 thru_hole oval (at 15.24 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(J10-Pad40)"))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(J10-Pad17)"))
    (pad 41 thru_hole oval (at 15.24 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "Net-(J10-Pad41)"))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(J10-Pad18)"))
    (pad 42 thru_hole oval (at 15.24 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /SPI_DC))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(J10-Pad19)"))
    (pad 43 thru_hole oval (at 15.24 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /RST))
    (pad 20 thru_hole oval (at 0 48.26 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /SPI_MOSI))
    (pad 44 thru_hole oval (at 15.24 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /SW_DOWN))
    (pad 21 thru_hole oval (at 0 50.8 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(J10-Pad21)"))
    (pad 45 thru_hole oval (at 15.24 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /SW_UP))
    (pad 22 thru_hole oval (at 0 53.34 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(J10-Pad22)"))
    (pad 46 thru_hole oval (at 15.24 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 +3V3))
    (pad 23 thru_hole oval (at 0 55.88 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(J10-Pad23)"))
    (pad 47 thru_hole oval (at 15.24 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(J10-Pad47)"))
    (pad 24 thru_hole oval (at 0 58.42 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(J10-Pad24)"))
    (pad 48 thru_hole oval (at 15.24 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-48_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:LGSwitch_SPST (layer F.Cu) (tedit 5A7F9A49)
    (at 137.922 128.016 90)
    (fp_text reference J8 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 /SW_UP))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module custom:LGSwitch_SPST (layer F.Cu) (tedit 5A7F9A49)
    (at 150.114 128.016 90)
    (fp_text reference J9 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 /SW_DOWN))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5A8082FD)
    (at 197.104 98.552 90)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 1.016 2.032 90) (layer B.SilkS))
    (fp_text value Measurement_Point_Round-SMD-Pad_Small (at 0 -2 90) (layer B.Fab))
    (pad 1 smd circle (at 0 0 90) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 /SPI_MOSI))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5A808303)
    (at 197.104 101.092 90)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -0.762 2.032 90) (layer B.SilkS))
    (fp_text value Measurement_Point_Round-SMD-Pad_Small (at 0 -2 90) (layer B.Fab))
    (pad 1 smd circle (at 0 0 90) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 /SPI_MISO))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 5A808300)
    (at 197.104 103.632)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference GND (at 2.032 2.286 270) (layer B.SilkS))
    (fp_text value Measurement_Point_Round-SMD-Pad_Small (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 182.88 129.032)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 181.864 99.06)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 173.99 144.272)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 188.214 143.002)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 122.682 92.202)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 122.682 96.012)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 130.048 121.412)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 173.736 132.08)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 142.494 140.97)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 120.65 105.41)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 125.476 138.176)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 125.476 140.97)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 188.214 137.414)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 145.542 96.012)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module custom:VIA-0.027 (layer F.Cu) (tedit 5A80FDD6)
    (at 122.682 98.298)
    (tags via)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 168.91 126.238)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.25) (layer F.SilkS))
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Mask)
      (net 76 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 172.974 126.238 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value R (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 42 /MCU_LED))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 76 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 116.078 87.376)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 116.078 149.606)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 197.612 149.606)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 197.866 87.376)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text RD (at 115.824 99.822) (layer B.SilkS))
  (gr_text LED (at 115.316 92.202) (layer B.SilkS))
  (gr_text DOWN (at 145.796 127.762 90) (layer F.SilkS))
  (gr_text UP (at 132.334 128.016 90) (layer F.SilkS))
  (gr_text Vcc (at 170.688 150.114 90) (layer F.SilkS))
  (gr_text GND (at 165.862 150.114 90) (layer F.SilkS))
  (gr_text GND (at 149.86 150.114 90) (layer F.SilkS))
  (gr_text RX (at 145.034 150.876 90) (layer F.SilkS))
  (gr_text TX (at 139.954 150.876 90) (layer F.SilkS))
  (gr_text 3v3 (at 115.824 134.62) (layer F.SilkS))
  (gr_text GND (at 115.57 137.16) (layer F.SilkS))
  (gr_text 3v3 (at 123.444 92.456) (layer F.SilkS))
  (gr_text 3v3 (at 163.83 92.202) (layer F.SilkS))
  (gr_text GND (at 163.576 115.062) (layer F.SilkS))
  (gr_text GND (at 133.35 92.202) (layer F.SilkS))
  (gr_text GND (at 189.484 146.812) (layer F.SilkS))
  (gr_text Vin (at 181.61 146.812) (layer F.SilkS))
  (gr_text "Teensy 3.6" (at 185.42 118.618 90) (layer F.SilkS))
  (gr_text CFAF240320W0-E1-1 (at 148.59 104.394 90) (layer F.SilkS))
  (gr_line (start 113.03 152.654) (end 113.03 84.328) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.66 152.654) (end 113.03 152.654) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.66 84.328) (end 113.03 84.328) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 200.66 152.654) (end 200.66 84.328) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 119.38 86.36) (xy 194.564 86.106) (xy 194.564 149.606) (xy 119.38 149.86)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 119.38 86.36) (xy 194.564 86.106) (xy 194.564 149.606) (xy 119.38 149.86)
      )
    )
  )
)
