(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 87)
    (tracks 162)
    (zones 0)
    (modules 4)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2286)
    (trace_clearance 0.228575)
    (zone_clearance 0.152375)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad19)")
  (net 2 "Net-(J1-Pad18)")
  (net 3 "Net-(J1-Pad17)")
  (net 4 "Net-(J1-Pad16)")
  (net 5 "Net-(J1-Pad15)")
  (net 6 "Net-(J1-Pad14)")
  (net 7 "Net-(J1-Pad13)")
  (net 8 "Net-(J1-Pad12)")
  (net 9 "Net-(J1-Pad11)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad9)")
  (net 12 "Net-(J1-Pad8)")
  (net 13 "Net-(J1-Pad7)")
  (net 14 "Net-(J1-Pad6)")
  (net 15 "Net-(J1-Pad5)")
  (net 16 "Net-(J1-Pad4)")
  (net 17 "Net-(J1-Pad3)")
  (net 18 "Net-(J1-Pad2)")
  (net 19 "Net-(J1-Pad1)")
  (net 20 "Net-(J2-Pad1)")
  (net 21 "Net-(J2-Pad2)")
  (net 22 "Net-(J2-Pad3)")
  (net 23 "Net-(J2-Pad4)")
  (net 24 "Net-(J2-Pad5)")
  (net 25 "Net-(J2-Pad6)")
  (net 26 "Net-(J2-Pad7)")
  (net 27 "Net-(J2-Pad8)")
  (net 28 "Net-(J2-Pad9)")
  (net 29 "Net-(J2-Pad10)")
  (net 30 "Net-(J2-Pad11)")
  (net 31 "Net-(J2-Pad12)")
  (net 32 "Net-(J2-Pad13)")
  (net 33 "Net-(J2-Pad14)")
  (net 34 "Net-(J2-Pad15)")
  (net 35 "Net-(J2-Pad16)")
  (net 36 "Net-(J2-Pad17)")
  (net 37 "Net-(J2-Pad18)")
  (net 38 "Net-(J2-Pad19)")
  (net 39 "Net-(J3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.228575)
    (trace_width 0.2286)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
  )
  (net_class "High Power" ""
    (clearance 0.228575)
    (trace_width 0.4318)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad19)")
  )
  (net_class Pad39 ""
    (clearance 0.228575)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J3-Pad1)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x19_Pitch2.54mm (layer B.Cu) (tedit 5BA66716)
    (at 91.44 57.15 180)
    (descr "Through hole straight pin header, 1x19, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x19 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x19 (at 0 -48.05 180) (layer B.Fab))
    (fp_text user %R (at 0 -22.86 90) (layer B.Fab))
    (pad 19 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad19)"))
    (pad 18 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad18)"))
    (pad 17 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad17)"))
    (pad 16 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x19_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x19_Pitch2.54mm (layer B.Cu) (tedit 5BA6671D)
    (at 109.22 102.87)
    (descr "Through hole straight pin header, 1x19, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x19 2.54mm single row")
    (fp_text reference J2 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value Conn_01x19 (at 0 -48.05) (layer B.Fab))
    (fp_text user %R (at 0 -22.86 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad12)"))
    (pad 13 thru_hole oval (at 0 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 0 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 0 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 0 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad16)"))
    (pad 17 thru_hole oval (at 0 -40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at 0 -43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad18)"))
    (pad 19 thru_hole oval (at 0 -45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad19)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x19_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5BA662AA)
    (at 100.33 88.9)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Footprints:HTSSOP-38_4.4x9.7mm_Pitch0.5mm" (layer F.Cu) (tedit 5BA654B6)
    (at 100.33 80.01)
    (descr "TSSOP38: plastic thin shrink small outline package; 38 leads; body width 4.4 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot510-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -5.9) (layer F.SilkS))
    (fp_text value PCA9956B (at 0 5.9) (layer F.Fab))
    (fp_text user %R (at -0.075 3.5) (layer F.Fab))
    (pad 38 smd rect (at 3.05 -4.6) (size 1.35 0.45) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J2-Pad19)"))
    (pad 37 smd rect (at 3.05 -4) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J2-Pad18)"))
    (pad 36 smd rect (at 3.05 -3.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J2-Pad17)"))
    (pad 35 smd rect (at 3.05 -3) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-Pad16)"))
    (pad 34 smd rect (at 3.05 -2.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J2-Pad15)"))
    (pad 33 smd rect (at 3.05 -2) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J2-Pad14)"))
    (pad 32 smd rect (at 3.05 -1.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J2-Pad13)"))
    (pad 31 smd rect (at 3.05 -1) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J2-Pad12)"))
    (pad 30 smd rect (at 3.05 -0.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J2-Pad11)"))
    (pad 29 smd rect (at 3.05 0) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J2-Pad10)"))
    (pad 28 smd rect (at 3.05 0.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J2-Pad9)"))
    (pad 27 smd rect (at 3.05 1) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J2-Pad8)"))
    (pad 26 smd rect (at 3.05 1.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J2-Pad7)"))
    (pad 25 smd rect (at 3.05 2) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J2-Pad6)"))
    (pad 24 smd rect (at 3.05 2.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J2-Pad5)"))
    (pad 23 smd rect (at 3.05 3) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J2-Pad4)"))
    (pad 22 smd rect (at 3.05 3.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J2-Pad3)"))
    (pad 21 smd rect (at 3.05 4) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (pad 20 smd rect (at 3.05 4.6) (size 1.35 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J2-Pad1)"))
    (pad 19 smd rect (at -3.05 4.6) (size 1.35 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad19)"))
    (pad 18 smd rect (at -3.05 4) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad18)"))
    (pad 17 smd rect (at -3.05 3.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad17)"))
    (pad 16 smd rect (at -3.05 3) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad16)"))
    (pad 15 smd rect (at -3.05 2.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad15)"))
    (pad 14 smd rect (at -3.05 2) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad14)"))
    (pad 13 smd rect (at -3.05 1.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 12 smd rect (at -3.05 1) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad12)"))
    (pad 11 smd rect (at -3.05 0.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad11)"))
    (pad 10 smd rect (at -3.05 0) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 9 smd rect (at -3.05 -0.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad9)"))
    (pad 8 smd rect (at -3.05 -1) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad8)"))
    (pad 7 smd rect (at -3.05 -1.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad7)"))
    (pad 6 smd rect (at -3.05 -2) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at -3.05 -2.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad5)"))
    (pad 4 smd rect (at -3.05 -3) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at -3.05 -3.5) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -3.05 -4) (size 1.35 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -3.05 -4.6) (size 1.35 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J1-Pad1)"))
    (pad 39 smd rect (at 0 0) (size 3 5.04) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at -1 2) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at 0 2) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at 1 2) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at -1 1) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at 0 1) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at 1 1) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at 1 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at -1 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at 1 -1) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at -1 -1) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at 0 -1) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at -1 -2) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at 1 -2) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 thru_hole circle (at 0 -2) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (pad 39 smd rect (at 0 0) (size 3 5.04) (layers B.Cu F.Paste F.Mask)
      (net 39 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-38_4.4x9.7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "(c)\npackom.net\n2018" (at 100.33 99.06) (layer B.SilkS))
  (gr_text "THSSOP\n38" (at 100.33 93.345) (layer B.SilkS))
  (gr_text 37 (at 107.315 59.69) (layer B.SilkS))
  (gr_text 38 (at 107.315 57.15) (layer B.SilkS))
  (gr_text 36 (at 107.315 62.23) (layer B.SilkS))
  (gr_text 35 (at 107.315 64.77) (layer B.SilkS))
  (gr_text 32 (at 107.315 72.39) (layer B.SilkS))
  (gr_text 34 (at 107.315 67.31) (layer B.SilkS))
  (gr_text 31 (at 107.315 74.93) (layer B.SilkS))
  (gr_text 30 (at 107.315 77.47) (layer B.SilkS))
  (gr_text 33 (at 107.315 69.85) (layer B.SilkS))
  (gr_text 25 (at 107.315 90.17) (layer B.SilkS))
  (gr_text 29 (at 107.315 80.01) (layer B.SilkS))
  (gr_text 27 (at 107.315 85.09) (layer B.SilkS))
  (gr_text 26 (at 107.315 87.63) (layer B.SilkS))
  (gr_text 28 (at 107.315 82.55) (layer B.SilkS))
  (gr_text 24 (at 107.315 92.71) (layer B.SilkS))
  (gr_text 23 (at 107.315 95.25) (layer B.SilkS))
  (gr_text 22 (at 107.315 97.79) (layer B.SilkS))
  (gr_text 21 (at 107.315 100.33) (layer B.SilkS))
  (gr_text 20 (at 107.315 102.87) (layer B.SilkS))
  (gr_text 19 (at 93.345 102.87) (layer B.SilkS))
  (gr_text 16 (at 93.345 95.25) (layer B.SilkS))
  (gr_text 17 (at 93.345 97.79) (layer B.SilkS))
  (gr_text 18 (at 93.345 100.33) (layer B.SilkS))
  (gr_text 14 (at 93.345 90.17) (layer B.SilkS))
  (gr_text 11 (at 93.345 82.55) (layer B.SilkS))
  (gr_text 12 (at 93.345 85.09) (layer B.SilkS))
  (gr_text 13 (at 93.345 87.63) (layer B.SilkS))
  (gr_text 15 (at 93.345 92.71) (layer B.SilkS))
  (gr_text 6 (at 93.345 69.85) (layer B.SilkS))
  (gr_text 7 (at 93.345 72.39) (layer B.SilkS))
  (gr_text 8 (at 93.345 74.93) (layer B.SilkS))
  (gr_text 9 (at 93.345 77.47) (layer B.SilkS))
  (gr_text 10 (at 93.345 80.01) (layer B.SilkS))
  (gr_text 5 (at 93.345 67.31) (layer B.SilkS))
  (gr_text 4 (at 93.345 64.77) (layer B.SilkS))
  (gr_text 3 (at 93.345 62.23) (layer B.SilkS))
  (gr_text 2 (at 93.345 59.69) (layer B.SilkS))
  (gr_text 1 (at 93.345 57.15) (layer B.SilkS))
  (gr_text "THSSOP\n38" (at 100.33 97.79) (layer F.SilkS))
  (gr_text 35 (at 107.315 64.77) (layer F.SilkS))
  (gr_text 38 (at 107.315 57.15) (layer F.SilkS))
  (gr_text 36 (at 107.315 62.23) (layer F.SilkS))
  (gr_text 37 (at 107.315 59.69) (layer F.SilkS))
  (gr_text 34 (at 107.315 67.31) (layer F.SilkS))
  (gr_text 33 (at 107.315 69.85) (layer F.SilkS))
  (gr_text 31 (at 107.315 74.93) (layer F.SilkS))
  (gr_text 32 (at 107.315 72.39) (layer F.SilkS))
  (gr_text 30 (at 107.315 77.47) (layer F.SilkS))
  (gr_text 29 (at 107.315 80.01) (layer F.SilkS))
  (gr_text 28 (at 107.315 82.55) (layer F.SilkS))
  (gr_text 26 (at 107.315 87.63) (layer F.SilkS))
  (gr_text 27 (at 107.315 85.09) (layer F.SilkS))
  (gr_text 25 (at 107.315 90.17) (layer F.SilkS))
  (gr_text 24 (at 107.315 92.71) (layer F.SilkS))
  (gr_text 23 (at 107.315 95.25) (layer F.SilkS))
  (gr_text 22 (at 107.315 97.79) (layer F.SilkS))
  (gr_text 21 (at 107.315 100.33) (layer F.SilkS))
  (gr_text 20 (at 107.315 102.87) (layer F.SilkS))
  (gr_text 15 (at 93.345 92.71) (layer F.SilkS))
  (gr_text 12 (at 93.345 85.09) (layer F.SilkS))
  (gr_text 13 (at 93.345 87.63) (layer F.SilkS))
  (gr_text 17 (at 93.345 97.79) (layer F.SilkS))
  (gr_text 18 (at 93.345 100.33) (layer F.SilkS))
  (gr_text 16 (at 93.345 95.25) (layer F.SilkS))
  (gr_text 11 (at 93.345 82.55) (layer F.SilkS))
  (gr_text 14 (at 93.345 90.17) (layer F.SilkS))
  (gr_text 19 (at 93.345 102.87) (layer F.SilkS))
  (gr_text 10 (at 93.345 80.01) (layer F.SilkS))
  (gr_text 9 (at 93.345 77.47) (layer F.SilkS))
  (gr_text 8 (at 93.345 74.93) (layer F.SilkS))
  (gr_text 7 (at 93.345 72.39) (layer F.SilkS))
  (gr_text 6 (at 93.345 69.85) (layer F.SilkS))
  (gr_text 5 (at 93.345 67.31) (layer F.SilkS))
  (gr_text 4 (at 93.345 64.77) (layer F.SilkS))
  (gr_text 3 (at 93.345 62.23) (layer F.SilkS))
  (gr_text 2 (at 93.345 59.69) (layer F.SilkS))
  (gr_text 1 (at 93.345 57.15) (layer F.SilkS))
  (gr_text * (at 98.679 75.946) (layer F.SilkS))
  (gr_line (start 90.17 104.14) (end 90.17 55.88) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.49 104.14) (end 90.17 104.14) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.49 55.88) (end 110.49 104.14) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.17 55.88) (end 110.49 55.88) (layer Edge.Cuts) (width 0.15))
  (gr_text Pad (at 100.33 91.44) (layer F.SilkS))
  (zone (net 39) (net_name "Net-(J3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.152375))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.98 104.14) (xy 106.68 104.14) (xy 106.68 55.88) (xy 93.98 55.88)
      )
    )
  )
)
