(kicad_pcb (version 20170123) (host pcbnew no-vcs-found-4f2ed1b~58~ubuntu16.04.1)
  (general
    (links 56)
    (no_connects 0)
    (area 88.871667 56.507499 126.742499 86.1425)
    (thickness 1.6)
    (drawings 6)
    (tracks 299)
    (zones 0)
    (modules 29)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(R3-Pad1)")
  (net 2 "Net-(R8-Pad1)")
  (net 3 NO2)
  (net 4 VDD)
  (net 5 VREF)
  (net 6 "Net-(Q5-Pad3)")
  (net 7 GNDD)
  (net 8 SCALE_2)
  (net 9 "Net-(Q1-Pad3)")
  (net 10 "Net-(Q1-Pad2)")
  (net 11 "Net-(Q1-Pad1)")
  (net 12 "Net-(Q2-Pad1)")
  (net 13 "Net-(Q2-Pad2)")
  (net 14 "Net-(Q2-Pad3)")
  (net 15 "Net-(Q3-Pad3)")
  (net 16 SCALE_1)
  (net 17 "Net-(Q4-Pad3)")
  (net 18 "Net-(Q6-Pad3)")
  (net 19 GND)
  (net 20 PWM)
  (net 21 CO)
  (net 22 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net CO)
    (add_net GND)
    (add_net GNDD)
    (add_net NO2)
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(Q4-Pad3)")
    (add_net "Net-(Q5-Pad3)")
    (add_net "Net-(Q6-Pad3)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net PWM)
    (add_net SCALE_1)
    (add_net SCALE_2)
    (add_net VDD)
    (add_net VREF)
  )
  (module rmap:MICS-4514 (layer B.Cu) (tedit 59136C75)
    (at 113.03 71.12)
    (fp_text reference U1 (at -5.08 0 270) (layer B.SilkS))
    (fp_text value MICS-4514 (at 0 -5.08) (layer B.Fab))
    (pad A smd rect (at -1.27 -2.54) (size 0.6 2) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(R3-Pad1)"))
    (pad B smd rect (at 0 -2.54) (size 0.6 2) (layers B.Cu B.Paste B.Mask)
      (net 21 CO))
    (pad C smd rect (at 1.27 -2.54) (size 0.6 2) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(R8-Pad1)"))
    (pad D smd rect (at 3.175 -1.27 270) (size 0.6 2) (layers B.Cu B.Paste B.Mask)
      (net 3 NO2))
    (pad E smd rect (at 3.175 1.27 270) (size 0.6 2) (layers B.Cu B.Paste B.Mask))
    (pad F smd rect (at 1.27 2.54) (size 0.6 2) (layers B.Cu B.Paste B.Mask)
      (net 4 VDD))
    (pad G smd rect (at 0 2.54) (size 0.6 2) (layers B.Cu B.Paste B.Mask)
      (net 5 VREF))
    (pad H smd rect (at -1.27 2.54) (size 0.6 2) (layers B.Cu B.Paste B.Mask)
      (net 4 VDD))
    (pad J smd rect (at -3.175 1.27 270) (size 0.6 2) (layers B.Cu B.Paste B.Mask)
      (net 5 VREF))
    (pad K smd rect (at -3.175 -1.27 270) (size 0.6 2) (layers B.Cu B.Paste B.Mask))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58A0C5EF)
    (at 116.84 67.31 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 SCALE_1))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GNDD))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q4-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58A0C603)
    (at 111.76 82.55 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q8 (at 0 3.175 180) (layer F.SilkS))
    (fp_text value BC849 (at 0 2.5 180) (layer F.Fab) hide)
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q2-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58A0C43D)
    (at 122.555 67.31 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.5 180) (layer F.Fab) hide)
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q6-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GNDD))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 SCALE_1))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 58A0C54E)
    (at 93.98 68.58)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P2 (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 12.55) (layer F.Fab) hide)
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 +5V))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VDD))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VREF))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GNDD))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C5F3)
    (at 110.49 66.04)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1M (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 CO))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 GNDD))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C5F6)
    (at 110.49 71.12)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 100K (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 CO))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q4-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C60A)
    (at 118.745 82.55 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 560 (at 0 2.1 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 VREF))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 +5V))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58A0C5FC)
    (at 122.555 74.93 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.5 180) (layer F.Fab) hide)
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q5-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GNDD))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 SCALE_2))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C55C)
    (at 101.6 62.23)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at -0.635 1.905) (layer F.SilkS))
    (fp_text value 100 (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 GNDD))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58A0C554)
    (at 101.6 58.42)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 1.905) (layer F.SilkS))
    (fp_text value 22u (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 22 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C565)
    (at 104.14 76.2)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q5-Pad3)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 NO2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C5FF)
    (at 110.49 76.2)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Q3-Pad3)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 CO))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C55F)
    (at 104.14 66.04)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0.635 -1.905) (layer F.SilkS))
    (fp_text value 1M (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 GNDD))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 NO2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C5E9)
    (at 115.929999 59.964999 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.535001 -0.994999 180) (layer F.SilkS))
    (fp_text value 75 (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58A0C446)
    (at 119.739999 59.964999 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q7 (at -0.275001 -3.535001 180) (layer F.SilkS))
    (fp_text value BC849 (at 0 2.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C613)
    (at 107.95 82.55 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 47 (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q2-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58A0C616)
    (at 104.14 82.55)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -3.175) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q2-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q2-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C559)
    (at 108.309999 59.964999 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.535001 0.275001 180) (layer F.SilkS))
    (fp_text value 47k (at 0 2.1 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 PWM))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58A0C5F9)
    (at 116.84 74.93 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.5 180) (layer F.Fab) hide)
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Q3-Pad3)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GNDD))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 SCALE_2))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C546)
    (at 95.25 58.42)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 1.905) (layer F.SilkS))
    (fp_text value 100 (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 +5V))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C60E)
    (at 115.57 82.55 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 17R4 (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C5EC)
    (at 123.549999 59.964999 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.535001 0.275001 180) (layer F.SilkS))
    (fp_text value 21R5 (at 0 2.1 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 GND))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58A0C5E5)
    (at 112.119999 59.964999)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0.275001 2.900001) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.5) (layer F.Fab) hide)
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58A0C54A)
    (at 95.25 62.23)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.905) (layer F.SilkS))
    (fp_text value 22u (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GNDD))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 58A0C551)
    (at 96.52 68.58)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 12.55) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 PWM))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 SCALE_1))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 SCALE_2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 CO))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 NO2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C562)
    (at 104.14 71.12)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 100K (at 0 2.1) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q6-Pad3)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 NO2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A0C569)
    (at 100.33 82.55 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 47k (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 PWM))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Q2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58A0C606)
    (at 123.19 82.55 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at 0 3.175 180) (layer F.SilkS))
    (fp_text value ZENER (at 0 2.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 VREF))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GNDD))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "Ver 2" (at 120.65 83.185) (layer B.SilkS))
  (gr_text rmap.cc (at 97.79 83.185) (layer B.SilkS))
  (gr_line (start 92.075 85.725) (end 92.075 57.15) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.095 85.725) (end 92.075 85.725) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.095 57.15) (end 125.095 85.725) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.075 57.15) (end 125.095 57.15) (layer Edge.Cuts) (width 0.1))
  (zone (net 19) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.095 85.725) (xy 92.075 85.725) (xy 92.075 57.15) (xy 125.095 57.15) (xy 125.095 85.09)
      )
    )
  )
  (zone (net 19) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.075 57.15) (xy 125.095 57.15) (xy 125.095 85.725) (xy 92.075 85.725)
      )
    )
  )
)
