<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="43.130175" x2="0" y2="4.33604375" width="0" layer="20"/>
<wire x1="0" y1="4.33604375" x2="4.33604375" y2="0" width="0" layer="20" curve="90"/>
<wire x1="4.33604375" y1="0" x2="68.138225" y2="0" width="0" layer="20"/>
<wire x1="68.138225" y1="0" x2="72.2736" y2="4.135375" width="0" layer="20" curve="90"/>
<wire x1="72.2736" y1="4.135375" x2="72.2736" y2="43.30850625" width="0" layer="20"/>
<wire x1="72.2736" y1="43.30850625" x2="69.17630625" y2="46.4058" width="0" layer="20" curve="90"/>
<wire x1="69.17630625" y1="46.4058" x2="3.275625" y2="46.4058" width="0" layer="20"/>
<wire x1="3.275625" y1="46.4058" x2="0" y2="43.130175" width="0" layer="20" curve="90"/>
<text>CAM+</text>
<text>CAM-</text>
<text>LED+</text>
<text>LED+</text>
<text>LED-</text>
<text>CAMERA
-       + </text>
<text>RV-Project.Com</text>
<text>Camera Switch Adapter</text>
<text>Rev C</text>
<text>3-25-2018</text>
<text>10A Max 2 oz/Ft^2 Copper</text>
<text>12V</text>
<text>GND</text>
<hole x="5.08" y="22.86" drill="3.7973"/>
<hole x="68.58" y="22.86" drill="3.7973"/>
<text>POWER
+     -</text>
<text>LED-</text>
<text>SwitchA</text>
<text>SwitchB</text>
<text>TVS Status</text>
<text>Camera On</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="MO1-18AWG">
</package>
<package name="D041-3.5MIL">
</package>
<package name="1/4W_AXIAL">
<description>Standard Axial 1/4Watt Resistor&lt;p&gt;0.45" footprint</description>
</package>
<package name="251SMALL">
</package>
<package name="ART_CHEROKEE_MEDIUM">
</package>
<package name="WAFER2PIN">
</package>
<package name="1CH_RECEIVE_RELAY">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP8" library="a-lib" package="MO1-18AWG" value="LED1">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP9" library="a-lib" package="MO1-18AWG" value="LED-">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP10" library="a-lib" package="MO1-18AWG" value="LED2">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="D1" library="a-lib" package="D041-3.5MIL" value="TVS-SD041">
<attribute name="NAME"/>
</element>
<element name="R1" library="a-lib" package="1/4W_AXIAL" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="a-lib" package="1/4W_AXIAL" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="a-lib" package="251SMALL" value="5A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="a-lib" package="ART_CHEROKEE_MEDIUM" value="Cherokee Medium">
<attribute name="VALUE" value="Cherokee Medium"/>
</element>
<element name="J1" library="a-lib" package="WAFER2PIN" value="WAFER2PHORIZONTAL"/>
<element name="J2" library="a-lib" package="WAFER2PIN" value="WAFER2PHORIZONTAL"/>
<element name="RY1" library="a-lib" package="1CH_RECEIVE_RELAY" value="WIRELESS_RELAY_1CHANNEL"/>
<element name="JP1" library="a-lib" package="MO1-18AWG" value="LED-">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP2" library="a-lib" package="MO1-18AWG" value="SwitchA">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP3" library="a-lib" package="MO1-18AWG" value="SwitchB">
<attribute name="AMPERAGE" value="10A"/>
</element>
</elements>
<signals>
<signal name="N$9">
<contactref element="JP8" pad="P$1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="JP10" pad="P$1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="RY1" pad="GND"/>
<contactref element="D1" pad="A"/>
<contactref element="JP9" pad="P$1"/>
<contactref element="JP1" pad="P$1"/>
<contactref element="J1" pad="P$2"/>
<contactref element="J2" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="C"/>
<contactref element="F1" pad="P$1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="RY1" pad="12V"/>
<contactref element="RY1" pad="COM"/>
<contactref element="JP3" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="RY1" pad="NO"/>
<contactref element="F1" pad="P$2"/>
<contactref element="R2" pad="2"/>
<contactref element="J2" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="JP2" pad="P$1"/>
<contactref element="J1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
