(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 35)
    (no_connects 0)
    (area 134.544999 52.502999 179.399001 90.499001)
    (thickness 1.6)
    (drawings 10)
    (tracks 84)
    (zones 0)
    (modules 15)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 3.5)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.4)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 65.024 65.532)
    (visible_elements FFFFDE7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(F1-Pad1)")
  (net 6 "Net-(R2-Pad2)")
  (net 7 "Net-(R3-Pad2)")
  (net 8 "Net-(U1-Pad1)")
  (net 9 "Net-(U1-Pad2)")
  (net 10 "Net-(U1-Pad3)")
  (net 11 "Net-(U1-Pad6)")
  (net 12 "Net-(U1-Pad7)")
  (net 13 "Net-(U1-Pad8)")
  (net 14 "Net-(U1-Pad9)")
  (net 15 "Net-(U1-Pad10)")
  (net 16 "Net-(U1-Pad11)")
  (net 17 "Net-(U1-Pad13)")
  (net 18 "Net-(U1-Pad18)")
  (net 19 "Net-(U1-Pad20)")
  (net 20 "Net-(U1-Pad21)")
  (net 21 "Net-(U1-Pad24)")
  (net 22 "Net-(U1-Pad26)")
  (net 23 "Net-(U1-Pad28)")
  (net 24 "Net-(U1-Pad29)")
  (net 25 "Net-(U1-Pad30)")
  (net 26 "Net-(P5-Pad1)")
  (net 27 "Net-(P5-Pad2)")
  (net 28 "Net-(P5-Pad3)")
  (net 29 "Net-(R5-Pad2)")
  (net 30 "Net-(P6-Pad1)")
  (net 31 +5V)
  (net 32 "Net-(U1-Pad25)")
  (net 33 "Net-(P4-Pad2)")
  (net 34 "Net-(P4-Pad3)")
  (net 35 "Net-(P7-Pad1)")
  (net 36 "Net-(P8-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
  )
  (net_class power ""
    (clearance 0.4)
    (trace_width 3.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Resistors_ThroughHole:Resistor_Vertical_RM5mm (layer F.Cu) (tedit 0)
    (at 155.956 73.914 180)
    (descr "Resistor, Vertical, RM 5mm, 1/3W,")
    (tags "Resistor, Vertical, RM 5mm, 1/3W,")
    (fp_text reference R5 (at 2.70002 -3.29946 180) (layer F.SilkS))
    (fp_text value "20 ohm" (at 0 4.50088 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.49936 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 26 "Net-(P5-Pad1)"))
    (pad 2 thru_hole circle (at 2.5019 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(R5-Pad2)"))
  )
  (module arduino_mini (layer F.Cu) (tedit 592B377C)
    (at 157.48 61.976 180)
    (descr "30 pins DIL package, elliptical pads, width 600mil (arduino mini)")
    (tags "DIL arduino mini")
    (fp_text reference U1 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value arduino_mini (at -1.6764 3.3274 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -19.05 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U1-Pad1)"))
    (pad 2 thru_hole oval (at -16.51 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U1-Pad2)"))
    (pad 3 thru_hole oval (at -13.97 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(U1-Pad3)"))
    (pad 4 thru_hole oval (at -11.43 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(R3-Pad2)"))
    (pad 5 thru_hole oval (at -8.89 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(R2-Pad2)"))
    (pad 6 thru_hole oval (at -6.35 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(U1-Pad6)"))
    (pad 7 thru_hole oval (at -3.81 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U1-Pad7)"))
    (pad 8 thru_hole oval (at -1.27 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(U1-Pad8)"))
    (pad 9 thru_hole oval (at 1.27 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U1-Pad9)"))
    (pad 10 thru_hole oval (at 3.81 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U1-Pad10)"))
    (pad 11 thru_hole oval (at 6.35 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U1-Pad11)"))
    (pad 12 thru_hole oval (at 8.89 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 +5V))
    (pad 13 thru_hole oval (at 11.43 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(U1-Pad13)"))
    (pad 14 thru_hole oval (at 13.97 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole oval (at 16.51 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad1)"))
    (pad 16 thru_hole oval (at 16.51 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P4-Pad3)"))
    (pad 17 thru_hole oval (at 13.97 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(P4-Pad2)"))
    (pad 18 thru_hole oval (at 11.43 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(U1-Pad18)"))
    (pad 19 thru_hole oval (at 8.89 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 20 thru_hole oval (at 6.35 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(U1-Pad20)"))
    (pad 21 thru_hole oval (at 3.81 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(U1-Pad21)"))
    (pad 22 thru_hole oval (at 1.27 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(P7-Pad1)"))
    (pad 23 thru_hole oval (at -1.27 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(P8-Pad1)"))
    (pad 24 thru_hole oval (at -3.81 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U1-Pad24)"))
    (pad 25 thru_hole oval (at -6.35 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U1-Pad25)"))
    (pad 26 thru_hole oval (at -8.89 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U1-Pad26)"))
    (pad 27 thru_hole oval (at -11.43 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(R5-Pad2)"))
    (pad 28 thru_hole oval (at -13.97 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U1-Pad28)"))
    (pad 29 thru_hole oval (at -16.51 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U1-Pad29)"))
    (pad 30 thru_hole oval (at -19.05 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U1-Pad30)"))
    (model arduino_nano.wrl
      (at (xyz -0.978 -0.385 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 592B3185)
    (at 150.114 73.406 270)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D2 (at 6.35 0 270) (layer F.SilkS))
    (fp_text value D_Schottky (at 5.08 -0.508 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 90) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 -0.00254 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad1)"))
  )
  (module freetronics_footprints:screw_terminal (layer F.Cu) (tedit 5800DEC5)
    (at 136.906 88.392 90)
    (fp_text reference P1 (at 2.54 1.27 90) (layer F.SilkS))
    (fp_text value "POWER +" (at 2.54 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(F1-Pad1)"))
    (pad 1 thru_hole circle (at 5 0 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(F1-Pad1)"))
    (pad 1 thru_hole circle (at 0 7 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(F1-Pad1)"))
    (pad 1 thru_hole circle (at 5 7 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(F1-Pad1)"))
  )
  (module freetronics_footprints:screw_terminal (layer F.Cu) (tedit 5800DEC1)
    (at 136.906 78.486 90)
    (fp_text reference P2 (at 2.54 1.27 90) (layer F.SilkS))
    (fp_text value "POWER -" (at 2.54 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 5 0 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 7 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 5 7 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module freetronics_footprints:1X03 (layer F.Cu) (tedit 5800EA77)
    (at 161.29 73.914)
    (fp_text reference P5 (at 0.3 0) (layer Eco1.User))
    (fp_text value CONN_01X03 (at 2.6 1.6) (layer Eco1.User) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(P5-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(P5-Pad3)"))
  )
  (module freetronics_footprints:screw_terminal (layer F.Cu) (tedit 5800DEC9)
    (at 169.672 88.392 90)
    (fp_text reference P3 (at 2.54 1.27 90) (layer F.SilkS))
    (fp_text value "CONTROLLER +" (at 5.08 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad1)"))
    (pad 1 thru_hole circle (at 5 0 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad1)"))
    (pad 1 thru_hole circle (at 0 7 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad1)"))
    (pad 1 thru_hole circle (at 5 7 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad1)"))
  )
  (module freetronics_footprints:screw_terminal (layer F.Cu) (tedit 5800DECB)
    (at 169.672 78.486 90)
    (fp_text reference P6 (at 2.54 1.27 90) (layer F.SilkS))
    (fp_text value CONTROLLER- (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P6-Pad1)"))
    (pad 1 thru_hole circle (at 5 0 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P6-Pad1)"))
    (pad 1 thru_hole circle (at 0 7 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P6-Pad1)"))
    (pad 1 thru_hole circle (at 5 7 90) (size 2.8 2.8) (drill 1.85) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P6-Pad1)"))
  )
  (module Diodes_ThroughHole:Diode_TO-220_Vertical (layer F.Cu) (tedit 5800EE15)
    (at 164.084 82.296 180)
    (descr "TO-220, Diode, Vertical,")
    (tags "TO-220, Diode, Vertical,")
    (fp_text reference D1 (at 2.54762 -3.92938 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 2.794 -1.27 180) (layer F.Fab))
    (fp_text user A (at 6.858 0.127 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (model Diodes_ThroughHole.3dshapes/Diode_TO-220_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module arduino:BladeFuse-CarType (layer F.Cu) (tedit 592B2950)
    (at 157.226 87.884)
    (fp_text reference F1 (at -0.1 -5.2) (layer F.SilkS))
    (fp_text value FUSE (at -3.302 -3.5814) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.11 0) (size 3.54 3.54) (drill 2.54) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 2.03 0) (size 3.54 3.54) (drill 2.54) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at -7.11 -0.1) (size 3.54 3.54) (drill 2.54) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(F1-Pad1)"))
    (pad 1 thru_hole circle (at -2.03 0) (size 3.54 3.54) (drill 2.54) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(F1-Pad1)"))
    (model Fuse_Holders_and_Fuses.3dshapes/BladeFuse-CarType.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module uart:uart (layer F.Cu) (tedit 592B3B30)
    (at 136.398 61.468 270)
    (fp_text reference P4 (at 0 0 270) (layer Eco1.User) hide)
    (fp_text value uart (at 1.27 1.27 270) (layer Eco1.User) hide)
    (fp_text user GND (at 7.6 -1.9 270) (layer F.SilkS))
    (fp_text user RX (at 2.54 -1.905 270) (layer F.SilkS))
    (fp_text user TX (at 5.08 -1.905 270) (layer F.SilkS))
    (fp_text user VCC (at -0.1 -1.9 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 +5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "Net-(P4-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 166.116 77.978 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.32892 -3.50012 180) (layer F.SilkS))
    (fp_text value ".05 ohm" (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 30 "Net-(P6-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 174.244 65.786 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 4.05892 -3.50012 180) (layer F.SilkS))
    (fp_text value 560 (at 3.81 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 30 "Net-(P6-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(R2-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 162.56 58.42)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R3 (at 4.05892 -3.50012) (layer F.SilkS))
    (fp_text value "10k ohm" (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(R3-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 170.18 62.23 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R4 (at 4.05892 -3.50012 180) (layer F.SilkS))
    (fp_text value "560 ohm" (at 3.81 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(R3-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 GND))
  )
  (gr_line (start 179.324 90.424) (end 134.874 90.424) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.874 52.578) (end 179.324 52.578) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.874 90.424) (end 134.874 52.578) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.324 52.578) (end 179.324 90.424) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text B- (at 147.32 76.2) (layer F.SilkS))
  (gr_text C- (at 167.894 75.438) (layer F.SilkS))
  (gr_text C+ (at 167.64 85.598) (layer F.SilkS))
  (gr_text B+ (at 146.812 84.836) (layer F.SilkS))
  (gr_text "Sean D'Epagnier" (at 152.4 66.04) (layer F.SilkS))
  (gr_text "controller\nv0.2" (at 151.384 82.296) (layer F.SilkS))
)
