(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 369)
    (zones 0)
    (modules 74)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.635)
    (user_trace_width 2.032)
    (user_trace_width 6.35)
    (trace_clearance 0.2)
    (zone_clearance 0.381)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.635)
    (via_min_drill 0.3048)
    (user_via 0.635 0.3048)
    (user_via 0.889 0.508)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 133.35 118.11)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C2-Pad2)")
  (net 2 "Net-(C2-Pad1)")
  (net 3 GND)
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C7-Pad1)")
  (net 6 "Net-(C11-Pad1)")
  (net 7 "Net-(C12-Pad2)")
  (net 8 "Net-(C14-Pad2)")
  (net 9 "Net-(C17-Pad1)")
  (net 10 "Net-(D1-Pad2)")
  (net 11 "Net-(D2-Pad2)")
  (net 12 GNDREF)
  (net 13 "Net-(D3-Pad1)")
  (net 14 "Net-(P1-Pad3)")
  (net 15 "Net-(P1-Pad2)")
  (net 16 "Net-(Q1-Pad4)")
  (net 17 "Net-(Q2-Pad5)")
  (net 18 "Net-(Q2-Pad4)")
  (net 19 "Net-(Q7-Pad1)")
  (net 20 "Net-(R20-Pad1)")
  (net 21 "Net-(TP3-Pad1)")
  (net 22 "Net-(TP6-Pad1)")
  (net 23 "Net-(TP7-Pad1)")
  (net 24 "Net-(TP10-Pad1)")
  (net 25 "Net-(C10-Pad1)")
  (net 26 "Net-(D1-Pad1)")
  (net 27 "Net-(R3-Pad2)")
  (net 28 "Net-(R4-Pad2)")
  (net 29 "Net-(R5-Pad2)")
  (net 30 "Net-(R6-Pad2)")
  (net 31 "Net-(R14-Pad2)")
  (net 32 "Net-(R23-Pad2)")
  (net 33 "Net-(C5-Pad1)")
  (net 34 "Net-(C10-Pad2)")
  (net 35 "Net-(Q1-Pad5)")
  (net 36 "Net-(R1-Pad1)")
  (net 37 "Net-(R2-Pad1)")
  (net 38 "Net-(R9-Pad2)")
  (net 39 "Net-(R10-Pad1)")
  (net 40 "Net-(TP24-Pad1)")
  (net 41 "Net-(TP25-Pad1)")
  (net 42 "Net-(TP26-Pad1)")
  (net 43 "Net-(TP27-Pad1)")
  (net 44 "Net-(TP29-Pad1)")
  (net 45 "Net-(P1-Pad4)")
  (net 46 "Net-(TP14-Pad1)")
  (net 47 "Net-(TP15-Pad1)")
  (net 48 "Net-(TP20-Pad1)")
  (net 49 "Net-(TP21-Pad1)")
  (net 50 "Net-(TP22-Pad1)")
  (net 51 "Net-(R11-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net GNDREF)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(Q1-Pad4)")
    (add_net "Net-(Q1-Pad5)")
    (add_net "Net-(Q2-Pad4)")
    (add_net "Net-(Q2-Pad5)")
    (add_net "Net-(Q7-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(TP10-Pad1)")
    (add_net "Net-(TP14-Pad1)")
    (add_net "Net-(TP15-Pad1)")
    (add_net "Net-(TP20-Pad1)")
    (add_net "Net-(TP21-Pad1)")
    (add_net "Net-(TP22-Pad1)")
    (add_net "Net-(TP24-Pad1)")
    (add_net "Net-(TP25-Pad1)")
    (add_net "Net-(TP26-Pad1)")
    (add_net "Net-(TP27-Pad1)")
    (add_net "Net-(TP29-Pad1)")
    (add_net "Net-(TP3-Pad1)")
    (add_net "Net-(TP6-Pad1)")
    (add_net "Net-(TP7-Pad1)")
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 123.19 123.19)
    (fp_text reference TP11 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C11-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 113.03 100.33)
    (fp_text reference TP2 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(C12-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 602AB902)
    (at 140.97 118.11)
    (fp_text reference TP34 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(R23-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 125.73 110.49)
    (fp_text reference TP33 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(R20-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 123.19 110.49)
    (fp_text reference TP32 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(R2-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 143.51 120.65)
    (fp_text reference TP31 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(R1-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 135.89 118.11)
    (fp_text reference TP30 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(R11-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 138.43 118.11)
    (fp_text reference TP29 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(TP29-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 120.65 110.49)
    (fp_text reference TP28 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(C17-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 135.89 120.65)
    (fp_text reference TP27 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(TP27-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 133.35 118.11)
    (fp_text reference TP26 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(TP26-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 138.43 125.73)
    (fp_text reference TP25 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(TP25-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 135.89 125.73)
    (fp_text reference TP24 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(TP24-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 118.11 110.49)
    (fp_text reference TP23 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(C14-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 133.35 128.27)
    (fp_text reference TP22 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(TP22-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 602AB926)
    (at 135.89 128.27)
    (fp_text reference TP21 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(TP21-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 130.81 125.73)
    (fp_text reference TP20 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(TP20-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 133.35 125.73)
    (fp_text reference TP15 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(TP15-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 130.81 128.27)
    (fp_text reference TP14 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(TP14-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 143.51 118.11)
    (fp_text reference TP12 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(P1-Pad4)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 138.43 123.19)
    (fp_text reference TP10 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(TP10-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 130.81 130.81)
    (fp_text reference TP9 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 135.89 123.19)
    (fp_text reference TP7 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(TP7-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 138.43 120.65)
    (fp_text reference TP6 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(TP6-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 140.97 120.65)
    (fp_text reference TP3 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(TP3-Pad1)"))
  )
  (module t_connectors:Header4_254 (layer F.Cu) (tedit 5F63AD14)
    (at 152.908 126.9365 90)
    (fp_text reference P1 (at 0.635 -4.064 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -0.5 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.62 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "Net-(P1-Pad4)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${T_LIBS}/3d/t_connectors/022112042.stp
      (offset (xyz 3.81 0 1.651))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 133.392 116.078)
    (descr "SMT capacitor, 0402")
    (fp_text reference R11 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R11-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 114.046 123.19)
    (fp_text reference TP18 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(R6-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 602AB0D7)
    (at 114.046 120.65)
    (fp_text reference TP17 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(R5-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 114.046 118.11)
    (fp_text reference TP16 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(R4-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 602AB0B0)
    (at 114.046 115.57)
    (fp_text reference TP13 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(R3-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 114.046 125.73)
    (fp_text reference TP19 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(R14-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 114.046 113.03)
    (fp_text reference TP1 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(D1-Pad1)"))
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 130.937 111.125 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R23 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R23-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 132.207 98.044 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R22 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(Q7-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 136.144 97.155)
    (descr "SMT capacitor, 0402")
    (fp_text reference R21 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 129.667 104.013)
    (descr "SMT capacitor, 0402")
    (fp_text reference R20 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R20-Pad1)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 141.351 109.474 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R17 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 10M (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q2-Pad4)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 132.969 114.215 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R13 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q1-Pad4)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 145.5 123.6345 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R10 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P1-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 145.542 121.8565)
    (descr "SMT capacitor, 0402")
    (fp_text reference R9 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R9-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 147.32 105.156 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R7 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q2-Pad5)"))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C10-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 141.732 111.379 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R2 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q2-Pad4)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 129.667 114.808 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R1 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q1-Pad4)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 125.857 97.409 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 0 -1.85) (layer F.SilkS))
    (fp_text value BAV3004 (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 GNDREF))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 127.381 115.062 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C18 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C17-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 125.928 115.077 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C17 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C17-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 125.857 118.152 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C14 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C14-Pad2)"))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 140.166 97.409)
    (descr "SMT capacitor, 0402")
    (fp_text reference C12 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C10-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 144.695 97.409)
    (descr "SMT capacitor, 0402")
    (fp_text reference C10 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C10-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_misc:BQ40Z80RSMR (layer F.Cu) (tedit 0)
    (at 129.986 120.73)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value BQ40Z50RSMR-R1 (at 0 0) (layer F.SilkS))
    (fp_text user Designator9 (at -3.302 -3.9878) (layer F.SilkS))
    (fp_text user .Designator (at 0.049985 -0.216596) (layer Dwgs.User))
    (fp_text user .Designator (at 0.049985 -0.216596) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 33 smd rect (at 0 0) (size 1.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 32 smd rect (at -1.4 -2.00102) (size 0.192474 0.91009) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C17-Pad1)"))
    (pad 31 smd rect (at -1.000001 -1.951246) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R1-Pad1)"))
    (pad 30 smd rect (at -0.599999 -1.951246) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R2-Pad1)"))
    (pad 29 smd rect (at -0.2 -1.951246) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 28 smd rect (at 0.2 -1.951246) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R20-Pad1)"))
    (pad 27 smd rect (at 0.599999 -1.951246) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R23-Pad2)"))
    (pad 26 smd rect (at 1.000001 -1.951246) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R11-Pad2)"))
    (pad 25 smd rect (at 1.4 -2.00102) (size 0.192474 0.91009) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(TP26-Pad1)"))
    (pad 24 smd rect (at 2.00102 -1.4 90) (size 0.192474 0.91009) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(TP29-Pad1)"))
    (pad 23 smd rect (at 1.951246 -1.000001 90) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(TP27-Pad1)"))
    (pad 22 smd rect (at 1.951246 -0.599999 90) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(TP6-Pad1)"))
    (pad 21 smd rect (at 1.951246 -0.2 90) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(TP3-Pad1)"))
    (pad 20 smd rect (at 1.951246 0.2 90) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(TP7-Pad1)"))
    (pad 19 smd rect (at 1.951246 0.599999 90) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R9-Pad2)"))
    (pad 18 smd rect (at 1.951246 1.000001 90) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R10-Pad1)"))
    (pad 17 smd rect (at 2.00102 1.4 90) (size 0.192474 0.91009) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(TP10-Pad1)"))
    (pad 16 smd rect (at 1.4 2.00102) (size 0.192474 0.91009) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(TP25-Pad1)"))
    (pad 15 smd rect (at 1.000001 1.951246) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(TP24-Pad1)"))
    (pad 14 smd rect (at 0.599999 1.951246) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 13 smd rect (at 0.2 1.951246) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(TP21-Pad1)"))
    (pad 12 smd rect (at -0.2 1.951246) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(TP15-Pad1)"))
    (pad 11 smd rect (at -0.599999 1.951246) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(TP22-Pad1)"))
    (pad 10 smd rect (at -1.000001 1.951246) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(TP20-Pad1)"))
    (pad 9 smd rect (at -1.4 2.00102) (size 0.192474 0.91009) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(TP14-Pad1)"))
    (pad 8 smd rect (at -2.00102 1.4 90) (size 0.192474 0.91009) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 7 smd rect (at -1.951246 1.000001 90) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at -1.951246 0.599999 90) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C11-Pad1)"))
    (pad 5 smd rect (at -1.951246 0.2 90) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at -1.951246 -0.2 90) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C2-Pad2)"))
    (pad 3 smd rect (at -1.951246 -0.599999 90) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at -1.951246 -1.000001 90) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -2.048942 -1.4) (size 0.814189 0.192474) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C14-Pad2)"))
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 128.486 112.73 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R16 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.12 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 126.111 129.498 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R15 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C11-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 602AACD0)
    (at 127.254 129.498 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R14 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R14-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res2512W (layer F.Cu) (tedit 58A46288)
    (at 126.873 135.001 270)
    (fp_text reference R8 (at 0.2 0.1 90) (layer F.SilkS))
    (fp_text value 100 (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 1.5 270) (size 7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 -1.5 270) (size 7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R14-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/R2512W.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 118.486 123.73)
    (descr "SMT capacitor, 0402")
    (fp_text reference R6 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R6-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 118.486 121.23)
    (descr "SMT capacitor, 0402")
    (fp_text reference R5 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R5-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 118.486 118.73)
    (descr "SMT capacitor, 0402")
    (fp_text reference R4 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R4-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 118.486 116.23)
    (descr "SMT capacitor, 0402")
    (fp_text reference R3 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R3-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_smd_transistors:sc70 (layer F.Cu) (tedit 5B9F0B6A)
    (at 130.486 101.23 90)
    (descr SC70)
    (fp_text reference Q7 (at 0 -0.3302 90) (layer F.SilkS))
    (fp_text value BSS-123 (at 0 0.3302 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.6604 1.016 90) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(Q7-Pad1)"))
    (pad 2 smd rect (at 0.6604 1.016 90) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (pad 3 smd rect (at 0 -1.016 90) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (model ${T_LIBS}/3d/t_smd_transistors/SC-70.stp
      (offset (xyz -0.635 -1.143 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_smd_transistors:PQFN_3x3 (layer F.Cu) (tedit 5BB76E5A)
    (at 138.8835 101.6525 270)
    (fp_text reference Q4 (at 2.73304 -2.42824 90) (layer F.SilkS))
    (fp_text value N_MOS_8 (at 0.2 0.1 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0 90) (layer F.Fab))
    (pad 9 smd rect (at 0.6 -0.5 270) (size 1 1) (layers F.Paste))
    (pad 9 smd rect (at -0.6 -0.5 270) (size 1 1) (layers F.Paste))
    (pad 8 smd rect (at 0 -0.8 270) (size 2.25 1.7) (layers F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 8 smd rect (at -1 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 7 smd rect (at -0.333 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 6 smd rect (at 0.333 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 5 smd rect (at 1 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 4 smd rect (at 1 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at 0.333 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at -0.333 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (pad 1 smd rect (at -1 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (model ${T_LIBS}/3d/t_smd_transistors/TDFN-8-EP_3x3mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module t_smd_transistors:PQFN_3x3 (layer F.Cu) (tedit 5BB76E5A)
    (at 143.986 106.73 270)
    (fp_text reference Q2 (at 2.73304 -2.42824 90) (layer F.SilkS))
    (fp_text value P_MOS_8 (at 0.2 0.1 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0 90) (layer F.Fab))
    (pad 9 smd rect (at 0.6 -0.5 270) (size 1 1) (layers F.Paste))
    (pad 9 smd rect (at -0.6 -0.5 270) (size 1 1) (layers F.Paste))
    (pad 8 smd rect (at 0 -0.8 270) (size 2.25 1.7) (layers F.Mask)
      (net 17 "Net-(Q2-Pad5)"))
    (pad 8 smd rect (at -1 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q2-Pad5)"))
    (pad 7 smd rect (at -0.333 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q2-Pad5)"))
    (pad 6 smd rect (at 0.333 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q2-Pad5)"))
    (pad 5 smd rect (at 1 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q2-Pad5)"))
    (pad 4 smd rect (at 1 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q2-Pad4)"))
    (pad 3 smd rect (at 0.333 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 2 smd rect (at -0.333 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 1 smd rect (at -1 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (model ${T_LIBS}/3d/t_smd_transistors/TDFN-8-EP_3x3mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module t_smd_transistors:PQFN_3x3 (layer F.Cu) (tedit 5BB76E5A)
    (at 138.8835 106.73 270)
    (fp_text reference Q1 (at 2.73304 -2.42824 90) (layer F.SilkS))
    (fp_text value N_MOS_8 (at 0.2 0.1 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0 90) (layer F.Fab))
    (pad 9 smd rect (at 0.6 -0.5 270) (size 1 1) (layers F.Paste))
    (pad 9 smd rect (at -0.6 -0.5 270) (size 1 1) (layers F.Paste))
    (pad 8 smd rect (at 0 -0.8 270) (size 2.25 1.7) (layers F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 8 smd rect (at -1 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 7 smd rect (at -0.333 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 6 smd rect (at 0.333 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 5 smd rect (at 1 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad5)"))
    (pad 4 smd rect (at 1 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q1-Pad4)"))
    (pad 3 smd rect (at 0.333 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -0.333 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C10-Pad1)"))
    (pad 1 smd rect (at -1 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C10-Pad1)"))
    (model ${T_LIBS}/3d/t_smd_transistors/TDFN-8-EP_3x3mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Fuse:Fuse_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 132.986 107.23)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags fuse)
    (attr smd)
    (fp_text reference F1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value FUSE (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(C10-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 134.8555 101.4025 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value Diode_TVS_SMA (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 128.486 108.28 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value Diode_TVS_SMA (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 124.968 126.661 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C11 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C11-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 126.851 126.833)
    (descr "SMT capacitor, 0402")
    (fp_text reference C9 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 126.958 124.714)
    (descr "SMT capacitor, 0402")
    (fp_text reference C8 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 100pF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 128.651 126.661 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C7 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 120.986 121.78 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C6 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C2-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 120.986 116.78 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C5 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 120.986 124.28 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C3 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 120.986 119.28 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C2 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 107.315 146.685) (end 107.315 94.615) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 159.385 146.685) (end 107.315 146.685) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 159.385 94.615) (end 159.385 146.685) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 107.315 94.615) (end 159.385 94.615) (layer Edge.Cuts) (width 0.05))
  (zone (net 17) (net_name "Net-(Q2-Pad5)") (layer F.Cu) (hatch edge 0.508)
    (priority 100)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.923 107.823) (xy 143.891 107.823) (xy 143.891 105.537) (xy 145.923 105.537)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 50)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.75 146.05) (xy 107.95 146.05) (xy 107.95 95.25) (xy 158.75 95.25)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 100)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.75 146.05) (xy 107.95 146.05) (xy 107.95 95.25) (xy 142.875 95.25) (xy 158.75 95.25)
      )
    )
  )
  (zone (net 35) (net_name "Net-(Q1-Pad5)") (layer F.Cu) (hatch edge 0.508)
    (priority 100)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.859 105.3465) (xy 143.129 105.3465) (xy 143.129 107.2515) (xy 141.478 107.188) (xy 141.478 107.8865)
        (xy 138.8745 107.823) (xy 138.811 100.457) (xy 141.859 100.457)
      )
    )
  )
)
