(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4~bpo8+1)
  (general
    (links 119)
    (no_connects 2)
    (area 86.150001 57.3 171.723829 101.2274)
    (thickness 1.6)
    (drawings 15)
    (tracks 198)
    (zones 0)
    (modules 54)
    (nets 27)
  )
  (page USLetter)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 100 70)
    (visible_elements FFFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Earth)
  (net 2 /ID_SD)
  (net 3 /ID_SC)
  (net 4 +3V3)
  (net 5 /V+_UNREG)
  (net 6 "Net-(D2-Pad2)")
  (net 7 /VIN+)
  (net 8 /VIN-)
  (net 9 "Net-(JP1-Pad1)")
  (net 10 "Net-(JP2-Pad1)")
  (net 11 "Net-(Q2-Pad1)")
  (net 12 +5V)
  (net 13 /SDA)
  (net 14 /SCL)
  (net 15 "Net-(C2-Pad1)")
  (net 16 "Net-(C2-Pad2)")
  (net 17 "Net-(C3-Pad1)")
  (net 18 "Net-(D1-Pad2)")
  (net 19 "Net-(R8-Pad1)")
  (net 20 "Net-(R9-Pad2)")
  (net 21 /Power/5V_REG)
  (net 22 /Power/V+_PROT)
  (net 23 "Net-(C10-Pad1)")
  (net 24 "Net-(C11-Pad1)")
  (net 25 "Net-(C11-Pad2)")
  (net 26 "Net-(C13-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /ID_SC)
    (add_net /ID_SD)
    (add_net /SCL)
    (add_net /SDA)
    (add_net Earth)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad2)")
  )
  (net_class LowImp ""
    (clearance 0.1524)
    (trace_width 0.75)
    (via_dia 0.9)
    (via_drill 0.6)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net +5V)
    (add_net /Power/5V_REG)
    (add_net /Power/V+_PROT)
    (add_net /V+_UNREG)
    (add_net /VIN+)
    (add_net /VIN-)
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
  )
  (module Housings_SSOP:TSSOP-16-1EP_4.4x5mm_Pitch0.65mm (layer Top) (tedit 54130A77)
    (at 123.25 94 270)
    (descr "FE Package; 16-Lead Plastic TSSOP (4.4mm); Exposed Pad Variation BB; (see Linear Technology 1956f.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at -3.25 4 360) (layer F.SilkS))
    (fp_text value LM43600 (at 0 3.55 270) (layer F.Fab))
    (pad 1 smd rect (at -2.775 -2.275 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 25 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at -2.775 -1.625 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 25 "Net-(C11-Pad2)"))
    (pad 3 smd rect (at -2.775 -0.975 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 24 "Net-(C11-Pad1)"))
    (pad 4 smd rect (at -2.775 -0.325 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 23 "Net-(C10-Pad1)"))
    (pad 5 smd rect (at -2.775 0.325 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 21 /Power/5V_REG))
    (pad 6 smd rect (at -2.775 0.975 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (pad 7 smd rect (at -2.775 1.625 270) (size 1.05 0.45) (layers Top F.Paste F.Mask))
    (pad 8 smd rect (at -2.775 2.275 270) (size 1.05 0.45) (layers Top F.Paste F.Mask))
    (pad 9 smd rect (at 2.775 2.275 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 26 "Net-(C13-Pad2)"))
    (pad 10 smd rect (at 2.775 1.625 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (pad 11 smd rect (at 2.775 0.975 270) (size 1.05 0.45) (layers Top F.Paste F.Mask))
    (pad 12 smd rect (at 2.775 0.325 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 22 /Power/V+_PROT))
    (pad 13 smd rect (at 2.775 -0.325 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 22 /Power/V+_PROT))
    (pad 14 smd rect (at 2.775 -0.975 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 22 /Power/V+_PROT))
    (pad 15 smd rect (at 2.775 -1.625 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (pad 16 smd rect (at 2.775 -2.275 270) (size 1.05 0.45) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (pad 17 smd rect (at 0.735 1.3425 270) (size 1.47 0.895) (layers Top F.Paste F.Mask)
      (net 1 Earth) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.735 0.4475 270) (size 1.47 0.895) (layers Top F.Paste F.Mask)
      (net 1 Earth) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.735 -0.4475 270) (size 1.47 0.895) (layers Top F.Paste F.Mask)
      (net 1 Earth) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.735 -1.3425 270) (size 1.47 0.895) (layers Top F.Paste F.Mask)
      (net 1 Earth) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.735 1.3425 270) (size 1.47 0.895) (layers Top F.Paste F.Mask)
      (net 1 Earth) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.735 0.4475 270) (size 1.47 0.895) (layers Top F.Paste F.Mask)
      (net 1 Earth) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.735 -0.4475 270) (size 1.47 0.895) (layers Top F.Paste F.Mask)
      (net 1 Earth) (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.735 -1.3425 270) (size 1.47 0.895) (layers Top F.Paste F.Mask)
      (net 1 Earth) (solder_paste_margin_ratio -0.2))
    (model Housings_SSOP.3dshapes/TSSOP-16-1EP_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_lib:VIA-0.6mm (layer Top) (tedit 58CA2173)
    (at 124.25 95)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 Earth) (zone_connect 2))
  )
  (module local_lib:VIA-0.6mm (layer Top) (tedit 58CA2173)
    (at 123.25 95)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 Earth) (zone_connect 2))
  )
  (module local_lib:VIA-0.6mm (layer Top) (tedit 58CA2173)
    (at 122.25 95)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 Earth) (zone_connect 2))
  )
  (module local_lib:VIA-0.6mm (layer Top) (tedit 58CA2173)
    (at 124.25 94)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 Earth) (zone_connect 2))
  )
  (module local_lib:VIA-0.6mm (layer Top) (tedit 58CA2173)
    (at 123.25 94)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 Earth) (zone_connect 2))
  )
  (module local_lib:VIA-0.6mm (layer Top) (tedit 58CA2173)
    (at 122.25 94)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 Earth) (zone_connect 2))
  )
  (module local_lib:VIA-0.6mm (layer Top) (tedit 58CA2173)
    (at 124.25 93)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 Earth) (zone_connect 2))
  )
  (module local_lib:VIA-0.6mm (layer Top) (tedit 58CA2173)
    (at 123.25 93)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 Earth) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58AA84A8)
    (at 131.5 94 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -3.5 0 270) (layer F.SilkS))
    (fp_text value 4u7 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 22 /Power/V+_PROT))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_lib:Socket_Strip_Straight_2x20_Pitch2.54mm (layer Bottom) (tedit 58C865E8)
    (at 132.5 73.5)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference J2 (at -26.46 3.5) (layer F.SilkS))
    (fp_text value Raspberry_Pi_2_3 (at 0 3.81) (layer B.Fab))
    (pad 1 thru_hole rect (at -24.13 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at -24.13 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 +5V))
    (pad 3 thru_hole oval (at -21.59 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /SDA))
    (pad 4 thru_hole oval (at -21.59 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 +5V))
    (pad 5 thru_hole oval (at -19.05 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /SCL))
    (pad 6 thru_hole oval (at -19.05 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 7 thru_hole oval (at -16.51 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at -16.51 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at -13.97 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 10 thru_hole oval (at -13.97 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at -11.43 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at -11.43 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at -8.89 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at -8.89 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 15 thru_hole oval (at -6.35 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at -6.35 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at -3.81 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 18 thru_hole oval (at -3.81 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at -1.27 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at -1.27 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 21 thru_hole oval (at 1.27 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 1.27 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 3.81 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 3.81 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 6.35 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 26 thru_hole oval (at 6.35 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 8.89 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /ID_SD))
    (pad 28 thru_hole oval (at 8.89 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /ID_SC))
    (pad 29 thru_hole oval (at 11.43 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at 11.43 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 31 thru_hole oval (at 13.97 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at 13.97 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 33 thru_hole oval (at 16.51 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 34 thru_hole oval (at 16.51 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 35 thru_hole oval (at 19.05 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at 19.05 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 21.59 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 21.59 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 24.13 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 40 thru_hole oval (at 24.13 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 105.5 83.25)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -3.49942 0.01191) (layer F.SilkS))
    (fp_text value 1k0 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 20 "Net-(R9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer Top) (tedit 54130A77)
    (at 147 84 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -3.5 270) (layer F.SilkS))
    (fp_text value INA219 (at 0 3.5 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 16 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 15 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 4 +3V3))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 14 /SCL))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 13 /SDA))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 9 "Net-(JP1-Pad1)"))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 10 "Net-(JP2-Pad1)"))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer Top) (tedit 58C9FDA6)
    (at 161.5 96.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (fp_text reference MHSE (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer Top) (tedit 58C9FD9D)
    (at 103.5 96.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (fp_text reference MHSW (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer Top) (tedit 58C9FD8C)
    (at 161.5 73.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (fp_text reference MHNE (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu))
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 58AAD9A4)
    (at 150.5 86.5)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference JP1 (at 3 0) (layer F.SilkS))
    (fp_text value A0 (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 9 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 1 Earth))
  )
  (module Resistors_SMD:R_0402 (layer Top) (tedit 58AAD9A4)
    (at 150.5 88)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference JP2 (at 3 0) (layer F.SilkS))
    (fp_text value A1 (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 10 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers Top F.Paste F.Mask)
      (net 1 Earth))
  )
  (module _div:_FAIRCHILD-MOSFET-SuperSOT-6 (layer Top) (tedit 58C8246E)
    (at 140 92.75 180)
    (fp_text reference Q1 (at 1 -4.75 450) (layer F.SilkS))
    (fp_text value FDC602P (at 1 -4.62 180) (layer F.Fab))
    (pad S smd rect (at 1.9 -2.62 180) (size 0.62 1.22) (layers Top F.Paste F.Mask)
      (net 22 /Power/V+_PROT))
    (pad D smd rect (at 0.95 -2.62 180) (size 0.62 1.22) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (pad G smd rect (at 1.9 0 180) (size 0.62 1.22) (layers Top F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad D smd rect (at 0 -2.62 180) (size 0.62 1.22) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (pad D smd rect (at 0.95 0 180) (size 0.62 1.22) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (pad D smd rect (at 0 0 180) (size 0.62 1.22) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0.035 0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58AA84A8)
    (at 147 79)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58C8665B)
    (at 152.5 82.46 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.5 -0.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 15 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 16 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_6.3x5.7 (layer Top) (tedit 58AA8B43)
    (at 147 95 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.7")
    (attr smd)
    (fp_text reference C3 (at -6 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 -4.56 270) (layer F.Fab))
    (fp_text user + (at -1.79 -0.06 270) (layer F.Fab))
    (fp_text user + (at -4.28 3.01 270) (layer F.SilkS))
    (fp_text user %R (at 0 4.56 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0 90) (size 3.5 1.6) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2.7 0 90) (size 3.5 1.6) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58AA84A8)
    (at 142 94 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 3.5 0 450) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58AA84A8)
    (at 103.51191 89.49942 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 3 0 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Standard (layer Top) (tedit 586432E5)
    (at 152.5 95 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at -5 0 360) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 4.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers Top F.Paste F.Mask)
      (net 17 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers Top F.Paste F.Mask)
      (net 18 "Net-(D1-Pad2)"))
    (model Diodes_SMD.3dshapes/SMA_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer Top) (tedit 58645DC7)
    (at 133.5 94 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at -3.5 0 270) (layer F.SilkS))
    (fp_text value MMSZ5256 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers Top F.Paste F.Mask)
      (net 22 /Power/V+_PROT))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers Top F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.2 1.2 1.2))
      (rotate (xyz 0 0 0))
    )
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuse_SMD1206_HandSoldering (layer Top) (tedit 58C86671)
    (at 156 94.91 90)
    (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann 433 Series, Hand Soldering,")
    (tags "Fuse Sicherung SMD1206 Littlefuse-Wickmann 433 Series Hand Soldering ")
    (attr smd)
    (fp_text reference F1 (at 5 0 180) (layer F.SilkS))
    (fp_text value 800mA (at -0.15 2.5 90) (layer F.Fab))
    (pad 1 smd rect (at -2.09 0 180) (size 2.03 2.65) (layers Top F.Paste F.Mask)
      (net 18 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2.09 0 180) (size 2.03 2.65) (layers Top F.Paste F.Mask)
      (net 5 /V+_UNREG))
    (model SMD_Packages.3dshapes/SMD-1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.16 0.17 0.17))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_4pol (layer Top) (tedit 58C85F53)
    (at 162.5 88.81 90)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J1 (at -3.19 0 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x04 (at 3.81 4.50088 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 7 /VIN+))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 5 /V+_UNREG))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 8 /VIN-))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_4pol.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer Top) (tedit 58CA1389)
    (at 117.75 81 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 1.75 1.75 180) (layer F.SilkS))
    (fp_text value DMG2305UX (at 0 2.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers Top F.Paste F.Mask)
      (net 11 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers Top F.Paste F.Mask)
      (net 12 +5V))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers Top F.Paste F.Mask)
      (net 21 /Power/5V_REG))
    (model TO_SOT_Packages_SMD.3dshapes\SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 156.5 81.19 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 1.5 2.19 180) (layer F.SilkS))
    (fp_text value 10 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 7 /VIN+))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 16 "Net-(C2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 156.5 83.73 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -1.5 4.73 180) (layer F.SilkS))
    (fp_text value 10 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 8 /VIN-))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 15 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 141 84.5 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -4 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 13 /SDA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 143 84.5 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -4 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 14 /SCL))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 139 84.5 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -4 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 9 "Net-(JP1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 137 84.5 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -4 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 10 "Net-(JP2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 136 94 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.5 0 450) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 113.5 77.5)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 3.25 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 19 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 108.25 81)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at -3.99942 0.01191) (layer F.SilkS))
    (fp_text value 3k9 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 3 /ID_SC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 108.25 79)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at -3.99942 0.01191 180) (layer F.SilkS))
    (fp_text value 3k9 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 2 /ID_SD))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58CA1332)
    (at 113.5 83.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 3.75 -1 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 11 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer Top) (tedit 54130A77)
    (at 107.51191 89.49942 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at -4.75058 -0.01191 180) (layer F.SilkS))
    (fp_text value 24LC04 (at 0 3.5 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 2 /ID_SD))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 3 /ID_SC))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 20 "Net-(R9-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers Top F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6_Handsoldering (layer Top) (tedit 5883693A)
    (at 113.5 80.5)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U5 (at -3.75 2.5 180) (layer F.SilkS))
    (fp_text value DMMT5401 (at 0 2.9) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers Top F.Paste F.Mask)
      (net 19 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers Top F.Paste F.Mask)
      (net 19 "Net-(R8-Pad1)"))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers Top F.Paste F.Mask)
      (net 19 "Net-(R8-Pad1)"))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers Top F.Paste F.Mask)
      (net 11 "Net-(Q2-Pad1)"))
    (pad 6 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers Top F.Paste F.Mask)
      (net 21 /Power/5V_REG))
    (pad 5 smd rect (at 1.35 0) (size 1.56 0.65) (layers Top F.Paste F.Mask)
      (net 12 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer Top) (tedit 58C9FD70)
    (at 103.5 73.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (fp_text reference MHNW (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58AA84A8)
    (at 129.5 94 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -3.5 0 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 22 /Power/V+_PROT))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58AA84A8)
    (at 113.5 90 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 1.5 -1.75 180) (layer F.SilkS))
    (fp_text value 2u2 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 23 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58AA84A8)
    (at 127.5 91.5 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 1.25 2.5 180) (layer F.SilkS))
    (fp_text value 470n (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 24 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 25 "Net-(C11-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58AA84A8)
    (at 113.5 85.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at -4 0 360) (layer F.SilkS))
    (fp_text value 4u7 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 21 /Power/5V_REG))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58AA84A8)
    (at 115 94 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 4 0 450) (layer F.SilkS))
    (fp_text value 18p (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 21 /Power/5V_REG))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 26 "Net-(C13-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58AA84A8)
    (at 113.5 87.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at -4 0 360) (layer F.SilkS))
    (fp_text value 22u (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 21 /Power/5V_REG))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 117 94 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 4 0 270) (layer F.SilkS))
    (fp_text value 1M (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 21 /Power/5V_REG))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 26 "Net-(C13-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58AADA1D)
    (at 119 94 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at -4 0 90) (layer F.SilkS))
    (fp_text value 255k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 26 "Net-(C13-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 1 Earth))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_lib:VIA-0.6mm (layer Top) (tedit 58CA2173)
    (at 122.25 93)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 Earth) (zone_connect 2))
  )
  (module Symbols:OSHW-Logo2_14.6x12mm_SilkScreen (layer Bottom) (tedit 0)
    (at 132.5 82 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module local_lib:WE-SPC_4838 (layer Top) (tedit 58CDEA07)
    (at 123 86 180)
    (fp_text reference L1 (at 0 4 180) (layer F.SilkS))
    (fp_text value L (at 0 -4 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.75 180) (size 5.3 2) (layers Top F.Paste F.Mask)
      (net 25 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 0 1.75 180) (size 5.3 2) (layers Top F.Paste F.Mask)
      (net 21 /Power/5V_REG))
    (model Inductors.3dshapes/self_cms_we-tpc_XL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "Raspberry Pi Zero Power Monitor Hat\nRev. 0 (Prototype)" (at 132.5 91) (layer B.SilkS))
  (dimension 23 (width 0.3) (layer Dwgs.User)
    (gr_text "23.000 mm" (at 96.65 85 270) (layer Dwgs.User))
    (feature1 (pts (xy 103.5 96.5) (xy 95.3 96.5)))
    (feature2 (pts (xy 103.5 73.5) (xy 95.3 73.5)))
    (crossbar (pts (xy 98 73.5) (xy 98 96.5)))
    (arrow1a (pts (xy 98 96.5) (xy 97.413579 95.373496)))
    (arrow1b (pts (xy 98 96.5) (xy 98.586421 95.373496)))
    (arrow2a (pts (xy 98 73.5) (xy 97.413579 74.626504)))
    (arrow2b (pts (xy 98 73.5) (xy 98.586421 74.626504)))
  )
  (dimension 30 (width 0.3) (layer Dwgs.User)
    (gr_text "30.000 mm" (at 92.65 85 270) (layer Dwgs.User))
    (feature1 (pts (xy 103.5 100) (xy 91.3 100)))
    (feature2 (pts (xy 103.5 70) (xy 91.3 70)))
    (crossbar (pts (xy 94 70) (xy 94 100)))
    (arrow1a (pts (xy 94 100) (xy 93.413579 98.873496)))
    (arrow1b (pts (xy 94 100) (xy 94.586421 98.873496)))
    (arrow2a (pts (xy 94 70) (xy 93.413579 71.126504)))
    (arrow2b (pts (xy 94 70) (xy 94.586421 71.126504)))
  )
  (dimension 3.5 (width 0.3) (layer Dwgs.User)
    (gr_text "3.500 mm" (at 96.65 71.75 90) (layer Dwgs.User))
    (feature1 (pts (xy 103.5 70) (xy 95.3 70)))
    (feature2 (pts (xy 103.5 73.5) (xy 95.3 73.5)))
    (crossbar (pts (xy 98 73.5) (xy 98 70)))
    (arrow1a (pts (xy 98 70) (xy 98.586421 71.126504)))
    (arrow1b (pts (xy 98 70) (xy 97.413579 71.126504)))
    (arrow2a (pts (xy 98 73.5) (xy 98.586421 72.373496)))
    (arrow2b (pts (xy 98 73.5) (xy 97.413579 72.373496)))
  )
  (dimension 58 (width 0.3) (layer Dwgs.User)
    (gr_text "58.000 mm" (at 132.5 61.65) (layer Dwgs.User))
    (feature1 (pts (xy 161.5 73.5) (xy 161.5 60.3)))
    (feature2 (pts (xy 103.5 73.5) (xy 103.5 60.3)))
    (crossbar (pts (xy 103.5 63) (xy 161.5 63)))
    (arrow1a (pts (xy 161.5 63) (xy 160.373496 63.586421)))
    (arrow1b (pts (xy 161.5 63) (xy 160.373496 62.413579)))
    (arrow2a (pts (xy 103.5 63) (xy 104.626504 63.586421)))
    (arrow2b (pts (xy 103.5 63) (xy 104.626504 62.413579)))
  )
  (dimension 65 (width 0.3) (layer Dwgs.User)
    (gr_text "65.000 mm" (at 132.5 58.65) (layer Dwgs.User))
    (feature1 (pts (xy 165 72.5) (xy 165 57.3)))
    (feature2 (pts (xy 100 72.5) (xy 100 57.3)))
    (crossbar (pts (xy 100 60) (xy 165 60)))
    (arrow1a (pts (xy 165 60) (xy 163.873496 60.586421)))
    (arrow1b (pts (xy 165 60) (xy 163.873496 59.413579)))
    (arrow2a (pts (xy 100 60) (xy 101.126504 60.586421)))
    (arrow2b (pts (xy 100 60) (xy 101.126504 59.413579)))
  )
  (dimension 29 (width 0.3) (layer Dwgs.User)
    (gr_text "29.000 mm" (at 118 66.65) (layer Dwgs.User))
    (feature1 (pts (xy 132.5 73.5) (xy 132.5 65.3)))
    (feature2 (pts (xy 103.5 73.5) (xy 103.5 65.3)))
    (crossbar (pts (xy 103.5 68) (xy 132.5 68)))
    (arrow1a (pts (xy 132.5 68) (xy 131.373496 68.586421)))
    (arrow1b (pts (xy 132.5 68) (xy 131.373496 67.413579)))
    (arrow2a (pts (xy 103.5 68) (xy 104.626504 68.586421)))
    (arrow2b (pts (xy 103.5 68) (xy 104.626504 67.413579)))
  )
  (gr_line (start 165 73) (end 165 97) (angle 90) (layer Edge.Cuts) (width 0.00001))
  (gr_arc (start 162 73) (end 162 70) (angle 90) (layer Edge.Cuts) (width 0.00001))
  (gr_line (start 103 100) (end 162 100) (angle 90) (layer Edge.Cuts) (width 0.00001))
  (gr_arc (start 162 97) (end 165 97) (angle 90) (layer Edge.Cuts) (width 0.00001))
  (gr_line (start 100 73) (end 100 97) (angle 90) (layer Edge.Cuts) (width 0.00001))
  (gr_arc (start 103 97) (end 103 100) (angle 90) (layer Edge.Cuts) (width 0.00001))
  (gr_line (start 103 70) (end 162 70) (angle 90) (layer Edge.Cuts) (width 0.00001))
  (gr_arc (start 103 73) (end 100 73) (angle 90) (layer Edge.Cuts) (width 0.00001))
  (zone (net 1) (net_name Earth) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100 70) (xy 165 70) (xy 165 100) (xy 100 100)
      )
    )
  )
  (zone (net 1) (net_name Earth) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100 70) (xy 165 70) (xy 165 100) (xy 100 100)
      )
    )
  )
  (zone (net 1) (net_name Earth) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 124.65 96.25) (xy 125.75 96.25) (xy 125.75 97.3) (xy 124.65 97.3)
      )
    )
  )
  (zone (net 25) (net_name "Net-(C11-Pad2)") (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 125.75 90.7) (xy 124.65 90.7) (xy 124.65 91.75) (xy 125.75 91.75)
      )
    )
  )
  (zone (net 22) (net_name /Power/V+_PROT) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.0255))
    (polygon
      (pts
        (xy 122.7 96.25) (xy 124.45 96.25) (xy 124.45 97.3) (xy 122.7 97.3)
      )
    )
  )
)
