(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6002)
    (drawings 101)
    (tracks 471)
    (zones 0)
    (modules 18)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/"))
  )
  (net 0 "")
  (net 1 /Gnd)
  (net 2 /+5V)
  (net 3 /Din)
  (net 4 /HV7)
  (net 5 /HV1)
  (net 6 /HV8)
  (net 7 /HV2)
  (net 8 /HV9)
  (net 9 /HV3)
  (net 10 /HV10)
  (net 11 /HV4)
  (net 12 /HV11)
  (net 13 /HV5)
  (net 14 /HV12)
  (net 15 /HV6)
  (net 16 /Anode)
  (net 17 "Net-(J5-Pad20)")
  (net 18 "Net-(J5-Pad19)")
  (net 19 "Net-(J6-Pad20)")
  (net 20 "Net-(J6-Pad19)")
  (net 21 /ClockHV)
  (net 22 /ExtHV)
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /+5V)
    (add_net /Anode)
    (add_net /ClockHV)
    (add_net /Din)
    (add_net /ExtHV)
    (add_net /Gnd)
    (add_net /HV1)
    (add_net /HV10)
    (add_net /HV11)
    (add_net /HV12)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net "Net-(J5-Pad19)")
    (add_net "Net-(J5-Pad20)")
    (add_net "Net-(J6-Pad19)")
    (add_net "Net-(J6-Pad20)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 5BD3AB2E)
    (at 187.96 76.2)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 5BD3AB20)
    (at 127 76.2)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 5BD3AB56)
    (at 172.72 110.49)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 5BD3AB4D)
    (at 142.24 110.49)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 5BD3AB68)
    (at 214.63 121.92)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 5BD3AB3B)
    (at 100.33 121.92)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 5BD3AB5E)
    (at 203.2 110.49)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_2x09_Pitch2.54mm (layer B.Cu) (tedit 5BD4748F)
    (at 162.56 78.74 270)
    (descr "Through hole straight socket strip, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x09 2.54mm double row")
    (fp_text reference J2 (at -1.27 2.33 270) (layer B.SilkS) hide)
    (fp_text value NX2 (at -5.08 -10.16) (layer B.SilkS) hide)
    (fp_text user %R (at -1.27 2.33 270) (layer B.Fab))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Gnd))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /+5V))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /HV7))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV1))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV8))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV2))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV9))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV3))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV10))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV4))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV11))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV5))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV12))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV6))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x09_Pitch2.54mm.wrl
      (offset (xyz -1.269999980926514 -10.15999984741211 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x09_Pitch2.54mm (layer B.Cu) (tedit 5BD47497)
    (at 132.08 78.74 270)
    (descr "Through hole straight socket strip, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x09 2.54mm double row")
    (fp_text reference J3 (at -1.27 2.33 270) (layer B.SilkS) hide)
    (fp_text value NX3 (at -5.08 -10.16) (layer B.SilkS) hide)
    (fp_text user %R (at -1.27 2.33 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV6))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV12))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV5))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV11))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV4))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV10))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV3))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV9))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV2))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV8))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV1))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /HV7))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /+5V))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Gnd))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x09_Pitch2.54mm.wrl
      (offset (xyz -1.269999980926514 -10.15999984741211 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x09_Pitch2.54mm (layer B.Cu) (tedit 5BD4749E)
    (at 101.6 78.74 270)
    (descr "Through hole straight socket strip, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x09 2.54mm double row")
    (fp_text reference J4 (at -1.27 2.33 270) (layer B.SilkS) hide)
    (fp_text value NX4 (at -5.08 -10.16) (layer B.SilkS) hide)
    (fp_text user %R (at -1.27 2.33 270) (layer B.Fab))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Gnd))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /+5V))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /HV7))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV1))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV8))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV2))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV9))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV3))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV10))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV4))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV11))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV5))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV12))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV6))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x09_Pitch2.54mm.wrl
      (offset (xyz -1.269999980926514 -10.15999984741211 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_2x10_Pitch2.54mm (layer F.Cu) (tedit 58CD5449)
    (at 105.41 93.98)
    (descr "Through hole angled socket strip, 2x10, 2.54mm pitch, 8.51mm socket length, double rows")
    (tags "Through hole angled socket strip THT 2x10 2.54mm double row")
    (fp_text reference J5 (at -5.65 -2.27) (layer F.SilkS))
    (fp_text value Out (at -5.65 25.13) (layer F.Fab))
    (fp_text user %R (at -5.65 -2.27) (layer F.Fab))
    (pad 20 thru_hole oval (at -2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J5-Pad20)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J5-Pad19)"))
    (pad 18 thru_hole oval (at -2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Gnd))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /+5V))
    (pad 16 thru_hole oval (at -2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 14 thru_hole oval (at -2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /HV7))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV1))
    (pad 12 thru_hole oval (at -2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV8))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV2))
    (pad 10 thru_hole oval (at -2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV9))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV3))
    (pad 8 thru_hole oval (at -2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV10))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV4))
    (pad 6 thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV11))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV5))
    (pad 4 thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV12))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV6))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Angled_2x10_Pitch2.54mm.wrl
      (offset (xyz -1.269999980926514 -11.42999982833862 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x10_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 208.28 93.98)
    (descr "Through hole angled pin header, 2x10, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x10 2.54mm double row")
    (fp_text reference J6 (at 5.655 -2.27) (layer F.SilkS))
    (fp_text value In (at 5.655 25.13) (layer F.Fab))
    (fp_text user %R (at 5.31 11.43 90) (layer F.Fab))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J6-Pad20)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J6-Pad19)"))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Gnd))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /+5V))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /HV7))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV1))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV8))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV2))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV9))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV3))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV10))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV4))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV11))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV5))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV12))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV6))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x09_Pitch2.54mm (layer B.Cu) (tedit 5BD47482)
    (at 193.04 78.74 270)
    (descr "Through hole straight socket strip, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x09 2.54mm double row")
    (fp_text reference J1 (at -1.27 2.33 270) (layer B.SilkS) hide)
    (fp_text value NX1 (at -5.08 -10.16) (layer B.SilkS) hide)
    (fp_text user %R (at -1.27 2.33 270) (layer B.Fab))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Gnd))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /+5V))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /HV7))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV1))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV8))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV2))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV9))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV3))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV10))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV4))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV11))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV5))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV12))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV6))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x09_Pitch2.54mm.wrl
      (offset (xyz -1.269999980926514 -10.15999984741211 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 5BD3AB44)
    (at 111.76 110.49)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 203.2 120.65 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5BD470FF)
    (at 129.54 88.9 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value HVX (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /ClockHV))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Anode))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /ExtHV))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 5BD470F1)
    (at 156.21 76.454 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J9 (at 4.385 -2.27 90) (layer F.SilkS) hide)
    (fp_text value "Ext HV" (at 4.385 4.81 90) (layer F.Fab))
    (fp_text user %R (at 2.77 1.27 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /ExtHV))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Gnd))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 5BD47111)
    (at 147.32 91.44 90)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J7 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Clock (at 1.27 22.65 90) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 180) (layer F.Fab))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Gnd))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /+5V))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Din))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /HV7))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV1))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV8))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV2))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV9))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV3))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV10))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV4))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV11))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV5))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV12))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV6))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /ClockHV))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /ClockHV))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Din (at 165.1 93.98) (layer F.SilkS))
  (gr_text Din (at 165.1 86.36) (layer F.SilkS))
  (gr_text 12 (at 149.86 86.36) (layer F.SilkS))
  (gr_text 10 (at 154.94 86.36) (layer F.SilkS))
  (gr_text 11 (at 152.4 86.36) (layer F.SilkS))
  (gr_text 9 (at 157.48 86.36) (layer F.SilkS))
  (gr_text 7 (at 162.56 86.36) (layer F.SilkS))
  (gr_text 8 (at 160.02 86.36) (layer F.SilkS))
  (gr_text 6 (at 149.86 93.98) (layer F.SilkS))
  (gr_text 5 (at 152.4 93.98) (layer F.SilkS))
  (gr_text 4 (at 154.94 93.98) (layer F.SilkS))
  (gr_text 3 (at 157.48 93.98) (layer F.SilkS))
  (gr_text 2 (at 160.02 93.98) (layer F.SilkS))
  (gr_text 1 (at 162.56 93.98) (layer F.SilkS))
  (gr_text 9 (at 111.76 73.66) (layer B.SilkS))
  (gr_text 7 (at 116.84 73.66) (layer B.SilkS))
  (gr_text Din (at 119.38 73.66) (layer B.SilkS))
  (gr_text Gnd (at 121.92 73.66) (layer B.SilkS))
  (gr_text 10 (at 109.22 73.66) (layer B.SilkS))
  (gr_text 8 (at 114.3 73.66) (layer B.SilkS))
  (gr_text 12 (at 104.14 73.66) (layer B.SilkS))
  (gr_text A (at 101.6 73.66) (layer B.SilkS))
  (gr_text 11 (at 106.68 73.66) (layer B.SilkS))
  (gr_text 11 (at 137.16 73.66) (layer B.SilkS))
  (gr_text 9 (at 142.24 73.66) (layer B.SilkS))
  (gr_text 10 (at 139.7 73.66) (layer B.SilkS))
  (gr_text Din (at 149.86 73.66) (layer B.SilkS))
  (gr_text A (at 132.08 73.66) (layer B.SilkS))
  (gr_text Gnd (at 152.4 73.66) (layer B.SilkS))
  (gr_text 12 (at 134.62 73.66) (layer B.SilkS))
  (gr_text 7 (at 147.32 73.66) (layer B.SilkS))
  (gr_text 8 (at 144.78 73.66) (layer B.SilkS))
  (gr_text 11 (at 167.64 73.66) (layer B.SilkS))
  (gr_text 9 (at 172.72 73.66) (layer B.SilkS))
  (gr_text 10 (at 170.18 73.66) (layer B.SilkS))
  (gr_text Din (at 180.34 73.66) (layer B.SilkS))
  (gr_text A (at 162.56 73.66) (layer B.SilkS))
  (gr_text Gnd (at 182.88 73.66) (layer B.SilkS))
  (gr_text 12 (at 165.1 73.66) (layer B.SilkS))
  (gr_text 7 (at 177.8 73.66) (layer B.SilkS))
  (gr_text 8 (at 175.26 73.66) (layer B.SilkS))
  (gr_text 9 (at 203.2 73.66) (layer B.SilkS))
  (gr_text Din (at 210.82 73.66) (layer B.SilkS))
  (gr_text Gnd (at 213.36 73.66) (layer B.SilkS))
  (gr_text 12 (at 195.58 73.66) (layer B.SilkS))
  (gr_text 11 (at 198.12 73.66) (layer B.SilkS))
  (gr_text 8 (at 205.74 73.66) (layer B.SilkS))
  (gr_text A (at 193.04 73.66) (layer B.SilkS))
  (gr_text 10 (at 200.66 73.66) (layer B.SilkS))
  (gr_text 7 (at 208.28 73.66) (layer B.SilkS))
  (gr_text 5 (at 198.12 81.28) (layer B.SilkS))
  (gr_text 4 (at 200.66 81.28) (layer B.SilkS))
  (gr_text Din (at 210.82 81.28) (layer B.SilkS))
  (gr_text A (at 193.04 81.28) (layer B.SilkS))
  (gr_text 1 (at 208.28 81.28) (layer B.SilkS))
  (gr_text 3 (at 203.2 81.28) (layer B.SilkS))
  (gr_text 2 (at 205.74 81.28) (layer B.SilkS))
  (gr_text 6 (at 195.58 81.28) (layer B.SilkS))
  (gr_text 5V (at 213.36 81.28) (layer B.SilkS))
  (gr_text 5 (at 167.64 81.28) (layer B.SilkS))
  (gr_text 6 (at 165.1 81.28) (layer B.SilkS))
  (gr_text 1 (at 177.8 81.28) (layer B.SilkS))
  (gr_text 4 (at 170.18 81.28) (layer B.SilkS))
  (gr_text 2 (at 175.26 81.28) (layer B.SilkS))
  (gr_text 5V (at 182.88 81.28) (layer B.SilkS))
  (gr_text Din (at 180.34 81.28) (layer B.SilkS))
  (gr_text A (at 162.56 81.28) (layer B.SilkS))
  (gr_text 3 (at 172.72 81.28) (layer B.SilkS))
  (gr_text 5 (at 137.16 81.28) (layer B.SilkS))
  (gr_text 1 (at 147.32 81.28) (layer B.SilkS))
  (gr_text 6 (at 134.62 81.28) (layer B.SilkS))
  (gr_text 5V (at 152.4 81.28) (layer B.SilkS))
  (gr_text A (at 132.08 81.28) (layer B.SilkS))
  (gr_text 2 (at 144.78 81.28) (layer B.SilkS))
  (gr_text Din (at 149.86 81.28) (layer B.SilkS))
  (gr_text 3 (at 142.24 81.28) (layer B.SilkS))
  (gr_text 4 (at 139.7 81.28) (layer B.SilkS))
  (gr_text 5V (at 121.92 81.28) (layer B.SilkS))
  (gr_text Din (at 119.38 81.28) (layer B.SilkS))
  (gr_text 1 (at 116.84 81.28) (layer B.SilkS))
  (gr_text 2 (at 114.3 81.28) (layer B.SilkS))
  (gr_text 3 (at 111.76 81.28) (layer B.SilkS))
  (gr_text 4 (at 109.22 81.28) (layer B.SilkS))
  (gr_text 5 (at 106.68 81.28) (layer B.SilkS))
  (gr_text 6 (at 104.14 81.28) (layer B.SilkS))
  (gr_text A (at 101.6 81.28) (layer B.SilkS))
  (gr_text Anode (at 107.315 93.98) (layer F.SilkS))
  (gr_text Anode (at 206.375 93.98) (layer F.SilkS))
  (gr_text "Anode\nSelect" (at 132.08 85.725) (layer F.SilkS))
  (gr_text ClockHV (at 134.62 90.805 270) (layer F.SilkS))
  (gr_text "Ext HV" (at 129.54 90.805 270) (layer F.SilkS))
  (gr_text "Ext HV" (at 158.75 78.105 270) (layer F.SilkS))
  (gr_text Gnd (at 156.21 78.105 270) (layer F.SilkS))
  (gr_text "nixies.us\nMulti-Board v0.1" (at 201.93 121.285) (layer B.Mask))
  (gr_text Gnd (at 169.545 88.9) (layer F.SilkS))
  (gr_text 5V (at 169.545 91.44) (layer F.SilkS))
  (gr_text ClockHV (at 145.415 90.17) (layer F.SilkS))
  (gr_line (start 218.44 72.39) (end 96.52 72.39) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 218.44 125.73) (end 218.44 72.39) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 96.52 125.73) (end 218.44 125.73) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 96.52 72.39) (end 96.52 125.73) (layer Edge.Cuts) (width 0.127))
  (zone (net 1) (net_name /Gnd) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.155 73.025) (xy 217.805 73.025) (xy 217.805 125.095) (xy 97.155 125.095)
      )
    )
  )
)
