(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 42)
    (zones 0)
    (modules 7)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J10-Pad4)")
  (net 2 "Net-(J10-Pad3)")
  (net 3 "Net-(J10-Pad1)")
  (net 4 "Net-(J10-Pad2)")
  (net 5 "Net-(J10-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J10-Pad3)")
    (add_net "Net-(J10-Pad4)")
    (add_net "Net-(J10-Pad5)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 27.94 49.53)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REFa (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 46.99 49.53)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REFb (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 46.99 100.33)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REFd (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 27.94 100.33)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REFc (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 41.91 64.77)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "MIDI EXT" (at 0 22.65) (layer F.Fab))
    (fp_text user %R (at 0 10.16 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J10-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J10-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J10-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J10-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J10-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J10-Pad4)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J10-Pad3)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J10-Pad2)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MJC:MIDI-5-pin-DIN-180 (layer F.Cu) (tedit 6063DE1F)
    (at 29.21 86.36 270)
    (fp_text reference J8 (at -6.825 -9.635 90) (layer F.SilkS))
    (fp_text value MIDI-IN (at -3.015 8.635 90) (layer F.Fab))
    (pad 3 thru_hole circle (at -7.5 -5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 5 -7.5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(J10-Pad1)"))
    (pad 5 thru_hole circle (at -5 -7.5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(J10-Pad2)"))
    (pad 1 thru_hole rect (at 7.5 -5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 -5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask))
    (pad E2 thru_hole circle (at 5.08 5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask))
    (pad E1 thru_hole circle (at -5.08 5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module MJC:MIDI-5-pin-DIN-180 (layer F.Cu) (tedit 6063DE1F)
    (at 29.21 63.5 270)
    (fp_text reference J9 (at -6.825 -9.635 90) (layer F.SilkS))
    (fp_text value MIDI-OUT (at -3.015 8.635 90) (layer F.Fab))
    (pad E1 thru_hole circle (at -5.08 5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask))
    (pad E2 thru_hole circle (at 5.08 5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 -5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(J10-Pad5)"))
    (pad 1 thru_hole rect (at 7.5 -5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -5 -7.5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J10-Pad4)"))
    (pad 4 thru_hole circle (at 5 -7.5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(J10-Pad3)"))
    (pad 3 thru_hole circle (at -7.5 -5 270) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask))
  )
  (gr_line (start 53.34 43.18) (end 53.34 106.68) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 21.59 43.18) (end 53.34 43.18) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 21.59 43.18) (end 21.59 106.68) (layer Edge.Cuts) (width 0.05))
  (gr_text . (at 39.37 63.5) (layer F.SilkS))
  (gr_text "MIDI\nIN" (at 24.13 99.06 90) (layer B.SilkS))
  (gr_text "MIDI\nOUT" (at 24.13 50.8 90) (layer B.SilkS))
  (gr_text "Off-board MIDI v1 - MJCulross (KD5RXT)" (at 50.8 74.93 90) (layer B.SilkS))
  (gr_text "Off-board MIDI v1 - MJCulross (KD5RXT)" (at 50.8 74.93 90) (layer F.SilkS))
  (gr_text 47 (at 33.02 81.28) (layer F.SilkS))
  (gr_text 47 (at 33.02 77.47) (layer F.SilkS))
  (gr_text "IN-4\n\nIN-5\n\nOUT-4\n\nOUT-5\n\nGND\n\nOUT-5\n\nOUT-4\n\nIN-5\n\nIN-4" (at 45.72 74.93) (layer F.SilkS))
  (gr_text "MIDI\nIN" (at 24.13 99.06 90) (layer F.SilkS))
  (gr_text "MIDI\nOUT" (at 24.13 50.8 90) (layer F.SilkS))
  (gr_line (start 53.34 106.68) (end 21.59 106.68) (layer Edge.Cuts) (width 0.05))
)
