(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers")
    )
  )
  (net 0 "")
  (net 1 "GNDREF")
  (net 2 "VCC")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(ATTINY85-Pad7)")
  (net 5 "Net-(ATTINY85-Pad3)")
  (net 6 "Net-(ATTINY85-Pad6)")
  (net 7 "Net-(ATTINY85-Pad2)")
  (net 8 "Net-(ATTINY85-Pad5)")
  (net 9 "Net-(ATTINY85-Pad1)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 175.925 149.5 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "attinyspeakersimple.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole roundrect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "GNDREF") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.00mm:PinSocket_1x02_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5A19A42F)
    (at 170.5 149.8 90)
    (descr "Through hole straight socket strip, 1x02, 2.00mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.00mm single row")
    (property "Sheetfile" "attinyspeakersimple.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -2.8 -2.3 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02" (at 0 4.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_1x02_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm_Socket" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 168.48 145.7 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "attinyspeakersimple.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "ATTINY85" (at 3.9 4.02 180) (layer "F.SilkS"))
    (fp_text value "ATtiny85-20PU" (at 3.81 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(ATTINY85-Pad1)") (pinfunction "~{RESET}/PB5") (pintype "bidirectional"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(ATTINY85-Pad2)") (pinfunction "XTAL1/PB3") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(ATTINY85-Pad3)") (pinfunction "XTAL2/PB4") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(ATTINY85-Pad5)") (pinfunction "AREF/PB0") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(ATTINY85-Pad6)") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(ATTINY85-Pad7)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 165.6 147.35 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "attinyspeakersimple.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Rfilt" (at 2.54 0.1 90) (layer "F.SilkS"))
    (fp_text value "68" (at 2.74 -1.2 90) (layer "F.Fab"))
    (fp_text user "Rfilt" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -0.15 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.2 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(ATTINY85-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 167.7 149.8 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "attinyspeakersimple.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 1.25 -1.1 unlocked) (layer "F.SilkS"))
    (fp_text value ".1" (at 1.25 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 182.88 149.3)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (property "Sheetfile" "attinyspeakersimple.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 182.88 134.62)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (property "Sheetfile" "attinyspeakersimple.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 165.4 140.1 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
    (property "Sheetfile" "attinyspeakersimple.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 1.3 1 90) (layer "F.SilkS"))
    (fp_text value ".1" (at 1.38 0.264 90) (layer "F.Fab"))
    (fp_text user "1uF" (at 1.25 -0.9 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 180.725 139.475)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "attinyspeakersimple.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "ICSP" (at 1.075 -2.175) (layer "B.SilkS"))
    (fp_text value "Conn_02x03_Odd_Even" (at 1.27 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(ATTINY85-Pad6)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(ATTINY85-Pad7)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(ATTINY85-Pad5)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(ATTINY85-Pad1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 165.9 134.6 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "attinyspeakersimple.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -3.1 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06" (at 0 15.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "GNDREF") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole rect (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(ATTINY85-Pad7)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(ATTINY85-Pad6)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(ATTINY85-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(ATTINY85-Pad2)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "attinyspeaker:makerlogo" (layer "B.Cu")
    (tedit 0)
    (at 171.4 142.8 180)
    (attr smd)
    (fp_text reference "REF**" (at 0.15 0 unlocked) (layer "B.SilkS") hide)
    (fp_text value "makerlogo" (at 0 -1 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab"))
  )
  (gr_line (start 164.1 151.4) (end 164.1 132.588) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 184.7088 132.588) (end 184.7088 151.4) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 184.7088 151.4) (end 164.1 151.4) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 164.1 132.588) (end 184.7088 132.588) (layer "Edge.Cuts") (width 0.05))
  (gr_text "+" (at 169.4 148.7) (layer "B.SilkS"))
  (gr_text "GND" (at 180.3 149.9 90) (layer "B.SilkS"))
  (gr_text "PB3" (at 178.7 133.1 180) (layer "B.SilkS"))
  (gr_text "SPKR" (at 171.5 148.2) (layer "B.SilkS"))
  (gr_text "PB1" (at 173.6 133.1468 180) (layer "B.SilkS"))
  (gr_text "-" (at 173.4 149 180) (layer "B.SilkS"))
  (gr_text "PB2" (at 171.1 133.1468 180) (layer "B.SilkS"))
  (gr_text "GND" (at 165.8 132.9944 180) (layer "B.SilkS"))
  (gr_text "VCC" (at 168.5 133.0452 180) (layer "B.SilkS"))
  (gr_text "VCC" (at 174.4388 149.7104 90) (layer "B.SilkS"))
  (gr_text "PB0" (at 176.1 133.1468 180) (layer "B.SilkS"))
  (gr_text "attiny85\naudio\nclass" (at 175.4 141.9) (layer "B.SilkS"))
  (gr_text "GND" (at 183.5 146.5) (layer "F.SilkS"))
  (gr_text "RST" (at 178.8 144.6 90) (layer "F.SilkS"))
  (gr_text "PB1" (at 173.4 136.144 -180) (layer "F.SilkS"))
  (gr_text "PB3" (at 178.8 136.1 180) (layer "F.SilkS"))
  (gr_text "-" (at 173.3 148.9 180) (layer "F.SilkS"))
  (gr_text "PB2" (at 171 136.144 -180) (layer "F.SilkS"))
  (gr_text "MOSI" (at 184.4 142 90) (layer "F.SilkS"))
  (gr_text "+" (at 169.5 148.7) (layer "F.SilkS"))
  (gr_text "SCK" (at 178.8 142 90) (layer "F.SilkS"))
  (gr_text "PB0" (at 176.1 136.0932 -180) (layer "F.SilkS"))
  (gr_text "VCC" (at 168.4 136.144 180) (layer "F.SilkS"))
  (gr_text "VCC" (at 183.4 137.6) (layer "F.SilkS"))
  (gr_text "GND" (at 165.9 136.144 180) (layer "F.SilkS"))
  (gr_text "+\n" (at 174.5388 148.5 90) (layer "F.SilkS"))
  (gr_text "-" (at 180 148.7 180) (layer "F.SilkS"))
  (gr_text "MISO" (at 178.8 139.2 90) (layer "F.SilkS"))
  (gr_text "BATTERY" (at 177.5 147.7) (layer "F.SilkS"))
  (zone (net 1) (net_name "GNDREF") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184.6 151.3)
        (xy 164.2 151.2)
        (xy 164.2 132.8)
        (xy 184.5 132.8)
      )
    )
  )
  (zone (net 1) (net_name "GNDREF") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184.6 151.2)
        (xy 164.3 151.2)
        (xy 164.3 132.8)
        (xy 184.5 132.8)
      )
    )
  )
)
