(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerber")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(AE1-Pad1)")
  (net 3 "+5V")
  (net 4 "Vdrive")
  (net 5 "Net-(U7-XTAL_OUT)")
  (net 6 "unconnected-(J1-Pin_45-Pad45)")
  (net 7 "unconnected-(J1-Pin_46-Pad46)")
  (net 8 "unconnected-(J1-Pin_47-Pad47)")
  (net 9 "unconnected-(J1-Pin_48-Pad48)")
  (net 10 "unconnected-(J1-Pin_49-Pad49)")
  (net 11 "Net-(J8-VBUS)")
  (net 12 "Earth")
  (net 13 "Net-(J9-Pin_1)")
  (net 14 "unconnected-(J9-Pin_35-Pad35)")
  (net 15 "unconnected-(J9-Pin_36-Pad36)")
  (net 16 "unconnected-(J9-Pin_37-Pad37)")
  (net 17 "unconnected-(J9-Pin_38-Pad38)")
  (net 18 "unconnected-(J9-Pin_39-Pad39)")
  (net 19 "unconnected-(J9-Pin_40-Pad40)")
  (net 20 "Net-(U6-Pin_4)")
  (net 21 "Net-(J12-CC1)")
  (net 22 "unconnected-(J12-SBU1-PadA8)")
  (net 23 "Net-(J12-CC2)")
  (net 24 "unconnected-(J12-SBU2-PadB8)")
  (net 25 "Net-(J13-VBUS)")
  (net 26 "Net-(U2-USBDM)")
  (net 27 "MMC3_D0")
  (net 28 "MMC3_D1")
  (net 29 "PC6")
  (net 30 "MMC3_D2")
  (net 31 "PC7")
  (net 32 "MMC3_CMD")
  (net 33 "PE0")
  (net 34 "MMC3_CK")
  (net 35 "PB6")
  (net 36 "MMC1_DETECT")
  (net 37 "PB8")
  (net 38 "Net-(U7-XTAL_IN)")
  (net 39 "Net-(U7-LNA)")
  (net 40 "UART1_TX")
  (net 41 "Net-(U4-VOUTR+)")
  (net 42 "UART1_RX")
  (net 43 "MMC3_D3")
  (net 44 "Net-(U4-VOUTL+)")
  (net 45 "unconnected-(U1-PB12-Pad118)")
  (net 46 "unconnected-(U1-PB10-Pad119)")
  (net 47 "unconnected-(U1-PE1-Pad12)")
  (net 48 "unconnected-(U1-PE4-Pad13)")
  (net 49 "unconnected-(U1-PC3-Pad120)")
  (net 50 "unconnected-(U1-PI8-Pad121)")
  (net 51 "unconnected-(U1-PB9-Pad16)")
  (net 52 "unconnected-(U1-PA4-Pad17)")
  (net 53 "unconnected-(U1-PA6-Pad18)")
  (net 54 "LCD_B0")
  (net 55 "LCD_B1")
  (net 56 "LCD_B2")
  (net 57 "LCD_B3")
  (net 58 "LCD_B4")
  (net 59 "LCD_B5")
  (net 60 "LCD_B6")
  (net 61 "LCD_B7")
  (net 62 "LCD_G0")
  (net 63 "LCD_G1")
  (net 64 "LCD_G2")
  (net 65 "LCD_G3")
  (net 66 "LCD_G4")
  (net 67 "LCD_G5")
  (net 68 "LCD_G6")
  (net 69 "LCD_G7")
  (net 70 "LCD_R0")
  (net 71 "LCD_R1")
  (net 72 "LCD_R2")
  (net 73 "LCD_R3")
  (net 74 "LCD_R4")
  (net 75 "LCD_R5")
  (net 76 "LCD_R6")
  (net 77 "LCD_R7")
  (net 78 "LCD_DATA_EN")
  (net 79 "LCD_V_SYNC")
  (net 80 "LCD_H_SYNC")
  (net 81 "LCD_CLK")
  (net 82 "/Audio/VCOM")
  (net 83 "BOOT1")
  (net 84 "BOOT0")
  (net 85 "BOOT2")
  (net 86 "unconnected-(U1-PD8-Pad57)")
  (net 87 "unconnected-(U1-PG3-Pad58)")
  (net 88 "SPI5_MOSI")
  (net 89 "SPI5_MISO")
  (net 90 "SPI5_CS")
  (net 91 "SPI5_CLK")
  (net 92 "unconnected-(U1-PB13-Pad66)")
  (net 93 "unconnected-(U1-PB5-Pad67)")
  (net 94 "UART4_RX")
  (net 95 "unconnected-(U1-PA12-Pad69)")
  (net 96 "unconnected-(U1-VBAT_RTC-Pad70)")
  (net 97 "CTP_INT")
  (net 98 "LCD_BL_EN")
  (net 99 "ANA0")
  (net 100 "ANA1")
  (net 101 "unconnected-(U1-VBUS_OTG-Pad84)")
  (net 102 "unconnected-(U1-ETH_MDIO-Pad85)")
  (net 103 "unconnected-(U1-ETH_MDC-Pad86)")
  (net 104 "unconnected-(U1-PG8-Pad88)")
  (net 105 "unconnected-(U1-ETH_TD3-Pad90)")
  (net 106 "unconnected-(U1-ETH_TD2-Pad91)")
  (net 107 "unconnected-(U1-ETH_TD1-Pad92)")
  (net 108 "unconnected-(U1-ETH_TD0-Pad93)")
  (net 109 "unconnected-(U1-ETH_TCTL-Pad94)")
  (net 110 "unconnected-(U1-ETH_TCLK-Pad95)")
  (net 111 "unconnected-(U1-ETH_RCLK-Pad97)")
  (net 112 "unconnected-(U1-ETH_RD3-Pad98)")
  (net 113 "unconnected-(U1-ETH_RD2-Pad99)")
  (net 114 "unconnected-(U1-ETH_RD1-Pad100)")
  (net 115 "unconnected-(U1-ETH_RD0-Pad101)")
  (net 116 "unconnected-(U1-ETH_RCTL-Pad102)")
  (net 117 "USB2_P")
  (net 118 "USB2_N")
  (net 119 "USB1_P")
  (net 120 "USB1_N")
  (net 121 "unconnected-(U1-PG5-Pad110)")
  (net 122 "WIFI_INT")
  (net 123 "unconnected-(U1-PA10-Pad123)")
  (net 124 "unconnected-(U1-PF13-Pad125)")
  (net 125 "unconnected-(U1-PF12-Pad126)")
  (net 126 "unconnected-(U1-PF10-Pad127)")
  (net 127 "unconnected-(U1-PI11-Pad122)")
  (net 128 "UART4_TX")
  (net 129 "unconnected-(U1-PA15-Pad130)")
  (net 130 "SWDIO")
  (net 131 "SWCLK")
  (net 132 "MMC1_D0")
  (net 133 "MMC1_D1")
  (net 134 "MMC1_D2")
  (net 135 "MMC1_D3")
  (net 136 "MMC1_CK")
  (net 137 "unconnected-(U1-PZ3-Pad141)")
  (net 138 "unconnected-(U1-PZ0-Pad144)")
  (net 139 "unconnected-(U1-PZ6-Pad145)")
  (net 140 "MMC1_CMD")
  (net 141 "unconnected-(U1-PZ7-Pad147)")
  (net 142 "unconnected-(U2-~{DTR}-Pad1)")
  (net 143 "unconnected-(U2-~{RTS}-Pad2)")
  (net 144 "unconnected-(U2-~{RI}-Pad5)")
  (net 145 "unconnected-(U2-~{DSR}-Pad7)")
  (net 146 "unconnected-(U2-~{DCD}-Pad8)")
  (net 147 "unconnected-(U2-~{CTS}-Pad9)")
  (net 148 "unconnected-(U2-CBUS2-Pad10)")
  (net 149 "unconnected-(U2-3V3OUT-Pad13)")
  (net 150 "unconnected-(U2-CBUS1-Pad17)")
  (net 151 "unconnected-(U2-CBUS0-Pad18)")
  (net 152 "unconnected-(U2-CBUS3-Pad19)")
  (net 153 "WIFI_UP")
  (net 154 "CTP_RESET")
  (net 155 "unconnected-(J5-SHIELD-PadP1)")
  (net 156 "I2C1_SCL")
  (net 157 "I2C1_SDA")
  (net 158 "Net-(D1-BA)")
  (net 159 "Net-(U1-USB1_N)")
  (net 160 "Net-(U1-USB1_P)")
  (net 161 "Net-(U1-USB2_N)")
  (net 162 "Net-(U1-USB2_P)")
  (net 163 "Net-(U2-USBDP)")
  (net 164 "Net-(D2-K)")
  (net 165 "/Power & Debug/USB_N")
  (net 166 "/Power & Debug/USB_P")
  (net 167 "Net-(D1-GA)")
  (net 168 "Net-(D1-RA)")
  (net 169 "LED_R")
  (net 170 "LED_G")
  (net 171 "LED_B")
  (net 172 "KEY_WP")
  (net 173 "Net-(U7-RES12K)")
  (net 174 "Net-(U7-U0RXD)")
  (net 175 "Net-(U7-U0TXD)")
  (net 176 "SAI1_SCK_B")
  (net 177 "SAI1_MCLK_B")
  (net 178 "SAI1_SD_B")
  (net 179 "SAI1_FS_B")
  (net 180 "SAI1_SD_A")
  (net 181 "unconnected-(U3-~{OC2}-Pad5)")
  (net 182 "unconnected-(U3-~{OC1}-Pad8)")
  (net 183 "unconnected-(U4-DOUT-Pad3)")
  (net 184 "unconnected-(U4-LRCK1-Pad4)")
  (net 185 "unconnected-(U4-BCK1-Pad5)")
  (net 186 "unconnected-(U4-SCKI1-Pad6)")
  (net 187 "unconnected-(U4-ZEROR-Pad13)")
  (net 188 "unconnected-(U4-ZEROL-Pad14)")
  (net 189 "unconnected-(U4-VOUTR--Pad17)")
  (net 190 "unconnected-(U4-VOUTL--Pad19)")
  (net 191 "unconnected-(U4-VINL-Pad25)")
  (net 192 "unconnected-(U4-VINR-Pad26)")
  (net 193 "unconnected-(U4-~{MS{slash}ADR{slash}IFMD}-Pad27)")
  (net 194 "unconnected-(U7-VDD_RTC-Pad5)")
  (net 195 "unconnected-(U7-TOUT-Pad6)")
  (net 196 "unconnected-(U7-XPD_DCDC-Pad8)")
  (net 197 "unconnected-(U7-MTMS-Pad9)")
  (net 198 "unconnected-(U7-MTDI-Pad10)")
  (net 199 "unconnected-(U7-MTCK-Pad12)")
  (net 200 "unconnected-(U7-MTDO-Pad13)")
  (net 201 "unconnected-(U7-GPIO2-Pad14)")
  (net 202 "unconnected-(U7-GPIO0-Pad15)")
  (net 203 "unconnected-(U7-GPIO4-Pad16)")
  (net 204 "unconnected-(U7-GPIO5-Pad24)")
  (net 205 "+3V3")
  (net 206 "NRST")
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 63.2 35.2)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mmc.kicad_sch")
    (property "Sheetname" "MMC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 3.2 0 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0.2 6.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 136 "MMC1_CK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 60 40)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mmc.kicad_sch")
    (property "Sheetname" "MMC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at -3 -0.2 90) (layer "F.SilkS"))
    (fp_text value "47K" (at 0 4.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 135 "MMC1_D3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_6.3x6.3_H3" (layer "F.Cu")
    (at 43.6 93.15 90)
    (descr "Choke, SMD, 6.3x6.3mm 3mm height")
    (tags "Choke SMD")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L1" (at 0 5.8 90) (layer "F.SilkS"))
    (fp_text value "20uH" (at 0 4.45 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.75 0 90) (size 1.5 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 2.75 0 90) (size 1.5 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(U6-Pin_4)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_6.3x6.3_H3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_5x5.3" (layer "F.Cu")
    (at 28.2 39.2 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "USB")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 -3.6 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at -0.2 3.6 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.2 0 90) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 11 "Net-(J8-VBUS)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.2 0 90) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 21.8 40.4)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "USB")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -2.6 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.8 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 37.8 94.25)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 0 2.95) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.68) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_5x5.3" (layer "F.Cu")
    (at 62.8 99.4)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at -5 0 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0.2 -3.6) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.2 0) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 2.2 0) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "F.Cu")
    (at 76 108.8 -90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Schottky diode")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D2" (at 3.2 -0.2 -180) (layer "F.SilkS"))
    (fp_text value "TVS" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 164 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 12 "Earth") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_FFC-FPC:Hirose_FH12-6S-0.5SH_1x06-1MP_P0.50mm_Horizontal" (layer "F.Cu")
    (at 52 109 -90)
    (descr "Hirose FH12, FFC/FPC connector, FH12-6S-0.5SH, 6 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J11" (at -2.8 5.6 90) (layer "F.SilkS") hide)
    (fp_text value "CTP" (at 0.8 -3.8 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.7 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "CTP_RESET") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at -0.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -0.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 0.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "CTP_INT") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 0.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "I2C1_SCL") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 1.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "I2C1_SDA") (pinfunction "Pin_6") (pintype "passive"))
    (pad "MP" smd rect (at -3.15 1.4 270) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "MP" smd rect (at 3.15 1.4 270) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Hirose_FH12-6S-0.5SH_1x06-1MP_P0.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_C_Receptacle_G-Switch_GT-USB-7010ASV" (layer "F.Cu")
    (at 66.18 117.425)
    (descr "USB Type C, right-angle, SMT, https://datasheet.lcsc.com/lcsc/2204071530_G-Switch-GT-USB-7010ASV_C2988369.pdf")
    (tags "USB C Type-C Receptacle SMD")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "USB 2.0-only Type-C Receptacle connector")
    (property "ki_keywords" "usb universal serial bus type-C USB2.0")
    (attr smd)
    (fp_text reference "J12" (at 5.62 -0.625 -90) (layer "F.SilkS"))
    (fp_text value "USB_DEBUG" (at -6.58 2.775 90) (layer "F.SilkS" knockout))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "A1" smd rect (at -3.2 -3.725) (size 0.6 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A4" smd rect (at -2.4 -3.725) (size 0.6 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "Net-(D2-K)") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" smd rect (at -1.25 -3.725) (size 0.3 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(J12-CC1)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.25 -3.725) (size 0.3 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "/Power & Debug/USB_P") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.25 -3.725) (size 0.3 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "/Power & Debug/USB_N") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd rect (at 1.25 -3.725) (size 0.3 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "unconnected-(J12-SBU1-PadA8)") (pinfunction "SBU1") (pintype "bidirectional+no_connect"))
    (pad "A9" smd rect (at 2.4 -3.725) (size 0.6 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "Net-(D2-K)") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" smd rect (at 3.2 -3.725) (size 0.6 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B1" smd rect (at 3.2 -3.725) (size 0.6 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B4" smd rect (at 2.4 -3.725) (size 0.6 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "Net-(D2-K)") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" smd rect (at 1.75 -3.725) (size 0.3 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(J12-CC2)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect (at 0.75 -3.725) (size 0.3 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "/Power & Debug/USB_P") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" smd rect (at -0.75 -3.725) (size 0.3 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "/Power & Debug/USB_N") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" smd rect (at -1.75 -3.725) (size 0.3 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "unconnected-(J12-SBU2-PadB8)") (pinfunction "SBU2") (pintype "bidirectional+no_connect"))
    (pad "B9" smd rect (at -2.4 -3.725) (size 0.6 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "Net-(D2-K)") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" smd rect (at -3.2 -3.725) (size 0.6 1.24) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 -3.125) (size 1 2.1) (drill oval 0.6 1.7) (layers "*.Cu" "*.Mask")
      (net 12 "Earth") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 1.075) (size 1 1.8) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask")
      (net 12 "Earth") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 -3.125) (size 1 2.1) (drill oval 0.6 1.7) (layers "*.Cu" "*.Mask")
      (net 12 "Earth") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 1.075) (size 1 1.8) (drill oval 0.6 1.4) (layers "*.Cu" "*.Mask")
      (net 12 "Earth") (pinfunction "SHIELD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_G-Switch_GT-USB-7010ASV.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 69.2 104.6)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at 2.25 0 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.68) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 62.8 37.6)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mmc.kicad_sch")
    (property "Sheetname" "MMC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at -3 -0.2 90) (layer "F.SilkS"))
    (fp_text value "47K" (at 0 5.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 140 "MMC1_CMD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 20.2 45.8)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "USB")
    (property "ki_description" "Dual power-distribution switcher")
    (property "ki_keywords" "2-chanel power-distribution USB")
    (attr smd)
    (fp_text reference "U3" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "TPS2042D" (at 0 3.4) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pinfunction "IN1") (pintype "power_in"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "~{EN1}") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "~{EN2}") (pintype "input"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 181 "unconnected-(U3-~{OC2}-Pad5)") (pinfunction "~{OC2}") (pintype "open_collector+no_connect"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J13-VBUS)") (pinfunction "OUT2") (pintype "power_out"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J8-VBUS)") (pinfunction "OUT1") (pintype "power_out"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 182 "unconnected-(U3-~{OC1}-Pad8)") (pinfunction "~{OC1}") (pintype "open_collector+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 84.6 100.2 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at -2.4 0.4 180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 2.4 0.2 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_FFC-FPC:Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal" (layer "F.Cu")
    (at 55.65 67.25 -90)
    (descr "Hirose FH12, FFC/FPC connector, FH12-40S-0.5SH, 40 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Generic connector, single row, 01x40, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J9" (at 0.15 0.05 90) (layer "F.SilkS"))
    (fp_text value "AFY480272A0" (at 0 -3.95 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.7 90) (layer "F.Fab"))
    (pad "1" smd rect (at 9.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(J9-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 9.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Vdrive") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 8.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 8.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "+3V3") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 7.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "LCD_R0") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 7.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "LCD_R1") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 6.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "LCD_R2") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 6.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "LCD_R3") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 5.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "LCD_R4") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 5.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "LCD_R5") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 4.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "LCD_R6") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 4.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "LCD_R7") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at 3.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "LCD_G0") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 3.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "LCD_G1") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at 2.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "LCD_G2") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at 2.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "LCD_G3") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at 1.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "LCD_G4") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at 1.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "LCD_G5") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at 0.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "LCD_G6") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at 0.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "LCD_G7") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at -0.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "LCD_B0") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at -0.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "LCD_B1") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect (at -1.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "LCD_B2") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at -1.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "LCD_B3") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at -2.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "LCD_B4") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at -2.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "LCD_B5") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at -3.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "LCD_B6") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at -3.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "LCD_B7") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at -4.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at -4.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "LCD_CLK") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at -5.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "+3V3") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at -5.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "LCD_H_SYNC") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at -6.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "LCD_V_SYNC") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at -6.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "LCD_DATA_EN") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd rect (at -7.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "unconnected-(J9-Pin_35-Pad35)") (pinfunction "Pin_35") (pintype "passive+no_connect"))
    (pad "36" smd rect (at -7.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "unconnected-(J9-Pin_36-Pad36)") (pinfunction "Pin_36") (pintype "passive+no_connect"))
    (pad "37" smd rect (at -8.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "unconnected-(J9-Pin_37-Pad37)") (pinfunction "Pin_37") (pintype "passive+no_connect"))
    (pad "38" smd rect (at -8.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "unconnected-(J9-Pin_38-Pad38)") (pinfunction "Pin_38") (pintype "passive+no_connect"))
    (pad "39" smd rect (at -9.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(J9-Pin_39-Pad39)") (pinfunction "Pin_39") (pintype "passive+no_connect"))
    (pad "40" smd rect (at -9.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "unconnected-(J9-Pin_40-Pad40)") (pinfunction "Pin_40") (pintype "passive+no_connect"))
    (pad "MP" smd rect (at -11.65 1.4 270) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "MP" smd rect (at 11.65 1.4 270) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Hirose_FH12-40S-0.5SH_1x40-1MP_P0.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6" (layer "F.Cu")
    (at 37.8 91.25)
    (descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Generic connector, double row, 02x03, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "U6" (at -4.5 0.25 90) (layer "F.SilkS"))
    (fp_text value "R1218NO41" (at -3 -0.25 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Vdrive") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(U6-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at 1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J9-Pin_1)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_5x5.3" (layer "F.Cu")
    (at 28.4 46.4)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "USB")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 5) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 3.7) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.2 0) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 25 "Net-(J13-VBUS)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.2 0) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 63.5 109.425 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at 15.02 82.9325 270) (layer "F.SilkS") hide)
    (fp_text value "5K1" (at -0.1 -1.975) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 21 "Net-(J12-CC1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "components:HRS_DM3AT-SF-PEJM5" (layer "F.Cu")
    (at 64.2375 31.8375 180)
    (descr "Micro SD card holder with push-to-eject feature.")
    (property "AVAILABILITY" "Unavailable")
    (property "DESCRIPTION" "DM3 RA SMT microSD memory card push/push")
    (property "MANUFACTURER" "Hirose")
    (property "MF" "Hirose")
    (property "MP" "DM3AT-SF-PEJM5")
    (property "PACKAGE" "None")
    (property "PARTREV" "n/a")
    (property "PRICE" "None")
    (property "STANDARED" "manufacturer recommendation")
    (property "Sheetfile" "mmc.kicad_sch")
    (property "Sheetname" "MMC")
    (attr smd)
    (fp_text reference "J5" (at -3.98677 -2.43602 180) (layer "F.SilkS"))
    (fp_text value "BOOT_SD" (at 8.4375 7.4375 270) (layer "F.SilkS" knockout))
    (fp_text user "PCB Edge" (at -4.75766 15.525 180) (layer "F.Fab"))
    (pad "1" smd rect (at 3.2 0 180) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "MMC1_D2") (pinfunction "DAT2") (pintype "bidirectional"))
    (pad "2" smd rect (at 2.1 0 180) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "MMC1_D3") (pinfunction "CD/DAT3") (pintype "bidirectional"))
    (pad "3" smd rect (at 1 0 180) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "MMC1_CMD") (pinfunction "CMD") (pintype "bidirectional"))
    (pad "4" smd rect (at -0.1 0 180) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "5" smd rect (at -1.2 0 180) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "MMC1_CK") (pinfunction "CLK") (pintype "bidirectional"))
    (pad "6" smd rect (at -2.3 0 180) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "7" smd rect (at -3.4 0 180) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "MMC1_D0") (pinfunction "DAT0") (pintype "bidirectional"))
    (pad "8" smd rect (at -4.5 0 180) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "MMC1_D1") (pinfunction "DAT1") (pintype "bidirectional"))
    (pad "P1" smd rect (at -6.4 4.3 180) (size 1 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "unconnected-(J5-SHIELD-PadP1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "P2" smd rect (at -6.4 14.65 180) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "unconnected-(J5-SHIELD-PadP1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "P3" smd rect (at 7.1 15.1 180) (size 1.3 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "unconnected-(J5-SHIELD-PadP1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "P4" smd rect (at 4.75 0 180) (size 1 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "unconnected-(J5-SHIELD-PadP1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "SWA" smd rect (at -6.4 10.5 180) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "+3V3") (pintype "bidirectional"))
    (pad "SWB" smd rect (at -5.45 0 180) (size 0.7 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "MMC1_DETECT") (pintype "bidirectional"))
  )
  (footprint "Package_SO:SSOP-20_3.9x8.7mm_P0.635mm" (layer "F.Cu")
    (at 80.9 106.7225)
    (descr "SSOP20: plastic shrink small outline package; 24 leads; body width 3.9 mm; lead pitch 0.635; (see http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT231X.pdf)")
    (tags "SSOP 0.635")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Full Speed USB to Full Handshake UART, SSOP-20")
    (property "ki_keywords" "FTDI USB UART interface converter")
    (attr smd)
    (fp_text reference "U2" (at 0 -5.4) (layer "F.SilkS"))
    (fp_text value "FT231XS" (at 0 5.4) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.6 -2.8575) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "unconnected-(U2-~{DTR}-Pad1)") (pinfunction "~{DTR}") (pintype "output+no_connect"))
    (pad "2" smd rect (at -2.6 -2.2225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "unconnected-(U2-~{RTS}-Pad2)") (pinfunction "~{RTS}") (pintype "output+no_connect"))
    (pad "3" smd rect (at -2.6 -1.5875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "+3V3") (pinfunction "VCCIO") (pintype "power_in"))
    (pad "4" smd rect (at -2.6 -0.9525) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "UART4_TX") (pinfunction "RXD") (pintype "input"))
    (pad "5" smd rect (at -2.6 -0.3175) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "unconnected-(U2-~{RI}-Pad5)") (pinfunction "~{RI}") (pintype "input+no_connect"))
    (pad "6" smd rect (at -2.6 0.3175) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd rect (at -2.6 0.9525) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "unconnected-(U2-~{DSR}-Pad7)") (pinfunction "~{DSR}") (pintype "input+no_connect"))
    (pad "8" smd rect (at -2.6 1.5875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "unconnected-(U2-~{DCD}-Pad8)") (pinfunction "~{DCD}") (pintype "input+no_connect"))
    (pad "9" smd rect (at -2.6 2.2225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "unconnected-(U2-~{CTS}-Pad9)") (pinfunction "~{CTS}") (pintype "input+no_connect"))
    (pad "10" smd rect (at -2.6 2.8575) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "unconnected-(U2-CBUS2-Pad10)") (pinfunction "CBUS2") (pintype "bidirectional+no_connect"))
    (pad "11" smd rect (at 2.6 2.8575) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "Net-(U2-USBDP)") (pinfunction "USBDP") (pintype "bidirectional"))
    (pad "12" smd rect (at 2.6 2.2225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(U2-USBDM)") (pinfunction "USBDM") (pintype "bidirectional"))
    (pad "13" smd rect (at 2.6 1.5875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "unconnected-(U2-3V3OUT-Pad13)") (pinfunction "3V3OUT") (pintype "power_out+no_connect"))
    (pad "14" smd rect (at 2.6 0.9525) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "+3V3") (pinfunction "~{RESET}") (pintype "input"))
    (pad "15" smd rect (at 2.6 0.3175) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "16" smd rect (at 2.6 -0.3175) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "17" smd rect (at 2.6 -0.9525) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "unconnected-(U2-CBUS1-Pad17)") (pinfunction "CBUS1") (pintype "bidirectional+no_connect"))
    (pad "18" smd rect (at 2.6 -1.5875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "unconnected-(U2-CBUS0-Pad18)") (pinfunction "CBUS0") (pintype "bidirectional+no_connect"))
    (pad "19" smd rect (at 2.6 -2.2225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "unconnected-(U2-CBUS3-Pad19)") (pinfunction "CBUS3") (pintype "bidirectional+no_connect"))
    (pad "20" smd rect (at 2.6 -2.8575) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "UART4_RX") (pinfunction "TXD") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-20_3.9x8.7mm_P0.635mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 78.4 118.2 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP7" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "GND" (at 0 1.55) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 55 32.6 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "mmc.kicad_sch")
    (property "Sheetname" "MMC")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C15" (at 0.2 -3 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0.2 -1.6 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_5x5.3" (layer "F.Cu")
    (at 71 99.4 180)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C13" (at -4.8 0 90) (layer "F.SilkS"))
    (fp_text value "100uF" (at 0 3.7) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.2 0 180) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 2.2 0 180) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 70.2 35 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mmc.kicad_sch")
    (property "Sheetname" "MMC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at -3.2 -0.2 90) (layer "F.SilkS"))
    (fp_text value "47K" (at 0 -7) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 133 "MMC1_D1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 46.8 86.4 90)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 1.6 0) (layer "F.SilkS"))
    (fp_text value "LED-" (at -1.8 0.6 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45 90) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 90) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 13 "Net-(J9-Pin_1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 42.6 88.2 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at -0.4 3.2 180) (layer "F.SilkS"))
    (fp_text value "10R" (at -0.4 1.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 13 "Net-(J9-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric" (layer "F.Cu")
    (at 73.6 111.4 -90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Schottky diode")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D3" (at 3 0 -180) (layer "F.SilkS"))
    (fp_text value "TVS" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 12 "Earth") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 1 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric" (layer "F.Cu")
    (at 66.2 106 90)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Resettable fuse, polymeric positive temperature coefficient")
    (property "ki_keywords" "resettable fuse PTC PPTC polyfuse polyswitch")
    (attr smd)
    (fp_text reference "F1" (at 3 0.2 180) (layer "F.SilkS"))
    (fp_text value "2A" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 164 "Net-(D2-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 3 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 55.8 102.8 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 3 0 90) (layer "F.SilkS"))
    (fp_text value "10K" (at -3 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 154 "CTP_RESET") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 84.6 118.2 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP5" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "5V" (at 0 1.55) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 3 "+5V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 69.2 37.6 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mmc.kicad_sch")
    (property "Sheetname" "MMC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -3.2 0.2 90) (layer "F.SilkS"))
    (fp_text value "47K" (at -0.2 -5.8) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 132 "MMC1_D0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_FFC-FPC:Hirose_FH12-50S-0.5SH_1x50-1MP_P0.50mm_Horizontal" (layer "F.Cu")
    (at 19.95 101.5 -90)
    (descr "Hirose FH12, FFC/FPC connector, FH12-50S-0.5SH, 50 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Generic connector, double row, 02x25, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J1" (at 0 -3.7 90) (layer "F.SilkS") hide)
    (fp_text value "MY-TFT070CV2" (at -0.1 -4.85 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.7 90) (layer "F.Fab"))
    (pad "1" smd rect (at 12.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 11.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 11.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "+3V3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 10.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "+3V3") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 10.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 9.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 9.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "LCD_B0") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 8.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "LCD_B1") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 8.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "LCD_B2") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 7.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "LCD_B3") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 7.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "LCD_B4") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 6.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "LCD_B5") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at 6.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "LCD_B6") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 5.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "LCD_B7") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at 5.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "LCD_G0") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at 4.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "LCD_G1") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at 4.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "LCD_G2") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at 3.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "LCD_G3") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at 3.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "LCD_G4") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at 2.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "LCD_G5") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at 2.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "LCD_G6") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at 1.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "LCD_G7") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect (at 1.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "LCD_R0") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at 0.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "LCD_R1") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at 0.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "LCD_R2") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at -0.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "LCD_R3") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at -0.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "LCD_R4") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at -1.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "LCD_R5") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at -1.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "LCD_R6") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at -2.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "LCD_R7") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at -2.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at -3.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "LCD_BL_EN") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at -3.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "+3V3") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at -4.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 205 "+3V3") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd rect (at -4.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "CTP_INT") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" smd rect (at -5.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "CTP_RESET") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd rect (at -5.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "I2C1_SCL") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" smd rect (at -6.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "I2C1_SDA") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" smd rect (at -6.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" smd rect (at -7.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "LCD_DATA_EN") (pinfunction "Pin_40") (pintype "passive"))
    (pad "41" smd rect (at -7.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "LCD_V_SYNC") (pinfunction "Pin_41") (pintype "passive"))
    (pad "42" smd rect (at -8.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "LCD_H_SYNC") (pinfunction "Pin_42") (pintype "passive"))
    (pad "43" smd rect (at -8.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "LCD_CLK") (pinfunction "Pin_43") (pintype "passive"))
    (pad "44" smd rect (at -9.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_44") (pintype "passive"))
    (pad "45" smd rect (at -9.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "unconnected-(J1-Pin_45-Pad45)") (pinfunction "Pin_45") (pintype "passive+no_connect"))
    (pad "46" smd rect (at -10.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "unconnected-(J1-Pin_46-Pad46)") (pinfunction "Pin_46") (pintype "passive+no_connect"))
    (pad "47" smd rect (at -10.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "unconnected-(J1-Pin_47-Pad47)") (pinfunction "Pin_47") (pintype "passive+no_connect"))
    (pad "48" smd rect (at -11.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "unconnected-(J1-Pin_48-Pad48)") (pinfunction "Pin_48") (pintype "passive+no_connect"))
    (pad "49" smd rect (at -11.75 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "unconnected-(J1-Pin_49-Pad49)") (pinfunction "Pin_49") (pintype "passive+no_connect"))
    (pad "50" smd rect (at -12.25 -1.85 270) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_50") (pintype "passive"))
    (pad "MP" smd rect (at -14.15 1.4 270) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "MP" smd rect (at 14.15 1.4 270) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Hirose_FH12-50S-0.5SH_1x50-1MP_P0.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 80.6 99.8)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C21" (at -2.4 0.2 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 -2) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 32.8 89.2 90)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at -0.2 -2.2 180) (layer "F.SilkS"))
    (fp_text value "LED+" (at 1.4 -1.6 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45 90) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 90) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 4 "Vdrive") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 58.4 35.2)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "mmc.kicad_sch")
    (property "Sheetname" "MMC")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at -3 0 90) (layer "F.SilkS"))
    (fp_text value "47K" (at 0 7) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 134 "MMC1_D2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 69 109.425)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.825 180) (layer "F.SilkS"))
    (fp_text value "5K1" (at 0 1.82) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 23 "Net-(J12-CC2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (at 81.6 118.2 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP6" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "3V3" (at 0 1.55) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 205 "+3V3") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 37.8 88.25)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "lcd.kicad_sch")
    (property "Sheetname" "LCD")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 0 -3.25) (layer "F.SilkS"))
    (fp_text value "0.22uF" (at 0 -1.45) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Vdrive") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 77.2 108.6)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R27" (at -3 -0.4 90) (layer "B.SilkS"))
    (fp_text value "27R" (at -0.2 -1.82) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 165 "/Power & Debug/USB_N") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 26 "Net-(U2-USBDM)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 36 54 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP151_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at 2.8 -0.8 90) (layer "B.SilkS"))
    (fp_text value "27R" (at 0 -1.82) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 162 "Net-(U1-USB2_P)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 117 "USB2_P") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "components:QFN50P500X500X90-33N" (layer "B.Cu")
    (at 35.645 26.6)
    (property "A_MAX" "0.9")
    (property "BALL_COLUMNS" "")
    (property "BALL_ROWS" "")
    (property "BODY_DIAMETER" "")
    (property "B_MAX" "0.3")
    (property "B_MIN" "0.2")
    (property "B_NOM" "0.25")
    (property "D2_NOM" "3.7")
    (property "DMAX" "")
    (property "DMIN" "")
    (property "DNOM" "")
    (property "D_MAX" "5.05")
    (property "D_MIN" "4.95")
    (property "D_NOM" "5.0")
    (property "E2_NOM" "3.7")
    (property "EMAX" "")
    (property "EMIN" "")
    (property "ENOM" "0.5")
    (property "E_MAX" "5.05")
    (property "E_MIN" "4.95")
    (property "E_NOM" "5.0")
    (property "IPC" "")
    (property "JEDEC" "")
    (property "L_MAX" "0.45")
    (property "L_MIN" "0.35")
    (property "L_NOM" "0.4")
    (property "MANUFACTURER" "Espressif")
    (property "PACKAGE_TYPE" "")
    (property "PARTREV" "2.0")
    (property "PINS" "")
    (property "PIN_COLUMNS" "")
    (property "PIN_COUNT_D" "8.0")
    (property "PIN_COUNT_E" "8.0")
    (property "SNAPEDA_PACKAGE_ID" "")
    (property "STANDARD" "IPC 7351B")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "THERMAL_PAD" "")
    (property "VACANCIES" "")
    (clearance 0.19)
    (attr smd)
    (fp_text reference "U7" (at 0.175 4.135 180) (layer "B.SilkS"))
    (fp_text value "ESP8285" (at 9.7 -4.135 180) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.445 1.75) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 205 "+3V3") (pinfunction "VDDA") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.445 1.25) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 39 "Net-(U7-LNA)") (pinfunction "LNA") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.445 0.75) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 205 "+3V3") (pinfunction "VDD3P3") (pintype "power_in"))
    (pad "4" smd roundrect (at -2.445 0.25) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 205 "+3V3") (pinfunction "VDD3P3") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.445 -0.25) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 194 "unconnected-(U7-VDD_RTC-Pad5)") (pinfunction "VDD_RTC") (pintype "power_in+no_connect"))
    (pad "6" smd roundrect (at -2.445 -0.75) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 195 "unconnected-(U7-TOUT-Pad6)") (pinfunction "TOUT") (pintype "output+no_connect"))
    (pad "7" smd roundrect (at -2.445 -1.25) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 153 "WIFI_UP") (pinfunction "CHIP_EN") (pintype "input"))
    (pad "8" smd roundrect (at -2.445 -1.75) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 196 "unconnected-(U7-XPD_DCDC-Pad8)") (pinfunction "XPD_DCDC") (pintype "bidirectional+no_connect"))
    (pad "9" smd roundrect (at -1.75 -2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 197 "unconnected-(U7-MTMS-Pad9)") (pinfunction "MTMS") (pintype "bidirectional+no_connect"))
    (pad "10" smd roundrect (at -1.25 -2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 198 "unconnected-(U7-MTDI-Pad10)") (pinfunction "MTDI") (pintype "bidirectional+no_connect"))
    (pad "11" smd roundrect (at -0.75 -2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 205 "+3V3") (pinfunction "VDDPST") (pintype "power_in"))
    (pad "12" smd roundrect (at -0.25 -2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 199 "unconnected-(U7-MTCK-Pad12)") (pinfunction "MTCK") (pintype "bidirectional+no_connect"))
    (pad "13" smd roundrect (at 0.25 -2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 200 "unconnected-(U7-MTDO-Pad13)") (pinfunction "MTDO") (pintype "bidirectional+no_connect"))
    (pad "14" smd roundrect (at 0.75 -2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 201 "unconnected-(U7-GPIO2-Pad14)") (pinfunction "GPIO2") (pintype "bidirectional+no_connect"))
    (pad "15" smd roundrect (at 1.25 -2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 202 "unconnected-(U7-GPIO0-Pad15)") (pinfunction "GPIO0") (pintype "bidirectional+no_connect"))
    (pad "16" smd roundrect (at 1.75 -2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 203 "unconnected-(U7-GPIO4-Pad16)") (pinfunction "GPIO4") (pintype "bidirectional+no_connect"))
    (pad "17" smd roundrect (at 2.445 -1.75) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 205 "+3V3") (pinfunction "VDDPST") (pintype "power_in"))
    (pad "18" smd roundrect (at 2.445 -1.25) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 30 "MMC3_D2") (pinfunction "SD_DATA_2") (pintype "bidirectional"))
    (pad "19" smd roundrect (at 2.445 -0.75) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 43 "MMC3_D3") (pinfunction "SD_DATA_3") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 2.445 -0.25) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 32 "MMC3_CMD") (pinfunction "SD_CMD") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 2.445 0.25) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 34 "MMC3_CK") (pinfunction "SD_CLK") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 2.445 0.75) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 27 "MMC3_D0") (pinfunction "SD_DATA_0") (pintype "bidirectional"))
    (pad "23" smd roundrect (at 2.445 1.25) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 28 "MMC3_D1") (pinfunction "SD_DATA_1") (pintype "bidirectional"))
    (pad "24" smd roundrect (at 2.445 1.75) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 204 "unconnected-(U7-GPIO5-Pad24)") (pinfunction "GPIO5") (pintype "bidirectional+no_connect"))
    (pad "25" smd roundrect (at 1.75 2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 174 "Net-(U7-U0RXD)") (pinfunction "U0RXD") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 1.25 2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 175 "Net-(U7-U0TXD)") (pinfunction "U0TXD") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 0.75 2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 5 "Net-(U7-XTAL_OUT)") (pinfunction "XTAL_OUT") (pintype "output"))
    (pad "28" smd roundrect (at 0.25 2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 38 "Net-(U7-XTAL_IN)") (pinfunction "XTAL_IN") (pintype "input"))
    (pad "29" smd roundrect (at -0.25 2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 205 "+3V3") (pinfunction "VDDD") (pintype "power_in"))
    (pad "30" smd roundrect (at -0.75 2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 205 "+3V3") (pinfunction "VDDA") (pintype "power_in"))
    (pad "31" smd roundrect (at -1.25 2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 173 "Net-(U7-RES12K)") (pinfunction "RES12K") (pintype "input"))
    (pad "32" smd roundrect (at -1.75 2.445 270) (size 0.81 0.27) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.03)
      (net 206 "NRST") (pinfunction "~{EXT_RST}") (pintype "input"))
    (pad "33" smd rect (at 0 0) (size 3.7 3.7) (layers "B.Cu" "B.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
  )
  (footprint "Connector_USB:USB_A_Molex_67643_Horizontal" (layer "B.Cu")
    (at 27.31 62.5 90)
    (descr "USB type A, Horizontal, https://www.molex.com/pdm_docs/sd/676433910_sd.pdf")
    (tags "USB_A Female Connector receptacle")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "USB")
    (property "ki_description" "USB Type A connector")
    (property "ki_keywords" "connector USB")
    (attr through_hole)
    (fp_text reference "J8" (at 3.5 5.49 90) (layer "B.SilkS"))
    (fp_text value "USB_1" (at 3.5 3.44 270) (layer "B.SilkS" knockout))
    (fp_text user "${REFERENCE}" (at 3.5 -3.7 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.5) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J8-VBUS)") (pinfunction "VBUS") (pintype "power_in"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 120 "USB1_N") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at 4.5 0 90) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 119 "USB1_P") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at 7 0 90) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole circle (at -3.07 -2.71 90) (size 3 3) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.07 -2.71 90) (size 3 3) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_Molex_67643_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 36 51.55 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP151_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at 2.8 -0.25 90) (layer "B.SilkS"))
    (fp_text value "27R" (at 0 -0.25) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 161 "Net-(U1-USB2_N)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 118 "USB2_N") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "B.Cu")
    (at 84.6 34.58 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Generic connector, single row, 01x05, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 4.6 -5.02 90) (layer "B.SilkS"))
    (fp_text value "SWDIO" (at 2.6 -2.02 90) (layer "B.SilkS" knockout))
    (fp_text user "${REFERENCE}" (at 0 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 205 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 131 "SWCLK") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 130 "SWDIO") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 206 "NRST") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_A_Molex_67643_Horizontal" (layer "B.Cu")
    (at 27.36 80.1 90)
    (descr "USB type A, Horizontal, https://www.molex.com/pdm_docs/sd/676433910_sd.pdf")
    (tags "USB_A Female Connector receptacle")
    (property "Sheetfile" "usb.kicad_sch")
    (property "Sheetname" "USB")
    (property "ki_description" "USB Type A connector")
    (property "ki_keywords" "connector USB")
    (attr through_hole)
    (fp_text reference "J13" (at 3.4 5.44 90) (layer "B.SilkS"))
    (fp_text value "USB_2" (at 3.4 3.44 270) (layer "B.SilkS" knockout))
    (fp_text user "${REFERENCE}" (at 3.5 -3.7 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.5) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(J13-VBUS)") (pinfunction "VBUS") (pintype "power_in"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 118 "USB2_N") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at 4.5 0 90) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 117 "USB2_P") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at 7 0 90) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole circle (at -3.07 -2.71 90) (size 3 3) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.07 -2.71 90) (size 3 3) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_Molex_67643_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 33.195 32.2 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 2.4 0) (layer "B.SilkS"))
    (fp_text value "10pF" (at 5 0.2 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(U7-XTAL_IN)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RF_Antenna:Texas_SWRA117D_2.4GHz_Left" (layer "B.Cu")
    (at 21.2 27.8 -90)
    (descr "http://www.ti.com/lit/an/swra117d/swra117d.pdf")
    (tags "PCB antenna")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "Dipole antenna")
    (property "ki_keywords" "dipole antenna")
    (attr exclude_from_pos_files)
    (net_tie_pad_groups "1,2")
    (fp_text reference "AE1" (at -4.8 -1.2 90) (layer "B.SilkS"))
    (fp_text value "Antenna_Dipole" (at -3.95 -1.21 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -4.55 6.4 90) (layer "B.Fab"))
    (pad "1" connect rect (at 0 0 270) (size 0.5 0.5) (layers "B.Cu")
      (net 2 "Net-(AE1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "2" thru_hole rect (at 2.1 0 270) (size 0.9 0.5) (drill 0.3) (layers "*.Cu")
      (net 1 "GND") (pinfunction "2") (pintype "input") (zone_connect 2))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 25.645 28.6 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C16" (at 2.4 0) (layer "B.SilkS"))
    (fp_text value "2.4pF" (at -3.8 0 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(AE1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 36 46.8 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP151_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at 2.8 1 90) (layer "B.SilkS"))
    (fp_text value "27R" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 159 "Net-(U1-USB1_N)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 120 "USB1_N") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "components:MYCYA151C256N256D65CT" (layer "B.Cu")
    (at 59.5 63.5 180)
    (descr "MYC-YA151C-256N256D-65-C-T-5")
    (tags "Undefined or Miscellaneous")
    (property "Height" "3.5")
    (property "Manufacturer_Name" "MYIR")
    (property "Manufacturer_Part_Number" "MYC-YA151C-256N256D-65-C-T")
    (property "Mouser Part Number" "885-MCA151CN256D65CT")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/MYIR/MYC-YA151C-256N256D-65-C-T?qs=e8oIoAS2J1SxKfhSw3h3gA%3D%3D")
    (property "Sheetfile" "STM32MP151_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Embedded Module ARM Cortex-A7, ARM Cortex-M4 650MHz 256MB 256MB")
    (attr smd)
    (fp_text reference "U1" (at 0 0) (layer "B.SilkS"))
    (fp_text value "MYC-YA151C-256N256D" (at 0 0) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd oval (at -18.5 18.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "2" smd oval (at -18.5 17.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "MMC3_D0") (pinfunction "MMC3_D0") (pintype "passive"))
    (pad "3" smd oval (at -18.5 16.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "MMC3_D1") (pinfunction "MMC3_D1") (pintype "passive"))
    (pad "4" smd oval (at -18.5 15.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "MMC3_D2") (pinfunction "MMC3_D2") (pintype "passive"))
    (pad "5" smd oval (at -18.5 14.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "MMC3_D3") (pinfunction "MMC3_D3") (pintype "passive"))
    (pad "6" smd oval (at -18.5 13.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "MMC3_CK") (pinfunction "MMC3_CK") (pintype "passive"))
    (pad "7" smd oval (at -18.5 12.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "MMC3_CMD") (pinfunction "MMC3_CMD") (pintype "passive"))
    (pad "8" smd oval (at -18.5 11.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "9" smd oval (at -18.5 10.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "PC6") (pinfunction "PC6") (pintype "passive"))
    (pad "10" smd oval (at -18.5 9.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "PC7") (pinfunction "PC7") (pintype "passive"))
    (pad "11" smd oval (at -18.5 8.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "PE0") (pinfunction "PE0") (pintype "passive"))
    (pad "12" smd oval (at -18.5 7.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "unconnected-(U1-PE1-Pad12)") (pinfunction "PE1") (pintype "passive"))
    (pad "13" smd oval (at -18.5 6.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "unconnected-(U1-PE4-Pad13)") (pinfunction "PE4") (pintype "passive"))
    (pad "14" smd oval (at -18.5 5.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "PB6") (pinfunction "PB6") (pintype "passive"))
    (pad "15" smd oval (at -18.5 4.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "PB8") (pinfunction "PB8") (pintype "passive"))
    (pad "16" smd oval (at -18.5 3.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "unconnected-(U1-PB9-Pad16)") (pinfunction "PB9") (pintype "passive"))
    (pad "17" smd oval (at -18.5 2.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "unconnected-(U1-PA4-Pad17)") (pinfunction "PA4") (pintype "passive"))
    (pad "18" smd oval (at -18.5 1.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "unconnected-(U1-PA6-Pad18)") (pinfunction "PA6") (pintype "passive"))
    (pad "19" smd oval (at -18.5 0.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "MMC1_DETECT") (pinfunction "PB7") (pintype "passive"))
    (pad "20" smd oval (at -18.5 -0.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_3") (pintype "passive"))
    (pad "21" smd oval (at -18.5 -1.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 54 "LCD_B0") (pinfunction "PD9") (pintype "passive"))
    (pad "22" smd oval (at -18.5 -2.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 55 "LCD_B1") (pinfunction "PG12") (pintype "passive"))
    (pad "23" smd oval (at -18.5 -3.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 56 "LCD_B2") (pinfunction "PG10") (pintype "passive"))
    (pad "24" smd oval (at -18.5 -4.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 57 "LCD_B3") (pinfunction "PD10") (pintype "passive"))
    (pad "25" smd oval (at -18.5 -5.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 58 "LCD_B4") (pinfunction "PI4") (pintype "passive"))
    (pad "26" smd oval (at -18.5 -6.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 59 "LCD_B5") (pinfunction "PI5") (pintype "passive"))
    (pad "27" smd oval (at -18.5 -7.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 60 "LCD_B6") (pinfunction "PI6") (pintype "passive"))
    (pad "28" smd oval (at -18.5 -8.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "LCD_B7") (pinfunction "PI7") (pintype "passive"))
    (pad "29" smd oval (at -18.5 -9.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_4") (pintype "passive"))
    (pad "30" smd oval (at -18.5 -10.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 62 "LCD_G0") (pinfunction "PE14") (pintype "passive"))
    (pad "31" smd oval (at -18.5 -11.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 63 "LCD_G1") (pinfunction "PE6") (pintype "passive"))
    (pad "32" smd oval (at -18.5 -12.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "LCD_G2") (pinfunction "PH13") (pintype "passive"))
    (pad "33" smd oval (at -18.5 -13.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "LCD_G3") (pinfunction "PH14") (pintype "passive"))
    (pad "34" smd oval (at -18.5 -14.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 66 "LCD_G4") (pinfunction "PH15") (pintype "passive"))
    (pad "35" smd oval (at -18.5 -15.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "LCD_G5") (pinfunction "PI0") (pintype "passive"))
    (pad "36" smd oval (at -18.5 -16.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "LCD_G6") (pinfunction "PI1") (pintype "passive"))
    (pad "37" smd oval (at -18.5 -17.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "LCD_G7") (pinfunction "PI2") (pintype "passive"))
    (pad "38" smd oval (at -18.5 -18.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_5") (pintype "passive"))
    (pad "39" smd oval (at -17.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_6") (pintype "passive"))
    (pad "40" smd oval (at -16.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "LCD_R0") (pinfunction "PH2") (pintype "passive"))
    (pad "41" smd oval (at -15.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "LCD_R1") (pinfunction "PH3") (pintype "passive"))
    (pad "42" smd oval (at -14.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "LCD_R2") (pinfunction "PH8") (pintype "passive"))
    (pad "43" smd oval (at -13.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "LCD_R3") (pinfunction "PH9") (pintype "passive"))
    (pad "44" smd oval (at -12.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "LCD_R4") (pinfunction "PH10") (pintype "passive"))
    (pad "45" smd oval (at -11.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "LCD_R5") (pinfunction "PH11") (pintype "passive"))
    (pad "46" smd oval (at -10.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 76 "LCD_R6") (pinfunction "PH12") (pintype "passive"))
    (pad "47" smd oval (at -9.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "LCD_R7") (pinfunction "PE15") (pintype "passive"))
    (pad "48" smd oval (at -8.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "LCD_DATA_EN") (pinfunction "PE13") (pintype "passive"))
    (pad "49" smd oval (at -7.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "LCD_V_SYNC") (pinfunction "PI9") (pintype "passive"))
    (pad "50" smd oval (at -6.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "LCD_H_SYNC") (pinfunction "PI10") (pintype "passive"))
    (pad "51" smd oval (at -5.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "LCD_CLK") (pinfunction "PG7") (pintype "passive"))
    (pad "52" smd oval (at -4.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_7") (pintype "passive"))
    (pad "53" smd oval (at -3.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 206 "NRST") (pinfunction "NRST") (pintype "passive"))
    (pad "54" smd oval (at -2.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "BOOT1") (pinfunction "BOOT1") (pintype "passive"))
    (pad "55" smd oval (at -1.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "BOOT0") (pinfunction "BOOT0") (pintype "passive"))
    (pad "56" smd oval (at -0.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "BOOT2") (pinfunction "BOOT2") (pintype "passive"))
    (pad "57" smd oval (at 0.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "unconnected-(U1-PD8-Pad57)") (pinfunction "PD8") (pintype "passive"))
    (pad "58" smd oval (at 1.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "unconnected-(U1-PG3-Pad58)") (pinfunction "PG3") (pintype "passive"))
    (pad "59" smd oval (at 2.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 156 "I2C1_SCL") (pinfunction "PF14") (pintype "passive"))
    (pad "60" smd oval (at 3.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 157 "I2C1_SDA") (pinfunction "PF15") (pintype "passive"))
    (pad "61" smd oval (at 4.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_8") (pintype "passive"))
    (pad "62" smd oval (at 5.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "SPI5_MOSI") (pinfunction "PF11") (pintype "passive"))
    (pad "63" smd oval (at 6.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "SPI5_MISO") (pinfunction "PH7") (pintype "passive"))
    (pad "64" smd oval (at 7.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 90 "SPI5_CS") (pinfunction "PH5") (pintype "passive"))
    (pad "65" smd oval (at 8.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "SPI5_CLK") (pinfunction "PH6") (pintype "passive"))
    (pad "66" smd oval (at 9.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "unconnected-(U1-PB13-Pad66)") (pinfunction "PB13") (pintype "passive"))
    (pad "67" smd oval (at 10.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "unconnected-(U1-PB5-Pad67)") (pinfunction "PB5") (pintype "passive"))
    (pad "68" smd oval (at 11.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 94 "UART4_RX") (pinfunction "PA11") (pintype "passive"))
    (pad "69" smd oval (at 12.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "unconnected-(U1-PA12-Pad69)") (pinfunction "PA12") (pintype "passive"))
    (pad "70" smd oval (at 13.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 96 "unconnected-(U1-VBAT_RTC-Pad70)") (pinfunction "VBAT_RTC") (pintype "passive"))
    (pad "71" smd oval (at 14.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 205 "+3V3") (pinfunction "3V3_OUT") (pintype "passive"))
    (pad "72" smd oval (at 15.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "+5V") (pinfunction "VDD_5V_1") (pintype "passive"))
    (pad "73" smd oval (at 16.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "+5V") (pinfunction "VDD_5V_2") (pintype "passive"))
    (pad "74" smd oval (at 17.5 -19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_9") (pintype "passive"))
    (pad "75" smd oval (at 18.5 -18.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_10") (pintype "passive"))
    (pad "76" smd oval (at 18.5 -17.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 172 "KEY_WP") (pinfunction "KEY_WP") (pintype "passive"))
    (pad "77" smd oval (at 18.5 -16.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 154 "CTP_RESET") (pinfunction "PE11") (pintype "passive"))
    (pad "78" smd oval (at 18.5 -15.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "CTP_INT") (pinfunction "PE12") (pintype "passive"))
    (pad "79" smd oval (at 18.5 -14.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "LCD_BL_EN") (pinfunction "PI3") (pintype "passive"))
    (pad "80" smd oval (at 18.5 -13.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 169 "LED_R") (pinfunction "PA3") (pintype "passive"))
    (pad "81" smd oval (at 18.5 -12.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "ANA0") (pinfunction "ANA0") (pintype "passive"))
    (pad "82" smd oval (at 18.5 -11.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "ANA1") (pinfunction "ANA1") (pintype "passive"))
    (pad "83" smd oval (at 18.5 -10.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 170 "LED_G") (pinfunction "PA5") (pintype "passive"))
    (pad "84" smd oval (at 18.5 -9.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "unconnected-(U1-VBUS_OTG-Pad84)") (pinfunction "VBUS_OTG") (pintype "passive"))
    (pad "85" smd oval (at 18.5 -8.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "unconnected-(U1-ETH_MDIO-Pad85)") (pinfunction "ETH_MDIO") (pintype "passive"))
    (pad "86" smd oval (at 18.5 -7.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "unconnected-(U1-ETH_MDC-Pad86)") (pinfunction "ETH_MDC") (pintype "passive"))
    (pad "87" smd oval (at 18.5 -6.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 171 "LED_B") (pinfunction "PC0") (pintype "passive"))
    (pad "88" smd oval (at 18.5 -5.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 104 "unconnected-(U1-PG8-Pad88)") (pinfunction "PG8") (pintype "passive"))
    (pad "89" smd oval (at 18.5 -4.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_11") (pintype "passive"))
    (pad "90" smd oval (at 18.5 -3.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "unconnected-(U1-ETH_TD3-Pad90)") (pinfunction "ETH_TD3") (pintype "passive"))
    (pad "91" smd oval (at 18.5 -2.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "unconnected-(U1-ETH_TD2-Pad91)") (pinfunction "ETH_TD2") (pintype "passive"))
    (pad "92" smd oval (at 18.5 -1.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "unconnected-(U1-ETH_TD1-Pad92)") (pinfunction "ETH_TD1") (pintype "passive"))
    (pad "93" smd oval (at 18.5 -0.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 108 "unconnected-(U1-ETH_TD0-Pad93)") (pinfunction "ETH_TD0") (pintype "passive"))
    (pad "94" smd oval (at 18.5 0.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 109 "unconnected-(U1-ETH_TCTL-Pad94)") (pinfunction "ETH_TCTL") (pintype "passive"))
    (pad "95" smd oval (at 18.5 1.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 110 "unconnected-(U1-ETH_TCLK-Pad95)") (pinfunction "ETH_TCLK") (pintype "passive"))
    (pad "96" smd oval (at 18.5 2.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_12") (pintype "passive"))
    (pad "97" smd oval (at 18.5 3.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 111 "unconnected-(U1-ETH_RCLK-Pad97)") (pinfunction "ETH_RCLK") (pintype "passive"))
    (pad "98" smd oval (at 18.5 4.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 112 "unconnected-(U1-ETH_RD3-Pad98)") (pinfunction "ETH_RD3") (pintype "passive"))
    (pad "99" smd oval (at 18.5 5.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 113 "unconnected-(U1-ETH_RD2-Pad99)") (pinfunction "ETH_RD2") (pintype "passive"))
    (pad "100" smd oval (at 18.5 6.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 114 "unconnected-(U1-ETH_RD1-Pad100)") (pinfunction "ETH_RD1") (pintype "passive"))
    (pad "101" smd oval (at 18.5 7.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 115 "unconnected-(U1-ETH_RD0-Pad101)") (pinfunction "ETH_RD0") (pintype "passive"))
    (pad "102" smd oval (at 18.5 8.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 116 "unconnected-(U1-ETH_RCTL-Pad102)") (pinfunction "ETH_RCTL") (pintype "passive"))
    (pad "103" smd oval (at 18.5 9.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_13") (pintype "passive"))
    (pad "104" smd oval (at 18.5 10.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 162 "Net-(U1-USB2_P)") (pinfunction "USB2_P") (pintype "passive"))
    (pad "105" smd oval (at 18.5 11.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 161 "Net-(U1-USB2_N)") (pinfunction "USB2_N") (pintype "passive"))
    (pad "106" smd oval (at 18.5 12.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_14") (pintype "passive"))
    (pad "107" smd oval (at 18.5 13.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 160 "Net-(U1-USB1_P)") (pinfunction "USB1_P") (pintype "passive"))
    (pad "108" smd oval (at 18.5 14.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 159 "Net-(U1-USB1_N)") (pinfunction "USB1_N") (pintype "passive"))
    (pad "109" smd oval (at 18.5 15.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_15") (pintype "passive"))
    (pad "110" smd oval (at 18.5 16.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 121 "unconnected-(U1-PG5-Pad110)") (pinfunction "PG5") (pintype "passive"))
    (pad "111" smd oval (at 18.5 17.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 122 "WIFI_INT") (pinfunction "PD13") (pintype "passive"))
    (pad "112" smd oval (at 18.5 18.5 90) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_16") (pintype "passive"))
    (pad "113" smd oval (at 17.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_17") (pintype "passive"))
    (pad "114" smd oval (at 16.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 176 "SAI1_SCK_B") (pinfunction "PF8") (pintype "passive"))
    (pad "115" smd oval (at 15.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 177 "SAI1_MCLK_B") (pinfunction "PF7") (pintype "passive"))
    (pad "116" smd oval (at 14.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 178 "SAI1_SD_B") (pinfunction "PF6") (pintype "passive"))
    (pad "117" smd oval (at 13.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 179 "SAI1_FS_B") (pinfunction "PF9") (pintype "passive"))
    (pad "118" smd oval (at 12.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "unconnected-(U1-PB12-Pad118)") (pinfunction "PB12") (pintype "passive"))
    (pad "119" smd oval (at 11.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "unconnected-(U1-PB10-Pad119)") (pinfunction "PB10") (pintype "passive"))
    (pad "120" smd oval (at 10.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "unconnected-(U1-PC3-Pad120)") (pinfunction "PC3") (pintype "passive"))
    (pad "121" smd oval (at 9.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "unconnected-(U1-PI8-Pad121)") (pinfunction "PI8") (pintype "passive"))
    (pad "122" smd oval (at 8.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 127 "unconnected-(U1-PI11-Pad122)") (pinfunction "PI11") (pintype "passive"))
    (pad "123" smd oval (at 7.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "unconnected-(U1-PA10-Pad123)") (pinfunction "PA10") (pintype "passive"))
    (pad "124" smd oval (at 6.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_18") (pintype "passive"))
    (pad "125" smd oval (at 5.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 124 "unconnected-(U1-PF13-Pad125)") (pinfunction "PF13") (pintype "passive"))
    (pad "126" smd oval (at 4.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 125 "unconnected-(U1-PF12-Pad126)") (pinfunction "PF12") (pintype "passive"))
    (pad "127" smd oval (at 3.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "unconnected-(U1-PF10-Pad127)") (pinfunction "PF10") (pintype "passive"))
    (pad "128" smd oval (at 2.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "UART4_TX") (pinfunction "PG11") (pintype "passive"))
    (pad "129" smd oval (at 1.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 180 "SAI1_SD_A") (pinfunction "PB2") (pintype "passive"))
    (pad "130" smd oval (at 0.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 129 "unconnected-(U1-PA15-Pad130)") (pinfunction "PA15") (pintype "passive"))
    (pad "131" smd oval (at -0.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 130 "SWDIO") (pinfunction "SWDIO") (pintype "passive"))
    (pad "132" smd oval (at -1.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "SWCLK") (pinfunction "SWCLK") (pintype "passive"))
    (pad "133" smd oval (at -2.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_19") (pintype "passive"))
    (pad "134" smd oval (at -3.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 132 "MMC1_D0") (pinfunction "MMC1_D0") (pintype "passive"))
    (pad "135" smd oval (at -4.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "MMC1_D1") (pinfunction "MMC1_D1") (pintype "passive"))
    (pad "136" smd oval (at -5.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 134 "MMC1_D2") (pinfunction "MMC1_D2") (pintype "passive"))
    (pad "137" smd oval (at -6.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 135 "MMC1_D3") (pinfunction "MMC1_D3") (pintype "passive"))
    (pad "138" smd oval (at -7.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 136 "MMC1_CK") (pinfunction "MMC1_CK") (pintype "passive"))
    (pad "139" smd oval (at -8.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 140 "MMC1_CMD") (pinfunction "MMC1_CMD") (pintype "passive"))
    (pad "140" smd oval (at -9.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_20") (pintype "passive"))
    (pad "141" smd oval (at -10.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 137 "unconnected-(U1-PZ3-Pad141)") (pinfunction "PZ3") (pintype "passive"))
    (pad "142" smd oval (at -11.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "UART1_TX") (pinfunction "PZ2") (pintype "passive"))
    (pad "143" smd oval (at -12.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "UART1_RX") (pinfunction "PZ1") (pintype "passive"))
    (pad "144" smd oval (at -13.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 138 "unconnected-(U1-PZ0-Pad144)") (pinfunction "PZ0") (pintype "passive"))
    (pad "145" smd oval (at -14.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 139 "unconnected-(U1-PZ6-Pad145)") (pinfunction "PZ6") (pintype "passive"))
    (pad "146" smd oval (at -15.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 153 "WIFI_UP") (pinfunction "PH4") (pintype "passive"))
    (pad "147" smd oval (at -16.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 141 "unconnected-(U1-PZ7-Pad147)") (pinfunction "PZ7") (pintype "passive"))
    (pad "148" smd oval (at -17.5 19.5 180) (size 0.6 1.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GND_21") (pintype "passive"))
    (model "MYC-YA151C-256N256D-65-C-T.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_DIP_SPSTx03_Slide_6.7x9.18mm_W8.61mm_P2.54mm_LowProfile" (layer "B.Cu")
    (at 67.805 95.96 180)
    (descr "SMD 3x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 6.7x9.18mm (see e.g. https://www.ctscorp.com/wp-content/uploads/219.pdf), SMD, LowProfile")
    (tags "SMD DIP Switch SPST Slide 8.61mm 338mil SMD LowProfile")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol")
    (property "ki_keywords" "dip switch")
    (attr smd)
    (fp_text reference "SW1" (at 0 5.65) (layer "B.SilkS"))
    (fp_text value "BOOT" (at -0.005 -5.84) (layer "B.SilkS" knockout))
    (fp_text user "${REFERENCE}" (at 2.58 0 90) (layer "B.Fab"))
    (fp_text user "on" (at 0.4275 3.8825) (layer "B.Fab"))
    (pad "1" smd rect (at -4.305 2.54 180) (size 2.44 1.12) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "BOOT0") (pintype "passive"))
    (pad "2" smd rect (at -4.305 0 180) (size 2.44 1.12) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "BOOT1") (pintype "passive"))
    (pad "3" smd rect (at -4.305 -2.54 180) (size 2.44 1.12) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "BOOT2") (pintype "passive"))
    (pad "4" smd rect (at 4.305 -2.54 180) (size 2.44 1.12) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "+5V") (pintype "passive"))
    (pad "5" smd rect (at 4.305 0 180) (size 2.44 1.12) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "+5V") (pintype "passive"))
    (pad "6" smd rect (at 4.305 2.54 180) (size 2.44 1.12) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_DIP_SPSTx03_Slide_6.7x9.18mm_W8.61mm_P2.54mm_LowProfile.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "B.Cu")
    (at 42.8 32.8 90)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 0.6 -1.6 90) (layer "B.SilkS"))
    (fp_text value "WiFi_Rx" (at 0.8 4 180) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.45 90) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 90) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 174 "Net-(U7-U0RXD)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 35.795 22.445)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 0 -3) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.68) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "B.Cu")
    (at 42.8 35 90)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP4" (at -0.4 -1.6 90) (layer "B.SilkS"))
    (fp_text value "WiFi_Tx" (at -0.6 3.8 180) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.45 90) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 90) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 175 "Net-(U7-U0TXD)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 67 20.4 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C18" (at 0.2 -2.8 90) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_6x6mm_H9.5mm" (layer "B.Cu")
    (at 78.36 95.525 90)
    (descr "tactile push button, 6x6mm e.g. PTS645xx series, height=9.5mm")
    (tags "tact sw push 6mm smd")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr smd)
    (fp_text reference "SW2" (at 5.725 0.04 180) (layer "B.SilkS"))
    (fp_text value "RESET" (at -6.275 -2.96 180) (layer "B.SilkS" knockout))
    (fp_text user "${REFERENCE}" (at 0 4.05 90) (layer "B.Fab"))
    (pad "1" smd rect (at -3.975 2.25 90) (size 1.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 206 "NRST") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 3.975 2.25 90) (size 1.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 206 "NRST") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -3.975 -2.25 90) (size 1.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 3.975 -2.25 90) (size 1.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_PUSH_6mm_H9.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 28.445 27.8 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C17" (at 0.2 -1.8) (layer "B.SilkS"))
    (fp_text value "10pF" (at -0.155 2.8 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(U7-LNA)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(AE1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_RGB_PLCC-6" (layer "B.Cu")
    (at 35 64 180)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (property "Sheetfile" "STM32MP151_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED, 6 pin package")
    (property "ki_keywords" "LED RGB diode")
    (attr smd)
    (fp_text reference "D1" (at 3.6 -0.3 90) (layer "B.SilkS"))
    (fp_text value "LED_RGB" (at -3.4 0.1 90) (layer "B.SilkS"))
    (pad "1" smd rect (at -1.55 1.1 90) (size 0.7 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "RK") (pintype "passive"))
    (pad "2" smd rect (at -1.55 0 90) (size 0.7 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "GK") (pintype "passive"))
    (pad "3" smd rect (at -1.55 -1.1 90) (size 0.7 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "BK") (pintype "passive"))
    (pad "4" smd rect (at 1.55 -1.1 90) (size 0.7 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 158 "Net-(D1-BA)") (pinfunction "BA") (pintype "passive"))
    (pad "5" smd rect (at 1.55 0 90) (size 0.7 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 167 "Net-(D1-GA)") (pinfunction "GA") (pintype "passive"))
    (pad "6" smd rect (at 1.55 1.1 90) (size 0.7 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 168 "Net-(D1-RA)") (pinfunction "RA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_RGB_PLCC-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 58 88 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP151_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at -0.2 2 -270) (layer "B.SilkS"))
    (fp_text value "4K7" (at -3 0.2) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 156 "I2C1_SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 39.595 32.2 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at -2.4 0) (layer "B.SilkS"))
    (fp_text value "10pF" (at -5 0.205 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(U7-XTAL_OUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 35.6 77.2 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP151_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at 0 1.82) (layer "B.SilkS"))
    (fp_text value "220R" (at 0 -1.82) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 169 "LED_R") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 168 "Net-(D1-RA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "B.Cu")
    (at 31.045 28.645 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L2" (at -2.6 0) (layer "B.SilkS"))
    (fp_text value "1.6nH" (at -5.245 0.245 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(U7-LNA)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 77.2 111)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R28" (at -3 0.8 90) (layer "B.SilkS"))
    (fp_text value "27R" (at 0 1.8) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 166 "/Power & Debug/USB_P") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 163 "Net-(U2-USBDP)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm" (layer "B.Cu")
    (at 36.395 32.2)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "Four pin crystal, GND on pins 2 and 4")
    (property "ki_keywords" "quartz ceramic resonator oscillator")
    (attr smd)
    (fp_text reference "Y2" (at 0 2.45) (layer "B.SilkS"))
    (fp_text value "26MHz" (at 0.005 3.8) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "Net-(U7-XTAL_IN)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 1.1 0.85) (size 1.4 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "Net-(U7-XTAL_OUT)") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -1.1 0.85) (size 1.4 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 55 88 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP151_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at -0.2 -1.8 -270) (layer "B.SilkS"))
    (fp_text value "4K7" (at -3 -0.2) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 157 "I2C1_SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_5x5.3" (layer "B.Cu")
    (at 59.4 32.2 -90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C12" (at 0.2 3.8 90) (layer "B.SilkS"))
    (fp_text value "10uF" (at 4.8 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.2 0 270) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 2.2 0 270) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 32.8 21 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -4.4 0 -180) (layer "B.SilkS"))
    (fp_text value "10K" (at -3 0) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 153 "WIFI_UP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PCM3060:SOP65P640X120-28N" (layer "B.Cu")
    (at 69 26.4 -90)
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (attr smd)
    (fp_text reference "U4" (at 0 -6 90) (layer "B.SilkS"))
    (fp_text value "PCM3060PWR" (at -0.2 6 90) (layer "B.SilkS"))
    (pad "1" smd roundrect (at -2.87 4.225 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 156 "I2C1_SCL") (pinfunction "MC/SCL/FMT") (pintype "input"))
    (pad "2" smd roundrect (at -2.87 3.575 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 157 "I2C1_SDA") (pinfunction "MD/SDA/DEMP") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.87 2.925 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 183 "unconnected-(U4-DOUT-Pad3)") (pinfunction "DOUT") (pintype "output"))
    (pad "4" smd roundrect (at -2.87 2.275 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 184 "unconnected-(U4-LRCK1-Pad4)") (pinfunction "LRCK1") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -2.87 1.625 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 185 "unconnected-(U4-BCK1-Pad5)") (pinfunction "BCK1") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.87 0.975 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 186 "unconnected-(U4-SCKI1-Pad6)") (pinfunction "SCKI1") (pintype "input"))
    (pad "7" smd roundrect (at -2.87 0.325 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 205 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "8" smd roundrect (at -2.87 -0.325 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 1 "GND") (pinfunction "DGND") (pintype "power_in"))
    (pad "9" smd roundrect (at -2.87 -0.975 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 176 "SAI1_SCK_B") (pinfunction "SCKI2") (pintype "input"))
    (pad "10" smd roundrect (at -2.87 -1.625 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 177 "SAI1_MCLK_B") (pinfunction "BCK2") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -2.87 -2.275 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 179 "SAI1_FS_B") (pinfunction "LRCK2") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -2.87 -2.925 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 178 "SAI1_SD_B") (pinfunction "DIN") (pintype "input"))
    (pad "13" smd roundrect (at -2.87 -3.575 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 187 "unconnected-(U4-ZEROR-Pad13)") (pinfunction "ZEROR") (pintype "output+no_connect"))
    (pad "14" smd roundrect (at -2.87 -4.225 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 188 "unconnected-(U4-ZEROL-Pad14)") (pinfunction "ZEROL") (pintype "output+no_connect"))
    (pad "15" smd roundrect (at 2.87 -4.225 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 206 "NRST") (pinfunction "~{RST}") (pintype "input"))
    (pad "16" smd roundrect (at 2.87 -3.575 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 1 "GND") (pinfunction "SGND") (pintype "power_in"))
    (pad "17" smd roundrect (at 2.87 -2.925 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 189 "unconnected-(U4-VOUTR--Pad17)") (pinfunction "VOUTR-") (pintype "output+no_connect"))
    (pad "18" smd roundrect (at 2.87 -2.275 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 41 "Net-(U4-VOUTR+)") (pinfunction "VOUTR+") (pintype "output"))
    (pad "19" smd roundrect (at 2.87 -1.625 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 190 "unconnected-(U4-VOUTL--Pad19)") (pinfunction "VOUTL-") (pintype "output+no_connect"))
    (pad "20" smd roundrect (at 2.87 -0.975 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 44 "Net-(U4-VOUTL+)") (pinfunction "VOUTL+") (pintype "output"))
    (pad "21" smd roundrect (at 2.87 -0.325 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 82 "/Audio/VCOM") (pinfunction "VCOM") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 2.87 0.325 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 1 "GND") (pinfunction "AGND2") (pintype "power_in"))
    (pad "23" smd roundrect (at 2.87 0.975 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 1 "GND") (pinfunction "AGND1") (pintype "power_in"))
    (pad "24" smd roundrect (at 2.87 1.625 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 3 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "25" smd roundrect (at 2.87 2.275 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 191 "unconnected-(U4-VINL-Pad25)") (pinfunction "VINL") (pintype "input"))
    (pad "26" smd roundrect (at 2.87 2.925 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 192 "unconnected-(U4-VINR-Pad26)") (pinfunction "VINR") (pintype "input"))
    (pad "27" smd roundrect (at 2.87 3.575 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 193 "unconnected-(U4-~{MS{slash}ADR{slash}IFMD}-Pad27)") (pinfunction "~{MS/ADR/IFMD}") (pintype "input"))
    (pad "28" smd roundrect (at 2.87 4.225 270) (size 1.57 0.41) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.05)
      (net 1 "GND") (pinfunction "MODE") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 35.6 73.4 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP151_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R25" (at 0 1.82) (layer "B.SilkS"))
    (fp_text value "220R" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 170 "LED_G") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 167 "Net-(D1-GA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 83 98.2 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 1 1.8 270) (layer "B.SilkS"))
    (fp_text value "10K" (at 3 0.4) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 206 "NRST") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 3 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 66.4 31.4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C19" (at -3.2 0) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0.2 -1.6) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 35.6 69.8 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP151_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R26" (at 0 1.82) (layer "B.SilkS"))
    (fp_text value "220R" (at 0 3) (layer "User.1"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 171 "LED_B") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 158 "Net-(D1-BA)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 36 49.15 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "STM32MP151_Dev_Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at 2.8 0.35 90) (layer "B.SilkS"))
    (fp_text value "27R" (at 0 -1.82) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 160 "Net-(U1-USB1_P)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2222222222)
      (net 119 "USB1_P") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Audio:Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal" (layer "B.Cu")
    (at 79.8 23 180)
    (descr "3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)")
    (tags "3.5mm audio cui horizontal jack stereo")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Audio Jack, 3 Poles (Stereo / TRS)")
    (property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector")
    (attr smd)
    (fp_text reference "J2" (at 0 9.9) (layer "B.SilkS"))
    (fp_text value "AudioJack3" (at 1.6 -9.8 180) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "" np_thru_hole circle (at 0 -4.5 180) (size 1.7 1.7) (drill 1.7) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 0 2.5 180) (size 1.7 1.7) (drill 1.7) (layers "*.Cu" "*.Mask"))
    (pad "R" smd rect (at 3.7 1.6 180) (size 2.8 2.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "Net-(U4-VOUTR+)") (pintype "passive"))
    (pad "S" smd rect (at -3.7 3.6 180) (size 2.8 2.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "Net-(U4-VOUTL+)") (pintype "passive"))
    (pad "T" smd rect (at -3.7 -5.8 180) (size 2.8 2.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "/Audio/VCOM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (at 47.4 118.8 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at -4.4 -4.2) (layer "B.SilkS"))
    (fp_text value "UART4" (at -2.6 -1.2) (layer "B.SilkS" knockout))
    (fp_text user "${REFERENCE}" (at 0 -3.81) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 94 "UART4_RX") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 128 "UART4_TX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 30.6 32.6 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R29" (at 0 1.82 90) (layer "B.SilkS"))
    (fp_text value "12K" (at 0 -1.82 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 173 "Net-(U7-RES12K)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "B.Cu")
    (at 39.995 23.245 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "WIFI.kicad_sch")
    (property "Sheetname" "WIFI")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C14" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 2.4 0.2) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:Texas_DRT-3" (layer "B.Cu")
    (at 70.975 110.6 90)
    (descr "Texas Instrument DRT-3 1x0.8mm Pitch 0.7mm http://www.ti.com/lit/ds/symlink/tpd2eusb30.pdf")
    (tags "DRT-3 1x0.8mm Pitch 0.7mm")
    (property "Sheetfile" "debug.kicad_sch")
    (property "Sheetname" "Power & Debug")
    (property "ki_description" "2-Channel ESD Protection for Super-Speed USB 3.0 Interface, DRT-3")
    (property "ki_keywords" "ESD protection USB 3.0")
    (attr smd)
    (fp_text reference "U5" (at -1.6 0.2 180) (layer "B.SilkS"))
    (fp_text value "TPD2EUSB30" (at 1.6 -1.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.5 90) (layer "B.Fab"))
    (pad "1" smd rect (at -0.35 -0.425 90) (size 0.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 166 "/Power & Debug/USB_P") (pinfunction "D+") (pintype "passive"))
    (pad "2" smd rect (at 0.35 -0.425 90) (size 0.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 165 "/Power & Debug/USB_N") (pinfunction "D-") (pintype "passive"))
    (pad "3" smd rect (at 0 0.425 90) (size 0.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "Earth") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Texas_DRT-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_5x5.3" (layer "B.Cu")
    (at 59.4 20.4 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 5.0x5.3mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C20" (at 0 -3.8 90) (layer "B.SilkS"))
    (fp_text value "10uF" (at 4.8 0) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.2 0 90) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 205 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 2.2 0 90) (size 3 1.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_5x5.3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 87 121) (end 15 121)
    (layer "Edge.Cuts"))
  (gr_line (start 15 15) (end 87 15)
    (layer "Edge.Cuts"))
  (gr_line (start 87 15) (end 87 121)
    (layer "Edge.Cuts"))
  (gr_line (start 15 121) (end 15 15)
    (layer "Edge.Cuts"))
  (gr_text "BOOT2" (at 61.8 99.2) (layer "B.SilkS"))
  (gr_text "BOOT0" (at 61.8 94.2) (layer "B.SilkS"))
  (gr_text "https://github.com/BasicCode" (at 44.1 117) (layer "B.SilkS" knockout))
  (gr_text "BOOT1" (at 61.8 96.6) (layer "B.SilkS"))
  (gr_text "REV B" (at 20.7 120) (layer "B.SilkS"))
  (gr_text "STM32MP151 DEV BOARD" (at 44.5 119) (layer "B.SilkS"))
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 87 121) (xy 51 121))
    (height -5.8)
    (gr_text "36.0000 mm" (at 69 125.65) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 87 121) (xy 87 15))
    (height 9.6)
    (gr_text "106.0000 mm" (at 95.45 68 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 87 121) (xy 87 68))
    (height 6)
    (gr_text "53.0000 mm" (at 91.85 94.5 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 15 121) (xy 87 121))
    (height 7.8)
    (gr_text "72.0000 mm" (at 53 130.6) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 1) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 15 15)
        (xy 87 15)
        (xy 87 121)
        (xy 15 121)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F&B.Cu") (name "Antenna") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 15 15)
        (xy 21 15)
        (xy 21 31)
        (xy 15 31)
      )
    )
  )
)
