<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="34.3" y1="8.4" x2="34.3" y2="24.13" width="0" layer="20"/>
<wire x1="34.3" y1="24.13" x2="33.03" y2="25.4" width="0" layer="20" curve="90"/>
<wire x1="33.03" y1="25.4" x2="1.27" y2="25.4" width="0" layer="20"/>
<wire x1="1.27" y1="25.4" x2="0" y2="24.13" width="0" layer="20" curve="90"/>
<wire x1="0" y1="24.13" x2="0" y2="8.4" width="0" layer="20"/>
<text>Swap Drive</text>
<text>LM3406 - 1.2A </text>
<text>Rev B</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="LQH55">
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0402K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0204 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1005</description>
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="PocketNC">
<packages>
<package name="HTSSOP-14">
</package>
<package name="PCIE_64_SMART_BOARD">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CB" library="adafruit" package="C0603" value="22nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="PocketNC" package="HTSSOP-14" value="LM3406">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$7" library="adafruit" package="LQH55" value="L-13uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CC" library="adafruit" package="C0603" value="100nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CF" library="adafruit" package="C0603" value="100nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="PocketNC" package="PCIE_64_SMART_BOARD" value=""/>
<element name="U$5" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$6" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="2N7002P" library="adafruit" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="R0603" value="460">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RED" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GRN" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="460">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="adafruit" package="R0603" value="460">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="adafruit" package="C0603" value=".1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R-ON" library="adafruit" package="R0805" value="148k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CO" library="adafruit" package="C1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="B340A">
<attribute name="PROD_ID" value="DIO-09886"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C0805" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0805" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0402K" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R2010" value=".166">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="P$3"/>
<contactref element="CB" pad="1"/>
</signal>
<signal name="SW">
<contactref element="CB" pad="2"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="U$7" pad="1"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="GND">
<contactref element="CC" pad="1"/>
<contactref element="CF" pad="1"/>
<contactref element="U$1" pad="P$7"/>
<contactref element="U$1" pad="P$15"/>
<contactref element="U$2" pad="P$49"/>
<contactref element="U$2" pad="P$60"/>
<contactref element="U$2" pad="P$25"/>
<contactref element="U$2" pad="P$13"/>
<contactref element="U$2" pad="P$53"/>
<contactref element="U$2" pad="GND@1"/>
<contactref element="U$2" pad="GND@2"/>
<contactref element="U$2" pad="GND@3"/>
<contactref element="2N7002P" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="LS-">
<contactref element="U$1" pad="P$6"/>
<contactref element="CO" pad="2"/>
<contactref element="U$2" pad="P$36"/>
<contactref element="U$2" pad="P$35"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="LS+">
<contactref element="U$7" pad="2"/>
<contactref element="U$1" pad="P$5"/>
<contactref element="CO" pad="1"/>
<contactref element="U$2" pad="P$33"/>
<contactref element="U$2" pad="P$34"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="VCC@1"/>
<contactref element="U$2" pad="VCC@2"/>
<contactref element="U$2" pad="VCC@3"/>
<contactref element="R-ON" pad="2"/>
<contactref element="U$1" pad="P$14"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U$1" pad="P$13"/>
<contactref element="U$1" pad="P$12"/>
</signal>
<signal name="RON">
<contactref element="U$1" pad="P$10"/>
<contactref element="R-ON" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="P$9"/>
<contactref element="CC" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="P$11"/>
<contactref element="CF" pad="2"/>
</signal>
<signal name="DIR">
<contactref element="U$2" pad="P$57@1"/>
</signal>
<signal name="SCL">
<contactref element="U$2" pad="P$45"/>
</signal>
<signal name="SDA">
<contactref element="U$2" pad="P$14"/>
</signal>
<signal name="3V">
<contactref element="U$2" pad="P$12"/>
<contactref element="R7" pad="2"/>
<contactref element="GRN" pad="A"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="ENBL-IN">
<contactref element="2N7002P" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="U$2" pad="P$22@1"/>
</signal>
<signal name="N$8">
<contactref element="GRN" pad="C"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="ENBL-OUT">
<contactref element="2N7002P" pad="3"/>
<contactref element="R7" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="RED" pad="A"/>
<contactref element="U$1" pad="P$8"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="1"/>
<contactref element="RED" pad="C"/>
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
