<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="49.53" y2="0" width="0" layer="20"/>
<wire x1="49.53" y1="0" x2="49.53" y2="24.13" width="0" layer="20"/>
<wire x1="49.53" y1="24.13" x2="0" y2="24.13" width="0" layer="20"/>
<wire x1="0" y1="24.13" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.032" y="22.098" drill="3.048"/>
<hole x="2.032" y="2.032" drill="3.048"/>
<hole x="47.498" y="2.032" drill="3.048"/>
<hole x="47.498" y="22.098" drill="3.048"/>
<text>ReDesigned By
Özay Turay
a.k.a Simon/CGTr
http://www.commodore.gen.tr
Original Design By
Peter Edwards
a.k.a sweetlilmre
http://www.sweetlilmre.com</text>
<text>Tapuino</text>
<text>Type A
Version
1.02</text>
<text>Mini</text>
</plain>
<libraries>
<library name="sj_connectors">
<description>&lt;b&gt;Popular Connectors Library&lt;/b&gt;
&lt;p&gt;
Popular Connectors Library is a set of components for using popular connectors in your schematic and board designs.</description>
<packages>
<package name="1X04_SQR">
<description>1x04 - 0.1" Pin Header Package (First Pin Square, Other Pins Octagon)</description>
</package>
<package name="1X06_SQR">
<description>1x06 - 0.1" Pin Header Package (First Pin Square, Other Pins Octagon)</description>
</package>
<package name="1X05_SQR">
<description>1x05 - 0.1" Pin Header Package (First Pin Square, Other Pins Octagon)</description>
</package>
<package name="1X02_SQR">
<description>1x02 - 0.1" Pin Header Package (First Pin Square, Other Pins Octagon)</description>
</package>
</packages>
</library>
<library name="sj_standart">
<description>&lt;b&gt;Standart Components Library&lt;/b&gt;
&lt;p&gt;Standart Components Library is a set of standart components for using in your schematic and board designs.</description>
<packages>
<package name="DIP06">
<description>6-pin Dual In Line Package</description>
</package>
<package name="RESISTOR_PTH_0.3">
<description>Resistor (0.3" Pin Spacing) Package</description>
</package>
<package name="TO-92">
<description>TO-92 (Type A) Package</description>
</package>
</packages>
</library>
<library name="sj_arduino">
<description>&lt;b&gt;Arduino Clones Library&lt;/b&gt;
&lt;p&gt;
Arduino Clones Library is a set of components for using cheap Arduino clones in your schematic and board designs.</description>
<packages>
<package name="PROMINI_A">
<description>Arduino Pro Mini Package (Type A)</description>
</package>
</packages>
</library>
<library name="sj_temp">
<description>&lt;b&gt;Temporary Library&lt;/b&gt;
&lt;p&gt;Temporary Library is for duplicating and modifying components and working on them.</description>
<packages>
<package name="OSHW-LOGO-L">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="sj_connectors" package="1X04_SQR" value="LCD">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="sj_connectors" package="1X06_SQR" value="SD">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="sj_connectors" package="1X05_SQR" value="BTN">
<attribute name="VALUE"/>
</element>
<element name="OK1" library="sj_standart" package="DIP06" value="4N25">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="sj_connectors" package="1X06_SQR" value="C64">
<attribute name="VALUE"/>
</element>
<element name="R5" library="sj_standart" package="RESISTOR_PTH_0.3" value="330">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="sj_arduino" package="PROMINI_A" value="Arduino ProMini">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="sj_standart" package="TO-92" value="2N2222">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="sj_standart" package="TO-92" value="2N2222">
<attribute name="VALUE"/>
</element>
<element name="R1" library="sj_standart" package="RESISTOR_PTH_0.3" value="1K">
<attribute name="VALUE"/>
</element>
<element name="R2" library="sj_standart" package="RESISTOR_PTH_0.3" value="1K">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="sj_connectors" package="1X02_SQR" value="&lt;R">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="sj_connectors" package="1X02_SQR" value="&lt;W">
<attribute name="VALUE"/>
</element>
<element name="R3" library="sj_standart" package="RESISTOR_PTH_0.3" value="220">
<attribute name="VALUE"/>
</element>
<element name="R4" library="sj_standart" package="RESISTOR_PTH_0.3" value="220">
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="sj_temp" package="OSHW-LOGO-L" value="OSHW-LOGOL"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="IC1" pad="VCC"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="OK1" pad="2"/>
<contactref element="OK1" pad="4"/>
<contactref element="IC1" pad="GND@1"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="CS">
<contactref element="JP2" pad="6"/>
<contactref element="IC1" pad="10*"/>
</signal>
<signal name="NEXT">
<contactref element="JP3" pad="2"/>
<contactref element="IC1" pad="A0"/>
</signal>
<signal name="PREV">
<contactref element="JP3" pad="3"/>
<contactref element="IC1" pad="A1"/>
</signal>
<signal name="ABORT">
<contactref element="JP3" pad="4"/>
<contactref element="IC1" pad="A2"/>
</signal>
<signal name="SELECT">
<contactref element="JP3" pad="5"/>
<contactref element="IC1" pad="A3"/>
</signal>
<signal name="SENSE">
<contactref element="JP4" pad="6"/>
<contactref element="IC1" pad="5*"/>
</signal>
<signal name="WRITE1">
<contactref element="JP4" pad="5"/>
<contactref element="IC1" pad="8"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="READ1">
<contactref element="JP4" pad="4"/>
<contactref element="IC1" pad="3*"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="MOTOR1">
<contactref element="JP4" pad="3"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="MOTOR2">
<contactref element="R5" pad="2"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="MOTOR3">
<contactref element="OK1" pad="5"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="A4"/>
</signal>
<signal name="SCL">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="A5"/>
</signal>
<signal name="READ2">
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="WRITE2">
<contactref element="Q2" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="WRITE3">
<contactref element="Q2" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="WRITE4">
<contactref element="JP6" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="READ3">
<contactref element="Q1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="READ4">
<contactref element="JP5" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="JP2" pad="3"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="MOSI">
<contactref element="JP2" pad="4"/>
<contactref element="IC1" pad="11*"/>
</signal>
<signal name="SCK">
<contactref element="JP2" pad="5"/>
<contactref element="IC1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
