(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 59)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 7)
    (tracks 258)
    (zones 0)
    (modules 7)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.08 5.08)
    (pad_drill 3.556)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad8)")
  (net 6 "Net-(J1-Pad7)")
  (net 7 "Net-(J1-Pad17)")
  (net 8 "Net-(J1-Pad9)")
  (net 9 "Net-(J1-Pad10)")
  (net 10 "Net-(J1-Pad11)")
  (net 11 "Net-(J1-Pad4)")
  (net 12 "Net-(J1-Pad3)")
  (net 13 "Net-(J1-Pad2)")
  (net 14 "Net-(J1-Pad1)")
  (net 15 "Net-(J1-Pad16)")
  (net 16 "Net-(J1-Pad15)")
  (net 17 "Net-(J1-Pad14)")
  (net 18 "Net-(J1-Pad13)")
  (net 19 "Net-(J2-Pad3)")
  (net 20 "Net-(J2-Pad4)")
  (net 21 "Net-(J2-Pad5)")
  (net 22 "Net-(J2-Pad6)")
  (net 23 "Net-(J2-Pad7)")
  (net 24 "Net-(J2-Pad8)")
  (net 25 "Net-(J2-Pad9)")
  (net 26 "Net-(J2-Pad10)")
  (net 27 "Net-(J2-Pad11)")
  (net 28 "Net-(J2-Pad12)")
  (net 29 "Net-(J2-Pad13)")
  (net 30 "Net-(J2-Pad14)")
  (net 31 "Net-(J2-Pad15)")
  (net 32 "Net-(J2-Pad16)")
  (net 33 "Net-(J2-Pad17)")
  (net 34 "Net-(J2-Pad18)")
  (net 35 "Net-(J2-Pad19)")
  (net 36 "Net-(J2-Pad20)")
  (net 37 "Net-(J2-Pad21)")
  (net 38 "Net-(J2-Pad23)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5AAB942A)
    (at 138.43 92.71 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value "" (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5AAB9437)
    (at 138.43 115.57 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value "" (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AAB93FC)
    (at 141.605 128.27 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C3 (at 1.25 -2.11 180) (layer F.SilkS))
    (fp_text value "" (at 1.25 2.11 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module GPIB-IF:GPIB_conn_male (layer F.Cu) (tedit 5AAB93DD)
    (at 123.19 107.95 270)
    (descr "standard male GPIB connector")
    (tags "GPIB HPIB IEEE488")
    (fp_text reference J1 (at 12.192 -7.874 270) (layer F.SilkS))
    (fp_text value "" (at -15.748 -7.493 270) (layer F.SilkS))
    (pad 6 thru_hole circle (at -1.0795 -2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at -3.2385 -2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad5)"))
    (pad 8 thru_hole circle (at 3.2385 -2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad8)"))
    (pad 7 thru_hole circle (at 1.0795 -2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad7)"))
    (pad 18 thru_hole circle (at -1.0795 2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 19 thru_hole circle (at 1.0795 2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 20 thru_hole circle (at 3.2385 2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 17 thru_hole circle (at -3.2385 2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad17)"))
    (pad 9 thru_hole circle (at 5.3975 -2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at 7.5565 -2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at 9.7155 -2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at 11.8745 -2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 21 thru_hole circle (at 5.3975 2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 22 thru_hole circle (at 7.5565 2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 23 thru_hole circle (at 9.7155 2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 24 thru_hole circle (at 11.8745 2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4 thru_hole circle (at -5.3975 -2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at -7.5565 -2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at -9.7155 -2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at -11.8745 -2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad1)"))
    (pad 16 thru_hole circle (at -5.3975 2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad16)"))
    (pad 15 thru_hole circle (at -7.5565 2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad15)"))
    (pad 14 thru_hole circle (at -9.7155 2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad14)"))
    (pad 13 thru_hole circle (at -11.8745 2.1463 270) (size 1.4 1.4) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J1-Pad13)"))
    (pad 25 thru_hole circle (at -23.4061 0 270) (size 5.08 5.08) (drill 3.556) (layers *.Cu *.Mask F.SilkS))
    (pad 26 thru_hole circle (at 23.4061 0 270) (size 5.08 5.08) (drill 3.556) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Angled_2x13_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 154.94 91.44)
    (descr "Through hole angled pin header, 2x13, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x13 2.54mm double row")
    (fp_text reference J2 (at 5.655 -2.27) (layer F.SilkS))
    (fp_text value CONN_02X13 (at 5.655 32.75) (layer F.Fab))
    (fp_text user %R (at 5.31 15.24 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x13_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-24W_7.5x15.4mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 138.43 115.57)
    (descr "24-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -8.8) (layer F.SilkS))
    (fp_text value SN75162B (at 0 8.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-Pad3)"))
    (pad 2 smd rect (at -4.7 -5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J2-Pad7)"))
    (pad 3 smd rect (at -4.7 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad17)"))
    (pad 4 smd rect (at -4.7 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad9)"))
    (pad 5 smd rect (at -4.7 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 6 smd rect (at -4.7 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad7)"))
    (pad 7 smd rect (at -4.7 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 8 smd rect (at -4.7 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 9 smd rect (at -4.7 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad11)"))
    (pad 10 smd rect (at -4.7 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad10)"))
    (pad 11 smd rect (at -4.7 5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -4.7 6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 13 smd rect (at 4.7 6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J2-Pad5)"))
    (pad 14 smd rect (at 4.7 5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 4.7 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J2-Pad23)"))
    (pad 16 smd rect (at 4.7 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J2-Pad21)"))
    (pad 17 smd rect (at 4.7 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-Pad19)"))
    (pad 18 smd rect (at 4.7 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J2-Pad17)"))
    (pad 19 smd rect (at 4.7 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J2-Pad15)"))
    (pad 20 smd rect (at 4.7 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J2-Pad13)"))
    (pad 21 smd rect (at 4.7 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J2-Pad11)"))
    (pad 22 smd rect (at 4.7 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J2-Pad9)"))
    (pad 23 smd rect (at 4.7 -5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 4.7 -6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-24W_7.5x15.4mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 138.43 92.71)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -7.5) (layer F.SilkS))
    (fp_text value SN75160B (at 0 7.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J2-Pad7)"))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad3)"))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad13)"))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad14)"))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad15)"))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad16)"))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J2-Pad4)"))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J2-Pad6)"))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J2-Pad8)"))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J2-Pad10)"))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J2-Pad12)"))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J2-Pad14)"))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J2-Pad16)"))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J2-Pad18)"))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J2-Pad20)"))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Mattis Lind" (at 146.685 83.185) (layer F.SilkS))
  (gr_text www.datormuseum.se (at 145.415 132.715) (layer F.SilkS))
  (gr_line (start 112.395 80.01) (end 112.395 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.29 80.01) (end 112.395 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.29 85.725) (end 161.29 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.29 135.89) (end 161.29 85.725) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.395 135.89) (end 161.29 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name "Net-(C1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.29 135.89) (xy 112.395 135.89) (xy 112.395 80.01) (xy 161.29 80.01)
      )
    )
  )
  (zone (net 2) (net_name "Net-(C1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.29 135.89) (xy 112.395 135.89) (xy 112.395 80.01) (xy 161.29 80.01)
      )
    )
  )
)
