(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 1195)
    (zones 0)
    (modules 54)
    (nets 59)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.254000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 D3)
  (net 2 LA)
  (net 3 LB)
  (net 4 LC)
  (net 5 LD)
  (net 6 D2)
  (net 7 D1)
  (net 8 LE)
  (net 9 LG)
  (net 10 LF)
  (net 11 LH)
  (net 12 GND)
  (net 13 5V)
  (net 14 VCC)
  (net 15 SRCLK)
  (net 16 RCLK)
  (net 17 OE)
  (net 18 SER)
  (net 19 10)
  (net 20 11)
  (net 21 "Net-(J1-Pad10)")
  (net 22 14)
  (net 23 15)
  (net 24 16)
  (net 25 17)
  (net 26 18)
  (net 27 19)
  (net 28 20)
  (net 29 21)
  (net 30 22)
  (net 31 23)
  (net 32 "Net-(R2-Pad2)")
  (net 33 "Net-(R3-Pad2)")
  (net 34 "Net-(R4-Pad2)")
  (net 35 "Net-(R5-Pad2)")
  (net 36 "Net-(R6-Pad2)")
  (net 37 "Net-(R7-Pad2)")
  (net 38 "Net-(R8-Pad2)")
  (net 39 "Net-(R9-Pad2)")
  (net 40 BA)
  (net 41 BB)
  (net 42 BD)
  (net 43 D0)
  (net 44 BC)
  (net 45 D6)
  (net 46 BH)
  (net 47 BG)
  (net 48 BF)
  (net 49 BE)
  (net 50 "Net-(U1-Pad9)")
  (net 51 "Net-(U2-Pad9)")
  (net 52 "Net-(U3-Pad1)")
  (net 53 D4)
  (net 54 D5)
  (net 55 D7)
  (net 56 "Net-(U3-Pad18)")
  (net 57 "Net-(U3-Pad20)")
  (net 58 "Net-(R1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 10)
    (add_net 11)
    (add_net 14)
    (add_net 15)
    (add_net 16)
    (add_net 17)
    (add_net 18)
    (add_net 19)
    (add_net 20)
    (add_net 21)
    (add_net 22)
    (add_net 23)
    (add_net 5V)
    (add_net BA)
    (add_net BB)
    (add_net BC)
    (add_net BD)
    (add_net BE)
    (add_net BF)
    (add_net BG)
    (add_net BH)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net GND)
    (add_net LA)
    (add_net LB)
    (add_net LC)
    (add_net LD)
    (add_net LE)
    (add_net LF)
    (add_net LG)
    (add_net LH)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad18)")
    (add_net "Net-(U3-Pad20)")
    (add_net OE)
    (add_net RCLK)
    (add_net SER)
    (add_net SRCLK)
    (add_net VCC)
  )
  (module AOR_custom:AOR_LOGO (layer F.Cu) (tedit 5C26ADAA)
    (at 133.858 125.222)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 147.701 69.3674)
    (fp_text reference D22 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 LH))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 D1))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CF1EB29)
    (at 108.585 57.15)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CF1EB29)
    (at 160.655 57.15)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CF1EB29)
    (at 149.86 153.035)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 110.0074 48.387)
    (fp_text reference D1 (at -1.8034 2.667) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 D3))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 LA))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 120.06072 48.387)
    (fp_text reference D2 (at -1.69672 2.667) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 D3))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 LB))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 130.11404 48.387)
    (fp_text reference D3 (at -1.84404 2.667) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 LC))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 D3))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 126.7206 115.316)
    (fp_text reference D4 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 LD))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 D2))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 126.7206 130.285066)
    (fp_text reference D5 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 D2))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 LA))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 126.7206 145.254132)
    (fp_text reference D6 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 LD))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 D1))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 126.7206 160.2232)
    (fp_text reference D7 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 LA))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 D1))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 140.16736 48.387)
    (fp_text reference D8 (at -1.73736 2.667) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 D3))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 LD))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 134.7229 115.316)
    (fp_text reference D9 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 D2))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 LE))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 134.7229 130.285066)
    (fp_text reference D10 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 LB))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 D2))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 134.7229 145.254132)
    (fp_text reference D11 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 D1))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 LE))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 134.7229 160.2232)
    (fp_text reference D12 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 D1))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 LB))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 150.22068 48.387)
    (fp_text reference D13 (at -1.63068 2.667) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 LE))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 D3))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 139.7 61.3664)
    (fp_text reference D14 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 D3))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 LG))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 139.7 69.3674)
    (fp_text reference D15 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 D1))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 LG))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 142.7252 115.316)
    (fp_text reference D16 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 LF))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 D2))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 142.7252 130.285066)
    (fp_text reference D17 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 D2))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 LC))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 142.7252 145.254132)
    (fp_text reference D18 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 LF))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 D1))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 142.7252 160.2232)
    (fp_text reference D19 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 LC))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 D1))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 160.274 48.387)
    (fp_text reference D20 (at -1.524 2.667) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 D3))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 LF))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 147.701 61.3664)
    (fp_text reference D21 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 LH))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 D3))
  )
  (module Connector_IDC:IDC-Header_2x10_P2.54mm_Vertical (layer B.Cu) (tedit 59DE0251)
    (at 119.888 94.234)
    (descr "Through hole straight IDC box header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x10 2.54mm double row")
    (fp_text reference J1 (at 1.27 6.604) (layer B.SilkS))
    (fp_text value Conn_01x20 (at 1.27 -29.464) (layer B.Fab))
    (fp_text user %R (at 1.27 -11.43) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 5V))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 VCC))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 SRCLK))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 RCLK))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 OE))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 SER))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 10))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 11))
    (pad 10 thru_hole oval (at 2.54 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 14))
    (pad 12 thru_hole oval (at 2.54 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 15))
    (pad 13 thru_hole oval (at 0 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 16))
    (pad 14 thru_hole oval (at 2.54 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 17))
    (pad 15 thru_hole oval (at 0 -17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 18))
    (pad 16 thru_hole oval (at 2.54 -17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 19))
    (pad 17 thru_hole oval (at 0 -20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 20))
    (pad 18 thru_hole oval (at 2.54 -20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 21))
    (pad 19 thru_hole oval (at 0 -22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 22))
    (pad 20 thru_hole oval (at 2.54 -22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 23))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 119.888 103.378 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 270) (layer B.SilkS))
    (fp_text value Conn_01x02 (at 0 -4.87 270) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 GND))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 113.03 82.296 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.8 90) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0 90) (size 1 0.5) (layers B.Cu B.Mask)
      (net 14 VCC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 90) (size 1 0.5) (layers B.Cu B.Mask)
      (net 21 "Net-(J1-Pad10)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.876 86.36 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 LA))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 32 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 147.32 86.36 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 33 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 LB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 143.764 86.36 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 LC))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 34 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 140.208 86.36 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 35 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 LD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 136.652 86.36 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 LE))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 36 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 133.096 86.36 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 37 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 LF))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 129.54 86.36 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 LG))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 38 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 125.984 86.36 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 39 "Net-(R9-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 LH))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 110.6932 92.2274)
    (fp_text reference SW1 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 40 BA) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 D2))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 LG))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 20 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 158.6992 92.2274)
    (fp_text reference SW2 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 20 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 LH))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 D2))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 41 BB) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 110.6932 115.3668)
    (fp_text reference SW3 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 42 BD) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 D0))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 LD))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 19 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 110.6932 130.3528)
    (fp_text reference SW4 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 44 BC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 D0))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 LC))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 19 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 110.6932 145.3388)
    (fp_text reference SW5 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 41 BB) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 D0))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 LB))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 19 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 110.6932 160.3248)
    (fp_text reference SW6 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 40 BA) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 D0))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 LA))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 19 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 126.0348 63.0428)
    (fp_text reference SW7 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 20 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 58 "Net-(R1-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 GND))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 44 BC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 158.6992 115.3668)
    (fp_text reference SW9 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 19 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 LH))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 D0))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 46 BH) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 158.6992 130.3528)
    (fp_text reference SW10 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 19 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 LG))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 D0))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 47 BG) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 158.6992 145.3388)
    (fp_text reference SW11 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 19 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 LF))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 D0))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 48 BF) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 158.6992 160.3248)
    (fp_text reference SW12 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 19 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 LE))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 D0))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 49 BE) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 138.938 77.724 270)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -6 270) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 16 smd rect (at 2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 VCC))
    (pad 15 smd rect (at 2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 BA))
    (pad 14 smd rect (at 2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 SER))
    (pad 13 smd rect (at 2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 OE))
    (pad 12 smd rect (at 2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 RCLK))
    (pad 11 smd rect (at 2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 SRCLK))
    (pad 10 smd rect (at 2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 VCC))
    (pad 9 smd rect (at 2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad9)"))
    (pad 8 smd rect (at -2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 7 smd rect (at -2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 BH))
    (pad 6 smd rect (at -2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 BG))
    (pad 5 smd rect (at -2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 BF))
    (pad 4 smd rect (at -2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 BE))
    (pad 3 smd rect (at -2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 BD))
    (pad 2 smd rect (at -2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 BC))
    (pad 1 smd rect (at -2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 BB))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 138.938 93.472 270)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -6 270) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at -2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R4-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R5-Pad2)"))
    (pad 4 smd rect (at -2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R6-Pad2)"))
    (pad 5 smd rect (at -2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R7-Pad2)"))
    (pad 6 smd rect (at -2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R8-Pad2)"))
    (pad 7 smd rect (at -2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R9-Pad2)"))
    (pad 8 smd rect (at -2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 9 smd rect (at 2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at 2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 VCC))
    (pad 11 smd rect (at 2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 SRCLK))
    (pad 12 smd rect (at 2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 RCLK))
    (pad 13 smd rect (at 2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 OE))
    (pad 14 smd rect (at 2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad9)"))
    (pad 15 smd rect (at 2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R2-Pad2)"))
    (pad 16 smd rect (at 2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 138.176 105.156 90)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 -7.5 90) (layer F.SilkS))
    (fp_text value TPIC6595 (at 0 7.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -4.7 -4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 VCC))
    (pad 3 smd rect (at -4.7 -3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U2-Pad9)"))
    (pad 4 smd rect (at -4.7 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 D0))
    (pad 5 smd rect (at -4.7 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 D1))
    (pad 6 smd rect (at -4.7 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 D2))
    (pad 7 smd rect (at -4.7 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 D3))
    (pad 8 smd rect (at -4.7 3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 VCC))
    (pad 9 smd rect (at -4.7 4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 OE))
    (pad 10 smd rect (at -4.7 5.715 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 11 smd rect (at 4.7 5.715 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 12 smd rect (at 4.7 4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 RCLK))
    (pad 13 smd rect (at 4.7 3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 SRCLK))
    (pad 14 smd rect (at 4.7 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 D4))
    (pad 15 smd rect (at 4.7 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 D5))
    (pad 16 smd rect (at 4.7 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 D6))
    (pad 17 smd rect (at 4.7 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 D7))
    (pad 18 smd rect (at 4.7 -3.175 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U3-Pad18)"))
    (pad 19 smd rect (at 4.7 -4.445 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 20 smd rect (at 4.7 -5.715 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U3-Pad20)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CF1EB29)
    (at 119.38 153.035)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module AOR_custom:AOR_LOGO (layer B.Cu) (tedit 5C26ADAA)
    (at 134.62 128.524 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 112.776 72.136 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 VCC))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 58 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 5V (at 122.428 106.172 90) (layer B.SilkS))
  (gr_text GND (at 119.888 106.68 90) (layer B.SilkS))
  (gr_text "ACP3-W-PR2-PCB\nREV A, 6-2-2019" (at 134.112 120.396) (layer F.SilkS))
  (gr_text "ACP3-W-PR2-PCB\nREV A, 6-2-2019" (at 133.858 123.444) (layer B.SilkS))
  (gr_text "PIN 12 HIGH" (at 110.744 82.296 90) (layer B.SilkS))
  (gr_line (start 104.775 46.355) (end 164.465 46.355) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 104.775 166.37) (end 104.775 46.355) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 164.465 166.37) (end 164.465 46.355) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 104.775 166.37) (end 164.465 166.37) (layer Edge.Cuts) (width 0.2))
  (zone (net 12) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.775 46.355) (xy 164.465 46.355) (xy 164.465 166.37) (xy 105.41 166.37) (xy 104.775 166.37)
      )
    )
  )
  (zone (net 12) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.775 46.355) (xy 164.465 46.355) (xy 164.465 166.37) (xy 104.775 166.37)
      )
    )
  )
)
